**Sierra Leone (country code +232)**

Communication of 16.III.2018:

The *National Telecommunications Commission (NATCOM),* Freetown, announces the following update to the national numbering plan of Sierra Leone:

**Presentation of national ITU-T E.164 numbering plan
for country code 232**

a) Overview:

 The minimum number length (excluding the country code) is 8 digits.

 The maximum number length (excluding the country code) is 8 digits.

b) Link to the national database (or any applicable list) with assigned ITU-T E.164 numbers within the national numbering plan (if any): n/a

c) Link to the real-time database reflecting ported ITU-T E.164 numbers (if any): n/a

**Description of introduction of new resources for
national E.164 numbering plan for country code 232:**

| **NDC (national destination code) or leading digits of N(S)N (national (significant) number)** | **N(S)N number length** | **Usage of E.164 number** | **Time and date of introduction** | **Additional information** |
| --- | --- | --- | --- | --- |
| **Maximum length** | **Minimum length** |
| 31(NDC) | 8 | 8 | Non geographic number for QCELL Sierra Leone | 12:40PM, 16-03-2018 | New mobile Company that will be operational soonest in Sierra LeoneInternational dialling format:+232 31 XXX XXX |
| 34(NDC) | 8 | 8 | Non geographic number for QCELL Sierra Leone | 12:40PM, 16-03-2018 | New mobile Company that will be operational soonest in Sierra LeoneInternational dialling format:+232 34 XXX XXX |

Contact:

 Mr Abdul Bah
National Telecommunications Commission (NATCOM)
13 Regent Road
Hill Station, FREETOWN
Sierra Leone
Tel: +232 88 600 003 or +232 78 333 444
E-mail: abah@natcom.gov.sl
URL: [www.natcom.gov.sl](http://www.natcom.gov.sl)

Communication of 22.I.2018:

The *National Telecommunications Commission (NATCOM),* Freetown, announces the following update to the national numbering plan of Sierra Leone:

**Presentation of national ITU-T E.164 numbering plan
for country code 232**

a) Overview:

 The minimum number length (excluding the country code) is 8 digits.

 The maximum number length (excluding the country code) is 8 digits.

b) Link to the national database (or any applicable list) with assigned ITU-T E.164 numbers within the national numbering plan (if any): n/a

c) Link to the real-time database reflecting ported ITU-T E.164 numbers (if any): n/a

d) Description of introduction of new resource for national E.164 numbering plan for country code 232:

| **NDC (national destination code) or leading digits of N(S)N (national (significant) number)** | **N(S)N number length** | **Usage of E.164 number** | **Additional information** |
| --- | --- | --- | --- |
| **Maximum length** | **Minimum length** |
| 75(NDC) | 8 | 8 | Non-geographic number for Orange SL | 10-11-2017-13:00 |

International dialling format: +232 75X XXXXX

Contact:

Mr Abdul Bah

National Telecommunications Commission

3 Regent Road

Hill Station, FREETOWN

Sierra Leone

Tel: +232 88 600 003 or +232 78 333 444

E-mail: abah@natcom.gov.sl

URL: www.natcom.gov.sl

Communication of 28.IV.2015:

The *National Telecommunications Commission (NATCOM),* Freetown, announces the following update of the national numbering plan of Sierra Leone:

Table − Description of introduction of new resource for
national E.164 numbering plan for country code 232:

| *(1)* | *(2)* | *(3)* | *(4)* |
| --- | --- | --- | --- |
| *NDC (national destination code) or leading digits of N(S)N (national (significant) number)* | *N(S)N number length* | *Usage of E.164 number* | *Time and date of introduction* |
| *Maximum length* | *Minimum length* |
| 55 (NDC) | 8 | 8 | Non-geographic number for AFCOM (SL) | 15-04-2015-12:00 |
| 35 (NDC) | 8 | 8 | Non-geographic number for IPTEL (SL) | 15-04-2015-12:00 |
| 66 (NDC) | 8 | 8 | Non-geographic number for Onlime (SL) | 15-04-2015-12:00 |

International dialling format: +232 55X XXXXX
 +232 35X XXXXX
 +232 66X XXXXX

Contact:

 NATIONAL TELECOMMUNICATIONS COMMISSION
Mr Victor Findlay
13 Regent Road
Hill Station
FREETOWN
Sierra Leone
Tel: +23278366386
E-mail: vfindlay@natcom.gov.sl
URL: www.natcom.gov.sl

Communication of 11.VI.2012 :

The *National Telecommunications Commission (NATCOM),* Freetown, announces the following update of the national numbering plan of Sierra Leone:

|  |  |
| --- | --- |
| E.164 Country code | 232 |
| International prefix | 00 |
| National (long distance) prefix | 0 |
| Length of area code | Two digits |
| Length of subscriber number | Six digits· Fixed/geographic: two digit exchange code + four digit subscriber number in the form NN XXXX· Mobile/non-geographic: six digits, in the form YXXXXX |
| Short codes | Three to four digits |

Geographical numbering (fixed operators)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Locality* | *Operator* | *Area code* | *Exchange code* | *Subscriber number* |
| Freetown | Sierratel | 22 | 2N – 4N | XXX |
| Bo & Kenema | Sierratel | 32 | 2N – 4N | XXX |
| Makeni& Koidu | Sierratel | 52 | 2N – 4N | XXX |

Mobile and non- geographic numbers

| *Network* | *Area code(Network Destination Code (NDC))* | *Subscriber number* |
| --- | --- | --- |
| Airtel (SL) Ltd | 76 | XXXXXX |
| Airtel (SL) Ltd | 78 | XXXXXX |
| Airtel (SL) Ltd | 79 | XXXXXX |
| Africell (SL) Ltd | 30 | XXXXXX |
| Comium (SL) Ltd. | 33 | XXXXXX |
| Comium (SL) Ltd. | 34 | XXXXXX |
| Africell (SL) Ltd. | 77 | XXXXXX |
| Africell (SL) Ltd | 88 | XXXXXX |
| Datatel/Cellcom (GSM) | 40 | XXXXXX |
| Datatel/Cellcom (CDMA) | 50 | XXXXXX |
| Ambitel | 55 | XXXXXX |
| Sierratel (CDMA) | 25 | XXXXXX |
| Sierratel  | 21 | XXXXXX |
| Intergroup | 44 | XXXXXX |

X = 0 – 9 ; N= 2 – 9

Contact;

 National Telecommunications Commission (NATCOM)
13 Regent Road
Hill Station
FREETOWN
Sierra Leone
Tel: +232 22 235121
Fax: +232 22 235179
E-mail: sensokay60@yahoo.com
URL: www.natcomsl.com