|  |  |  |  |
| --- | --- | --- | --- |
| MWI - Malawi | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| The Chief Executive  Malawi Telecommunications Limited | Glyn Jones Road P.O. Box 537 Blantyre | TF : +265 620977 FAX : +265 624445 EMAIL : mtlceo@malawi.net | Contact Officer in the Centralizing Office: The Deputy Director (NS)  P.O. Box 80050 Maelema Blantyre 8 Malawi Telephone:+265 620000 |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Kanjedza (IMS)** | The Controller (SS) P.O. Box 537 Blantyre Malawi | TF : +265 677531 FAX : +265 674861 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 15°49'00''S 035°02'00''E | Frequency measurements | 300 MHz - 500 MHz | H24 |  |
| 15°49'00''S 035°02'00''E | Frequency measurements | 500 MHz - 18 GHz | H24 |  |
| 15°49'00''S 035°02'00''E | Field strength or power flux-density measurements | 9 kHz - 500 MHz | H24 |  |
| 15°49'00''S 035°02'00''E | Direction-finding measurements | 9 kHz - 500 MHz | H24 | 3 MHz to 30 MHz: three log-periodic antennas on one central mast.  10 MHz to 500 MHz: one vertical and one horizontal, remotely controlled, 360° rotatable log-periodic antennas.  10 kHz to 30 MHz: portable ferrite antennas with receiver KE 393 and direction-finder accessory NR 392. |
| 15°49'00''S 035°02'00''E | Bandwidth measurements | 0 - 1.2 GHz | H24 |  |
| 15°49'00''S 035°02'00''E | Automatic spectrum occupancy surveys | 9 kHz - 1000 MHz | H24 |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_