Access Network Transport

Standards Overview

October 2018 Q1/15 Meeting

Contact persons for the project updating:

|  |  |  |
| --- | --- | --- |
| Study Group 15 Advisor:  Mr. Hiroshi Ota  International Telecommunication  Union (ITU)  Place des Nations  1211 Geneva 20  Switzerland  Tel.: +41 22 730 6356  E-mail: [hiroshi.ota@itu.int](mailto:hiroshi.ota@itu.int) | Study Group 15 Chairman  Dr. Stephen J. Trowbridge  Nokia  5280 Centennial Trail  Boulder, Colorado 80303-1262  USA  Tel: +1 303 809 7423  E-mail: [steve.trowbridge@nokia.com](mailto:steve.trowbridge@nokia.com) | Question 1/15 Rapporteur  Mr. Jean-Marie Fromenteau  Corning Incorporated  Corning, NY 14831  USA  Tel: +49 9561 42 74 20  E-mail:  [fromentejm@corning.com](mailto:fromentejm@corning.com) |

Access Network Transport is an ITU-T Project dealing with studies and Recommendations on the Access Network.

Access Network Transport Standards Overview

Issue 31, October 2018

|  |
| --- |
| Revision Status Report: Major Updates of Version 31, Oct. 2018 |
| 1. Sections 7, 8 and 9 have been entirely reviewed and Annex 1 has been updated with   examples of deployment scenarios and references models of the major Access Network Transport technologies deployed today.   1. Annex 2.1, Standards related to ANT Technologies    * Historical standards and standards not directly related to broadband ANT Technologies have been deleted.    * BBF, ETSI and ISO/IEC standards have been reviewed and updated.    * IEEE 802.3 has been updated and IEEE 802.16 has been added.    * ITU-R BT.2400, F.1401 and F.1500 have been added.    * ITU-T G Suppl. 39, G.984.5 Amd1, G Suppl. 48 (HSP), G Suppl. 50 (TCadapt), G.993.2 Amd3 and Amd4, G.993.5 Cor2, G.994.1 Amd2, G.998.2 Cor1, G.9701 Cor5 and Amd5 have been added.    * ITU-T Y.2000 to 2012 series have been added. 2. Annex 2.2, Standards related to broadband ANT Infrastructure Elements (incl. maintenance and operation)     * Historical standards and standards not directly related to ANT Infrastructure Elements have been deleted.    * BBF and ETSI standards have been reviewed and updated.    * G Suppl. 59, G.650.1, G Suppl. 39, G Suppl. 44, G. Suppl. 46, G.996.2 Cor1 and Amd6, G.997.1 Cor1 and Amd2 G.997.2 Cor4 and Amd5 and G. Suppl. 62 have been added.    * ITU-T L.108, L.156, L 207, L315, L. 430 to 434 series and L Suppl. 35 have been added. |

Access Network Transport Standards Overview

Issue 31, October 2018

Introduction 5

1. Scope 5

2. References 6

3. Definitions 6

4. Abbreviations 7

5. Access Network Transport Reference Model 7

6. Access Network Transport functionality 7

7. Access Network Transport Interfaces 9

8. Access Network Transport Technologies 11

9. Overview of existing ANT standards 13

Annex 1 - Examples of deployment scenarios and references models of Access Network  
 Transport technologies 15

A1.1 Metallic Conductor Broadband Access 15

A1.1.1 Access Digital Subscriber Lines (DSL) technology 15

A1.1.2 Reference configuration for a generic xDSL system 15

A1.1.3 Example of VDSL system reference model 16

A1.1.4 Example of G.fast application reference model 17

A1.2 Fibre Optic Broadband Access 18

A1.2.1 Optical access network architecture 18

A1.2.2 Example of Access Network solutions using PON technology 20

A1.2.3 Reference configuration: example of XG-PON (as in ITU-T G.987.x series) 20

A1.2.4 Reference configuration: example of NG-PON2 (as in the ITU-T G.989.x series) 21

A1.3 Hybrid Fibre Coax (HFC) Broadband Access 23

A1.3.1 The DOCSIS network  23

A1.3.2 High performance network over coax (HiNoC) 25

A1.4 Fixed Wireless Access 26

A1.4.1 Broadband Wireless Access (BWA) in the fixed service 26

A1.5 Power Line Communications 29

Annex 2 - ANT-Relevant Standards 30

Annex 2.1 - Standards related to ANT Technologies 30

Annex 2.2 - Standards related to ANT Infrastructure Elements 68

Annex 3 - Rearrangement of the list of standards Annex 2 90

Annex 4 - List of Abbreviations 91

**ACCESS NETWORK TRANSPORT STANDARDS OVERVIEW**

Issue 31, OCTOBER 2018

# Introduction

In today's global communications world the traditional boundaries in network access between Telecommunication Network Operators, Private Network Providers, Satellite and Cable TV Networks and Information Technologies cease to exist.

Within the ITU-T, the study and development of Recommendations related to transport in the access network is being carried out in a number of different Study Groups, e.g. SG 9, 13, 15. Moreover, ITU-R and other standards bodies, forums and consortia are also active in this area.

Recognizing that without a strong coordination effort there is the danger of duplication of work as well as the development of incompatible and non-interoperable standards, the WTSC 96 designated Study Group 15 as **Lead Study Group** on **Access Network Transport (ANT) - reaffirmed at the WTSA-16 -** with the mandate to

1. study the appropriate core Questions (Question 1, 2 and 4/15)
2. define and maintain an overall (standards) framework, in collaboration with other SGs and standards bodies
3. coordinate, assign and prioritize the studies done by the Study Groups (recognizing their mandates) to ensure the development of consistent, complete and timely Recommendations.

Study Group 15 entrusted WP 1/15 (Network Access), under Question 1/15, with the task to manage and carry out the Lead Study Group activities on Access Network Transport.

# 1. Scope

This document defines an ANT on the background of the Recs. G.902 and GII Y.100 series and provides an overview of the existing ANT related standards released and/or prepared by the ITU and other standardization bodies.

The main purpose ofthe **ANT Standards Overview** is to identify

- Which standards exist

- Lack of standards

- Duplication and/or overlap

- Market needs

- Priorities.

Topics/standards under study/development are identified in the **ANT Standards Work Plan.**

The presentation of the standards overview consists of two matrixes identifying key elements of the access network transport technologies and a listing of the various standards organizations and their standards identified, including their titles and publication dates.

# 2. References

G.902 (ITU-T)

[ETSI EG 202 306](http://webapp.etsi.org/WorkProgram/Report_WorkItem.asp?WKI_ID=6237&curItemNr=2&totalNrItems=2&optDisplay=10&titleType=all&qSORT=HIGHVERSION&qETSI_ALL=&SearchPage=TRUE&qINCLUDE_SUB_TB=True&qINCLUDE_MOVED_ON=&qSTOP_FLG=N&qKEYWORD_BOOLEAN=OR&qCLUSTER_BOOLEAN=OR&qFREQUENCIES_BOOLEAN=OR&qTITLE=Access+networks+for+residential+customers&qSTOPPING_OUTDATED=&butExpertSearch=Search&includeNonActiveTB=FALSE&includeSubProjectCode=FALSE&qREPORT_TYPE=SUMMARY)

GII. Y.100 Recs. series (ITU-T)

ANT Standards Work Plan (Issue 29)

# 3. Definitions

The basic documents for the following definitions are G.902 (ITU-T) and ETSI EG 202 306.

**Access Network Transport (ANT):**

Based on definitions specified in G.902 the Access Network (AN) provides transport bearer capabilities for the provision of telecommunications services inside of the AN between a service node interface (SNI) providing customer access to a service node and each of the associated interfaces towards the Customer Premises Network(s) which are being grouped as XNI interfaces (this would include ISDN UNIs). An AN implementation comprises transmission media and access network element (NE) entities.

The XNI interface, following the intent of GII Recs. Y.100 series, is defined as “the interface between the user domain and the network domain at which the access network transport functions apply”.

Following the intent of GII Recs. Y.100 series, the Distribution Interface (DI) is defined as the interface inside the access network domain at which the access network transport functions apply.




Figure 1 - Access Network Transport functional model

An access network element can be configured and managed through a Qx interface that may be implemented at the q reference point. This q reference point is the access point for management information, configuration control, performance monitoring and maintenance as defined in ITU-T Rec. M.3010.

In principle there are no restrictions on the types and number of SNIs and XNIs that an Access Network may implement. The Access Network does not interpret (user) signaling and does not include Customer Premises Networks and/or terminal equipment respectively.

Note: The boxes in Figure 1 represent functions at the interfaces and do not necessarily imply actual equipment at the interface.

# 4. Abbreviations

The list of ANT related abbreviations is included into the Annex 4.

# 5. Access Network Transport Reference Model

Logical and physical representations of the Access Network Transport Reference Model (ANT RM) are presented in Figure 2. This Reference Models are based on the generic GII AN Reference Model and the basic model presented in G.902 (ITU-T) and ETSI EG 202 306 (ETSI - revised ETR 306). The logical representation shows the mutual relations of different ANs and relation to the other parts of the network and/or CPN respectively. The wide varieties of interfaces, architectures, applications, etc. for the ANT can be best understood through scenarios that could be found in Annex 1. The physical representation of the ANT RM includes those entities which provide the required transport bearer capabilities between a Service Node Interface (SNI) and each of the associated Customer Network Interfaces (XNIs). An Access Network may be configured and managed via a Q interface. Access network internal Distribution Interface DI represents the internal interfaces within the AN between the access NEs and in special cases could be presented as interface between two ANs.

# 6. Access Network Transport functionality

The ANT functions are dedicated from the G.902 where AN functions are divided into 5 groups:

1. User port functions
2. Service port functions
3. Core functions
4. Transport functions
5. AN-system management functions

With respect to this classification the following functions to the access network entities represented in the Access Network Transport Reference Model (ANT RM) are applied:

Service Port – service port, core and transport functions

User Port – user port, core and transport functions

Access Distribution Function – core and transport functions



Note: Logical reference point “L” is physically represented as access network Distribution Interface DI.

**a: Logical representation**



Note: The NT term is used for generic Network Termination for various services. For some services/configurations, the NT might be property of the customer and therefore integrated in the CPN; nevertheless it terminates the Access Network from a functional/physical point of view.

**b: Physical representation**

Figure 2 - Access Network Transport Reference Model

# Access Network Transport Interfaces

An Access Network as specified in G.902 is bounded by the customer premises network interfaces (XNIs) on the customer side, the service node interfaces (SNIs) at the core network side and a placement of the management Q interface. In addition to these interfaces, and with respect to the ANT functional model and ANT RM, there is an access network Distribution Interface DI specified representing the internal interfaces within the AN between the access NEs.

These interfaces could be deeper determined via following designation:

1. SNISn : between **S**ervice Function and Access Network (n- seq. number)
2. SNICn : between **C**ore Network and Access Network ( n- seq. number)
3. XNIXYn : between Access Network and CPN (x: type of access technology / y: medium)
4. Ln: between Access Networks (special case of DI)
5. Qn: between Access Network and Management Agent/Network
6. DIn: between Access Network and Network Elements (refer to Scenario 4 as an example)

The following basic physical interfaces are identified (others may be added):

##### SNI Interfaces

***Narrowband (up to 2MBit/s including)***

1. 2Mbit/s (according to ITU-T G.703)
2. Ethernet (IEEE 802.3) 2BASE-TL
3. ISDN PRA V2M (according to ETS 300 012)
4. ISDN BA
5. 64kbit/s and n x 64kbit/s (according to ITU-T G.703/V.24/X.21/V.35 and V.36)
6. POTS (a, b) with U2 signalization (Z interface according to ITU-T Q.512)
7. 2W ALL (according to ITU-T Q.552)
8. 4W ALL (according to ITU-T Q.553)
9. Narrowband Power Line Communications

***Broadband (above 2Mbit/s)***

1. Ethernet (IEEE 802.3) 2BASE-TL, 10PASS-TS
2. ATMF 25.6 (according to ATMF af-phy-0040.000)
3. 34 Mbit/s (according to ITU-T G.703)
4. Ethernet (IEEE 802.3) 100BASE-LX10, 100BASE- BX10
5. Ethernet (IEEE 802.3) 1000BASE-LX10, 1000BASE-BX10
6. 140 Mbit/s (according to ITU-T G.703)
7. STM-0 (ITU-T I.432.4)
8. STM-1 155 Mbit/s (according to ITU-T G.703 and/or G.957)
9. STM-4 622 Mbit/s (according to ITU-T G.957)
10. STM-16 2.5 Gbit/s (according to ITU-T G.957)
11. Broadband Power Line Communications
12. Ethernet (IEEE 802.3) 1000BASE-PX (1G-EPON)
13. Ethernet (IEEE 802.3)10GBASE-PR, 10/1GBASE-PRX (10G-EPON)
14. Passive Optical Network (“B-PON” according to ITU-T G.983 series and “G-PON” according to ITU-T G.984 series, “10G-PON” (XG-PON) according to ITU-T G.987 series and (XGS-PON) according to ITU-T G.9807 series, “40G-PON” (NG-PON2) according to ITU-T G.989 series,)
15. HDSL and SHDSL according to ITU-T G.991 series, ADSL and ADSL2 according to ITU-T G.992 series, VDSL and VDSL2 according to ITU-T G.993 series
16. G.fast according to ITU-T G.9700 and G.9701
17. HiNoC1.0 (100Mbits/s/channel over coaxial network according to J.195.1, J.195.2 and J.195.3)
18. HiNoC2.0 (1000Mbits/s/channel over coaxial network)
19. DOCSIS 1.0, DOCSIS 1.1, DOCSIS 2.0, DOCSIS 3.0, DOCSIS 3.1 and DOCSIS 3.1 Full Duplex

##### XNI Interfaces

***Narrowband (up to 2MBit/s including)***

1. 2Mbit/s (according to ITU-T G.703)
2. Ethernet (IEEE 802.3) 2BASE-TL
3. ISDN PA U2M / S2M (according to ETS 300 012)
4. ISDN BA Uk0 /S0 (according to ETS 300 012)
5. 64kbit/s and n x 64kbit/s (according to ITU-T G.703/V.24/X.21/V.35 and V.36)
6. POTS (a, b) with U2 signalization (Z interface according to ITU-T Q.512)
7. 2W ALL (according to ITU-T Q.552)
8. 4W ALL (according to ITU-T Q.553)
9. Narrowband Power Line Communications
10. IMT-2000 (Rec. ITU-R M.1457)
11. IMT-Advanced (Rec. ITU-R M.2012)

***Broadband (above 2Mbit/s)***

1. Ethernet (IEEE 802.3) 2BASE-TL, 10PASS-TS
2. ATMF 25.6 (according to ATMF af-phy-0040.000)
3. 34 Mbit/s (according to ITU-T G.703)
4. Ethernet (IEEE 802.3) 100BASE-LX10, 100BASE-BX10
5. Ethernet (IEEE 802.3) 1000BASE-LX10, 1000BASE-BX10
6. 140 Mbit/s (according to ITU-T G.703)
7. STM-0 (ITU-T I.432.4)
8. STM-1 155 Mbit/s (according to ITU-T G.703 and/or G.957)
9. STM-4 622 Mbit/s (according to ITU-T G.957)
10. STM-16 2.5 Gbit/s (according to ITU-T G.957)
11. Broadband Power Line Communications
12. IMT-2000 (Rec. ITU-R M.1457)
13. IMT-Advanced (Rec. ITU-R M.2012)
14. IMT-2000 and IMT-Advanced enhancements (Recs. ITU-R M.1457 and M.2012)
15. Ethernet (IEEE 802.3) 1000BASE-PX (1G-EPON)
16. Ethernet (IEEE 802.3) 10GBASE-PR, 10/1GBASE-PRX (10G-EPON)
17. Passive Optical Network (“BPON” according to ITU-T G.983 series and “GPON” according to ITU-T G.984 series, “10G-PON” (XG-PON) according to ITU-T G.987 series and (XGS-PON) according to ITU-T G.9807 series,“40G-PON” (NG-PON2) according to ITU-T G.989 series,)
18. HDSL and SHDSL according to ITU-T G.991 series, ADSL and ADSL2 according to ITU-T G.992 series, VDSL and VDSL2 according to ITU-T G.993 series
19. G.fast according to ITU-T G.9700 and G.9701
20. RLANs (Recommendation ITU-R M.1450)
21. Multiple Gigabit Wireless Systems (Recommendation ITU-R M.2003)
22. Broadband wireless access systems (Recommendation ITU-R M.1801)
23. HiNoC1.0 (100Mbits/s/channel over coaxial network according to J.195.1, J.195.2 and J.195.3)
24. HiNoC2.0 (1000Mbits/s/channel over coaxial network)
25. DOCSIS 1.0, DOCSIS 1.1, DOCSIS 2.0, DOCSIS 3.0, DOCSIS 3.1 and DOCSIS 3.1 Full Duplex

Management interfaces

1. F interface ( for interconnection between ANT NE and local terminal and/ or for interconnection of management system to the remote terminal )
2. Q interface (for connection of ANT NE and the management system)

# 8. Access Network Transport Technologies

Today’s Access Network Transport technologies enable the telecom and internet service providers to offer multi-services and applications (e.g. voice telephony, data, video, etc.) - including both legacy and emerging services - to a wide range of markets and customers, e.g. residential subscribers in SFUs (single family units) and MDUs (multi-dwelling units), businesses, public organizations like schools, hospitals, etc.. They may also be connected to other network infrastructures like for example base stations of mobile networks, security and monitoring networks and they may support wholesale and retail.  
   
Today’s Access Network Transport types can be classified as below according to the transmission medium of the physical path and used technology:

1. Metallic Conductor Broadband Access
   1. Integrated services digital network (ISDN)
   2. Digital Subscriber Lines (DSL) Technologies
      * HDSL (High bit rate DSL) and SHDSL (Single-pair high-speed DSL)
      * ADSL (Asymmetric DSL), ADSL2 and ADSL2plus
      * VDSL (Very-high speed DSL), VDSL2 and VDSL2 Vectoring
      * G.fast (fast access to subscriber terminals) /FTTdp
   3. Ethernet over copper (EoC)
2. Fibre Optic Broadband Access
   1. Point-to-Point (PtP) Ethernet
   2. Passive Optical Network (PON)
      * Early PON Protocols: OAN and B-PON
      * Gigabit PON: G-PON and 1G-EPON
      * 10-Gibabit PON: XG-PON, XGS-PON and 10G-EPON
      * 40-Gigabit PON: NG-PON2
      * Higher-Speed PON and Multiple-wavelength PON (MW-PON)
   3. Hybrid Fibre Access Technologies
      * Radio and Radio Frequency over Fibre
      * Wireless – Fibre Access Networks
3. Hybrid Fibre Coax (HFC) Broadband Access
   1. Ethernet Passive Optical Networks Protocol over Coax
   2. DOCSIS (Data-Over-Cables Service Interface Specification) Network
4. Fixed Wireless Access
5. Satellite
6. Power Line Communications (PLC)

Annex 1 depicts examples of deployment scenarios and references models of some major Access Network Transport technologies deployed today.

# 9. Overview of existing ANT standards

In order to classify the existing ANT standards, a matrix of ANT-related standards was developed from known public lists inputs from other ITU Study Groups, other standards development organizations (SDOs), Forums & consortia. The matrix is organized by Standards bodies alphabetically listed and then by standard numbers and titles. The current matrix is reported in Annex 2 and consists of two parts reported in Annex 2.1 and Annex 2.2.

The Annex 2.1 - Standards related to ANT Technologies – lists the ANT relevant standards by transmission medium and technology. Each standard is categorized by marking its type according to a code as below:  
General Aspects (Gen. Asp.) = General requirements, architecture and functions  
Medium: F= Fiber; C= Coax; P= Twisted pair; A= Wireless  
Technology: I= ISDN; D= DSL; G= G.fast; E= PtP; P= PON; H= HFC; W= Fixed Wireless Access and Satellite; L= PLC  
Additionally examples of deployment scenarios and references models of some major Access Network Transport technologies deployed today are shown in Annex 1.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Stds. Body** | **Number** | **Titles** | **Gen. Asp.** | **Medium** | | | | **Technology** | | | | | | | | **Public. Date** |
| F | **C** | **P** | A | I | **D** | **G** | **E** | **P** | **H** | **W** | **L** |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

**Sample format for standards matrix as in Annex 2.1**

The Annex 2.2 - Standards related to ANT Infrastructure Elements – lists the ANT relevant standards by transmission medium and infrastructure elements including operation and maintenance. Each standard is categorized by marking its type according to a code as below:  
General Aspects (Gen. Asp.) = General aspects on network infrastructure, design and management  
Medium: F= Fiber; C= Coax; P= Twisted pair; A= Wireless  
Infrastructure: N= Network engineering and infrastructure elements including node equipment and devices; E= Power supply and energy management; O= Operation and maintenance including network management; T = Testing; C= Conformance and interoperability; F = Optical cable technology;   
P = Copper cable technology; I = Cable installation technique

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Stds. Body** | **Number** | **Titles** | **Gen. Asp.** | **Medium** | | | | **Infrastructure** | | | | | | | | **Public. Date** |
| F | **C** | **P** | A | N | **E** | **O** | **T** | **C** | **F** | **P** | **I** |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Sample format for standards matrix as in Annex 2.2

The matrixes are updated through liaison to ITU-T, ITU-R, and standards organizations outside the ITU. It is planned to eventually replace this manual method for presenting the matrixes of standards with a web-based approach where a user could click on a portion of the ANT technologies and immediately obtain a list of relevant standards.

# Annex 1

**Examples of deployment scenarios and references models of   
Access Network Transport technologies**

### 

### A1.1 Metallic Conductor Broadband Access

### A1.1.1 Access Digital Subscriber Lines (DSL) technology Examples of ADSL2plus, VDSL2 and G.fast deployment

### 

### Figure 1.1 - Example of Access Network solutions using ADSL2plus, VDSL2 and G.fast technologies

### VDSL2 supports FTTCab (fiber to the cabinet), FTTC (fiber to the curb) and FTTB (fiber to the building) types of deployment. G.fast supports FTTdp (fiber to the distribution point) and FTTB (fiber to the building) types of deployment.

### 

### A1.1.2 Reference configuration for a generic xDSL system




Figure 1.2 – A reference configuration for a generic ITU-T G.99x system

### Figure 1.2 depicts a reference configuration for a generic xDSL system based on the reference configuration used for N-ISDN in ITU-T I.411. This reference configuration identifies the reference points in the context of access network and consists of seven elements: 1) Core network 2) Access network 3) Network termination 1 (NT1) 4) Network termination 2 (NT2) 5) Terminal adapter (TA) 6) User terminal 7) Access network management

### A1.1.3 Example of VDSL system reference model Figure 1.3 illustrates the ITU-T G.993.1 system VDSL reference model aligned with the reference configuration shown in Figure 1.2.

### 

### Figure 1.3 - ITU-T G.993.1 system VDSL reference model and its alignment with the generic reference configuration

The ITU-T G.993.1 system reference model shows the functional blocks necessary to illustrate a VDSL transmission system. With reference to the alignment with the generic reference configuration, the core network may contain the following functions:

– concentrator and/or switch;

– interface to the broadband and narrow-band network.

The VDSL access network consists of the following:

– VDSL Transceiver Unit-ONU (VTU-O);

– POTS splitter to separate the POTS and VDSL channels;

– copper loop plant.

The VDSL-NT1 may consist of the following functions:

– VDSL Transceiver Unit – Remote Terminal end (VTU-R);

– multiplexer/Demultiplexer;

– higher layer functions;

– interface to the user terminal or a home network.

The VDSL-NT2, the terminal adapter and the user terminal may share some or all of the NT1 functionalities.  
In ITU-T G.993.1, interfaces are defined at the V, U and T reference points namely U-O, U-R, V-O, and T-R interfaces.

A1.1.4 Example of G.fast application reference model  
Implementations complying with Recommendation ITU-T G.9701 for fast access to subscriber terminals (G.fast) are typically deployed in a fibre to the-distribution point (FTTdp) scenario. A FTTdp deployment may be a further evolution of a FTTx (e.g., FTTCab, FTTC and FTTB) deployment, taking the fibre deeper into the network, or it may be a FTTH deployment with a copper extension where installation of the fibre inside the customer premises is not possible. The optical distribution network that feeds the distribution point units (DPUs) may be based on point-to-multipoint (e.g., PON) or point-to-point (e.g., GbE) technologies.




Figure 1.4 – Application reference model for FTTdp with POTS

A key aspect of FTTdp deployment is the requirement that the customer should be able to self-install the equipment. Figure 1.4 provides an overview of the basic application reference model for customer self-install with POTS as the underlying narrowband service. Alternatively, the integrated services digital network (ISDN) may be used as the underlying narrowband service. This application model is very similar to the ITU-T G.993.2 generic application reference model for splitterless remote deployment. The DPU may contain one or multiple instantiations of the FTU-O and service splitter functionalities.

## 

## A1. 2. Fibre Optic Broadband Access

A1.2.1 Optical access network architecture

The optical section of a local access network system can be either active or passive and its architecture can be either point-to-point or point-to-multipoint. Figure 2.1 shows the considered architectures, which can be fibre to the home (FTTH), fibre to the cell site (FTTCell), fibre to the building/curb (FTTB/C), fibre to the cabinet (FTTCab), etc. The optical distribution network (ODN) is common to all the architectures shown in Figure 2.1; hence, the commonality of this system has the potential to generate large worldwide volumes.

## 

Figure 2.1 – Network architecture

NOTE – An ONU supporting FTTH has been commonly referred to as ONT (see [ITU-T G.987]).

The differences among these FTTx options are mainly due to the different services supported and the different locations of the ONUs rather than the ODN itself, so they can be treated as one. It must be noted that a single OLT optical interface might accommodate a combination of several scenarios described hereafter.

1) FTTB scenario

The FTTB scenario is divided into two scenarios, one for multi-dwelling units (MDU) and the other for businesses or mixed environments, multi-tenant units (MTUs). Each scenario has the following service categories:

1.1) FTTB for MDU-served residential users

* Asymmetric broadband services (e.g., IPTV, digital broadcast services, video on demand (VoD), file download, etc.).
* Symmetric broadband services (e.g., content broadcast, e-mail, file exchange, distance learning, telemedicine, online-games, etc.).
* POTS – The access network must be able to provide, in a flexible way, narrow-band telephone services using either emulation (complete replication of a legacy service) or simulation (providing a service that is almost the same as the legacy service).

1.2) FTTB for MTU-served business users

* Symmetric broadband services (e.g., group software, content broadcast, e-mail, file exchange, etc.).
* POTS – The access network must be able to provide, in a flexible way, narrow-band telephone services using either emulation (complete replication of a legacy service) or simulation (providing a service that is almost the same as the legacy service).
* Private line – The access network must be able to provide, in a flexible way, private-line services at several rates.

2) FTTCurb and FTTCab scenario

Within this scenario, the following service categories have been considered:

* Asymmetric broadband services (e.g., IPTV, digital broadcast services, VoD, file download, online-games, etc.).
* Symmetric broadband services (e.g., content broadcast, e-mail, file exchange, distance learning, telemedicine, etc.).
* POTS – The access network must be able to provide, in a flexible way, narrow-band telephone services using either emulation (complete replication of a legacy service) or simulation (providing a service that is almost the same as the legacy service).
* xDSL backhaul.

3) FTTH scenario

Within this scenario, the following service categories have been considered:

* Asymmetric broadband services (e.g., IPTV, digital broadcast services, VoD, file download, etc.).
* Symmetric broadband services (e.g., content broadcast, e-mail, file exchange, distance learning, telemedicine, online-games, etc.).
* POTS – The access network must be able to provide, in a flexible way, narrow-band telephone services using either emulation (complete replication of a legacy service) or simulation (providing a service that is almost the same as the legacy service).

4) FTTO scenario

Fibre to the office (FTTO) addresses business ONU dedicated to a small business customer. Within this scenario, the following service categories have been considered:

* Symmetric broadband services (e.g., group software, content broadcast, e-mail, file exchange, etc.).
* POTS – The access network must be able to provide, in a flexible way, narrow-band telephone services using either emulation (complete replication of a legacy service) or simulation (providing a service that is almost the same as the legacy service).
* Private line – The access network must be able to provide, in a flexible way, private line services at several rates.

5) FTTCell wireless scenario

Within this scenario, the ONU will be called a cell-site backhauling unit (CBU) and will have to offer connectivity to wireless base stations:

* Symmetric TDM services (e.g., 2G cell site backhaul);
* Symmetric/asymmetric packet-based broadband services (e.g., 3G/4G cell-site backhaul);
* Hot spots.

A1.2.2 Example of Access Network solutions using PON technology




Figure 2.2 – A summary of some PON deployment scenarios

Figure 2.2 represents exemplary scenarios of PON applications

A1.2.3 Reference configuration: example of XG-PON (as in the ITU-T G.987.x series)

A high level and simple reference configuration of XG-PON is depicted in Figure A2-3, which shows a very similar high level reference configuration of B-PON as in the ITU-T G.983.x series and G-PON as in the ITU-T G.984.x series of Recommendations.




Figure 2.3 – High-level reference configuration of XG-PON

In addition to Figure 2.3, when XG-PON is deployed with an RF video overlay service, the ODN can use a WDM device or an optical coupler/splitter to combine PON and RF video signals.




Figure 2.4 - Reference access network architecture

Figure 2.4 depicts the generic optical access network (OAN) reference architecture that applies to the XG-PON. It includes an OLT, ONUs and an optical distribution network between them. As shown in Figure 2.4, an XG-PON ODN can consist of a single passive optical distribution segment (ODS), or a group of passive ODSs interconnected with reach extenders (REs) [ITU T G.987].

A1.2.4 Reference configuration: example of NG-PON2 (as in the ITU-T G.989.x series)

1. Multi-wavelength PON system reference points

In a multiple wavelength passive optical network (PON) system, such as next generation passive optical network 2 (NG PON2), the optical line terminal (OLT) is conceptually composed of multiple OLT channel terminations (CTs) connected via a wavelength multiplexer (WM). The associated reference logical architecture and its reference points are presented in Figure 2.5.




Figure 2.5- NG-PON2 reference logical architecture

1. Network reference architecture

Figure 2.6 depicts the functional optical access network architecture and reference points that apply to NG-PON2 systems with legacy systems coexistence. The ODN consists of the splitter and the coexistence element (WDM) and, optionally, reach extenders may also be used in the ODN.




Figure 2.6 - Functional reference architecture and points  
for NG-PON2 system coexistence with legacy systems

## A1.3 Hybrid Fibre Coax (HFC) Broadband Access

## A1.3.1 The DOCSIS network

## The elements that participate in the provisioning of DOCSIS services are shown in Figure 3.1:

## 

## Figure 3.1 – The DOCSIS network

The CM connects to the operator's HFC network and to a home network, bridging packets between them. Many CPE devices can connect to the CMs' LAN interfaces. CPE devices can be embedded with the CM in a single device, or they can be separate standalone devices, as shown in Figure ‎3.1.   
CPE devices may use IPv4, IPv6 or both forms of IP addressing. Examples of typical CPE devices are home routers, set-top devices, personal computers, etc.

The CMTS connects the operator's back office and core network with the HFC network. Its main function is to forward packets between these two domains, and between upstream and downstream channels on the HFC network.

## Service goals

As cable operators have widely deployed high-speed data services on cable television systems, the demand for bandwidth has increased. Additionally, networks have scaled to such a degree that IPv4 address constraints are becoming a burden on network operations. It is thus appropriate to add new features to the DOCSIS Recommendations for the purpose of increasing channel capacity, enhancing network security, expanding addressability of network elements, and deploying new service offerings.

The DOCSIS system allows transparent bidirectional transfer of Internet protocol (IP) traffic, between the cable system head-end and customer locations, over an all-coaxial or hybrid-fibre/coax (HFC) cable network. This is shown in simplified form in Figure 3.2.




Figure 3.2 – Transparent IP traffic through the data-over-cable system

1.2. Reference architecture

The reference architecture for data-over-cable services and interfaces is shown in Figure ‎3.3




Figure 3.3 – Data-over-cable reference architecture

## A1.3.2 High performance network over coax (HiNoC) connected with fibre to the building

Typical scenario for HiNoC operation-deployment

Cable operators around the world are interested in deploying triple-play services over cable television systems while supporting existing analogue or digital TV broadcasting services. Most triple-play services with video content require a very high-speed access network.

In high-density residential or office areas, FTTB and coax solutions have been introduced. A typical network scenario is shown in Figure 3.4. The FTTB + coax network can be realized by the PON system in the distribution network and the HiNoC system in a coaxial network. Services such as analogue or digital TV, VoIP, Internet access and interactive services can be transferred over the network.




Figure 3.4 – FTTB + coax

## A1.4 Fixed Wireless Access

A1.4.1 Broadband Wireless Access (BWA) in the fixed service

1) Application and services

BWA systems operating in the fixed service should support a wide range of applications in use today and be extendable to support future services. The main user applications that can be foreseen today are as follows:

* Internet access (e.g. IP versions 4 and 6)
* LAN bridging and remote LAN access

The protocols could support bridged LAN service and remote LAN access capabilities.

* Videotelephony and videoconferencing
* Computer gaming
* Real-time video and audio
* Telemedicine; tele-education
* Telephony/voice services (e.g. VoIP)
* Voice-band modems and fax

The system could facilitate unicast, multicast, as well as broadcast services.

Fixed BWA systems can also be used to provide backhaul links for local area networks (LAN), metropolitan area networks (MAN), and cellular mobile networks, as well as synchronous digital hierarchy (SDH) rings.

2) Topology structures

There are four kinds of basic topology:

* A conventional point-to-point (P-P) topology where a station communicates directly with another station;
* A conventional point-to-multipoint (P-MP) topology where each subscriber unit (SU) communicates directly with a base station (BS);
* A multipoint-to-multipoint (MP-MP) with mesh network topology where SUs communicate with nearest neighbours and information is passed back through the mesh in a manner analogous to internet traffic;
* A combination of P-P, P-MP and MP-MP topology.

The main difference between the P-MP and MP-MP topology structures is that in the P-MP mode, traffic only occurs between BS and SUs while in the MP-MP topology traffic can occur directly between SUs and also can be routed further through other SUs. It should be noted that a P-P application may be used as an element link of P-MP or MP-MP topology, and that some backhaul links including mobile infrastructure may also use P-P application.

The above four topology structures, P-P, P-MP and MP-MP, or a combination structure of them, should be evaluated when being considered for implementation.

2.1) P-P deployment topology

In P-P systems, traffic is transmitted directly from one station to another. Uses for P-P systems also include backhaul links for LAN, MAN, and cellular mobile networks.




Figure 4.1 - Illustration of network deployment configuration based on P-P configuration

2.2) P-MP deployment topology

In P-MP systems, all data traffic (data, voice or multimedia) should go through the BS that shall serve as a radio resource supervisor.

Figure 4.2 shows an example deployment configuration. The BS can serve individual buildings, multiple subscribers in multiple buildings (using multiple radio links), or multiple subscribers in a single building by use of a single radio link and further in-building distribution systems. It shows the use of an optional repeater and route diversity in order to provide extended coverage and coverage in difficult areas. This does not imply the use of these features in all systems.

BWA base stations are deployed to form either contiguous cells or spot-type coverage.




Figure 4.2 Illustration of network deployment configuration based on P-MP configuration

2.3) MP-MP deployment topology

The system may support MP-MP with mesh network topology.

Figure 4.3 illustrates an example of MP-MP system with mesh network topology. The wireless mesh network consists of wireless nodes, which are either customer sites, relay nodes without originating/terminating traffic, or points of interface (PoI) to other networks such as ISP networks. The entire network shown in Figure 4.3 can be regarded as an MP-MP system. When at least one diversity route is available in the network, the system is specifically referred to as “an MP-MP system with mesh network topology” (see Recommendation ITU-R F.1704).




Figure 4.3 - Illustration of network deployment configuration based on MP-MP configuration

2.4) Combination P-P, P-MP and MP-MP deployment topology

Figure 4.4 illustrates an example of mix topology. In this case, the wireless network may have both P MP and MP-MP links and the BS supporting its SU may be connected to the other networks via backbone network.




Figure 4.4 - Illustration of network deployment based on combination P-P, P-MP

and MP-MP configuration

## A1.5 Power Line Communications (PLC)

The Power Line Communications technology, also called Power Line Telecommunications (or PLT) enables the provision of telecommunications narrowband and broadband services over the power line. The Access Network PLC technology is designed to provide the services to the user’s home through the external electricity grid, while the In-home PLC technology is designed to provide the services within the user’s home.

Figure 5.1 depicts a typical Power Line Communications solution for the Access



# Annex 2 - ANT-Relevant Standards

## Annex 2.1 - Standards related to ANT Technologies

Some of the listed Documents, may not be not publicly available. Interested people may contact the person mentioned under the responsible standardization group in the list of contacts in Section 3.2 of the ANT Standards Work Plan.

| **Organization of ANT Relevant Standards by Transmission Medium and Technology**  **General Aspects (Gen. Asp.) =** General requirements, architecture and functions **Medium:** **F**= Fiber; **C**= Coax; **P**= Twisted pair; **A**= Wireless **Technology: I**= ISDN; **D**= DSL; **G**= G.fast; **E**= PtP; **P**= PON, **H**= HFC, **W**= Fixed Wireless Access and Satellite, **L**= PLC |
| --- |

| **Stds** | **Number** | **Title** | **Gen.**  **Asp.** | | **Medium** | | | | | | | | | **Technology** | | | | | | | | | | | | | | **Public. Date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Body** |  |  |  | | **F** | | | **C** | | **P** | | **A** | | **I** | | **D** | | **G** | | **E** | | **P** | | **H** | | **W** | **L** |  |
| ATIS | 0600107 | Digital Hierarchy – Formats Specifications | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | Edition 2005 |
| ATIS | 0600413 | Network to Customer Installation Interfaces – Asymmetric Digital Subscriber Line (ADSL) Metallic Interface |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | Edition  March 1, 2009 |
| ATIS | 0600418 | HIGH BIT RATE DIGITAL SUBSCRIBER LINE - 2ND GENERATION (HDSL2/HDSL4) ISSUE 2 (S2015) \*\*\* (SUPPLEMENT A S2015) \*\*\* |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | Edition  June 1, 2004 |
| ATIS | 0600422 | Single-Pair High-Speed Digital Subscriber Line (SHDSL) Transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | Edition October 1, 2001 |
| ATIS | 0600424 | Interface Between Networks and Customer Installation Very-high-bit-rate Digital Subscriber Lines (VDSL) Metallic Interface (DMT based) |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | Edition  June 1, 2004 |
| ATIS | 0600427.01 | ATM-Based Multi-Pair Bonding |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | Edition November 1, 2004 |
| ATIS | 0600427.02 | Ethernet-based Multi-Pair Bonding |  | | |  | |  | | X | |  | |  | | X | |  | |  | | |  | |  |  |  | Edition  January 1, 2005 |
| ATIS | 0600427.03 | Multi-Pair Bonding Using Time-Division Inverse Multiplexing |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | Edition September 1, 2004 |
| ATIS | 0600601 | Integrated Services Digital Network (ISDN)- Basic Access Interface for Use on Metallic Loops for Application on the Network Side of the NT (Layer 1 Specification). |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition  June 1, 1999 |
| ATIS | 0600605 | Integrated Services Digital Network (ISDN) – Basic Access Interface for S and T Reference Points (Layer 1 Specification) |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition  July 1, 1991 |
| ATIS | 1000627 | Broadband ISDN – ATM Layer Functionality and Specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition  June 1, 2014 |
| ATIS | 1000640 | Broadband ISDN Network Node Interfaces and Inter-Network Interfaces - Rates and Formats Specifications |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition  August 1, 2001 |
| ATIS | T1.TR.28 | HIGH-BIT-RATE DIGITAL SUBSCRIBER LINE (HDSL) | X | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | February 1,  1994 |
| BBF | TR-xxx | Published BBF Technical Reports can be found at:  <https://www.broadband-forum.org/standards-and-software/technical-specifications/technical-reports> | X | | | X | | X | | X | | X | | X | | X | | X | | X | | X | | X | | X | X |  |
| EIA/TIA | EIA/TIA-547 | Network channel Terminal Equipment for DS1 Service |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | March-89 |
| ETSI | EG 202 306 | Transmission and Multiplexing (TM); Access networks for residential customers | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | V 1.2.1  (1998-05) |
| ETSI | TR 101 689-2 | Transmission and Multiplexing (TM); Terms and definitions in transport networks; Part 2: Access networks | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | V1.1.1 (2000-06) |
| ETSI | TS 101 135 | Transmission and Multiplexing (TM); High bit-rate Digital Subscriber Line (HDSL) transmission system on metallic local lines; HDSL core specification and applications for combined ISDN-BA and2 048 kbit/s transmission |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | V1.5.3 (2000-09) |
| SI | EN 301 217-1 | V interfaces at the digital Service Node (SN); Interfaces at VB5.2 reference point for the support of broadband or combined narrowband and broadband Access Networks (ANs); Part 1: Interface specification". |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V1.2.2 (1999-09) |
| ETSI | EN 301 141-1 | Integrated Services Digital Network (ISDN);  Narrowband Multi-service Delivery System (NMDS);  Part 1: NMDS interface specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V1.2.2  (1998-09) |
| ETSI | TR 101 177 | Broadband Radio Access Networks (BRAN); Requirements and architectures for broadband and fixed radio access networks (HIPERACCESS) | X | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.1.1  (1998-05) |
| ETSI | TR 101 173 | Broadband Radio Access Networks (BRAN); Inventory of broadband radio technologies and techniques | X | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.1.1  (1998-05) |
| ETSI  TM | TS 101 272 | Transmission and Multiplexing (TM);  Optical Access Networks (OANs) for evolving services; ATM Passive Optical Networks (PONs) and the transport of ATM over digital subscriber lines |  | | | X | |  | | X | |  | |  | | X | |  | |  | | X | |  | |  |  | V1.1.1  (1998-06) |
| ETSI  ATTM  TM4 | EN 302 217-3 | Fixed Radio Systems; Characteristics and requirements for point-to-point equipment and antennas; Part 3: Equipment operating in frequency bands where both frequency coordinated or uncoordinated deployment might be applied; Harmonized EN covering the essential requirements of article 3.2 of R&TTE Directive |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V2.2.1 (2014-04) |
| ETSI  ATTM  TM4 | EN 302 217-2-2 | Fixed Radio Systems; Characteristics and requirements for point-to-point equipment and antennas; Part 2-2: Digital systems operating in frequency bands where frequency co-ordination is applied; Harmonized EN covering the essential requirements of article 3.2 of the R&TTE Directive |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V2.2.1 (2014-04) |
| ETSI | EN 301 005-1 | V interfaces at the digital Service Node (SN); Interfaces at the VB5.1 reference point for the support of broadband or combined narrowband and broadband Access Networks (ANs); Part 1: Interface specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V1.1.4  (1998-05) |
| ETSI  ATTM  TM4 | EN 302 326-2 | Fixed Radio Systems; Multipoint Equipment and Antennas; Part 2: Harmonized EN covering the essential requirements of article 3.2 of the R&TTE Directive for Digital Multipoint Radio Equipment |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.2.2  (2007-06) |
| ETSI  ATTM  TM6 | ETR 080 | Transmission and Multiplexing (TM); ISDN basic rate access; Digital transmission system on metallic local lines |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition 2  (1996-11) |
| ETSI | ETR 085 | Transmission and Multiplexing (TM); Generic functional architecture of transport network | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | Edition 1  (1993-06) |
| ETSI | ETR 139 | Radio Equipment and Systems (RES); Radio in the Local Loop | X | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | Edition 1  (1994-11) |
| ETSI | ETR 248 | Transmission and Multiplexing (TM); Use of single mode fibre in the access network | | X | | | X | |  | |  | |  | |  | |  | |  | |  | |  | |  |  |  | Edition 1  (1996-01) |
| ETSI | ETR 326 | Transmission and Multiplexing (TM); Broadband Integrated Services Digital Network (B-ISDN) access | X | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition 1  (1996-11) |
| ETSI | EN 300 011-1 | Integrated Services Digital Network (ISDN); primary rate user-network interface; Part 1: Layer 1 specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V1.2.2 (2000-05) |
| ETSI | EN 300 012-1 | Integrated Services Digital Network (ISDN); basic rate user-network interface; Part 1:Layer 1 specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V1.2.2  (2000-05) |
| ETSI  TM3 | ETS 300 233 | Integrated Services Digital Network (ISDN); Access digital section for ISDN primary rate |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition 1  (1994-05) |
| ETSI  TM3 | ETS 300 297 | Access digital section for ISDN basic access |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition 1  (1995-05) |
| ETSI  TM3 | EN 300 299 | Broadband Integrated Services Digital Network (B-ISDN); Cell based user network access; Physical layer interfaces for B-ISDN applications |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V1.3.2 (2000-05) |
| ETSI  TM3 | ETS 300 300 | Broadband Integrated Services Digital Network (B-ISDN); Synchronous Digital Hierarchy (SDH) based user network interface; Physical layer interfaces for B-ISDN applications |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition 2  (1997-04) |
| ETSI  TISPAN | EN 300 324‑1 | V interfaces at the digital Local Exchange (LE); V5.1 interface for the support of Access Network (AN); Part 1: V5.1 interface specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V2.1.1 (2000-04) |
| ETSI  TISPAN | EN 300 347‑1 | V interfaces at the digital Local Exchange (LE); V5.2 interface for the support of Access Network (AN); Part 1: V5.2 interface specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | V2.2.2  (1999-12) |
| ETSI  TM3 | EN 300 463 | Transmission and Multiplexing (TM);Requirements of passive Optical Access Networks (OANs) to provide services up to 2 Mbit/s bearer capacity |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | V1.1.2 (2000-06) |
| ETSI  TM1 | ETS 300 681 | Transmission and Multiplexing (TM); Optical Distribution Network (ODN) for Optical Access Network (OAN) |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | Edition 1  (1997-06) |
| ETSI | EN 300 686 | Access and Terminals (AT); 34 Mbit/s and 140 Mbit/s digital leased lines (D34U, D34S, D140U, D140S); Network interface presentation |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | V1.2.1  (2001-07) |
| ETSI | EN 300 687 | Access and Terminals (AT); 34 Mbit/s digital leased lines (D34U and D34S); Connection characteristics |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | V1.2.1  (2001-07) |
| ETSI | EN 300 688 | Access and Terminals (AT); 140 Mbit/s digital leased lines (D140U and D140S); Connection characteristics. |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | V1.2.1  (2001-07) |
| ETSI  TM3 | ETS 300 742 | Transmission and Multiplexing (TM); Physical layer User Network Interface (UNI) for 2 048 kbit/s Asynchronous Transfer Mode (ATM) signals |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | Edition 1 (1997-04) |
| ETSI  TM3 | EN 300 766 | Access and Terminals (AT); Multiple 64 kbit/s digital unrestricted leased lines with octet integrity presented at a structured 2 048 kbit/s interface at either or both ends (D64M); Connection characteristics and network interface presentation |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | V1.2.1  (2001-07) |
| ETSI  TM | ETS 300 681 | Transmission and Multiplexing (TM); Optical Distribution Network (ODN) for OAN |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | Edition 1  (1997-06) |
| ETSI | ETS 300 354 | Broadband Integrated Services Digital Network (B-ISDN);B-ISDN Protocol Reference Model (PRM) |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition 1  (1995-08) |
| ETSI  TM3 | ETS 300 811 | Broadband Integrated Services Digital Network (B-ISDN); Transmission Convergence (TC) and Physical Media Dependent(PMD) sublayers for the SB reference point at a bit-rate of 25,6 Mbit/s over twisted pair cable |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | Edition 1  (1998-02) |
| ETSI | TBR 024 | Business Telecommunications; 34 Mbit/s digital unstructured and structured leased lines (D34U and D34S); Attachment requirements for terminal equipment interface. |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | Edition 1  (1997-07) |
| ETSI | TBR 025 | Business Telecommunications; 140 Mbit/s digital unstructured and structured leased lines (D140U and D140S); Attachment requirements for terminal equipment interface |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | Edition 1  (1997-07) |
| ETSI | TBR 012 | Business TeleCommunications (BTC); Open Network Provision (ONP) technical requirements; 2 048 kbit/s digital unstructured leased line (D2048U); Attachment requirements for terminal equipment interface |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | Edition 1  (1996-01) |
| ETSI | TBR 013 | Business TeleCommunications (BTC); 2 048 kbit/s digital structured leased lines (D2048S); Attachment requirements for terminal equipment interface |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | Edition 1  (1996-01) |
| ETSI | TBR 014 | Business TeleCommunications (BTC); 64 kbit/s digital unrestricted leased line with octet integrity (D64U); Attachment requirements for terminal equipment interface |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | Edition 1  (1996-01) |
| ETSI  ATTM  TM4 | TR 101 036-1 | Fixed Radio Systems; Generic wordings for standards on DFRS (Digital Fixed Radio Systems) characteristics; Part 1: General aspects and point-to-point equipment parameters |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.3.1 (2002-08) |
| ETSI  ATTM  TM4 | TR 101 274 | Transmission and Multiplexing (TM); Digital Radio Relay Systems (DRRS); Point-to-multipoint DRRS in the access network; Overview of different access techniques |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.1.1  (1998-06) |
| ETSI  ATTM  TM6 | TS 101 270-1/-2 | Transmission and Multiplexing (TM); Access transmission systems on metallic access cables; Very High Speed Digital Subscriber Line (VDSL); Part 1: Functional requirements, Part 2: Transceiver specification |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | Part 1: V1.4.1  (2005-10)  Part 2: V1.2.1 (2003-07) |
| ETSI  ATTM  TM6 | TS 101 271 | Access, Terminals, Transmission and Multiplexing (ATTM); Access transmission systems on metallic access cables; Very High Speed digital subscriber line system (VDSL2) [Recommendation ITU-T G.993.2 modified] |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | V.1.2.1  (2013-08) |
| ETSI  ATTM  TM6 | TS 101 388 | Access Terminals Transmission and Multiplexing (ATTM); Access transmission systems on metallic access cables; Asymmetric Digital Subscriber Line (ADSL) - European specific requirements [ITU-T Recommendation G.992.1 modified] |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | V1.4.1  (2007-08) |
| ETSI  ATTM  TM6 | TS 101 524 | Access, Terminals, Transmission and Multiplexing (ATTM); Access transmission system on metallic access cables; Symmetrical single pair high bit rate Digital Subscriber Line (SDSL); [ITU-T Recommendation G.991.2 (2005), modified]  Note: the originally two parts are merged to one (11/2000 ) |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | V1.5.1 (2010-08) |
| ETSI  ATTM  TM4 | TS 101 974 | Transmission and Multiplexing (TM);  Digital Radio Relay Systems (DRRS);  Radio specific SDH functionalities for transmission of sub-STM-0 |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.1.1  (2001-08) |
| ETSI  ATTM  TM4 | ETS 300 635 | Transmission and Multiplexing (TM);  Synchronous Digital Hierarchy (SDH);  Radio specific functional blocks for transmission of M x STM-N |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | Edition 1  (1996-10) |
| ETSI  ATTM  TM4 | ETS 300 785 | Transmission and Multiplexing (TM);  Synchronous Digital Hierarchy (SDH);  Radio specific functional blocks for transmission of M x sub-STM-1 |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | Edition 1  (1998-02) |
| ETSI  ATTMTM4 | TR 101 016 | Transmission and Multiplexing (TM); Digital Radio Relay Systems (DRRS);  Comparison and verification of performance prediction models |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.1.1  (1997-02) |
| ETSI  ATTMTM4 | TR 101 853 | Fixed Radio Systems; Point-to-point and Point-to-multipoint equipment; Rules for the co-existence of point-to-point and point-to-multipoint systems using different access methods in the same frequency band |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | V1.1.1  (2000-10) |
| ETSI AT2 | TS 102 639-1 | Access and Terminals, Transmission and Multiplexing (ATTM); Third Generation Transmission Systems for Interactive Cable Television Services - IP Cable Modems; Part 1: General |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | V1.1.1 (2009-04) |
| ETSI AT2 | TS 102 639-2 | Access and Terminals, Transmission and Multiplexing (ATTM); Third Generation Transmission Systems for Interactive Cable Television Services - IP Cable Modems; Part 2: Physical Layer [ITU-T Recommendation J.222.1 (07/2007), modified] |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | V1.1.1 (2009-04) |
| ETSI AT2 | TS 102 639-3 | Access and Terminals, Transmission and Multiplexing (ATTM); Third Generation Transmission Systems for Interactive Cable Television Services - IP Cable Modems; Part 3: Downstream Interface [ITU-T Recommendation J.210 (11/2006), modified] |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | V1.1.1 (2009-04) |
| ETSI AT2 | TS 102 639-4 | Access and Terminals, Transmission and Multiplexing (ATTM); Third Generation Transmission Systems for Interactive Cable Television Services - IP Cable Modems; Part 4: MAC and Upper Layer Protocols [ITU-T Recommendation J.222.2 (07/2007), modified] |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | V1.1.1 (2009-04) |
| ETSI AT2 | TS 102 639-5 V1.1.1 | Access and Terminals, Transmission and Multiplexing (ATTM); Third Generation Transmission Systems for Interactive Cable Television Services - IP Cable Modems; Part 5: Security Services [ITU-T Recommendation J.222.3 (07/2007), modified] |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | V1.1.1  (2009-04) |
| ETSI AT2 | TS 102 836-1 | Access, Terminals, Transmission and Multiplexing (ATTM); Lawful Interception (LI); Part 1: Interception of IP Telephony Service on Cable Operator's Broadband IP Network: Internal Network Interfaces |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | V1.1.1  (2009-11) |
| ETSI AT2 | TS 102 836-2 | Access, Terminals, Transmission and Multiplexing (ATTM); Lawful Interception (LI); Part 2: Interception of IP Data Service on Cable Operator's Broadband IP Network: Internal Network Interfaces |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | V1.1.1  (2009-11) |
| ETSI AT2 | TS 102 973 | Access Terminals, Transmission and Multiplexing (ATTM); Network Termination (NT) in Next Generation Network architectures | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | V1.1.1  (2008-09) |
| IEEE | 802.3-2018 2BASE-TL | Physical Layer specification up to 5.696 Mb/s point to point link over single copper wire pair - IEEE Std 802.3, Clause 61 and Clause 63 |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | 08/2018 |
| IEEE | 802.3-2018 10PASS-TS | Physical Layer specification up to 100 Mb/s point to point link over single copper wire pair – IEEE Std 802.3, Clause 61 and 62 |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | 08/2018 |
| IEEE | 802.3-2018 100BASE-LX1 and  100BASE-BX10 | Physical Layer specification for point-to-point 100 Mb/s Ethernet links over single-mode optical fiber - IEEE Std 802.3, Clause 56, Clause 58 and Clause 66 |  | | | X | |  | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 08/2018 |
| IEEE | 802.3-2018 1000BASE-LX10 and  1000BASE-BX10 | Physical Layer specification for point-to-point 1 Gb/s Ethernet links over single-mode optical fiber and multimode optical fiber- IEEE Std 802.3, Clause 56, Clause 59 and Clause 66 |  | | | X | |  | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 08/2018 |
| IEEE | 802.3-2018 1000BASE-PX | Physical Layer specification for point-to-multipoint 1 Gb/s connections over Ethernet-based passive optical networks (1G-EPON) - IEEE Std 802.3, Clause 56, Clause 60, Clause 64 and Clause 65 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 08/2018 |
| IEEE | 802.3-2018 10GBASE-PR and  10/1GBASE-PRX | Physical Layer specification for point-to-multipoint 10 Gb/s connections over Ethernet-based passive optical networks (10G-EPON) - IEEE Std 802.3, Clause 56, Clause 75, Clause 76 and Clause 77 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 08/2018 |
| IEEE | 802.3-2018 EPoC | Physical Layer Specifications and Management Parameters for Ethernet Passive Optical Networks Protocol over Coax (EPoC) – IEEE Std 802.3, Clause 100, Clause 101, Clause 102 and Clause 103 |  | | | X | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 08/2018 |
| IEEE | 802.16-2017 | IEEE Standard for Air Interface for Broadband Wireless Access Systems |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 03/2018 |
| IEEE | 802.16.1-2012 | IEEE Standard for WirelessMAN-Advanced Air Interface for Broadband Wireless Access Systems |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 09/2012 |
| IEEE | 802.16.1a-2013 | IEEE Standard for WirelessMAN-Advanced Air Interface for Broadband Wireless Access Systems --Amendment 2: Higher Reliability Networks |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 06/2013 |
| IEEE | 802.16.1b-2012 | IEEE Standard for WirelessMAN-Advanced Air Interface for Broadband Wireless Access Systems Amendment 1: Enhancements to Support Machine-to-Machine Applications |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 10/2012 |
| ISO | ISO/IEC 8877:1992 | Information technology — Telecommunications and information exchange between systems — Interface connector and contact assignments for ISDN Basic Access Interface located at reference points S and T |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 1992 |
| ISO/ IEC | 12139-1 | Information technology — Telecommunications and information exchange between systems — Power Line Communication(PLC) – High speed PLC Media Access Control(MAC) and Physical Layer(PHY) | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | X | May 2009 |
| ITU-R | BT.2400 (draft) | Draft new Report ITU-R BT.[GLOBAL PLATFORM] - Usage scenarios, requirements and technical elements of a global platform for the broadcasting service | X | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2017 |
| ITU-R | F.757-3 | Basic system requirements and performance objectives for fixed wireless access using mobile-derived technologies offering basic telephony service and data communication service | X | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 02/03 |
| ITU-R | F.757-4 | Basic system requirements and performance objectives for fixed wireless access using mobile | X | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 04/2011 |
| ITU-R | F.1332-1 | Radio-frequency signal transport through optical fibres | X | | | X | |  | |  | |  | |  | |  | |  | |  | |  | |  | | X |  | 05/99 |
| ITU-R | F.1399-1 | Vocabulary of terms for wireless access | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 05/01 |
| ITU-R | F.1400 | Performance and availability objectives for FWA to PSTN | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 05/99 |
| ITU-R | F.1401-1 | Considerations for the identification of possible frequency bands for fixed wireless access and related sharing studies. |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 01/04 |
| ITU-R | F.1402 | Frequency sharing criteria between land mobile wireless access systems and FWA using the same equipment type as mobile wireless access system |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 05/1999 |
| ITU-R | F.1490-1 | Generic requirements for fixed wireless access (FWA) systems | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 09/2007 |
| ITU-R | F.1499 | Radio transmission systems for fixed broadband wireless access (BWA) based on cable modem standard |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 05/00 |
| ITU-R | F.1500 | Preferred characteristics of systems in the fixed service using high altitude platforms operating in the bands 47.2‑47.5 GHz and 47.9-48.2 GHz |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 05/2000 |
| ITU-R | F.1569 | Technical and operational characteristics for the fixed service using high altitude platform stations in the band 27.5-28.5 and 31.0-31.3 GHz |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 05/02 |
| ITU-R | F.1704 | Characteristics of multipoint-to-multipoint fixed wireless systems with meshed network topology operating in frequency bands above about 17 GHz |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 01/05 |
| ITU-R | F.1763-1 | Radio interface standards for broadband wireless access systems in the fixed service operating below 66 GHz |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 02/2014 |
| ITU-R | F.2058 (Report) | Design techniques applicable to broadband fixed wireless access systems conveying Internet protocol packets or asynchronous transfer mode cells |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2006 |
| ITU-R | F.2086-1 (Report) | Technical and operational requirements for broadband wireless access in the fixed service | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2010 |
| ITU-R | F.2106-1 (Report) | Fixed Service applications using free-space optical links | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2010 |
| ITU-R | F.2107-1 (Report) | Characteristics and applications of fixed wireless systems operating in the 57 GHz to 130 GHz bands |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2012 |
| ITU-R | F.2060 (Report) | Fixed Service use in the IMT-2000 transport network | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2005 |
| ITU-R | F.2106-1 (Report) | Fixed Service applications using free-space optical links | X | | |  | |  | |  | |  | |  | |  | |  | |  | | |  | |  | X |  | 2010 |
| ITU-R | F.2107-1 (Report) | Characteristics and applications of fixed wireless systems operating in the 57 GHz to 130 GHz bands |  | | |  | |  | |  | |  | |  | |  | |  | |  | | |  | |  | X |  | 2012 |
| ITU‑R | [M.687-2](http://www.itu.int/rec/R-REC-M.687/en) | International Mobile Telecommunications-2000 (IMT-2000) | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 02-1997 |
| ITU‑R | [M.818-2](http://www.itu.int/rec/R-REC-M.818/en) | Satellite operation within IMT‑2000 | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 06-2003 |
| ITU-R | [M.819-2](http://www.itu.int/rec/R-REC-M.819/en) | International Mobile Telecommunications-2000  (IMT-2000) for developing countries | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 02-1997 |
| ITU‑R | [M.1036-](http://www.itu.int/rec/R-REC-M.1036/en)4 | Frequency arrangements for implementation of the terrestrial component of International Mobile Telecommunications-2000 (IMT-2000) in the bands  806-960 MHz, 1 710-2 025 MHz, 2 110-2 200 MHz and 2 500-2 690 MHz |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 03/2012 |
| ITU‑R | [M.1073](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1073).2 | Digital cellular land mobile telecommunication systems | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | June 2005 |
| ITU-R | [M.1079-2](http://www.itu.int/rec/R-REC-M.1079/en) | Performance and quality of service requirements for International Mobile Telecommunications-2000  (IMT-2000) | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 06-2003 |
| ITU‑R | [M.1167](http://www.itu.int/rec/R-REC-M.1167/en) | Framework for the satellite component of International Mobile Telecommunications-2000 (IMT-2000) | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 10-1995 |
| ITU‑R | [M.1224](http://www.itu.int/rec/R-REC-M.1224/en)-1 | Vocabulary of terms for IMT-2000 | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 03/2012 |
| ITU‑R | [M.1225](http://www.itu.int/rec/R-REC-M.1225/en) | Guidelines for evaluation of radio transmission technologies for IMT-2000 | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 02-1997 |
| ITU‑R | [M.1311](http://www.itu.int/rec/R-REC-M.1311/en) | Framework for modularity and radio commonality within IMT-2000 | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 10-1997 |
| ITU‑R | [M.1390](http://www.itu.int/rec/R-REC-M.1390/en) | Methodology for the Calculation of IMT‑2000 Terrestrial Spectrum Requirements |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 01-1999 |
| ITU‑R | [M.1391-1](http://www.itu.int/rec/R-REC-M.1391/en) | Methodology for the Calculation of IMT‑2000 Satellite Spectrum Requirements |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 03-2006 |
| ITU‑R | [M.1034-1](http://www.itu.int/rec/R-REC-M.1034/en) | Requirements for the radio interfaces for IMT-2000 | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 02-1997 |
| ITU‑R | [M.1450](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1450)-5 | Characteristics of broadband RLANs | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 04/2014 |
| ITU‑R | [M.1454](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1454) | E.i.r.p. density limit and operational restrictions for RLANs or other wireless access transmitters in order to ensure the protection of feeder links of NGSO systems in the MSS in the frequency band 5 150-5 250 MHz |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2000 |
| ITU-R | M.1457-12 | Detailed specifications of the terrestrial radio interfaces of International Mobile Telecommunications-2000 (IMT-2000) |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 02/2015  Supersedes M.1457-11 (02/2013) |
| ITU-R | M.1579-2 | Global circulation of IMT-2000 terrestrial terminals |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 01/2015  Supersedes  M.1579-1 (03/2012) |
| ITU‑R | [M.1651](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1651) | A method for assessing the required spectrum for broadband NWA systems including RLANs using the 5 GHz band |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2003 |
| ITU‑R | [M.1652](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1652)-1 | Dynamic Frequency Selection (DFS) in Wireless Access Systems (WAS) including Radio Local Area Networks (RLAN) for the purpose of protecting the radio determination service in the 5 GHz band |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 05/2011 |
| ITU‑R | [M.1653](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1653) | Operational and deployment requirements for WAS including RLANs in the MS to facilitate sharing between these systems and systems in the EESS (active) and the SRS (active) in the band 5 470-5 570 MHz within the 5 460‑5 725 MHz range |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2003 |
| ITU-R | [M.1768](http://www.itu.int/rec/R-REC-M.1768/en) | Methodology for calculation of spectrum requirements for the future development of the terrestrial component of IMT-2000 and systems beyond IMT-2000 |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 03-2006 |
| ITU‑R | [M.1797](http://www.itu.int/rec/R-REC-M.1797/en) | Vocabulary of terms for the land mobile service | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2007 |
| ITU‑R | [M.1801](http://www.itu.int/rec/R-REC-M.1801/en)-2 | Radio interface standards for broadband wireless access systems, including mobile and nomadic applications, in the mobile service operating below 6 GHz |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 02/2013 |
| ITU‑R | M.1850-2 | Detailed specifications of the radio interfaces for the satellite component of International Mobile Telecommunications-2000 (IMT-2000). |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 10/2014 |
| ITU-R | [M.2003](http://www.itu.int/rec/R-REC-M.2003-1-201501-I/en)-1 | Multiple Gigabit Wireless Systems | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 01/2015 |
| ITU-R | M.2012-2 | Detailed specifications of the terrestrial radio interfaces of International Mobile Telecommunications Advanced (IMT-Advanced) |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 09/2015 Supersedes M.2012-1 (02/2014) |
| ITU‑R | [M.2023](http://www.itu.int/pub/R-REP-M.2023/en) (Report) | Spectrum Requirements for IMT‑2000 | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2000 |
| ITU‑R | [M.2034](http://www.itu.int/itudoc/itu-r/publica/rep/m/2034.html) (Report) | Impact of radar detection requirements of dynamic frequency selection on 5 GHz wireless access system receivers |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2003 |
| ITU-R | M.2047-0 | Detailed specifications of the satellite radio interfaces of International Mobile Telecommunications-Advanced (IMT-Advanced) |  | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 12/2013 |
| ITU-R | [M.2074](http://www.itu.int/pub/R-REP-M/en) (Report) | Radio aspects for the terrestrial component of IMT-2000 and systems beyond IMT-2000(ex-[Doc. 8/115(Rev.1](http://www.itu.int/md/R03-SG08-C-0115/e))) | X | | |  | |  | |  | | X | |  | |  | |  | |  | | |  | |  | X |  | 2006 |
| ITU-R | S.579 | Availability objectives for a hypothetical reference circuit and a hypothetical reference digital path when used for telephony using pulse code modulation, or as part of an integrated services digital network hypothetical reference connection, in the fixed satellite service |  | | |  | |  | |  | | X | | X | |  | |  | |  | |  | |  | | X |  | 2001 |
| ITU-R | S.614 | Allowable error performance for a hypothetical reference digital path in the fixed-satellite service operating below 15 GHz when forming part of an international connection in an integrated services digital network |  | | |  | |  | |  | | X | | X | |  | |  | |  | |  | |  | | X |  | 1994 |
| ITU-R | S.1062 | Allowable error performance for a hypothetical reference digital path operating at or above the primary rate |  | | |  | |  | |  | | X | | X | |  | |  | |  | |  | |  | | X |  | 1999 |
| ITU-R | S.1420 | Performance for broadband integrated services digital network asynchronous transfer mode via satellite |  | | |  | |  | |  | | X | | X | |  | |  | |  | |  | |  | | X |  | 1999 |
| ITU-R | S.1424 | Availability objectives for a hypothetical reference digital path when used for the transmission of B-ISDN asynchronous transfer mode in the fixed-satellite service by geostationary orbit satellite systems using frequencies below 15 GHz |  | | |  | |  | |  | | X | | X | |  | |  | |  | |  | |  | | X |  | 2000 |
| ITU-R | S.1521 | Allowable error performance for a hypothetical reference digital path based on synchronous digital hierarchy |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 2001 |
| ITU-R | S.1711 | Performance enhancements of transmission control protocol (TCP) over satellite networks |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 2005 |
| ITU-R | S.1782 | Possibilities for global broadband Internet access by fixed-satellite service systems – 2007 | X | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 01/2007 |
| ITU-R | S.1806 | Availability objectives for hypothetical reference digital paths in the fixed-satellite service operating below 15 GHz – 2008 |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 08/2008 |
| ITU-R | S.1878 | Multi-carrier based transmission techniques for satellite systems – 2010 |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 12/2010 |
| ITU-R | S.1897 | Cross-layer QoS provisioning in IP-based hybrid satellite-terrestrial networks – 201 |  | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 01/2012 |
| ITU-R | http://www.itu.int/oth/R0A06000001/en | Guide to the use of ITU-R texts related to the land mobile service | X | | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  | | X |  | 2011 |
| ITU-T | G.177 | Transmission planning for voiceband services over hybrid internet/PSTN connections | X | | |  | |  | |  | |  | | X | |  | |  | |  | |  | |  | |  |  | 09/1999 |
| ITU‑T | G.702 | Digital hierarchy bit rates | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.703 | Physical/electrical characteristics of hierarchical digital interfaces | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 04/2016 |
| ITU‑T | G.707/Y.1322 | Network node interface for the synchronous digital hierarchy (SDH) | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 01/2007 |
| ITU-T | G.707/Y.1322  Amendment 1 | Network node interface for the synchronous digital hierarchy (SDH)  Amendment 1 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 07/2007 |
| ITU-T | G.707/Y.1322  Amendment 2 | Network node interface for the synchronous digital hierarchy (SDH)  Amendment 2 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 11/2009 |
| ITU‑T | G.775 | Loss of signal (LOS) and alarm indication signal (AIS) defect detection and clearance criteria | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 10/1998 |
| ITU‑T | G.783 | Physical characteristics of multiplexing equipment for the Synchronous Digital Hierarchy | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 03/2006 |
| ITU-T | G.783  Amendments  1, 2, 3, 4 | Physical characteristics of multiplexing equipment for the Synchronous Digital Hierarchy  Amendments 1, 2, 3, 4 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | Amd. 1 05/2008  Amd. 2 03/2010  Amd. 3 02/2012  Amd. 4 08/2013 Cor. 1 01/2015 |
| ITU‑T | G.802 | Interworking between networks based on different digital hierarchies and speech encoding laws  Blue Book Fascicle III.5 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.803 | Architectures of transport networks based on the synchronous digital hierarchy (SDH) | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 03/2000 |
| ITU-T | G.803  Amendment 1 | Architectures of transport networks based on the synchronous digital hierarchy (SDH)  Amendment 1 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 06/2005 |
| ITU‑T | G.805 | General transport network architecture | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 03/2000 |
| ITU-T | G.831 | Management capabilities of transport networks based on the synchronous digital hierarchy (SDH) | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 03/2000 |
| ITU‑T | G.902 | Framework Recommendation on functional access networks (AN) - Architecture and functions, access types, management and service node aspects | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 11/1995 |
| ITU‑T | G.921 | Digital sections based on the 2048 kbit/s hierarchy  Blue Book Fascicle III.5 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.950 | General considerations on digital line systems  Blue Book Fascicle III.5 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.951 | Digital line systems based on the 1544 kbit/s hierarchy on symmetric pair cables  Blue Book Fascicle III.5 |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.952 | Digital line systems based on the 2048 kbit/s hierarchy on symmetric pair cables  Blue Book Fascicle III.5 |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.953 | Digital line systems based on the 1544 kbit/s hierarchy on coaxial pair cables  Blue Book Fascicle III.5 |  | | |  | | X | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.954 | Digital line systems based on the 2048 kbit/s hierarchy on coaxial pair cables  Blue Book Fascicle III.5 |  | | |  | | X | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 11/1988 |
| ITU‑T | G.955 | Digital line systems based on the 1544 kbit/s and the 2048 kbit/s hierarchy on optical fibre cables |  | | | X | |  | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 11/1996 |
| ITU‑T | G.957 | Optical interfaces for equipments and systems relating to the synchronous digital hierarchy | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 03/2006 |
| ITU‑T | G.960 | Digital section for ISDN basic rate access |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/1993 |
| ITU‑T | G.961 | Digital transmission system on metallic local lines for ISDN basic rate access |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/1993 |
| ITU‑T | G.962 | Access digital section for ISDN primary rate access at  2048 kbit/s |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/1993 |
| ITU‑T | G.962  Amendment 1 | Access digital section for ISDN primary rate access at  2048 kbit/s  Amendment1 – Maintenance channel |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 06/1997 |
| ITU‑T | G.963 | Access digital section for ISDN primary rate at 1544 kbit/s |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/1993 |
| ITU‑T | G.964 | V interfaces at the digital local exchange (LE) -V5.1 interface (based on 2 048 kbit/s) for the support of access network (AN) |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/2001 |
| ITU‑T | G.965 | V interfaces at the digital local exchange (LE) -V5.2 interface (based on 2 048 kbit/s) for the support of access network (AN)" |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/2001 |
| ITU‑T | G.966 | Access Digital Section for B-ISDN (G.96x) |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU‑T | G.967.1 | V interfaces at the digital Service Node (SN); Interfaces at the VB5.1 reference point specification for the support of broadband or combined narrowband and broadband Access Networks (G.VB51) |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 06/1998 |
| ITU‑T | G.967.2 | V interfaces at the digital Service Node (SN); Interfaces at VB5.2 reference point specification for the support of broadband or combined narrowband and broadband Access Networks (G.VB52) |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU-T | G.967.3 | V-Interfaces at the service node (SN)- Protocol implementation conformance statements for Interfaces at VB5 reference points |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/2000 |
| ITU-T | Technical paper (12/2011) | Wireline broadband access networks and home networking | X | | | X | |  | | X | |  | |  | | X | |  | | X | | X | |  | |  |  | 12/2011 |
| ITU-T | G Suppl. 39  (02/2016) | Optical system design and engineering considerations | X | | | X | |  | |  | |  | |  | |  | |  | | X | | X | |  | |  |  | 02/2016 |
| ITU‑T | G.981 | PDH optical line systems for the local network |  | | | X | |  | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 01/1994 |
| ITU‑T | G.982 | Optical access networks to support services up to the ISDN primary rate or equivalent bit rates |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 11/1996 |
| ITU‑T | G.983.1 (01/2005) | Broadband optical access system based on Passive Optical Networks (PON) |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 01/2005  Erratum 1  03/2006 |
| ITU‑T | G.983.1 (2005)  Amendment 1 | Broadband optical access systems based on Passive Optical Networks (PON)  Amendment 1: PICS for OLT and ONU |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 05/ 2005 |
| ITU-T | G.983.3 (03/2001) | A broadband optical access system with increased service capability by wavelength allocation |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2001 |
| ITU-T | G.983.3 (2001) Amendment 1 | A broadband optical access system with increased  service capability by wavelength allocation  Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 06/ 2002 |
| ITU-T | G.983.3 (2001) Amendment 2 | A broadband optical access system with increased  service capability by wavelength allocation  Amendment 2 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 07/ 2005 |
| ITU-T | G.983.4 (11/2001) | A broadband optical access system with increased service capability using dynamic bandwidth assignment |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 11/2001  Corrigendum1  01/2005 |
| ITU-T | G.983.4 (2001)  Amendment 1 | A broadband optical access system with increased service capability using dynamic bandwidth assignment  Amendment 1: New Annex A – Performance  monitoring parameters |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 12/2003 |
| ITU-T | G.983.5 (01/2002) | A Broadband Optical Access System with Enhanced Survivability |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 01/2002 |
| ITU-T | G.984.1 (03/2008) | Gigabit-capable passive optical networks (GPON): General characteristics |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2008 |
| ITU-T | G.984.1 (2008)  Amendment 1 | Gigabit-capable passive optical networks (GPON): General characteristics  Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 10/2009 |
| ITU-T | G.984.1 (2008)  Amendment 2 | Gigabit-capable passive optical networks (GPON): General characteristics  Amendment 2 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 04/2012 |
| ITU-T | G.984.2 (03/2003) | Gigabit-capable Passive Optical Networks (GPON): Physical Media Dependent (PMD) layer specification |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2003 |
| ITU-T | G.984.2 (2003)  Amendment 1 | Gigabit-capable Passive Optical Networks  (G-PON): Physical Media Dependent (PMD) layer  specification  Amendment 1: New Appendix III – Industry best  practice for 2.488 Gbit/s downstream,  1.244 Gbit/s upstream G-PON |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 02/2006 |
| ITU-T | G.984.2 (2003)  Amendment 2 | Gigabit-capable Passive Optical Networks  (G-PON): Physical Media Dependent (PMD) layer  specification  Amendment 2 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2008 |
| ITU-T | G.984.3 (01/2014) | Gigabit-capable Passive Optical Networks (GPON): Transmission convergence layer specification |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 01/2014  Supersedes Ed. 1 - 02/2004, Ed. 2- 03/2008 and all related amendments |
| ITU-T | G.984.4 (02/2008) | Gigabit-capable Passive Optical Networks (GPON): ONT management and control interface specification |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 02/2008  Erratum 08/2009  Corrigendum1  03/2010 |
| ITU-T | G.984.4 (2008)  Amendment 1 | Gigabit-capable Passive Optical Networks (GPON): ONT management and control interface specification  Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 06/2009 |
| ITU-T | G.984.4 (2008)  Amendment 2 | Gigabit-capable passive optical networks (G-PON):  ONT management and control interface specification  Amendment 2: Changes and extensions to the  OMCI, editorial clarifications and corrections |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 11/2009 |
| ITU-T | G.984.4 (2008)  Amendment 3 | Gigabit-capable passive optical networks (G-PON):  ONT management and control interface specification  Amendment 3: Clarification of scope of application |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 07/2010 |
| ITU-T | G.Imp.984.4  (10/1999) | Implementers’ Guide for Recommendation ITU-T G.984.4  Second Revision |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 10/2009 |
| ITU-T | G.984.5 (05/2014) | Gigabit-capable Passive Optical Networks (G-PON): Enhancement band |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 05/2014  Supersedes Ed.1- 09/2007 and Amd.1-10/2009 |
| ITU-T | G.984.5 (05/2014) Amendment 1 | Gigabit-capable Passive Optical Networks (G-PON): Enhancement band  Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 05/2018 |
| ITU-T | G.984.6 (03/2008) | Gigabit-capable passive optical networks  (GPON): Reach extension |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2008 |
| ITU-T | G.984.6 (2008)  Amendment 1 | Gigabit-capable passive optical networks (GPON):  Reach extension  Amendment 1: Wavelength-converting, continuous mode, and 1:N-protected range extenders |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 11/2009 |
| ITU-T | G.984.6 (2008)  Amendment 2 | Gigabit-capable passive optical networks (G-PON):  Reach extension  Amendment 2 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 05/2012 |
| ITU-T | G.984.7 (07/2010) | Gigabit-capable passive optical networks (GPON): Long reach |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 07/2010 |
| ITU-T | G.985 (03/2003) | 100 Mbit/s point-to-point Ethernet based optical  access system |  | | | X | |  | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 03/2003  Corrigendum1 01/2005 |
| ITU-T | G.985 (2003)  Amendment 1 | 100 Mbit/s point-to-point Ethernet based optical  access system  Amendment 1: Silent start function of optical  network terminals |  | | | X | |  | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 01/2009 |
| ITU-T | G.986 (01/2010) | 1 Gbit/s point-to-point Ethernet-based optical  access system |  | | | X | |  | |  | |  | |  | |  | |  | | X | |  | |  | |  |  | 01/2010 |
| ITU-T | G.987 (06/2012) | 10-Gigabit-capable passive optical network  (XG-PON) systems: Definitions, abbreviations  and acronyms |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 06/2012 |
| ITU-T | G.987.1 (03/2016) | 10-Gigabit-capable passive optical networks  (XG-PON): General requirements |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2016  Supersedes  Ed.1 - 01/2010  and Amd.1 - 04/2012 |
| ITU-T | G.987.2 (02/2016) | 10-Gigabit-capable passive optical networks  (XG-PON): Physical media dependent (PMD)  layer specification |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 02/2016  Superseded Amd.1 – 02/2012  and Ed.2 -10/2010 and Ed.1 - 01/2010 |
| ITU-T | G.987.2 (2016) Amendment 1 | 10-Gigabit-capable passive optical networks  (XG-PON): Physical media dependent (PMD)  layer specification  Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 08/2017 |
| ITU-T | G.987.3 (01/2014) | 10-Gigabit-capable passive optical networks (XG-PON): Transmission convergence (TC) layer specification |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 01/2014  Supersedes  Ed. 1- 10/2010 and Amd.1 - 06/2012 |
| ITU-T | G.987.4 (06/2012) | 10 Gigabit-capable passive optical networks  (XG-PON): Reach extension |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 06/2012 |
| ITU-T | G Suppl. 48 (06/2010) | 10-Gigabit-capable passive optical networks: Interface between media access control with serializer/deserializer and physical medium dependent sublayers |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 06/2010 |
| ITU-T | G.989 (10/2015) | 40-Gigabit-capable passive optical network (NG PON2): Definitions, abbreviations and acronyms |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 10/2015 |
| ITU-T | G.989.1 (03/2013) | 40-Gigabit-capable passive optical networks  (NG-PON2): General requirements |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 03/2013 |
| ITU-T | G.989.1 (2013) Amendment 1 | 40-Gigabit-capable passive optical networks (NG-PON2): General requirements: Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 08/2015 |
| ITU-T | G.989.2 (12/2014) | 40-Gigabit-capable passive optical networks 2 (NG-PON2): Physical media dependent (PMD) layer specification |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 12/2014 |
| ITU-T | G.989.2 (2014)  Amendment 1 | 40-Gigabit-capable passive optical networks 2 (NG-PON2): Physical media dependent (PMD) layer specification  Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 04/2016 |
| ITU-T | G.989.2 (2014)  Amendment 2 | 40-Gigabit-capable passive optical networks 2 (NG-PON2): Physical media dependent (PMD) layer specification  Amendment 2 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 08/2017 |
| ITU-T | G.989.3 (10/2015) | 40-Gigabit-capable passive optical networks (NG PON2): Transmission Convergence Layer Specification |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 10/2015 |
| ITU-T | G.989.3 (2015)  Amendment 1 | 40-Gigabit-capable passive optical networks (NG PON2): Transmission Convergence Layer Specification Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 11/2016 |
| ITU-T | G Suppl. 63 (02/2018) (ex G.sup.TCadapt) | ITU-T G.989.3 TC layer operating in ITU T G.987.3 or ITU-T G.9807.1 TC layer mode |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 02/2018 |
| ITU-T | G Suppl. 64 (02/2018)  (ex G.sup.HSP) | PON transmission technologies above 10 Gb/s per wavelength |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 02/2018 |
| ITU-T | G Suppl. 50 (09/2011) | Overview of digital subscriber line Recommendations | X | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 09/2011 |
| ITU‑T | G.991.1 (10/1998) | High bit rate Digital Subscriber Line (HDSL) transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 10/1998 |
| ITU‑T | G.991.2 (12/2003) | Single-pair high-speed digital subscriber line (SHDSL) transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 12/2003  Erratum 1  04/2005 |
| ITU‑T | G.991.2 (2003)  Amendment 1 | Single-pair high-speed digital subscriber line (SHDSL) transceivers  Amendment 1 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 07/2004 |
| ITU‑T | G.991.2 (2003)  Amendment 2 | Single-pair high-speed digital subscriber line (SHDSL) transceivers  Amendment 2 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 02/2005  Erratum 1  11/2005 |
| ITU‑T | G.991.2 (2003)  Amendment 3 | Single-pair high-speed digital subscriber line (SHDSL) transceivers  Amendment 3 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 09/2005 |
| ITU‑T | G.992.1 (07/1999) | Asymmetric digital subscriber line (ADSL) transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 07/1999  Corrigendum1 11/2001  Corrigendum2  07/2002 |
| ITU‑T | G.992.1 (1999) Amendment 1 | Asymmetric digital subscriber line (ADSL) transceivers  Amendment 1: Revised Annex C, new Annex I  and new Appendix V |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 03/2003  Corrigendum1  12/2003 |
| ITU‑T | G.992.1 (10/2000) Annex H | Asymmetric digital subscriber line (ADSL) transceivers  Annex H: Specific requirements for a  synchronized symmetrical DSL (SSDSL) system  operating in the same cable binder as ISDN as  defined in ITU-T G.961 Appendix III |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 10/2000 |
| ITU‑T | G.992.2 (07/1999) | Splitterless asymmetric digital subscriber line (ADSL) transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 07/1999  Corrigendum1  07/2002 |
| ITU‑T | G.992.2 (1999)  Amendment 1 | Splitterless asymmetric digital subscriber line (ADSL) transceivers  Amendment 1: Revised Annex C |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 03/2003 |
| ITU‑T | G.992.2 (1999)  Amendment 2 | Splitterless asymmetric digital subscriber line (ADSL) transceivers  Amendment 2: New Appendix IV – Example  overlapped PSD masks for use in a TCM-ISDN  crosstalk environment |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 10/2003 |
| ITU-T | G.992.3 (04/2009) | Asymmetric digital subscriber line transceivers 2 (ADSL2) |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 04/2009  Corrigendum1  11/2009  Corrigendum2  06/2011  Corrigendum3  08/2013 |
| ITU-T | G.992.3 (2009)  Amendment 1 | Asymmetric digital subscriber line transceivers 2  (ADSL2)  Amendment 1: Channel initialization policies |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 03/2010 |
| ITU-T | G.992.3 (2009)  Amendment 2 | Asymmetric digital subscriber line transceivers 2  (ADSL2)  Amendment 2: Retrain on eoc protocol timeout |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 07/2010 |
| ITU-T | G.992.3 (2009)  Amendment 3 | Asymmetric digital subscriber line transceivers 2  (ADSL2)  Amendment 3: Scale factor for downstream  transmitter referred virtual noise, and corrigenda |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 11/2010 |
| ITU-T | G.992.3 (2009)  Amendment 4 | Asymmetric digital subscriber line transceivers 2  (ADSL2)  Amendment 4 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 10/2011 |
| ITU-T | G.992.3 (2009)  Amendment 5 | Asymmetric digital subscriber line transceivers 2  (ADSL2)  Amendment 5: Accuracy of test parameters |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 10/2012 |
| ITU‑T | G.992.4 (07/2002) | Splitterless asymmetric digital subscriber line  transceivers 2 (splitterless ADSL2) |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 07/2002 |
| ITU-T | G.992.5 (01/2009) | Asymmetric digital subscriber line 2 transceivers (ADSL2)– Extended bandwidth ADSL2 (ADSL2plus) |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 01/2009  Corrigendum1  11/2010 |
| ITU-T | G.993.1 (06/2004) | Very high speed digital subscriber line transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 06/2004 |
| ITU-T | G.993.2 (01/2015) | Very high speed digital subscriber line transceivers 2 (VDSL2) |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 01/2015 Corrigendum1  11/2016  Supersedes previous version 2011 with Cor. 1, Err 1 and all previous Amd. 1, 2, 3, 4, 5, 6 |
| ITU-T | G.993.2 (2015) Amendment 1 | Very high speed digital subscriber line transceivers 2 (VDSL2): Amendment 1 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 11/2015 |
| ITU-T | G.993.2 (2015) Amendment 2 | Very high speed digital subscriber line transceivers 2 (VDSL2): Amendment 2 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 13/2016 |
| ITU-T | G.993.2 (2015) Amendment 3 | Very high speed digital subscriber line transceivers 2 (VDSL2): Amendment 3 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 02/2018 |
| ITU-T | G.993.2 (2015) Amendment 4 | Very high speed digital subscriber line transceivers 2 (VDSL2): Amendment 4 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 05/2018 |
| ITU-T | G.993.5 (01/2015) | Self-FEXT cancellation (vectoring) for use with  VDSL2 transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 01/2015 Corrigendum1  11/2016  Corrigendum2  03/2018  Supersedes previous version 2010 with Cor. 1, 2 and all previous Amd. 1, 2, 3, 4, 5 |
| ITU-T | G.993.5 (2015) Amendment 1 | Self-FEXT cancellation (vectoring) for use with  VDSL2 transceivers – Amendment 1 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 12/2016 |
| ITU-T | G.993.5 (2015) Amendment 2 | Self-FEXT cancellation (vectoring) for use with  VDSL2 transceivers – Amendment 2 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 12/2017 |
| ITU‑T | G.994.1 (04/2017) | Handshake procedures for digital subscriber line transceivers  (This edition of this Recommendation integrates ITU-T G.994.1 (2012) and all its amendments and corrigenda. It does not add any new technical material). |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 04/2017 |
| ITU-T | G.994.1 (2017) Amendment 1 | Handshake procedures for digital subscriber line transceivers: Amendment 1 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 12/2017 |
| ITU-T | G.994.1 (2017) Amendment 2 | Handshake procedures for digital subscriber line transceivers: Amendment 2 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 03/2018 |
| ITU-T | G.998.1 (01/2005) | ATM-based multi-pair bonding |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 01/2005 |
| ITU-T | G.998.1(2005)  Amendment 1 | ATM-based multi-pair bonding  Amendment 1 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 08/2013 |
| ITU-T | G.998.2 (01/2005) | Ethernet-based multi-pair bonding |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 01/2005 Corrigendum1 03/2018 |
| ITU-T | G.998.2 (2005)  Amendment 1 | Ethernet-based multi-pair bonding  Amendment 1 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 12/2006 |
| ITU-T | G.998.2 (2005)  Amendment 2 | Ethernet-based multi-pair bonding  Amendment 2 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 12/2007 |
| ITU-T | G.998.2 (2005)  Amendment 3 | Ethernet-based multi-pair bonding  Amendment 3 – Intentional temporary shutdown  of some bonded lines |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 08/2013 |
| ITU-T | G.998.2 (2005) Amendment 4 | Ethernet-based multi-pair bonding  Amendment 4 |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 08/2015 |
| ITU-T | G.998.3 (01/2005) | Multi-pair bonding using time-division inverse  multiplexing |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 01/2005  Erratum 1  08/2005 |
| ITU-T | G.998.3 (2005)  Amendment 1 | Multi-pair bonding using time-division inverse  multiplexing  Amendment 1 – Intentional temporary shutdown  of some bonded lines |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 08/2013 |
| ITU-T | G.998.4 (01/2015) | Improved impulse noise protection for DSL  Transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 01/2015  Corrigendum1 08/2017  Supersedes previous version 2010 with Cor. 1,2,3,4,5 and previous Amd. 1,2,3,4 |
| ITU-T | G.999.1 (10/2009) | Interface between the link layer and the physical  layer for digital subscriber line (DSL)  transceivers |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 10/2009  Corrigendum1  04/2010 |
| ITU-T | G.999.1 (2009)  Amendment 1 | Interface between the link layer and the physical  layer for digital subscriber line (DSL)  transceivers  Amendment 1: Extension for flow control on the PHY-to-LINK data stream over gamma reference point |  | | |  | |  | | X | |  | |  | | X | |  | |  | |  | |  | |  |  | 04/2014 |
| ITU-T | G.9700 (04/2014) | Fast access to subscriber terminals (G.fast) – Power spectral density specification |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 04/2014 |
| ITU-T | G.9700 (2014) Amendment 1 | Fast access to subscriber terminals (G.fast) - Power spectral density specification: Amendment 1 |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 09/2016 |
| ITU-T | G.9700 (2014) Amendment 2 | Fast access to subscriber terminals (G.fast) - Power spectral density specification: Amendment 2 |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 06/2017 |
| ITU-T | G.9701 (12/2014) | Fast Access to Subscriber Terminals (G.fast) - Physical layer specification  This erratum also applies to ITU-T G.9701 (2014) Corrigenda 1, 2 and 3, and Amendments 1 and 2. |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 12/2014  Erratum 1 07/2017  Corrigendum1 Erratum 1 06/2017  Corrigendum1  11/2015  Corrigendum2  05/2016  Corrigendum3  04/2017  Corrigendum4  12/2107  Corrigendum5  08/2018 |
| ITU-T | G.9701 (2014)  Amendment 1 | Fast access to subscriber terminals (G.fast) - Physical layer specification  Amendment 1 |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 05/2016 |
| ITU-T | G.9701 (2014)  Amendment 2 | Fast access to subscriber terminals (G.fast) - Physical layer specification  Amendment 2 |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 07/2016 |
| ITU-T | G.9701 (2014)  Amendment 3 | Fast access to subscriber terminals (G.fast) - Physical layer specification  Amendment 3 |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 04/2017  Erratum 1 12/2017 |
| ITU-T | G.9701 (2014)  Amendment 4 | Fast access to subscriber terminals (G.fast) - Physical layer specification  Amendment 4 |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 12/2017 |
| ITU-T | G.9701 (2014)  Amendment 5 | Fast access to subscriber terminals (G.fast) - Physical layer specification  Amendment 5 |  | | |  | | X | | X | |  | |  | |  | | X | |  | |  | |  | |  |  | 08/2018 |
| ITU-T | G.9802 (04/2015) | Multiple Wavelength Passive Optical Networks (MW-PON) |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 04/2015 |
| ITU-T | G.9802 (2015) Amendment 1 | Control aspects of multiple wavelength passive optical networks: Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 08/2015 |
| ITU-T | G.9807.1 (06/2016) | 10-Gigabit-capable symmetric passive optical network (XGS-PON) |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 06/2016  Erratum 1 (03/17) |
| ITU-T | G.9807.1 (2016)  Amendment 1 | 10-Gigabit-capable symmetric passive optical network (XGS-PON)  Amendment 1 |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 10/2017 |
| ITU-T | G.9807.2 (08/2017) | 10 Gigabit-capable passive optical networks (XG(S)-PON): Reach extension |  | | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  | |  |  | 08/2017 |
| ITU-T | G Suppl.55 (ex G Suppl.RoF) (07/2015) | Radio-over-fiber (RoF) technologies and their applications |  | | | X | |  | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 07/2015 |
| ITU‑T | I.361 | B-ISDN ATM Layer Specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU‑T | I.410 | General aspects and principles relating to Recommendations on ISDN user-network interfaces  Blue Book Fascicle III.8 |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | I.411 | ISDN User-Network Interfaces - Reference Configurations |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/1993 |
| ITU‑T | I.412 | ISDN user-network interfaces - Interface structures and access capabilities  Blue Book Fascicle III.8 |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | I.413 | ISDN User-Network Interfaces - B-ISDN User-Network Interface |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/1993 |
| ITU‑T | I.414 | ISDN User-Network Interfaces - Overview of recommendations on layer 1 for ISDN and B-ISDN customer access |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 09/1997 |
| ITU‑T | I.420 | Basic user-network interface  Blue Book Fascicle III.8 |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | I.421 | Primary rate user-network interface  Blue Book Fascicle III.8 |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 11/1988 |
| ITU‑T | I.430 | Basic user-network interface - Layer 1 specification |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 11/1995 |
| ITU‑T | I.431 | Primary rate user-network interface - Layer 1 specification. |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 03/1993 |
| ITU‑T | I.432.1 | B-ISDN user-network interface physical layer specification – general characteristics |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU‑T | I.432.2 | B-ISDN UNI Physical layer specification for 155 520 kbit/s and 622 080 kbit/s |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU‑T | I.432.3 | B-ISDN UNI Physical layer specification for 1 544 kbit/s and 2 048 kbit/. |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU‑T | I.432.4 | B-ISDN UNI Physical layer specification for 51 840 kbit/s |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU‑T | I.432.5 | B-ISDN UNI Physical layer specification for 25 600 kbit/s |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 06/1997 |
| ITU‑T | I.460 | Multiplexing, rate adaption and support of existing interfaces |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 11/88 |
| ITU‑T | I.464 | Multiplexing, rate adaption and support of existing interfaces for restricted 64 kbit/s transfer capability |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 10/91 |
| ITU‑T | I.761 | Inverse multiplexing for ATM (IMA) | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | Approved 2000 |
| ITU-T | I.150 | B-ISDN asynchronous transfer mode functional characteristics |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 11/95 |
| ITU-T | I.480 | 1+1 protection switching for cell based physical layer | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | Approved 2000 |
| ITU-T | I.571 | Connection of VSAT based Private networks to the public ISDN |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 8/96 |
| ITU-T | I.572 | VSAT interconnection with the PSTN |  | | |  | |  | | X | |  | | X | |  | |  | |  | |  | |  | |  |  | 3/00 |
| ITU-T | I.762, former I.frac | Mapping over fractional physical links | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | approved 2000 |
| ITU-T | J.83 | Digital multi-programme systems for television, sound and data services for cable distribution | X | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.84 | Distribution of digital multi-programme signals for television, sound and data services through SMATV |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2001 |
| ITU-T | J.87 | Use of hybrid cable television links for the secondary distribution of television into the user’s premises |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2001 |
| ITU-T | J.93 | Requirements for conditional access in the secondary distribution of digital television on cable television systems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/1998 |
| ITU-T | J.112 | Transmission systems for interactive cable television services |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/1998 |
| ITU-T | J.112 Annex A | Transmission systems for interactive cable television services  Annex A |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2001 |
| ITU-T | J.112  Annex B | Transmission systems for interactive cable television services  Annex B |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2004 |
| ITU-T | J.112  Annex C | Transmission systems for interactive cable television services  Annex C |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 02/2002 |
| ITU-T | J.113 | Digital video broadcasting interaction channel through the PSTN/ISDN |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/1998 |
| ITU-T | J.118 | Access systems for interactive services in SMATV |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 05/2000 |
| ITU-T | J.122 | Second Generation Transmission Systems for Interactive Cable Television Services – IP Cable Modems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.126 | Embedded Cable Modem device specification |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.128 | Set-top Gateway specification for transmission systems for interactive cable television services |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 10/2008 |
| ITU-T | J.132 | Transport of MPEG-2 signals in SDH networks |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/1998 |
| ITU-T | J.150 | Transmission of digital multi-programme signals for television, sound and data services through multichannel, multipoint distribution systems (MMDS) |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/1998 |
| ITU-T | J.160(J.arch) | Architectural framework for the delivery of time-critical services over cable television networks using cable modems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 11/2005 |
| ITU-T | J.161(J.acr) | Audio/Video Codecs |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 06/2007 |
| ITU-T | J.162 (J.ncs) | Network-Based Call Signaling |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12(2007 |
| ITU-T | J.163(J.dqos) | Dynamic Quality-of-Service |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.164(J.em) | Event Messages |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.165(J.istp) | Internet Signaling Transport Protocol (ISTP) |  | | |  | |  | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 05/2003 |
| ITU-T | J.166(J.mibfrw) | MIBs Framework |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.167(J.mtadpv) | MTA Device Provisioning |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.168(J.mtamib) | MTA MIB |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2001 |
| ITU-T | J.169(J.ncsmib) | BNCS MI |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2001 |
| ITU-T | J.170 | IPCablecom security specification |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 11/2005 |
| ITU-T | J.171(J.tgcp) | IPCablecom Trunking Gateway Control Protocol (TGCP) |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2002 |
| ITU-T | J.175 (J.as) | Audio Server Protocol |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 11/2005 |
| ITU-T | J.176 (J.memmib) | IPCablecom Management Event Mechanism MIB |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 07/ 2002 |
| ITU-T | J.184(J.oob) | Digital Broadband Delivery System:  Out Of Band Transport |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2001 |
| ITU-T | J.185 | Transmission equipment for transferring multi-channel television signals over optical access networks by frequency modulation conversion |  | | | X | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 06/2012 |
| ITU-T | J.186 | Transmission equipment for multi-channel television signals over optical access networks by sub-carrier multiplexing (SCM) |  | | | X | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 6/2008 |
| ITU-T | J.190 | Home Network Architecture that supports IP-based and proprietary protocol-based multimedia services |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 7/2007 |
| ITU-T | J.191 | IP Feature Package to Enhance Cable Modems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | March 2004 |
| ITU-T | J.192 | A Residential Gateway to support the delivery of cable data services |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 11/2005 |
| ITU-T | J.195.1  (J.HiNoC-req) | Functional Requirements of high speed transmission over coaxial network connected with Fiber To The Building |  | | | X | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2016 Supersedes Ed.1 03/2013 |
| ITU -T | J.195.2  (J.HiNoC-phy) | PHY layer specification of high performance network over coax |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 10/2014 |
| ITU-T | J.195.3  (J.HiNoC-mac) | MAC layer specification of high performance network over coax |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 10/2014 |
| ITU-T | J.196.1  (J.HiNoC2-req) | Functional Requirements for Second-generation HiNoC |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2016 |
| ITU-T | J.196.2  (J.HiNoC2-phy) | Physical layer specification of second generation HiNoC |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 10/2016 |
| ITU-T | J.196.3 (J.HiNoC2-mac) | Media Access Control (MAC) layer specification of second generation HiNoC |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 10/2016 |
| ITU-T | J.223.1  (J.C-DOCSIS-req) | Functional Requirements for Cabinet DOCSIS (C-DOCSIS) |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 03/2016 |
| ITU-T | J.223.2 (J.C-DOCSIS-spec) | Cabinet DOCSIS (C-DOCSIS) System Specification |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 10/2016 |
| ITU-T | J.197 | High level requirements for a Digital Rights Management (DRM) bridge from a cable access network to a home network |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 11/2005 |
| ITU-T | J.210 | Downstream RF Interface for Cable Modem Termination Systems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | October 2006 |
| ITU-T | J.211 | Timing Interface for Cable Modem Termination Systems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | October 2006 |
| ITU-T | J.212 | Downstream External PHY Interface for Modular Cable Modem Termination Systems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | October 2006 |
| ITU-T | J.222.0 | Overview of third-generation transmission systems for interactive cable television services - IP cable modems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 12/2007 |
| ITU-T | J.222.1 | Physical layer specification for third-generation transmission systems for interactive cable television services - IP cable modems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 07/2007 |
| ITU-T | J.222.2 | MAC and Upper Layer protocols for third-generation transmission systems for interactive cable television services - IP cable modems |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 07/2007 |
| ITU-T | J.222.3 | Third-generation transmission systems for interactive cable television services - IP cable modems Security services |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 11/2007 |
| ITU-T | J.381 | Requirements for advanced digital cable transmission technologies |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 09/ 2012 |
| ITU-T | J.382 (J.atrans-spec) | Advanced digital downstream transmission systems for television, sound and data services for cable distribution |  | | |  | | X | |  | |  | |  | |  | |  | |  | |  | | X | |  |  | 01/2014 |
| ITU‑T | Q.512 | Digital exchange interfaces for subscriber access | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 02/1995 |
| ITU‑T | Q.551 | Transmission characteristics of digital exchanges | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 2001 |
| ITU‑T | Q.552 | Transmission characteristics at 2-wire analogue interfaces of digital exchanges | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 2001 |
| ITU‑T | Q.553 | Transmission characteristics at 4-wire analogue interfaces of digital exchanges | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 2001 |
| ITU‑T | Y.100 | General overview of the Global Information  Infrastructure standards development | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 06/1998 |
| ITU‑T | Y.110 | Global Information Infrastructure principles and  framework architecture | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 06/1998 |
| ITU‑T | Y.120 | Global Information Infrastructure scenario  methodology | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 06/1998  Corrigendum1  11/2000 |
| ITU‑T | Y.120  Annex A | Global information infrastructure scenario  methodology  Annex A: Examples of use | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 02/1999 |
| ITU-T | Y.2001 | General overview of NGN | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 12/2004 |
| ITU-T | Y.2002 | Overview of ubiquitous networking and of its support in NGN | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 10/2009 |
| ITU-T | Y.2006 | Description of capability set 1 of NGN release 1 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 02/2008 |
| ITU-T | Y.2007 | NGN capability set 2 | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 01/2010 |
| ITU-T | Y.2011 | General principles and general reference model for Next Generation Networks | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 10/2004 |
| ITU-T | Y.2012 | Functional requirements and architecture of next generation networks | X | | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  | |  |  | 04/2010 |
| ITU-T | V.90 | A digital modem and analogue modem pair for use on the public switched telephone network (PSTN) at data signaling rates up to 56000 bit/s downstream and up to 36600 bits/s upstream |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | Publication 1998 |
| ITU-T | V.91 | A digital modem operating at data signaling rates of up to 64 000 bit/s on a 4-wire circuit switched connection and on leased point-to-point 4-wire digital circuits |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | approval 1999 |
| ITU-T | V.92 | DATA COMMUNICATION OVER THE  TELEPHONE NETWORK  Simultaneous transmission of data and other signals  Enhancements to Recommendation V.90 |  | | |  | |  | | X | |  | |  | |  | |  | | X | |  | |  | |  |  | 11/2000 |

**Annex 2.2 - Standards related to ANT Infrastructure Elements**

Some of the listed Documents may not be publicly available. Interested people may contact the person mentioned under the responsible standardization group in the list of contacts in Section 3.1 of the ANT Standards Work Plan.

**Organization of ANT Relevant Standards by Transmission Medium and Infrastructure Elements  
 incl. Operation and Maintenance**

**General Aspects (Gen. Asp.)** = General aspects on network infrastructure, design and management  
**Medium:** **F**= Fiber; **C**= Coax; **P**= Twisted pair; **A**= Wireless  
**Infrastructure**: **N**= Network engineering and infrastructure elements including node equipment and devices; **E=** Power supply and energy management; **O**= Operation and maintenance including network management; **T** = Testing; **C**= Conformance and interoperability; **F** = Optical cable technology; **P** = Copper cable technology; **I** = Cable installation technique

| **Stds** | **Number** | **Title** | **Gen. Asp.** | **Medium** | | | | | **Infrastructure** | | | | | | | | | | **Public. Date** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Body** |  |  |  | **F** | | **C** | **P** | **A** | **N** | **E** | **O** | **T** | **C** | | | **F** | **P** | **I** |  |
| BBF | TR-xxx | Published BBF Technical Reports can be found at:  <https://www.broadband-forum.org/standards-and-software/technical-specifications/technical-reports> | X | X | | X | X | X | X | X | X | X | X | | |  |  |  |  |
| Cenelec | TR 50510 | Fibre optic access to end-user – A guideline to building of FTTX fibre optic network | X | X | |  |  |  | X | X |  |  |  | | | X |  | X | May 2012 |
| ETSI AT2 | TS 102 566 | Access, Terminals, Transmission and Multiplexing (ATTM) Common Requirements for Automated Distribution Frames (ADF) at Street Cabinet | X |  | |  | X |  | X |  | X |  |  | | |  |  |  | V1.1.1  (2007-09) |
| ETSI | EN 302 099 | Environmental Engineering (EE);  Powering of equipment in access network | X |  | |  |  |  | X | X |  |  |  | | |  |  |  | V2.1.1 (2014-08) |
| ETSI AT2 | ES 202 874-1 | Access, Terminals, Transmission and Multiplexing (ATTM); External Common Power Supply for Customer Premises Network and Access Equipment; Part 1: Functional Requirements | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2012-05) |
| ETSI AT2 | TS 102 874-3 | Access, Terminals, Transmission and Multiplexing (ATTM); External Common Power Supply for Customer Premises Network and Access Equipment; Part 3: CPS Type 1 implementation details | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2012-03) |
| ETSI AT2 | TS 102 874-4 | Access, Terminals, Transmission and Multiplexing (ATTM); External Common Power Supply for Customer Premises Network and Access Equipment; Part 4: CPS Type 2.b implementation details | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2012-03) |
| ETSI AT2 | TS 102 874-5 | Access, Terminals, Transmission and Multiplexing (ATTM); External Common Power Supply for Customer Premises Network and Access Equipment; Part 5: CPS Type 2.c implementation details | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2012-03) |
| ETSI AT2 | TS 102 874-6 | Access, Terminals, Transmission and Multiplexing (ATTM); External Common Power Supply for Customer Premises Network and Access Equipment; Part 6: CPS Type 2.d implementation details | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.1.1  (2012-02) |
| ETSI ATTM AT2 | TS 105 174-1 | Access, Terminals, Transmission and Multiplexing (ATTM); Broadband Deployment and Energy Management; Part 1: Overview, common and generic aspects | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2014-09) |
| ETSI ATTM AT2 | TR 105 174-2-1 | Access, Terminals, Transmission and Multiplexing (ATTM); Broadband Deployment - Energy Efficiency and Key Performance Indicators; Part 2: Network sites; Sub-part 1: Operator sites | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.1.1  (2009-10) |
| ETSI ATTM AT2 | TS 105 174-2-2 | Access, Terminals, Transmission and Multiplexing (ATTM); Broadband Deployment - Energy Efficiency and Key Performance Indicators; Part 2: Network sites; Sub-part 2: Data centres | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.1.1  (2009-10) |
| ETSI ATTM AT2 | TS 105 174-4-1 | Access, Terminals, Transmission and Multiplexing (ATTM); Broadband Deployment and Energy Management; Part 4: Access Networks; Sub-part 1: Fixed access networks (excluding cable | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2015-09) |
| ETSI AT2 | TR 105 174-5-1 | Access, Terminals, Transmission and Multiplexing (ATTM); Broadband Deployment - Energy Efficiency and Key Performance Indicators; Part 5: Customer network infrastructures; Sub-part 1: Homes (single-tenant) | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.1.1  (2009-10) |
| ETSI AT2 | TR 105 174-5-2 | Access, Terminals, Transmission and Multiplexing (ATTM); Broadband Deployment - Energy Efficiency and Key Performance Indicators; Part 5: Customer network infrastructures; Sub-part 2: Office premises (single-tenant) | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.1.1  (2009-10) |
| ETSI AT2 | TS 105 174-5-4 | Access, Terminals, Transmission and Multiplexing (ATTM); Broadband Deployment - Energy Efficiency and Key Performance Indicators; Part 5: Customer network infrastructures; Sub-part 4: Data centres (customer) | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.1.1  (2009-10) |
| ETSI ATTM AT2 | ES 205 200-1 | Access, Terminals, Transmission and Multiplexing (ATTM); Energy management; Global KPIs; Operational infrastructures; Part 1: General requirements | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2014-03) |
| ETSI ATTM AT2 | ES 205 200-2-1 | Access, Terminals, Transmission and Multiplexing (ATTM); Energy management; Global KPIs; Operational infrastructures; Part 2: Specific requirements; Sub-part 1: Data centres | X |  | |  |  |  |  | X | X |  |  | | |  |  |  | V1.2.1  (2014-03) |
| ETSI | EN 301 217-2 | V interfaces at the digital Service Node (SN); Interfaces at the VB5.2 reference point for the support of broadband or combined narrowband and broadband Access Networks (ANs); Part 2: Protocol Implementation Conformance Statement (PICS) proforma specification |  |  | |  | X |  |  |  |  |  | X | | |  |  |  | V1.1.3 (1999-09) |
| ETSI | EN 302 326-3 | Fixed Radio Systems; Multipoint Equipment and Antennas; Part 3: Harmonized EN covering the essential requirements of article 3.2 of the R&TTE Directive for Multipoint Radio Antennas |  |  | |  |  | X | X |  |  |  |  | | |  |  |  | V1.3.1 (02/2008) |
| ETSI | EN 301 754 | Telecommunications Management Network (TMN); Management interfaces associated with the VB5.2 reference point | X |  | |  | X |  |  |  | X |  |  | | |  |  |  | V1.1.1 (2001-09) |
| ETSI | ETR 240 | Transmission and Multiplexing (TM); Optical Access Networks (OANs); Operations and Maintenance (OAM) of OANs | X | X | |  |  |  |  |  | X |  |  | | |  |  |  | Edition 1 (1996-04) |
| ETSI AT2 | ES 203 069 | Access, Terminals, Transmission and Multiplexing (ATTM); Remote management of CPE over broadband networks; CPE WAN Management Protocol (CWMP) | X |  | |  |  |  |  |  | X |  |  | | |  |  |  | V1.2.1  (2011-09) |
| ETSI | ETR 240 | Transmission and Multiplexing (TM); Operations and maintenance of Optical Access Networks | X | X | |  |  |  |  |  | X |  |  | | |  |  |  | Edition 1  (1996-04) |
| ETSI | ETS 300 150 | Transmission and Multiplexing (TM); Protocol suites for Q interfaces for management of transmission systems | X |  | |  |  |  |  |  | X |  |  | | |  |  |  | Edition 1  (1992-11) |
| ETSI | ETS 300 376‑1 | Q3 interface at the Access Network (AN) for configuration management of V5 interfaces and associated user ports; Part 1: Q3 interface specification | X |  | |  |  |  |  |  | X |  |  | | |  |  |  | Edition 1  (1994-12) |
| ETSI | ETS 300 377‑1 | Q3 interface at the Local Exchange (LE) for configuration management of V5 interfaces and associated customer profiles; Part 1: Q3 interface specification | X |  | |  |  |  |  |  | X |  |  | | |  |  |  | Edition 1  (1994-12) |
| ETSI | ETS 300 378‑1 | Q3 interface at the Access Network (AN) for fault and performance management of V5 interfaces and associated user ports; Part 1: Q3 interface specification | X |  | |  |  |  |  |  | X |  |  | | |  |  |  | Edition 1  (1995-11) |
| ETSI | ETS 300 379‑1 | Q3 interface at the Local Exchange (LE) for fault and performance management of V5 interfaces and associated customer profiles; Part 1: Q3 interface specification | X |  | |  |  |  |  |  | X |  |  | | |  |  |  | Edition 1  (1995-11) |
| ETSI | TS 100 783 | Transmission and Multiplexing (TM); Passive optical components; Fibre optic fusion splices for single-mode optical fibre transmission systems for indoor and outdoor applications; Common requirements and conformance testing |  | X | |  |  |  | X |  |  | X |  | | | X |  | X | V1.2.1 (2004-08) |
| ETSI | TS 101 263 | Transmission and Multiplexing (TM); Passive optical components; Fibre optic mechanical splices for single-mode optical fibre communications systems for indoor and outdoor applications; Common requirements and conformance testing |  | X | |  |  |  | X |  |  | X |  | | | X |  | X | V1.2.1 (2004-07) |
| ETSI | ES 201 792 | Transmission and Multiplexing (TM); Passive optical components; Fibre optic patchcords for single mode optical fibre communication systems; Common requirements and conformance testing |  | X | |  |  |  | X |  |  | X |  | | | X |  |  | V1.1.1  (2000-08) |
| ETSI | ES 201 286 | Transmission and Multiplexing ™; Passive optical components; Connector-type optical fixed attenuators for single-mode optical fibre communications systems; Common requirements and conformance testing |  | X | |  |  |  | X |  |  | X |  | | | X |  |  | V1.1.1  (1999-06) |
| ETSI | ES 202 319 | Transmission and Multiplexing (TM); Passive optical components and cables; Optical fibre cables to be used for patchcord applications for single-mode optical fibre communication systems; Common requirements and conformance testing |  | X | |  |  |  | X |  |  | X |  | | | X |  |  | V1.1.1  (2004-06) |
| ETSI | ETS 300 644 | Transmission and Multiplexing (TM); Optical fibre cables for indoor applications |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | Edition 1  (1997-06) |
| ETSI | TS 101 573 | Access, Terminals, Transmission and Multiplexing (ATTM); General engineering of optical building cabling | X | X | |  |  |  | X |  |  |  |  | | | X |  | X | V1.1.1  (2012-09) |
| ETSI AT2 | TS 102 872 | Transmission and Multiplexing (ATTM); Copper External Network Testing Interface |  |  | |  | X |  |  |  | X | X |  | | |  |  |  | V1.1.1  (2010-07) |
| ETSI AT2 | TS 102 873 | Transmission and Multiplexing (ATTM); Optical External Network Testing |  | X | |  |  |  |  |  | X | X |  | | |  |  |  | V1.1.1  (2010-10) |
| ETSI ATTM | TS 101 548 | Access, Terminals, Transmission and Multiplexing (ATTM); European Requirements for Reverse Powering  of Remote Access Equipment | X |  | |  |  |  |  | X |  |  |  | | |  |  |  | V2.1.1 (2016-09) |
| ETSI ATTM | TS 101 548-1 | Access, Terminals, Transmission and Multiplexing (ATTM); European Requirements for Reverse Powering of Remote Access Equipment; Part 1: Twisted pair networks | X |  | |  |  |  |  | X |  |  |  | | |  |  |  | V2.2.1 (2018-06) |
| ICEA | S-84-608-2017 | Telecommunications Cable Filled, Polyolfin Insulated, Copper Conductor Technical Requirements |  |  | |  | X |  |  |  |  |  |  | | |  | X |  | January 1, 2017 |
| ICEA | S-85-625-2016 | Telecommunications Cable, Aircore Polyolefin Insulated, Copper Conductor Technical Requirements |  |  | |  | X |  |  |  |  |  |  | | |  | X |  | March 8, 2016 |
| ICEA | S-86-634-2001 | Buried Telecommunications Wire Filled, Polyolefin Insulated, Copper Conductor Technical Requirements |  |  | |  | X |  |  |  |  |  |  | | |  | X |  | January 1, 2011 |
| IEC | TR 62691 Edition 2.0 | Optical fibre cables – Guidelines to the installation of optical fibre cables |  | X | |  |  |  | X |  |  |  |  | | | X |  | X | 06/2016 |
| IEC | TR 62901  Edition 1.0 | Guidance for the selection of drop cables |  | X | |  |  |  | X |  |  |  |  | | | X |  | X | 03/2016 |
| IEEE | 802.16.2-2004 | IEEE Recommended Practice for Local and Metropolitan Area Networks Coexistence of Fixed Broadband Wireless Access Systems | X |  | |  |  | X | X |  | X |  |  | | |  |  |  | 03/2004  Reaffirmed: 03/2010 |
| IEEE | 1904.1-2017 | IEEE Standard for Service Interoperability in Ethernet Passive Optical Networks (SIEPON) |  | X | |  |  |  |  |  | X |  | X | | |  |  |  | 07/2017 |
| ITU-R | F.1400 | Performance and availability objectives for FWA to PSTN |  |  | |  |  | X | X |  | X |  |  | | |  |  |  | 05/99 |
| ITU-R | F.1569 | Technical and operational characteristics for the fixed service using high altitude platform stations in the band 27.5-28.5 and 31.0-31.3 GHz |  |  | |  |  | X | X |  | X |  |  | | |  |  |  | 05/02 |
| ITU-R | F.2058 (Report) | Design techniques applicable to broadband fixed wireless access systems conveying Internet protocol packets or asynchronous transfer mode cells |  |  | |  |  | X | X |  | X |  |  | | |  |  |  | 2006 |
| ITU-R | F.2086-1 (Report) | Technical and operational requirements for broadband wireless access in the fixed service | X |  | |  |  | X | X |  | X |  |  | | |  |  |  | 2010 |
| ITU-R | F.2106-1 (Report) | Fixed Service applications using free-space optical links | X |  | |  |  | X | X |  | X |  |  | | |  |  |  | 2010 |
| ITU-R | F.2107-1 (Report) | Characteristics and applications of fixed wireless systems operating in the 57 GHz to 130 GHz bands |  |  | |  |  | X | X |  | X |  |  | | |  |  |  | 2012 |
| ITU-R | F.2060 (Report) | Fixed Service use in the IMT-2000 transport network | X |  | |  |  | X | X |  | X |  |  | | |  |  |  | 2005 |
| ITU-R | F.2106-1 (Report) | Fixed Service applications using free-space optical links | X |  | |  |  | X | X |  | X |  |  | | |  |  |  | 2010 |
| ITU-R | F.2107-1 (Report) | Characteristics and applications of fixed wireless systems operating in the 57 GHz to 130 GHz bands |  |  | |  |  | X | X |  | X |  |  | | |  |  |  | 2012 |
| ITU‑R | [M.818-2](http://www.itu.int/rec/R-REC-M.818/en) | Satellite operation within IMT‑2000 | X |  | |  |  | X | X |  | X |  |  | | |  |  |  | 06-2003 |
| ITU‑R | [M.1036-](http://www.itu.int/rec/R-REC-M.1036/en)4 | Frequency arrangements for implementation of the terrestrial component of International Mobile Telecommunications-2000 (IMT-2000) in the bands  806-960 MHz, 1 710-2 025 MHz, 2 110-2 200 MHz and 2 500-2 690 MHz |  |  | |  |  | X | X |  |  |  |  | | |  |  |  | 03/2012 |
| ITU-R | [M.1079-2](http://www.itu.int/rec/R-REC-M.1079/en) | Performance and quality of service requirements for International Mobile Telecommunications-2000  (IMT-2000) |  |  | |  |  | X | X |  | X |  |  | | |  |  |  | 06-2003 |
| ITU‑R | [M.1225](http://www.itu.int/rec/R-REC-M.1225/en) | Guidelines for evaluation of radio transmission technologies for IMT-2000 | X |  | |  |  | X | X |  |  |  |  | | |  |  |  | 02-1997 |
| ITU‑R | [M.1390](http://www.itu.int/rec/R-REC-M.1390/en) | Methodology for the Calculation of IMT‑2000 Terrestrial Spectrum Requirements |  |  | |  |  | X | X |  |  |  |  | | |  |  |  | 01-1999 |
| ITU‑R | [M.1391-1](http://www.itu.int/rec/R-REC-M.1391/en) | Methodology for the Calculation of IMT‑2000 Satellite Spectrum Requirements |  |  | |  |  | X | X |  |  |  |  | | |  |  |  | 03-2006 |
| ITU‑R | [M.1454](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1454) | E.i.r.p. density limit and operational restrictions for RLANs or other wireless access transmitters in order to ensure the protection of feeder links of NGSO systems in the MSS in the frequency band 5 150-5 250 MHz |  |  | |  |  | X | X |  |  |  |  | | |  |  |  | 2000 |
| ITU‑R | [M.1651](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1651) | A method for assessing the required spectrum for broadband NWA systems including RLANs using the 5 GHz band |  |  | |  |  | X | X |  |  |  |  | | |  |  |  | 2003 |
| ITU‑R | [M.1653](http://www.itu.int/rec/recommendation.asp?type=folders&lang=e&parent=R-REC-M.1653) | Operational and deployment requirements for WAS including RLANs in the MS to facilitate sharing between these systems and systems in the EESS (active) and the SRS (active) in the band 5 470-5 570 MHz within the 5 460‑5 725 MHz range |  | |  |  |  | X | X |  | X |  |  | | |  |  |  | 2003 |
| ITU-R | [M.1768](http://www.itu.int/rec/R-REC-M.1768/en) | Methodology for calculation of spectrum requirements for the future development of the terrestrial component of IMT-2000 and systems beyond IMT-2000 |  |  | |  |  | X | X |  |  |  |  | | |  |  |  | 03-2006 |
| ITU-T | G.107 (06/2015) | The E-model: a computational model for use in transmission planning | X |  | |  |  |  | X |  |  |  |  | | |  |  |  | 06/2015 |
| ITU-T | G.108 (09/1999) | Application of the E-model: A planning guide | X |  | |  |  |  | X |  |  |  |  | | |  |  |  | 09/1999  Erratum 1 12/2000 |
| ITU-T | G.108 (1999)  Amendment 1 | Application of the E-model: A planning guide Amendment 1: New Appendix I - The relationship between and interaction of talker echo and absolute delay |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 09/2003 |
| ITU-T | G.108 (1999)  Amendment 2 | Application of the E-model: A planning guide Amendment 2: New Appendix II - Planning examples regarding delay in packet-based networks |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 03/2004 |
| ITU-T | G.108.1 | Guidance for assessing conversational speech transmission quality effects not covered by the E-model |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 05/2000 |
| ITU-T | G.108.2 (03/2007) | Transmission planning aspects of echo cancellers |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 03/2007 |
| ITU-T | G.108.2 (2007)  Amendment 1 | Transmission planning aspects of echo cancellers  Amendment 1: New Appendix III - Guidance for using echo cancellers to prevent low-level echo |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 10/2007 |
| ITU-T | G.109 (1999) | Definitions of categories of speech transmission quality | X |  | |  |  |  | X |  |  |  |  | | |  |  |  | 09/1999 |
| ITU-T | G.109 (1999)  Amendment 1 | Definitions of categories of speech transmission quality  Amendment1: New Appendix I – The E-model-based quality contours for predicting speech transmission quality and user satisfaction from time-varying transmission impairments | X |  | |  |  |  | X |  |  |  |  | | |  |  |  | 01/2007 |
| ITU‑T | G.114 (05/2003) | One-way transmission time |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 05/2003 |
| ITU‑T | G.114 (2003)  Amendment 1 | One-way transmission time  Amendment 1 |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 09/2003 |
| ITU‑T | G.114 (2003)  Amendment 2 | One-way transmission time  Amendment 2: New Appendix III – Delay variation on unshared access lines |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 11/2009 |
| ITU‑T | G.131 | Talker echo and its control |  |  | |  |  |  | X |  |  |  |  | | |  |  |  | 11/2003 |
| ITU‑T | G.174 | Transmission Performance Objectives for Terrestrial Digital Wireless Systems Using Portable Terminals to Access the PSTN |  |  | |  |  |  | X |  | X |  |  | | |  |  |  | 06/1994 |
| ITU‑T | G.601 | Terminology for cables | X | X | | X | X |  | X |  |  |  |  | | | X | X |  | 11/1988 |
| ITU‑T | G.602 | Reliability and availability of analogue cable transmission systems and associated equipments |  |  | |  | X |  | X |  | X |  |  | | |  |  |  | 11/1988 |
| ITU‑T | G.611 | Characteristics of symmetric cable pairs for analogue transmission |  |  | |  | X |  | X |  |  |  |  | | |  | X |  | 11/1988 |
| ITU‑T | G.612 | Characteristics of symmetric cable pairs designed for the transmission of systems with bit rates of the order of 6 to 34 Mbit/s |  |  | |  | X |  | X |  |  |  |  | | |  | X |  | 11/1988 |
| ITU‑T | G.613 | Characteristics of symmetric cable pairs usable wholly for the transmission of digital systems with a bit rate of up to 2 Mbit/s |  |  | |  | X |  | X |  |  |  |  | | |  | X |  | 11/1988 |
| ITU‑T | G.614 | Characteristics of symmetric pair star-quad cables designed earlier for analogue transmission systems and being used now for digital system transmission at bit rates of 6 to 34 Mbit/s |  |  | |  | X |  | X |  |  |  |  | | |  | X |  | 11/1988 |
| ITU‑T | G.621 | Characteristics of 0.7/2.9 mm coaxial cable pairs |  |  | | X |  |  | X |  |  |  |  | | |  | X |  | 11/1988 |
| ITU‑T | G.622 | Characteristics of 1.2/4.4 mm coaxial cable pairs |  |  | | X |  |  | X |  |  |  |  | | |  | X |  | 11/1988 |
| ITU‑T | G.623 | Characteristics of 2.6/9.5 mm coaxial cable pairs |  |  | | X |  |  | X |  |  |  |  | | |  | X |  | 11/1988 |
| ITU-T | Technical report (2015) | Technical Report on Optical fibres, cables and systems | X | X | |  |  |  | X |  |  |  |  | | | X |  |  | 2015 |
| ITU-T | G Suppl. 59 (02/2018) | Guidance on optical fibre and cable reliability | X | X | |  |  |  | X |  |  |  |  | | | X |  |  | 02/2018 |
| ITU‑T | G.650.1 (03/2018) | Definitions and test methods for linear, deterministic attributes of single-mode fibre and cable | X | X | |  |  |  | X |  |  | X |  | | | X |  |  | 03/2018 |
| ITU‑T | G.650.2 (08/2015) | Definitions and test methods for statistical and non-linear related attributes of single mode fibre and cable | X | X | |  |  |  | X |  |  | X |  | | | X |  |  | 08/2015 |
| ITU‑T | G.650.3 (08/2017) | Test methods for installed single-mode optical  fibre cable links | X | X | |  |  |  | X |  |  | X |  | | | X |  |  | 08/2017 |
| ITU‑T | G.651.1 (07/2007) | Characteristics of a 50/125 µm multimode graded index optical fibre cable for the optical access network |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 07/2007 |
| ITU‑T | G.651.1 (2007)  Amendment 1 | Characteristics of a 50/125 μm multimode graded  index optical fibre cable for the optical access  network  Amendment 1: New Appendix I – Historical  perspective on the evolution of the specification  of multimode optical fibre cable |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 12/2008 |
| ITU‑T | G.652 (11/2016) | Characteristics of a single-mode optical fibre and cable |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 11/2016  Supersedes  11/2009 |
| ITU‑T | G.657 (11/2016) | Characteristics of a bending-loss insensitive single-mode optical fibre and cable for the access network |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 11/2016  Supersedes  10/2012 |
| ITU‑T | G.772 | Protected monitoring points provided on digital transmission systems |  |  | |  |  |  | X |  |  | X |  | | |  |  |  | 03/1993 |
| ITU‑T | G.773 | Protocol suites for Q-interfaces for management of transmission systems |  |  | |  |  |  | X |  |  | X |  | | |  |  |  | 03/1993 |
| ITU‑T | G.821 | Error performance of an international digital connection operating at a bit rate below the primary rate and forming part of an Integrated Services Digital Network |  |  | |  |  |  | X |  | X | X |  | | |  |  |  | 12/2002 |
| ITU‑T | G.826 | End-to-end error performance parameters and objectives for international, constant bit-rate digital paths and connections |  |  | |  |  |  | X |  | X | X |  | | |  |  |  | 12/2002 |
| ITU‑T | G.827 | Availability parameters and objectives for path elements of international constant bit-rate digital paths at or above the primary rate |  |  | |  |  |  | X |  | X | X |  | | |  |  |  | 09/2003 |
| ITU‑T | G.901 | General considerations on digital sections and digital line systems Blue Book Fascicle III.5 | X |  | |  |  |  | X |  | X |  |  | | |  |  |  | 11/1988 |
| ITU‑T | G.902 | Framework Recommendation on functional access networks (AN) - Architecture and functions, access types, management and service node aspects | X |  | |  |  |  | X |  | X |  |  | | |  |  |  | 11/1995 |
| ITU-T | G Suppl. 39 (02/2016) | Optical system design and engineering considerations | X | X | |  |  |  | X |  |  |  |  | | |  |  |  | 02/2016 |
| ITU‑T | G.911 | Parameters and calculation methodologies for reliability and availability of fibre optic systems |  | X | |  |  |  | X |  | X |  |  | | |  |  |  | 04/ 1997 |
| ITU-T | G.983.2 (07/2005) | ONT management and control interface specification for B-PON |  | X | |  |  |  |  |  | X |  |  | | |  |  |  | 07/2005  Erratum 1  06/2006 |
| ITU-T | G.983.2 (2005)  Amendment 1 | ONT management and control interface specification for B-PON  Amendment 1: Omnibus improvements for OMCI |  | X | |  |  |  |  |  | X |  |  | | |  |  |  | 03/2006 |
| ITU-T | G.983.2 (2005)  Amendment 2 | ONT management and control interface specification for B-PON  Amendment 2 |  | X | |  |  |  |  |  | X |  |  | | |  |  |  | 01/2007 |
| ITU-T | G.Imp983.2 (02/2006) | Implementers’ Guide for ITU-T Rec. G.983.2 (07/2005)  ONT management and control interface specification for B-PON |  | X | |  |  |  |  |  | X |  |  | | |  |  |  | 02/2006 |
| ITU-T | G.988 (11/2017) | ONU management and control interface (OMCI)  specification |  | X | |  |  |  |  |  | X |  |  | | |  |  |  | 11/2017 |
| ITU-T | G Suppl. 44 (06/2007) | Test plan to verify B-PON interoperability |  | X | |  |  |  |  |  |  | X | X | | |  |  |  | (06/2007) |
| ITU-T | G Suppl. 46 (05/2009) | G-PON interoperability test plan between optical line terminations and optical network units |  | X | |  |  |  |  |  |  | X | X | | |  |  |  | (05/2009) |
| ITU-T | G. Suppl. 51 (06/2017) | Passive optical network protection consideration |  | X | |  |  |  | X | X |  |  |  | | |  |  |  | 06/2017 |
| ITU-T | G.995.2 (08/2015) | Enhanced common mode limits and measurement methods for customers premises equipment operating on copper pairs |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 08/2015 |
| ITU-T | G.996.1 | Test procedures for digital subscriber line (DSL)  transceivers |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 02/2001  Erratum 1  01/2003 |
| ITU-T | G.996.1  Amendment 1 | Test procedures for digital subscriber line (DSL)  transceivers  Amendment 1: New Annex B |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 03/2003 |
| ITU-T | G.996.2 (05/2009) | Single-ended line testing for digital subscriber lines (DSL) (This Recommendation includes the annexes E and F introduced by Amendment 1 (10/2009)) |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 05/2009  Includes  Amendment 1  10/2009  Corrigendum 1 (06/2018) |
| ITU-T | G.996.2 (2009)  Amendment 2 | Single-ended line testing for digital subscriber lines (DSL)  Amendment 2 |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 04/2012 |
| ITU-T | G.996.2 (2009)  Amendment 3 | Single-ended line testing for digital subscriber lines  (DSL)  Amendment 3: Definition of accuracy values for  MELT-PMD and MELT-P in Annex E |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 03/2013 |
| ITU-T | G.996.2 (2009)  Amendment 4 | Single-ended line testing for digital subscriber  lines (DSL)  Amendment 4: Updates to Annex E |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 08/2013 |
| ITU-T | G.996.2 (2009)  Amendment 5 | Single-ended line testing for digital subscriber  lines (DSL)  Amendment 5 |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 12/2017 |
| ITU-T | G.996.2 (2009)  Amendment 6 | Single-ended line testing for digital subscriber  lines (DSL)  Amendment 6 |  |  | |  | X |  |  |  |  | X |  | | |  |  |  | 06/2018 |
| ITU-T | G.997.1 (11/2016) | Physical layer management for digital subscriber line transceivers  This edition of this Recommendation integrates ITU-T G.997.1 (2012) and all its amendments and corrigenda. It does not add any new technical material. |  |  | |  | X |  | X |  | X |  |  | | |  |  |  | 11/2016 Corrigendum 1  03/2018 |
| ITU-T | G.997.1 (2016) Amendment 1 | Physical layer management for digital subscriber line transceivers: Amendment 1 |  |  | |  | X |  | X |  | X |  |  | | |  |  |  | 12/2017 |
| ITU-T | G.997.1  Amendment 2 (05/2018) | Physical layer management for digital subscriber line transceivers  Amendment 2 |  |  | |  | X |  | X |  | X |  |  | | |  |  |  | 05/2018 |
| ITU-T | G.997.2 (05/2015) | Physical layer management for G.fast transceivers |  |  | | X | X |  | X |  | X |  |  | | |  |  |  | 05/2015 Corrigendum 1 03/2016  Corrigendum 2 12/2016  Corrigendum 3  08/2017  Corrigendum 4  03/2018 |
| ITU-T | G.997.2 (2015)  Amendment 1 | Physical layer management for G.fast transceivers  Amendment 1 |  |  | | X | X |  | X |  | X |  |  | | |  |  |  | 05/2016 |
| ITU-T | G.997.2 (2015)  Amendment 2 | Physical layer management for G.fast transceivers  Amendment 2 |  |  | | X | X |  | X |  | X |  |  | | |  |  |  | 07/2016 |
| ITU-T | G.997.2 (2015)  Amendment 3 | Physical layer management for G.fast transceivers  Amendment 3 |  |  | | X | X |  | X |  | X |  |  | | |  |  |  | 04/2017 |
| ITU-T | G.997.2 (2015)  Amendment 4 | Physical layer management for G.fast transceivers  Amendment 4 |  |  | | X | X |  | X |  | X |  |  | | |  |  |  | 12/2017 |
| ITU-T | G.997.2 (2015)  Amendment 5 | Physical layer management for G.fast transceivers  Amendment 5 |  |  | | X | X |  | X |  | X |  |  | | |  |  |  | 08/2018 |
| ITU-T | G.Supp.62 (02/2018) | Gfast Certification |  |  | | X | X |  |  |  |  |  | X | | |  |  |  | 02/2018 |
| ITU‑T | G.8011.1/Y.1307 (11/2016) | Ethernet service characteristics | X |  | |  |  |  | X |  | X |  |  | | |  |  |  | 11/2016 |
| ITU‑T | G.8012/Y.1308 (08/2004) | Ethernet UNI And Ethernet Over Transport NNI | X |  | |  |  |  | X |  | X |  |  | | |  |  |  | 08/2004 |
| ITU‑T | G.8012/Y.1308 (2004)  Amendment 1 | Ethernet UNI And Ethernet Over Transport NNI  Amendment 1 | X |  | |  |  |  | X |  | X |  |  | | |  |  |  | 05/2006 |
| ITU‑T | G.8012/Y.1308 (2004)  Amendment 2 | Ethernet UNI And Ethernet Over Transport NNI  Amendment 2 | X |  | |  |  |  | X |  | X |  |  | | |  |  |  | 11/2016 |
| ITU-T | G.9801(08/2013) | Ethernet passive optical networks using OMCI |  | X | |  |  |  |  |  | X |  | X | | |  |  |  | 08/2013 |
| ITU-T | G.9801 Impl. Guide  (ex G.epon) (12/2104) | Conformance and interoperability test plans for OMCI-EPON |  | X | |  |  |  |  |  | X |  | X | | |  |  |  | 12/2014 |
| ITU-T | H.610 | Full-Service VDSL - System architecture and customer premises equipment |  |  | |  | X |  | X |  | X |  |  | | |  |  |  | 07/2003 |
| ITU-T | H.611 | Full-Service VDSL - Operations, Administration Maintenance & Provision aspects |  |  | |  | X |  | X |  | X |  |  | | |  |  |  | 07/2003 |
| ITU‑T | I.610 | B-ISDN operation and maintenance principles and functions |  |  | |  | X |  |  |  | X |  |  | | |  |  |  | 02/1999  Corrigendum 1  03/2000 |
| ITU‑T | I.610  Amendments 1, 2 | B-ISDN operation and maintenance principles and functions  Amendments 1, 2 |  |  | |  | X |  |  |  | X |  |  | | |  |  |  | Amd. 1 03/2000  Amd. 2 12/2006 |
| ITU-T | K.23 (11/1988) | Types of induced noise and description of noise voltage parameters for ISDN basic user networks |  |  | |  | X |  | X |  |  |  |  | | |  |  |  | 11/1988 |
| ITU-T | K.27 (03/2015) | Bonding configurations and earthing inside a telecommunication building  Q4/5 states that this is valid for UNI and NNI |  |  | |  |  |  | X |  | X |  |  | | |  |  | X | 03/2015 |
| ITU-T | K.34 (07/2003) | Classification of electromagnetic environmental conditions for telecommunications equipment - Fast transient and radio frequency phenomena |  |  | |  |  |  | X |  | X |  |  | | |  |  |  | 07/2003 |
| ITU-T | K.35 (05/1996) | Bonding configurations and earthing at remote electronic sites |  |  | |  |  |  | X |  | X |  |  | | |  |  | X | 05/1996 |
| ITU-T | K.38 (10/1996) | Radiated emission test procedure for physically large systems |  |  | |  |  |  | X |  |  | X |  | | |  |  |  | 10/1996 |
| ITU-T | K.43(07/2009) | Immunity requirements for telecommunication equipment |  |  | |  |  |  | X |  | X |  |  | | |  |  |  | 07/2009 |
| ITU-T | K 47 (05/2012) | Protection of telecommunication lines against direct lightning flashes |  |  | |  |  |  | X |  | X |  |  | | |  |  | X | 05/2012 |
| ITU-T | K.50 (12/2016) | Safe limits for operating voltages and currents of telecommunication systems powered over the network |  |  | |  |  |  | X | X | X |  |  | | |  |  |  | 12/2016 |
| ITU-T | K.51(06/2016) | Safety criteria for telecommunication equipment |  |  | |  |  |  | X |  | X |  |  | | |  |  |  | 06/2016 |
| ITU-T | K.48 (09/2006) | EMC requirements for telecommunication equipment - Product family Recommendation |  |  | |  |  |  | X |  | X |  |  | | |  |  |  | 09/2006 |
| ITU-T | K.20 (07/2017) | Resistibility of telecommunication equipment installed in a telecommunication centre to overvoltages and overcurrents |  |  | |  |  |  | X | X | X |  |  | | |  |  |  | 07/2017 |
| ITU-T | K.45 (12/2016) | Resistibility of telecommunication equipment installed in the access and trunk networks to overvoltages and overcurrents |  |  | |  |  |  | X | X | X |  |  | | |  |  |  | 12/2016 |
| ITU-T | K.73 (04/2008) | Shielding and bonding for cables between buildings |  | X | | X | X |  | X |  | X |  |  | | | X | X | X | 04/2008 |
| ITU-T | K 188 (12/2016) | Requirements for lightning protection of fibre to the distribution point equipment |  | X | |  |  |  | X |  | X |  |  | | | X |  | X | 12/2016 |
| ITU-T | Technical report (2017) | Guide on the use of ITU-T L-series Recommendations related to optical technologies for outside plant | X | X | | X | X |  | X |  |  |  |  | | | X | X | X | 2017 |
| ITU-T | L.19 (05/2010) | Multi-pair copper nework cable supporting shared multiple services such as POTS, ISDN and xDSL |  |  | |  | X |  | X |  |  |  |  | | |  | X |  | 05/2010 |
| ITU-T | L.75 (05/2008) | Test, acceptance and maintenance methods of copper subscriber pairs |  |  | |  | X |  | X |  | X | X |  | | |  | X |  | 05/2008 |
| ITU-T | L.76 (05/2008) | Copper loop requirements for various technologies including indoor and structured cabling |  |  | |  | X |  | X |  |  |  |  | | |  | X |  | 05/2008 |
| ITU-T | L.100/L10 (08/2015) | Optical fibre cables for duct and tunnel application |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 08/2015 |
| ITU-T | L.101/L.43 (08/2015) | Optical fibre cables for buried application |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 08/2015 |
| ITU-T | L.102/L.26 (08/2015) | Optical fibre cables for aerial application |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 08/2015 |
| ITU-T | L.103 (04/2016) | Optical fibre cables for indoor applications |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 04/2016  Supersedes L.59 |
| ITU-T | L.104/L.67  (10/20006) | Small count optical fibre cables for indoor applications |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 10/2006 |
| ITU-T | L.105/L.87 (07/2010) | Optical fibre cables for drop applications |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 07/2010 |
| ITU-T | L.106/L.58  (03/2004) | Optical fibre cables: Special needs for access networks |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 03/2004 |
| ITU-T | L.107/L.78  (05/2008) | Optical fibre cable construction for sewer duct applications |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 05/2008 |
| ITU-T | L.107/L.78 (2008)  Amendment 1 | Optical fibre cable construction for sewer duct applications  Amendement 1 |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 06/2010 |
| ITU-T | L.108(03/2018) | Optical fibre cable elements for microduct blowing-installation application |  | X | |  |  |  | X |  |  |  |  | | | X |  |  | 03/2018 |
| ITU-T | L.109/L.60 (09/2004) | Construction of optical/metallic hybrid cables |  | X | | X | X |  | X |  |  |  | |  | | X | X |  | 09/2004 |
| ITU-T | L.110 (08/2017) | Optical fibre cables for direct surface application |  | X | |  |  |  | X |  |  |  | |  | | X |  |  | 08/2017 |
| ITU-T | L.150/L.35 (10/1998) | Installation of optical fibre cables in the access network |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 10/ 1998 |
| ITU-T | L.150/L.35 (1998)  Amendment 1 | Installation of optical fibre cables in the access network  Amendment 1 |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 11/2007 |
| ITU-T | L.151/L.34 (10/1998) | Installation of Optical Fibre Ground Wire (OPGW) cable |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 10/1998 |
| ITU-T | L.152/L.38 (09/1999) | Use of trenchless techniques for the construction of underground infrastructures for telecommunication cable installation |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 09/1999 |
| ITU-T | L.153/L.48 (03/2003) | Mini-trench installation technique |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 03/2003 |
| ITU-T | L.154/L.49 (03/2003) | Micro-trench installation technique |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 03/2003 |
| ITU-T | L.155 (11/2016) | Low impact trenching technique for FTTx networks |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 11/2016 |
| ITU-T | L.156 (03/2018) | Air-assisted installation of optical fibre cables |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 03/2018 |
| ITU-T | L.157/L.61 (07/2004) | Optical fibre cable installation by floating technique |  | X | |  |  |  | X |  |  |  |  | | | X |  | X | 07/2004 |
| ITU-T | L.158/L.56 (05/2003) | Installation of optical fibre cables along railways |  | X | |  |  |  | X |  |  |  |  | | | X |  | X | 05/2003 |
| ITU-T | L.159/L.77  (05/2008) | Installation of cables in sewer ducts |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 05/2008 |
| ITU-T | L.160/L.82 (07/2010) | Optical cabling shared with multiple operators in buildings |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 07/2010 |
| ITU-T | L.160/L.82 (2010)  Amendment 1 | Optical cabling shared with multiple operators in buildings  Amendment 1 |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 12/2014 |
| ITU-T | L.161/L.46 (10/2000) | Protection of telecommunication cables and plant from biological attack |  | X | | X | X |  | X |  |  |  | | |  | X | X | X | 10/2000 |
| ITU-T | L.162 (11/2016) | Microduct technology and its applications |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 11/2016 |
| ITU-T | L.200/L.51 (04/2003) | Passive node elements for fibre optic networks – General principles and definitions for characterization and performance evaluation |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 04/2003 |
| ITU-T | L.201/L.13 (04/2003) | Performance requirements for passive optical nodes: Sealed closures for outdoor environments |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 04/2003 |
| ITU-T | L.202/L.50  (07/2010) | Requirements for passive optical nodes: Optical distribution frames for central office environments |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 07/2010 |
| ITU-T | L.203/L.44 (10/2000) | Electric power supply for equipment installed as outside plant |  |  | |  |  |  | X | X |  |  | | |  |  |  |  | 10/2000 |
| ITU-T | L.204/L.70 (11/2007) | Managing active electronics in the outside plant |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 11/2007 |
| ITU-T | L.205/L.11 (11/1988) | Joint use of tunnels by pipelines and telecommunication cables, and the standardization of underground duct plans |  |  | |  |  |  | X |  | X |  | | |  | X | X | X | 11/1988 |
| ITU-T | L.206 (08/2017) | Requirements for passive optical nodes – Outdoor optical cross-connect cabinet |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 08/2017 |
| ITU-T | L.207 (03/2018) | Passive node elements with automated ID tag detection |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 03/2018 |
| ITU-T | L.250/L.90 (02/2012) | Optical access network topologies for broadband services | X | X | |  |  |  | X |  |  |  | | |  |  |  |  | 02/2012 |
| ITU-T | L.251/L.72  (01/2008) | Databases for optical access network infrastructure |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 01/2008 |
| ITU-T | L.252/L.86  (07/2010) | Considerations on the installation site of branching components in passive optical networks for fibre to the home |  | X | |  |  |  | X |  |  |  | | |  |  |  |  | 07/2010 |
| ITU-T | L.253/L.47 (10/2000) | Access facilities using hybrid fibre/copper networks |  | X | | X | X |  | X |  |  |  | | |  |  |  |  | 10/2000 |
| ITU-T | L.254/L.62  (09/2004) | Practical aspects of unbundling services by multiple operators in copper access networks |  |  | |  | X |  | X |  |  |  |  | | |  |  |  | 09/2004 |
| ITU-T | L.255/L.17 (06/1995) | Implementation of connecting customers into the public switched telephone network (PSTN) via optical fibres |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 06/1995  Appendix 02/1997 |
| ITU-T | L.256/L.45 (10/2000) | Minimizing the effect on the environment from the outside plant in telecommunication networks | X |  | |  |  |  | X |  |  |  | | |  |  |  |  | 10/2000 |
| ITU-T | L.257/L.39 (05/2000) | Investigation of the soil before using trenchless techniques |  |  | |  |  |  | X |  |  |  | | |  |  |  | X | 05/2000 |
| ITU-T | L.258/L.63 (10/2004) | Safety procedures for outdoor installations |  |  | |  |  |  | X |  |  |  |  | | |  |  | X | 10/2004 |
| ITU-T | L.259/L.73 (04/2008) | Methods for inspecting and repairing underground plastic ducts |  |  | |  |  |  | X |  | X |  |  | | |  |  | X | 04/2008 |
| ITU-T | L.260/L.84 (07/2010) | Fast mapping of underground networks |  |  | |  |  |  | X |  | X |  | | |  |  |  | X | 07/2010 |
| ITU-T | L.261/L.89 (02/2012) | Design of suspension wires, telecommunication poles and guy-lines for optical access networks |  | X | |  |  |  | X |  |  |  | | |  | X |  | X | 02/2012 |
| ITU-T | L.262/L.94 (01/2015) | Use of global navigation satellite systems to create a referenced network map |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 01/2015 |
| ITU-T | L.300/L.25 (01/2015) | Optical fibre cable network maintenance |  | X | |  |  |  | X |  | X |  | | |  | X |  |  | 01/2015 |
| ITU-T | L.301/L.41 (05/2000) | Maintenance wavelength on fibres carrying signals |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 05/2000 |
| ITU-T | L.302/L.40  (10/2000) | Optical fibre outside plant maintenance support, monitoring and testing system |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 10/2000 |
| ITU-T | L.310 (04/2016) | Optical fibre maintenance depending on topologies of access networks |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 04/2016 |
| ITU-T | L.311/L.93 (05/2014) | Optical fibre cable maintenance support, monitoring and testing systems for optical fibre trunk networks |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 05/2014 |
| ITU-T | L.312/L.68 (10/2007) | Optical fibre cable maintenance support, monitoring and testing system for optical fibre cable networks carrying high total optical power |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 10/2007 |
| ITU-T | L.313/L.66 (05/2007) | Optical fibre cable maintenance criteria for in-service fibre testing in access networks |  | X | |  |  |  | X |  | X | X | | |  |  |  |  | 05/2007 |
| ITU-T | L.314/L.85 (07/2010) | Optical fibre identification for the maintenance of optical access networks |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 07/2010 |
| ITU-T | L.315 (03/2018) | Water detection in underground closures for the maintenance of optical fibre cable networks with optical monitoring system |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | 03/2018 |
| ITU-T | L.340/L.74 (04/2008) | Maintenance of cable tunnels |  | X | | X | X |  | X |  | X |  | | |  | X | X |  | 04/2008 |
| ITU-T | L.341/L.88 (07/2010) | Management of poles carrying overhead telecommunication lines |  | X | | X | X |  | X |  | X |  | | |  | X | X |  | 07/2010 |
| ITU-T | L.360/L.80 (05/2008) | Operations support system requirements for infrastructure and network elements management using ID technology |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 05/2008 |
| ITU.T | L.361/L.64 (10/2012) | ID tag requirements for infrastructure and network elements management |  |  | |  |  |  | X |  | X |  |  | | |  |  |  | 10/2012 |
| ITU-T | L.362/L.69 (06/2007) | Personal digital assistant requirements and relevant data structure for infrastructure and network elements management |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 06/2007 |
| ITU-T | L.390/L92 (10/2012) | Disaster management for outside plant facilities |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 10/2012 |
| ITU-T | L.391/L.81 (11/2009) | Monitoring systems for outside plant facilities |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 11/2009 |
| ITU-T | L.392 (04/2016) | Disaster management for improving network resilience and recovery with movable and deployable information and communication technology (ICT) resource units |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 04/2016 |
| ITU-T | L.400/L.12 (03/2008) | Optical fibre splices |  | X | |  |  |  | X |  |  |  | | |  |  |  | X | 03/2008 |
| ITU-T | L.401/L.31 (10/1996) | Optical fibre attenuators |  | X | |  |  |  | X |  |  |  | | |  |  |  | X | 10/1996 |
| ITU-T | L.402/L.36 (01/2015) | Single mode fibre optic connectors |  | X | |  |  |  | X |  |  |  | | |  |  |  | X | 01/2015 |
| ITU-T | L.403/L.37 (02/2007) | Fibre optic (non-wavelength selective) branching devices |  | X | |  |  |  | X |  |  |  | | |  |  |  | X | 02/2007 |
| ITU-T | L.404 (08/2017) | Field mountable single-mode optical fibre connectors |  | X | |  |  |  | X |  |  |  | | |  |  |  | X | 08/2017 |
| ITU-T | L.430/L.28 (10/2002) | External additional protection for marinized terrestrial cables |  |  | |  |  |  | X |  |  |  | | |  | X |  | X | (10/2002) |
| ITU-T | L.431/L.29 (01/2002) | As-laid report and maintenance/repair log for marinized terrestrial cable installation |  |  | |  |  |  | X |  | X |  | | |  | X |  | X | (01/2002) |
| ITU-T | L.432/L.30 (11/2007) | Markers on marinized terrestrial cables |  |  | |  |  |  | X |  | X |  | | |  | X |  | X | (11/2007) |
| ITU-T | L.433/L.54 (02/2004) | Splice closure for marinized terrestrial cables (MTC) |  |  | |  |  |  | X |  |  |  | | |  | X |  | X | (02/2004) |
| ITU-T | L.434/L.55 (11/2003) | Digital database for marine cables and pipelines |  |  | |  |  |  | X |  | X |  | | |  | X |  | X | (11/2003) |
| ITU-T | L Suppl. 35 (06/2017) | Framework of disaster management for network resilience and recovery |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | 06/2017) |
| ITU-T | M.3210.1 | TMN management services for IMT-2000 security management |  |  | |  |  | X |  |  | X |  | | |  |  |  |  | January 2001 |
| ITU-T | M.3211.1 | Fault and Performance Management of ISDN Access |  |  | |  | X |  | X |  | X |  | | |  |  |  |  | May 1996 |
| ITU-T | Q.824 series | Stages 2 and 3 description for Q3 interfaces |  |  | |  |  |  | X |  | X |  | | |  |  |  |  | October 1995 |
| ITU-T | Q.831.1 | Access Management for V5 |  |  | |  | X |  | X |  | X |  | | |  |  |  |  | 02/ 2000 |
| ITU-T | Q.832.1  Q.832.1 Cor 1 | VB5.1 Management |  |  | |  | X |  | X |  | X |  | | |  |  |  |  | June 1998 03/2001 |
| ITU-T | Q.832.2 | VB5.2 Management |  |  | |  | X |  | X |  | X |  | | |  |  |  |  | March 1999 |
| ITU-T | Q.833.1 | ADSL network element management – CMIP model |  |  | |  | X |  | X |  | X |  | | |  |  |  |  | January 2001 |
| ITU-T | Q.834.1 | ATM-PON requirements and managed entities for the network and network element views |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | June 2004 |
| ITU-T | Q.834.3 | A UML description for management interface requirements for Broadband Passive Optical Networks |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | June 2004 |
| ITU-T | Q.834.4  Q834.4 cor.1  Q834.4 Amd.1 | A CORBA interface specifications for Broadband Passive Optical Networks based on UML interface requirements |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | July 2003  January 2004  January 2004 |
| ITU-T | Q.838.1 | Requirements and analysis for the management interface of Ethernet passive optical networks (EPON) |  | X | |  |  |  | X |  | X |  | | |  |  |  |  | October 2004 |
| ITU‑T | Q.922 | ISDN data link layer specification for frame mode bearer services |  |  | |  | X |  | X |  | X |  | | |  |  |  |  | 02/1992 |
| ITU-T | Y.1001 | IP Framework – A framework for convergence of telecommunications network and IP network technologies | X |  | |  |  |  | X |  |  |  | | |  |  |  |  | November 2000 |
| ITU-T | Y.1231 | IP access network architecture |  | X | |  |  |  |  |  |  |  | | |  |  |  |  | November 2000 |
| ITU-T | Y.1401 | Principles of interworking |  | X | |  |  |  |  |  |  |  | | |  |  |  |  | February 2008 |
| ITU-T | Y.1541 | Network performance objectives for IP-based services |  | X | |  |  |  |  |  |  |  | | |  |  |  |  | 12/2011 |
| ITU-T | Y.1541  Amendment 1 | Network performance objectives for IP-based  services  Amendment 1: New Appendix XII –  Considerations for low speed access networks |  | X | |  |  |  |  |  |  |  | | |  |  |  |  | 12/2013 |

# Annex 3 - Rearrangement of the list of standards Annex 2

Work on a web-based ANT Standards Overview in order to make the huge Standardization List in ANNEX 2 more manageable and to concentrate on the major approved documents related to Access Network Transport is in progress. A pilot web-based “ANT Roadmap” has been realized using a new taxonomy for the approved Standards and Recommendations related to the Fiber Optic Broadband Access and extended with those related to Metallic Conductor Broadband Access. The taxonomy used for these ANT technologies is as below:

1. Access Network Architecture and Functions
2. Fibre Optic Broadband Access

2.1 General on optical system design

2.2 Point-to-Point (PtP)

2.3 Passive Optical Network (PON)

* Early PON Protocols: OAN and B-PON
* Gigabit PON: G-PON and 1G-EPON
* 10-Gibabit PON: XG-PON, XGS-PON and 10G-EPON
* 40-Gigabit PON: NG-PON2
* Higher Speed PON and Multiple-wavelength PON (MW-PON)
* ONU Management and Control Interfaces (OMCI) and other ONU considerations
* Protection and system power saving considerations
* Conformance and Interoperability

2.4 Hybrid Fibre Access Technologies

* Radio and Radio Frequency over Fibre
* Wireless – Fiber Access Networks

1. Metallic Conductor Broadband Access

3.1 Integrated services digital network (ISDN)

3.2 Digital Subscriber Lines (DSL) Technologies

* Overview DSL systems
* HDSL (High bit rate DSL)
* SHDSL (Single-pair high-speed DSL)
* ADSL (Asymmetric DSL)
* ADLS2 (Asymmetric DSL2) and ADLS2plus
* VDSL (Very-high speed DSL)
* VDSL2 (Very-high speed DSL2)
* VDSL2 Vectoring (Very-high speed DSL2 Vectoring)
* G.fast (fast access to subscriber terminal)

3.3 DSL techniques

* Spectrum management
* Handshake
* Physical layer management for transceivers
* Link layer /Physical layer interface
* Multi-pair bonding
* Impulse noise protection
* Reverse Powering
* Test procedures
* Conformance and Interoperability

3.4 Ethernet over copper (EoC)

Next objective is to extend the web-based “ANT Roadmap” with the approved Standards and Recommendations related to the “Hybrid Fibre Coax”, “Fixed Wireless Access” and “Wireline Access Network Infrastructure”.

# Annex 4 - List of Abbreviations

|  |  |
| --- | --- |
| AAL | ATM Adaptive Layer |
| ADPCM | Adaptive Differential Pulse Code Modulation |
| ADSL | Asymmetric Digital Subscriber Line |
| AF | Adaptation Function |
| AFE | Analogue Front End |
| AI | Adaptation-Interface |
| AMPS | Advanced Mobile Phone System |
| AN | Access Network |
| ANAI | Access Network Architecture and Interfaces |
| ANI | Access Network Interface |
| AN-SMF | Access Network System Management Function |
| ANT | Access Network Transport |
| ANT RM | Access Network Transport Reference Model |
| ANT SMF | Access Network Transport System Management Function |
| AP | Access Point |
| API | Application Programming Interface |
| ATM | Asynchronous Transfer Mode |
| ATMF | ATM Forum |
| ATTM | Access Terminals, Transmission and Multiplexing |
| ATU | ADSL Transceiver Unit |
| ATU-C | ADSL Transceiver Unit – Central Office End |
| ATU-R | ADSL Transceiver Unit – Remote End |
| AU | Adaptation Unit |
| B-ISDN | Broadband ISDN |
| B-ISUP | Broadband Integrated Service User Part |
| BA | Basic Access |
| BC | Bearer Channel |
| BM | Business Management layer |
| BRAN | Broadband Radio Access Networks |
| BS | Base Station |
| BSC | Base Station Controller |
| BSS | Base Station System |
| BTS | Base Transceiver Station |
| BWA | Broadband Wireless Access |
| CAP | Carrierless Amplitude Modulation  Carrier-less Amplitude and Phase |
| CATV | Cable Television |
| CATV | Community Antenna TV |
| CBDS | Connectionless Broadband Data Service |
| CD | Code Division |
| CDMA | Code Division Multiple Access |
| CDPD | Cellular Digital Packet Data |
| CE | Circuit Emulator |
| CE | Common Equipment |
| Cellco | Cellular company |
| CELP | Code Excited Linear Prediction |
| CF | Core Function |
| CLNAP | Connectionless Network Access Protocol |
| CN | Core Network |
| CO | Central Office |
| CORBA | Common Object Request Broker Architecture |
| CP | Customer Premises |
| CPE | Customer Premises Equipment |
| CPN | Customer Premises Network |
| CSU | Channel Service Unit |
| CT | Cordless Telephone |
| CT2 | Cordless Telephone 2nd generation |
| CTM | Cordless Terminal Mobility |
| CTR | Common Technical Regulation |
| D-AMPS | Digital Advanced Mobile Phone System |
| DAB | Digital Audio Broadcasting |
| DCA | Dynamic Channel Allocation |
| DCE | Data Circuit Terminating Equipment |
| DCME | Digital Circuit Multiplication Equipment |
| DCN | Data Communication Network |
| DCS | Digital Cellular System |
| DDI | Drop Distribution Interface |
| DECT | Digital Enhanced Cordless Telecommunications |
| DI | Drop Distribution Interface |
| DLC | Digital Loop Carrier |
| DLL | Digital Local Line |
| DMT | Discrete Multitone  Discrete Multi-tone Carrier |
| DQDB | Distributed Queue Dual Bus |
| DRRS | Digital Radio Relay Systems |
| DRU | Dual-mode Radio Unit |
| DS | (access) Digital Section |
| DSB | Digital Satellite Broadcast |
| DS-CDMA | Digital System Code Division Multiple Access |
| DSL | Digital Subscriber Line |
| DSP | Digital Signal Processing |
| DSS1 | Digital Subscriber Signaling 1 |
| DSU | Data Service Unit |
| DTE | Data Terminal Equipment |
| DTMF | Dual Tone Multi Frequency |
| DVB | Digital Video Broadcasting |
| DXI | Data exchange Interface |
| EIA/TIA | Electronic Industry Alliance/Telecommunications Industry Association) |
| EII | European Information Infrastructure |
| EMS | Element Management System |
| ENG/OB | Electronic News Gathering/Outside Broadcast |
| ESF | Extended Superframe |
| ET | Exchange Termination |
| FCS | Frame Check Sequence |
| FDD | Frequency Division Duplex |
| FDDI | Fiber Distributed Data Interface |
| FDM | Frequency-Division Multiplexing |
| FDMA | Frequency Division Multiple Access |
| FDX | Full – Duplex |
| FEC | Forward Error Connection  Forward Error Control |
| FPLMTS (old) | Future Public Land Mobile Telecommunication System |
| FR | Frame Relay |
| FSAN | Full Service Access Networks |
| FTTB | Fiber to the Building |
| FTTC | Fiber to the Curb |
| FTTCab | Fiber to the Cabinet |
| FTTH | Fiber to the Home |
| FWA | Fixed Wireless Access |
| GAP | Generic Access Profile |
| GII | Global Information Infrastructure |
| GK | GateKeeper |
| GMSK | Gaussian Minimum Shift Keying |
| GOS | Grade of Service |
| GPS | Global Positioning System |
| GSM | Global System for Mobile communications  Global System for Mobility |
| HDLC | High Level Data Link control |
| HDSL | High Speed Digital Subscriber Line |
| HEC | Header Error Check |
| HFC | Hybrid Fiber Coax |
| HIPERLAN | High Performance Radio Local Area Network |
| HSD | High Speed Data Channel |
| HSSI | High Speed Serial Interface |
| IAB | Internet Activity Board |
| ICG | Intersector Coordination Group |
| ICP | Intelligent Cellular Peripheral |
| ID code | Vendor identification code |
| IDCT | Inverted Discrete Cosign Transform |
| IDT | International Digital Trunk |
| IMT | International Mobile Telecommunication |
| IN | Intelligent Network |
| INI | Inter-network Interface |
| IP | Internet Protocol |
| IPDC | IP Device Control |
| IPR | Intellectual Property Rights |
| iptel | Internet Protocol Telephony (IETF Working Group) |
| IRD | Integrated Receiver Decoders |
| ISDN | Integrated Services Digital Network |
| ISDN-BA | ISDN basic access |
| ISUP | ISDN User Part |
| LAN | Local Area Network |
| LATA | Local Access Transport Area |
| LD-CELP | Low Delay CELP |
| LE | Local Exchange |
| LLC | Logical Link Control |
| LMCS | Local Multipoint Communications System |
| LMDS | Local Multipoint Distribution Systems |
| LOF | Loss of Frame |
| LS0 – 2 | DUPLEX bearer channel designators |
| LSD | Low Speed Data channel |
| LT | Line Termination |
| LTB | Line Termination Box |
| LTU | Line Termination Unit |
| MAC | Medium Access Control |
| MAP | Mobile Application Part |
| MCF | Message Communication Function |
| MCS | Multi-point Control Services (T.122) |
| MCU | Multi-point Control Unit |
| MDANT | Mediation Device ANT |
| MDSN | Mediation Device SN |
| MDS | Multipoint Distribution System |
| MDSL | Multi-rate Digital Subscriber Line |
| MFAF | MFA Forum |
| MGWS | Multiple Gigabit Wireless Systems |
| MIB | Management Information Base |
| MLP | Multi-Layer Protocol |
| MMDS | Multichannel Multipoint Distribution Systems |
| MMS | Multimedia Messaging Service |
| MMUSIC | Multiparty Multimedia Session Control (WG) |
| MSC | Mobile-services Switching Centre |
| MSC | Mobile Switching Centre |
| MSOH | Multiplexer Section Overhead |
| MTM | Maintenance Trunk Module |
| MUNI | Mid-Range User Network Interface |
| MVDS | Multipoint Video Distribution System |
| MWA | Mobile Wireless Access |
| N-AMPS | Narrow-Advanced Mobile Phone System |
| N-ISDN | Narrowband ISDN |
| NE | Network Element |
| NE | Network Element layer |
| NEF | Network Element Function |
| NEFANT | Network Element Function ANT |
| NEFSN | Network Element Function SN |
| NEXT | Near end crosstalk |
| NEM | Network Element Management layer |
| NM | Network Management layer |
| NIU | Network Interface Unit |
| NLPID | Network Layer Protocol Identifier |
| NMS | Network Management System |
| NNI | Network Node Interface |
| NNI-A | Network-to-Network-Interface Type A |
| NNI-B | Network-to-Network-Interface Type B |
| NSS | Network Switching System |
| NT  (NTU) | Network Terminating Unit  Network Termination  Network Termination Unit |
| NT1 | Network Termination 1 |
| NT2 | Network Termination 2 |
| NWA | Nomadic Wireless Access |
| OAM (OA&M) | Operation, Administration and Maintenance, Operation and Maintenance (used in ISDN related Recs.) |
| OAM&P | Operations, Administration, Maintenance and Provisioning |
| OAN | Optical Access Networks |
| OCP | Operations Control Point |
| ODF | Optical Distribution Frame |
| ODN | Optical Distribution Network |
| OLT | Optical Line Termination |
| OMG | Object Management Group |
| ON | Optical Network |
| ONE | Optical Network Element |
| ONP | Open Network Provision |
| ONU | Optical Network Unit |
| OPI | On-Premise-Interface |
| OPTIS | Overlapped PAM Transmission with Interlocking Spectra |
| OS | Operation System |
| OSF | Operations System Function |
| PACS | Personal Access Communications System |
| PAI | Premises-Attachment-Interface |
| PBX | Private Branch Exchange |
| PC | Personal Computer |
| PCM | Pulse Code Modulation |
| PCME | Packet Circuit Multiplication Equipment |
| PCS | Personal Communications Service |
| PDH | Packet Digital Hierarchy |
| PDH | Plesiochronous Digital Hierarchy |
| PDTC | Peripheral Digital Trunk Controller |
| PHS | Personal Handphone System |
| PHY | Physical Layer |
| PICS | Protocol Implementation Conformance Statement |
| PINT | PSTN Interworking (IETF) |
| PIXIT | Protocol Implementation eXtra Information for Testing |
| PL | Path Layer |
| PLCP | Physical Level Convergence Protocol |
| PMD | Physical Media Dependent (sublayer) |
| PMP | Point to Multipoint microwave radio |
| PMS-TC | Physical Media Specific – Transmission Convergence |
| PON | Passive Optical Network |
| POP | Point of Presence |
| POTS | Plain Old Telephony Service |
| PRA | Primary Rate Access |
| PRBS | Pseudo-Random Bit Sequence |
| PSD | Power Spectral Density |
| PSTN | Public Switched Telephone Network |
| PTM | Package Trunk Module |
| PTT | Postal, Telephone and Telegraph |
| q | Reference point |
| Q | Interface |
| QAM | Quadrature Amplitude Modulation |
| QANT-L1 | ANT Network Management Interface – Level 1 |
| QANT-L2 | ANT Network Management Interface – Level 2 |
| QOS | Quality of Service |
| QPSK | Quadrature Phase Shift Keying |
| QX | Network Management Interface |
| RAP | Radio local loop Access Profile |
| RBB | Residential Broadband |
| RDC | Remote Device Control |
| REG | Regenerator |
| RF | Radio Frequency |
| RFC | Designation for an Internet Standard |
| RITL | Radio in the Loop |
| RLL | Radio Local Loop |
| RMS | Root Mean Squared |
| RSOH | Regenerator Section Overhead |
| RSU | Remote Switch Unit |
| RT | Remote Terminal |
| RTP | Real Time Transport Protocol |
| RTTH | Radio to the Home |
| SAP | Service Access Point |
| SAR | Segmentation and Reassembly |
| SAT | Satellite |
| SBS | Selector Bank Subsystem |
| SCN | Switched Circuit Network |
| SCR | Selective Call Rejection |
| SD | Starting Delimiter |
| SDH | Synchronous Digital Hierarchy |
| SDL | Specification and Description Language |
| SDSL | Symmetrical high bit rate Digital Subscriber Line |
| SDO | Standards Development Organization |
| SECDED | single error correction, double error detection (code) |
| SG | Study Group (ITU, CCITT) |
| SLP | Service Location Protocol |
| SM | Service Module |
| SMATV | Satellite Master Antenna TeleVision |
| SMDS | Switched multi-megabit data service |
| SMF | System Management Function |
| SMG | Special Mobile Group |
| SMS | Short Message Service |
| SN | Service Node |
| SNI | Service Node Interface |
| SNMP | Simple Network Management Protocol |
| SN-SMF | Service Node System Management Function |
| SOHO | Small Office Home Office |
| SPF | Service Port Function |
| SPP | Service Provisioning Platform |
| SS7 | Signalling System No.7 |
| SSCOP | Service Specific Connection-Oriented Protocol |
| SSCS | Service Specific Functions sublayer |
| STC | ETSI Technical Sub-Committee |
| STM | Service Trunk Module |
| STM | Synchronous Transfer Mode |
| STP | Shielded Twisted Pair |
| STU | Set Top Unit |
| SUD | Single Use Device |
| T1/E1 | Primary rate transmission system |
| T/S | Interface(s) between ADSL network termination and Customer Installation or home network |
| TA | Terminal Adopter  Terminal Adapter |
| TAB | Tape Automated Bonding |
| TACS | Total Access Communications System |
| TBR | Technical Basis for Regulation (ETSI standard) |
| TC | Technical Committee |
| TC | Transmission Convergence (sublayer) |
| TCM | Time-Compressed Modulation  Time Compressed Multiplex |
| TCP | Termination Connection Point |
| TCP | Transmission Control Protocol |
| TCP/IP | Transmission Control Protocol/ Internet Protocol |
| TDD | Time Division Duplex |
| TDM | Time Division Multiplex |
| TDMA | Time Division Multiple Access |
| TE | Terminal Equipment |
| TF | Transport Function |
| TFU | Timing Frequency Unit |
| TII | Transport Independent Interface |
| TINA | Telecommunications Information Networking Architecture |
| TM | Transmission and Multiplexing |
| TM | Trunk Module |
| TM  (TML) | Transmission Media Layer |
| TMN | Telecommunications Management Network |
| TV | Television |
| UMTS | Universal Mobile Telecommunications System |
| UNI | User Network Interface |
| UPC | Usage Parameter Control |
| UPF | User Port Function |
| UTP | Unshielded Twisted Pair |
| VC | Virtual Channel |
| VC | Virtual Container |
| VDSL | Very high rate Digital Subscriber Line  Very high speed ADSL |
| VLR | Visitor Location Register |
| VOP |  |
| VP | Virtual Path |
| VPI | Virtual Path Identifier |
| VPN | Virtual Private Network |
| VSB | Vestigial SideBand |
| WBS | Wireless Base Station |
| WCTX | Wireless Centrex |
| WDM | Wavelength Division Multiplexing |
| WG | Working Group |
| WKTS | Wireless Key Telephone System |
| WL | Wireless Loop |
| WLL | Wireless Local Loop |
| WPBX | Wireless Private Branch Exchange |
| WT | Wireless Terminal |
| X | Interface |
| xDSL | Any of the various types of Digital Subscriber Lines (DSL)  All the different Digital Subscriber Lines |
| XNI | Customer to Network Interface  Access Network Interface |
| XTU | XDSL Transceiver Unit |
| xTU-C  (XTU-C) | xDSL central site terminal unit  XDSL Transceiver Unit – Central Office End |
| xTU-R  (XTU-R) | xDSL remote terminal unit  XDSL Transceiver Unit – Remote End |
| 2B1Q | 2 Binary 1 Quaternary |

# 

<!-- ################################## Update ################################## --> \_\_\_\_\_\_\_\_\_\_\_\_\_\_<!-- ################################## Update ################################## --></BASEFONT><!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN"><!-- saved from url=(0033)file://E:\ANSI-xDSL\ansixdsl.html --><BASEFONT size=2>