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ABSTRACT

This contribution proposes a Path Coupled QoS Request modification information flow for Section 8 of Draft TRQ.IPQOS.sig.cs1.

Introduction

This contribution provides a Path Coupled QoS Request modification information flow in support of the reference model in Figure 1.
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Figure 1 - Path-Coupled End-to-End flow

It was noted at the T1S1 meeting that the CF as  shown operates sometimes as a Call Server and others as a Policy function. It was recommended that these functions be separated. In figure 1 the CF is a policy function.

Proposal

Include the information flow found in Figure 2 into Section 8, and add a request modification flow for the Path-decoupled scenario.
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Figure 2 - Path Coupled QoS Request Modification Information Flow

The information flow in Figure 2 illustrates a scenario where the QoS request is “User Initiated” and is modified by the CF1. 
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