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Abstract:

This contribution proposes addition of a new sub-clause for clause 7 concerning an evolution of PSTN access elements (i.e., UAM, RUAM, PBX, AN)
1. Discussion

According to draft PSTN evolution to NGN [FGNGN-OD-00004] it seems to be useful and would make text more clearly by adding additional clause for the access methods evolution that are used in the scenarios.
2. Proposal 

It is proposed to add texts presented below as sub-clause 7.2 of draft PSTN evolution to NGN [FGNGN-OD-00004]. 

7.2 Evolution of PSTN access

Possible scenarios for evolution of PSTN access elements (i.e., UAM, RUAM, PBX, AN) may be as follows:

7.2.1 Evolution of PSTN access – UAM

In the first step User Access Module (UAM) is replaced by a RUAM or an Access Network (AN) or PBX as shown in Figure 7-1 (see clause 7.1.1) 

In the second step access elements (i.e., RUAM, AN, PBX) are replaced by Access Gateway.

There is also a direct way – UAM is replaced by AG (see clauses 7.1.2, 7.1.3).
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Figure 7-1: Evolution of PSTN access – UAM
7.2.2 Evolution of PSTN access – RUAM

Remote User Access Module (RUAM) is replaced by an Access Network (AN) or PBX as shown in Figure 7-2, and then they (i.e., AN, PBX) are replaced by Access Gateway.

There is also a direct way – RUAM is replaced by AG (see clause 7.1.1).
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Figure 7-2: Evolution of PSTN access - RUAM

7.2.3 Evolution of PSTN access – PBX

There is a possibility to connect directly PBX to AG or replace by AG as shown in Figure 7-3 (see clauses 7.1.1, 7.1.2, 7.1.3).
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Figure 7-3: Evolution of PSTN access - PBX

7.2.4 Evolution of PSTN access – AN

There is a possibility to connect directly AN to AG or replace by AG as shown in Figure 7-4 (see clauses 7.1.1, 7.1.2, 7.1.3).
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Figure 7-4: Evolution of PSTN access - AN
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