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1. Introduction 

At its second meeting FGNGN WG 5 drafted Outline of the draft technical specification NGN Security Framework (output document FGNGN-OD-0002 R1) that defined direction for the group’s future standardization work. 

This document identifies a list of the relevant to NGN security standards and proposes to use it as an input  to Section 5 (Overview of relevant global security standards) of the FGNGN-OD-0002 R1 output document.

2. List of the relevant security standards

· 3GPP TS 33.102, 3G Security; Security Architecture
· 3GPP TS 33.103, Universal Mobile Telecommunications System (UMTS); 3G Security; Integration Guidelines
· 3GPP TS 33.203, Access security for IP-based services
· 3GPP TS 33.210, Universal Mobile Telecommunications System (UMTS); 3G security; Network Domain Security (NDS); IP network layer security
· 3GPP TS 33.220, Generic Authentication Architecture (GAA);Generic bootstrapping architecture
· 3GPP TS 33.221, Generic Authentication Architecture (GAA); Support for subscriber certificates

· 3GPP TS 33.222, Generic Authentication Architecture (GAA); Access to Network Application Function using HTTPS
· 3GPP TS 33.234, 3G Security; Wireless Local Area Network (WLAN) interworking security
· 3GPP TS 33.246, Security of Multimedia Broadcast/Multicast Service
· 3GPP2 S.S0086, IMS Security Framework
· 3GPP2 X.P0028, WLAN-CDMA2000 Interworking Architecture
· 3GPP2 X.R0083, Broadcast/Multicast Service(BCMCS) Security Requirements
· IETF RFC 2617 (1999), HTTP Authentication: Basic and Digest Access Authentication
· IETF RFC 2406 (1998), IP Encapsulating Security Payload (ESP)
· IETF RFC 2401 (1998), Security Architecture for the Internet Protocol
· IETF RFC 2403 (1998), The Use of HMAC-MD5-96 within ESP and AH
· IETF RFC 2404 (1998), The Use of HMAC-SHA-1-96 within ESP and AH
· IETF RFC 3310 (2002), HTTP Digest Authentication Using AKA
· IETF RFC 3041 (2001), Privacy Extensions for Stateless Address Autoconfiguration in IPv6
· IETF RFC 2402 (1998), IP Authentication Header
· IETF RFC 2405 (1998), The ESP DES-CBC Cipher Algorithm With Explicit IV
· IETF RFC 2406 (1998), IP Encapsulating Security Payload (ESP)
· IETF RFC 2409 (1998), Internet Key Exchange (IKE)
· IETF RFC 3261, SIP: Session Initiation Protocol
· IETF RFC 3329 (2002), Security Mechanism Agreement for the Session Initiation Protocol (SIP)
· ITU-T Recommendation X.800, Security Architecture for Open Systems Interconnection for CCITT Applications
· ITU-T Recommendation X.805, Security Architecture for Systems Providing End-to-end Communications
3. Proposal

Accept the list of relevant security standards presented in Section 2 of this document as an input to Section 5 of the draft specification NGN Security Framework.
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