|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Received: 27 November 2019 | **Document 5D/11-E** |
| **2 December 2019** |
| **English only  TECHNOLOGY ASPECTS** |
| Director, Radiocommunication Bureau[[1]](#footnote-1),[[2]](#footnote-2) | |
| preliminary Evaluation report from the 5G Infrastructure Association on IMT-2020 proposal | |
|  | |

This contribution contains in Attachment 1 the preliminary evaluation report from the Independent Evaluation Group 5G Infrastructure Association (<http://www.itu.int/oth/R0A0600006E/en>). The report contains a detailed analysis of the analytical, inspection and simulation characteristics defined in ITU-R Reports M.2410-0, M.2411-0 and M.2412-0 [1] – [3] using a methodology described in Report ITU-R M.2412-0 [3].

The preliminary report contains analytical, simulation and inspection evaluation results. Updates to this preliminary report will be provided in the final report, which is due on 12 February 2020 for the 34th meeting of Working Party 5D.

The evaluation targets the SRIT proposal contained in ITU-R WP 5D/817-E [4] (3GPP), as well as the technically very similar proposals in ITU-R WP 5D/838-E [5] (People’s Republic of China) and ITU-R WP 5D/819-E [6] (Republic of Korea) and revisions in [7] and [8].

The attached evaluation report consists of 3 Parts:

• Part I: Administrative Aspects of 5G Infrastructure Association

• Part II: Technical Aspects of the work in 5G Infrastructure Association

• Part III: Conclusion

The report is structured according to the proposed structure in [9].

Attachment 1:

# Part I: Administrative aspects of 5G Infrastructure Association

# I-1 Name of the Independent Evaluation Group

The Independent Evaluation Group is called *5G Infrastructure Association*.

# I-2 Introduction and background of 5G Infrastructure Association

The 5G Infrastructure Association Independent Evaluation Group was launched by the 5G Infrastructure Association as part of 5G Public Private Partnership (5G PPP) in October 2016 by registration at ITU-R.

The 5G Public Private Partnership (5G PPP) is a sub-research program in Horizon 2020 of the European Commission. 5G Infrastructure Association is representing the private side in 5G PPP and the EU Commission the public side. The Association was founded end of 2013. The Contractual Arrangement on 5G PPP was signed by the EU Commission and representatives of 5G Infrastructure Association in December 2013. 5G PPP is structured in three program phases.

• In Phase 1 from July 1, 2015 to 2017 19 projects researched the basic concepts of 5G systems in all relevant areas and contributed to international standardization (<https://5g-ppp.eu/5g-ppp-phase-1-projects/>).

• Phase 2 started on June 1, 2017 with 23 projects (<https://5g-ppp.eu/5g-ppp-phase-2-projects/>). The focus of Phase 2 is on the optimization of the system and the preparation of trials.

• The Phase 3 is implemented with 14 projects (<https://5g-ppp.eu/5g-ppp-phase-3-projects/>)

* + Part 1: 3 Infrastructure Projects,
  + Part 2: 3 Automotive Projects and
  + Part 3: 8 Advanced 5G validation trials across multiple vertical industries. This phase is addressing the development of trial platforms especially with vertical industries, large scale trials, cooperative, connected and automated mobility, 5G long term evolution as well as international cooperation.

In each phase around 200 organizations are cooperating in the established projects.

The main key challenges of the 5G PPP Program are to deliver solutions, architectures, technologies and standards for the ubiquitous 5G communication infrastructures of the next decade:

• Providing 1000 times higher wireless area capacity and more varied service capabilities compared to 2010.

• Saving up to 90 % of energy per service provided. The main focus will be in mobile communication networks where the dominating energy consumption comes from the radio access network.

• Reducing the average service creation time cycle from 90 hours to 90 minutes.

• Creating a secure, reliable and dependable Internet with a “zero perceived” downtime for services provision.

• Facilitating very dense deployments of wireless communication links to connect over 7 trillion wireless devices serving over 7 billion people.

• Enabling advanced User controlled privacy.

The Independent Evaluation Group is currently supported by the following 5G PPP Phase 2 projects:

• 5G Essence,

• 5G MoNArch,

• 5G Xcast,

• One 5G and

• To-Euro-5G CSA

and the 5G PPP Phase 3 projects

• Clear5G,

• 5G Genesis,

• 5G VINNI,

• 5G Tours,

• Full3G CSA,

• Global5G.org CSA

and the 5G Infrastructure Association members

• Huawei,

• Intel,

• Nokia,

• Telenor and

• Turkcell.

This Evaluation Group is evaluating all 16 evaluation characteristics according to Table 1 by means of analytical, inspection and simulation activities in order to perform a full evaluation. For simulation purposes simulators at different Evaluation Group member are used, where different evaluation characteristics are mapped to different simulators. Simulators are being calibrated where needed in order to provide comparable results. Calibration results and the calibration approach are published (c.f. Section I-6) in order to provide this information to the other Independent Evaluation Groups to support the consensus building process in ITU-R WP 5D.

# I-3 Method of work

The 5G Infrastructure Association Evaluation Group is organized as Working Group in 5G PPP under the umbrella of the 5G Infrastructure Association. Evaluation activities are executed according to a commonly agreed plan and conducted work through e.g.:

• Physical meetings and frequent telephone conferences where the activities are planned and where action items are given and followed up.

• Frequent email and telephone discussions among partners on detailed issues on an ad-hoc basis.

• File sharing on the web.

• Participation in the ITU-R Correspondence Group dedicated to the   
IMT-Advanced evaluation topics.

In addition, the Evaluation Group participated in a workshop organized by 3GPP on October 24 and 25, 2018 in Brussels.

Open issues in the system description were discussed and clarified with 3GPP.

The Evaluation Group is participating in the ITU-R WP 5D Evaluation Workshop in December 2019 in Geneva, Switzerland on 10 – 11 December 2019 at the 33rd meeting of Working Party 5D. In that workshop the Evaluation Group will present the work method, work plan, channel model calibration status, baseline system calibration assumptions, and available evaluation results.

At and after the ITU-R workshop the Evaluation Group will have communication with other Evaluation Groups as well regarding calibration and is making material openly available.

Public information on the calibration work is available at the home page listed in Section I-6.

The assessment of the proponent submission and self-evaluation has been made by analytical, inspection and simulation methods as required in Reports ITU-R M.2410-0 [1], M.2411-0 [2] and M.2412-0 [3], see Table 1 in M.2412-0 [3] in Section 6 for details.

# I-4 Administrative contact details

Dr Werner Mohr, Working Group chair

Email: [werner.mohr@nokia.com](mailto:werner.mohr@nokia.com)

# I-5 Technical contact details

Members of the Evaluation Group:

|  |  |  |
| --- | --- | --- |
| [Hakan Batıkhan](mailto:hakan.batikhan@turkcell.com.tr) | Turkcell | [hakan.batikhan@turkcell.com.tr](mailto:hakan.batikhan@turkcell.com.tr) |
| Ioannis-Prodromos Belikaidis | WINGS ICT Solutions | [iobelika@wings-ict-solutions.eu](mailto:iobelika@wings-ict-solutions.eu) |
| Ömer Bulakci | Huawei | [Oemer.Bulakci@huawei.com](mailto:Oemer.Bulakci@huawei.com) |
| Jose Luis Carcel | Universitat Politecnica de Valencia | [jocarcer@iteam.upv.es](mailto:jocarcer@iteam.upv.es) |
| [Yang Changqing](mailto:changqing.yang@huawei.com) | Huawei | [changqing.yang@huawei.com](mailto:changqing.yang@huawei.com) |
| Marcos Rates Crippa | University of Kaiserslautern | [crippa@eit.uni-kl.de](mailto:crippa@eit.uni-kl.de) |
| Panagiotis Demestichas | WINGS ICT Solutions | [pdemest@wings-ict-solutions.eu](mailto:pdemest@wings-ict-solutions.eu) |
| [Salih Ergut](mailto:salih.ergut@turkcell.com.tr) | Turkcell | [salih.ergut@turkcell.com.tr](mailto:salih.ergut@turkcell.com.tr) |
| Manuel Fuentes | Universitat Politecnica de Valencia | [mafuemue@iteam.upv.es](mailto:mafuemue@iteam.upv.es) |
| Eduardo Garro | Universitat Politecnica de Valencia | [edgarcre@iteam.upv.es](mailto:edgarcre@iteam.upv.es) |
| Andreas Georgakopoulos | WINGS ICT Solutions | [andgeorg@wings-ict-solutions.eu](mailto:andgeorg@wings-ict-solutions.eu) |
| Ioannis Giannoulakis | National Centre for Scientific Research Demokritos | giannoul@iit.demokritos.gr |
| David Gomez-Barquero | Universitat Politecnica de Valencia | [dagobar@iteam.upv.es](mailto:dagobar@iteam.upv.es) |
| Marco Gramaglia | UC3M | [mgramagl@it.uc3m.es](mailto:mgramagl@it.uc3m.es) |
| Ole Grondalen | Telenor | [ole.grondalen@telenor.com](mailto:ole.grondalen@telenor.com) |
| [Nazli Guney](mailto:nazli.guney@turkcell.com.tr) | Turkcell | [nazli.guney@turkcell.com.tr](mailto:nazli.guney@turkcell.com.tr) |
| Marie-Helene Hamon | Orange | [mhelene.hamon@orange.com](mailto:mhelene.hamon@orange.com) |
| [Ahmet Kaplan](mailto:ahmet.kaplan@turkcell.com.tr) | Turkcell | [ahmet.kaplan@turkcell.com.tr](mailto:ahmet.kaplan@turkcell.com.tr) |
| Cemil Karakus | Turkcell | [cemil.karakus@turkcell.com.tr](mailto:cemil.karakus@turkcell.com.tr) |
| Evangelos Kosmatos | WINGS ICT Solutions | [vkosmatos@wings-ict-solutions.eu](mailto:vkosmatos@wings-ict-solutions.eu) |
| Anastasios Kourtis | National Centre for Scientific Research Demokritos | [kourtis@iit.demokritos.gr](mailto:kourtis@iit.demokritos.gr) |
| Fotis Lazarakis | National Centre for Scientific Research Demokritos | [flaz@iit.demokritos.gr](mailto:flaz@iit.demokritos.gr) |
| Ji Lianghai | University of Kaiserslautern | [ji@eit.uni-kl.de](mailto:ji@eit.uni-kl.de) |
| Hans-Peter Mayer | Nokia | [hans-peter.mayer.ext@nokia-bell-labs.com](mailto:hans-peter.mayer.ext@nokia-bell-labs.com) |
| Werner Mohr | Nokia | [werner.mohr@nokia.com](mailto:werner.mohr@nokia.com) |
| Volker Pauli | Nomor | [pauli@nomor.de](mailto:pauli@nomor.de) |
| [Athul Prasad](mailto:athul.prasad@nokia-bell-labs.com) | Nokia Bell-Labs | [athul.prasad@nokia-bell-labs.com](mailto:athul.prasad@nokia-bell-labs.com) |
| Christoph Schmelz | Nokia | [christoph.schmelz@nokia-bell-labs.com](mailto:christoph.schmelz@nokia-bell-labs.com) |
| Hans Schotten | DFKI/University of Kaiserslautern | [schotten@eit.uni-kl.de](mailto:schotten@eit.uni-kl.de) |
| Egon Schulz | Huawei | [egon.schulz@huawei.com](mailto:egon.schulz@huawei.com) |
| Vera Stravroulaki | WINGS ICT Solutions | [veras@wings-ict-solutions.eu](mailto:veras@wings-ict-solutions.eu) |
| Ingo Viering | Nomor | [viering@nomor.de](mailto:viering@nomor.de) |
| [Shangbin Wu](mailto:shangbin.wu@samsung.com) | Samsung | [shangbin.wu@samsung.com](mailto:shangbin.wu@samsung.com) |
| [Wu Yong](mailto:wuyong@huawei.com) | Huawei | [wuyong@huawei.com](mailto:wuyong@huawei.com) |
| Yu Jian | Huawei | jason.yujian@huawei.com |

# I-6 Other pertinent administrative information

5G Infrastructure Association and 5G PPP homepage:

<https://5g-ppp.eu/5g-ppp-imt-2020-evaluation-group/>

This homepage contains public information about e.g. calibration work that the 5G Infrastructure Association has performed in order to ensure reliable simulation results as well as the Interim and Final Evaluation Report (after it will become available in February 2020).

The specific calibration results that were performed for the system- and link-level simulations used in this Evaluation Report can be found in the following documents:

• System-level calibration results:

º White paper with description of calibration activities:

º Matlab calibration files

• Link-level calibration results:



# I-7 Structure of this Report

This Report consists of 3 Parts:

• Part I: Administrative Aspects of 5G Infrastructure Association

• Part II: Technical Aspects of the work in 5G Infrastructure Association

• Part III: Conclusion

The Report is structured according to the proposed structure in [9].

# Part II: Technical aspects of the work in 5G Infrastructure Association

# II-A What candidate technologies or portions of the candidate technologies this IEG is or might anticipate evaluating?

In this report, *preliminary* results are presented for the SRIT and RIT proposals in [4], [7] and [8] for IMT-2020 NR and LTE components with a focus on the 3GPP submission to ITU-R. The preliminary evaluation treats analytical, inspection and simulation evaluation. The complete simulation evaluations will be provided in the final evaluation report.

It should be noted that technically the proposal in [4] is nearly identical to the submission in [5]; [6] by the People’s Republic of China and the Republic of Korea. Updates to the submission in [7] and [8] are taken into account. Hence, this evaluation report is valid also as an evaluation report for these proposals.

Table 1

Summary of evaluation methodologies

|  |  |  |  |
| --- | --- | --- | --- |
| Characteristic for evaluation | High-level assessment method | Evaluation methodology in this Report | Related section of Reports ITU-R M.2410-0 and ITU-R M.2411-0 |
| Peak data rate | Analytical | § 7.2.2 | Report ITU-R M.2410-0, § 4.1 |
| Peak spectral efficiency | Analytical | § 7.2.1 | Report ITU-R M.2410-0, § 4.2 |
| User experienced data rate | Analytical for single band and single layer;  Simulation for multi-layer | § 7.2.3 | Report ITU-R M.2410-0, § 4.3 |
| 5th percentile user spectral efficiency | Simulation | § 7.1.2 | Report ITU-R M.2410-0, § 4.4 |
| Average spectral efficiency | Simulation | § 7.1.1 | Report ITU-R M.2410-0, § 4.5 |
| Area traffic capacity | Analytical | § 7.2.4 | Report ITU-R M.2410-0, § 4.6 |
| User plane latency | Analytical | § 7.2.6 | Report ITU-R M.2410-0, § 4.7.1 |
| Control plane latency | Analytical | § 7.2.5 | Report ITU-R M.2410-0, § 4.7.2 |
| Connection density | Simulation | § 7.1.3 | Report ITU-R M.2410-0, § 4.8 |
| Energy efficiency | Inspection | § 7.3.2 | Report ITU-R M.2410-0, § 4.9 |
| Reliability | Simulation | § 7.1.5 | Report ITU-R M.2410-0, § 4.10 |
| Mobility | Simulation | § 7.1.4 | Report ITU-R M.2410-0, § 4.11 |
| Mobility interruption time | Analytical | § 7.2.7 | Report ITU-R M.2410-0, § 4.12 |
| Bandwidth | Inspection | § 7.3.1 | Report ITU-R M.2410-0, § 4.13 |
| Support of wide range of services | Inspection | § 7.3.3 | Report ITU-R M.2411-0, § 3.1 |
| Supported spectrum band(s)/range(s) | Inspection | § 7.3.4 | Report ITU-R M.2411-0, § 3.2 |

In addition, evaluations of link budgets will be provided in the final evaluation Report.

# II-B Confirmation of utilization of the ITU-R evaluation guidelines in Report ITU‑R M.2412

5G Infrastructure Association confirms that the evaluation guidelines provided in Report ITU-R M.2412-0 [3] have been utilized.

# II-C Documentation of any additional evaluation methodologies that are or might be developed by the Independent Evaluation Group to complement the evaluation guidelines

The following additional evaluation methodologies have been applied by this Evaluation Group:

• Updating of already available link-level and system-level simulators according to the submitted RITs and SRITs as well as to ITU-R requirements

• These link-level and system-level simulators have been calibrated with respect to externally available results.

# II-D Verification as per Report ITU-R M.2411 of the compliance templates and the self-evaluation for each candidate technology as indicated in A)

This Interim Evaluation Report is summarizing the available evaluation results by end of November 2019. The evaluation template is completed in Section III-2. These results confirm the self-evaluation of the proponent 3GPP.

## II-D.1 Identify gaps/deficiencies in submitted material and/or self-evaluation

There were no gaps and deficiencies identified in the submission of 3GPP.

## II-D.2 Identify areas requiring clarifications

During the evaluation process open issues were clarified with 3GPP experts on assumptions and simulation methodologies.

# II-E Assessment as per Reports ITU-R M.2410, ITU-R M.2411 and ITU-R M.2412 for each candidate technology as indicated in A)

In the following Sections details on

• Detailed analysis/assessment and evaluation by the IEGs of the compliance templates submitted by the proponents per the Report ITU-R M.2411 section 5.2.4;

• Provide any additional comments in the templates along with supporting documentation for such comments;

• Analysis of the proponent’s self-evaluation by the IEG;

are provided.

Analytical, inspection evaluation and simulation-based evaluation

## II-E.1 Peak data rate

The ITU-R minimum requirements on peak data rate are given in [1]. The following requirements and remarks are extracted from [1]:

*Peak data rate is the maximum achievable data rate under ideal conditions (in bit/s), which is the received data bits assuming error-free conditions assignable to a single mobile station, when all assignable radio resources for the corresponding link direction are utilized (i.e. excluding radio resources that are used for physical layer synchronization, reference signals or pilots, guard bands and guard times).*

*Peak data rate is defined for a single mobile station. In a single band, it is related to the peak spectral efficiency in that band. Let W denote the channel bandwidth and denote the peak spectral efficiency in that band. Then the user peak data rate is given by:*

*Peak spectral efficiency and available bandwidth may have different values in different frequency ranges. In case bandwidth is aggregated across multiple bands, the peak data rate will be summed over the bands. Therefore, if bandwidth is aggregated across Q bands then the total peak data rate is:*

*where and (i = 1,…Q) are the component bandwidths and spectral efficiencies respectively.*

*The requirement is defined for the purpose of evaluation in the eMBB usage scenario.*

*The requirements for peak data are:*

– *Downlink peak data rate is 20 Gbit/s.*

*– Uplink peak data rate is 10 Gbit/s*

### II-E.1.1 Basic parameters

Peak data rate expression is defined for downlink (DL) and uplink (UL) transmissions with TDD (Time Division Duplex) and FDD (Frequency Division Duplex) techniques as:

where in:

• J is umber of aggregated carriers in a frequency band. It can reach integer values from 1 up to 16 in 5G NR and from 1 up to 32 in LTE.

• is the normalized scaling factor related to the proportion of resources used in the DL/UL ratio for the j component carrier. For FDD j=1 for DL and UL; and for TDD and other duplexing techniques for DL and UL, j is calculated based on the frame structure and the Slot Format Indicator (SFI).

º In TDD DL, considers the presence of Guard Period (GP) as part of theeffective BW. As a consequence, the impact of GP has to be considered later in the overhead ( calculation.

* is the maximum number of layers. For DL, it can reach integer values from 1 up 8; and for UL, it is defined from 1 up to 4.
* is the maximum modulation order. It is set to 8 (256QAM) for 5G NR and to 10 (1024QAM) for LTE.
* is the scaling factor used to reflect the capability mismatch between baseband and RF capability for both SA UE and NSA UE. Its use is also proposed to scale down the maximum throughput of NR UEs in EN-DC scenarios where there is LTE and NR hardware sharing.

º is signaled per band and per band per band combination as per UE capability signalling.

º There are two possible values, 1 or 0.75.

* is the maximum code rate. In 5G NR is set to 9 while in LTE depends on the maximum Transport block size (TBS) and the number of useful data bits.
* µ is the numerology set in 5G NR. In 5G NR it is defined in [10] and can reach integer values between 0 and 4. LTE unicast only considers numerologies equal to 0.
* is the average OFDM symbol duration in a subframe for numerology, µ, i.e.. It includes the impact of the CP insertion.
* is the maximum RB allocation in the available system bandwidth with numerology µ. In 5G NR, [11] specifies the UE supported maximum bandwidth for a given band or band combination. In LTE, the maximum RB allocation and available system bandwidth is specified in [12].
* is the is the overhead calculated as the average ratio of the number of REs occupied by L1/L2 control, synchronization signals, PBCH, reference signals and guard bands with respect to the total number of REs for the effective bandwidth in a 5G NR frame time product. More specific details about the overhead calculation in 5G NR and LTE are given in Annex A.

## II-E.1.2 5G NR

### II-E.1.2.1 Downlink

DL peak data rate is calculated for FDD (Table 2) and TDD modes (Table 3). For FDD, peak data rate is only calculated for the frequency range 1 (FR1) between 450 MHz and 6 000 MHz in order to ensure minimum efficiency levels. For TDD, peak data rate is calculated in both FR1 and FR2 (24.25 GHz – 52.6 GHz). Peak data rate values have been calculated per component carrier with SISO and MIMO schemes and different aggregated component carrier levels for both antenna configurations. Detailed parameter assumptions are given in Annex A.

#### II-E.1.2.1.1 FDD RIT

Considering an FDD configuration where all resources are assigned to DL transmissions, the obtained peak date rate values are calculated as follows:

Table 2

NR FDD DL peak data rate values

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SCS [kHz]** | | **Per CC BW (MHz)** | **Peak data rate per CC, SISO (Gbits/s)** | **Number of Layers** | **Peak data rate per CC, MIMO (Gbit/s)** | **Number of CC** | **Aggregated peak data rate SISO (Gbit/s)** | **Aggregated peak data rate MIMO (Gbit/s)** | **Req. (Gbit/s)** |
| FR1 | 15 | 50 | 0.30 | 8 | 2.40 | 16 | 4.81 | 38.54 | 20 |
| 30 | 100 | 0.60 | 4.87 | 9.75 | 78.05 |
| 60 | 100 | 0.59 | 4.78 | 9.57 | 76.62 |

#### II-E.1.2.1.2 TDD RIT

Following the same procedure, TDD DL peak data rate values are calculated:

Table 3

NR TDD DL peak data rate values

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SCS [kHz]** | | **Per CC BW (MHz)** | **Peak data rate per CC SISO (Gbit/s)** | **Number of Layers** | **Peak data rate per CC MIMO (Gbit/s)** | **Number of CC** | **Aggregated peak data rate SISO (Gbit/s)** | **Aggregated peak data rate MIMO (Gbit/s)** | **Req. (Gbit/s)** |
| FR1 | 15 | 50 | 0.22 | 8 | 1.80 | 16 | 3.61 | 28.94 | 20 |
| 30 | 100 | 0.45 | 3.66 | 7.32 | 58.62 |
| 60 | 100 | 0.44 | 3.59 | 7.19 | 57.52 |
| FR2 | 60 | 200 | 0.89 | 6 | 5.39 | 13.19 | 86.31 |
| 120 | 400 | 1.80 | 10.85 | 26.51 | 173.57 |

### II-E.1.2.2 Uplink

UL peak data rate is calculated for FDD (Table 4) and TDD modes (Table 5). For FDD, peak data rate is only evaluated in FR1. For TDD, peak data rate is calculated in both FR1 and FR2. Same SISO and MIMO assumptions with single and carrier aggregation levels are considered. The rest of assumptions is described in Annex A.

#### II-E.1.2.2.1 FDD RIT

Table 4

NR FDD UL RIT

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SCS [kHz]** | | **Per CC BW (MHz)** | **Peak data rate per CC, SISO (Gbits/s)** | **Number of Layers** | **Peak data rate per CC, MIMO (Gbit/s)** | **Number of CC** | **Aggregated peak data rate SISO (Gbit/s)** | **Aggregated peak data rate MIMO (Gbit/s)** | **Req. (Gbit/s)** |
| FR1 | 15 | 50 | 0.30 | 4 | 1.22 | 16 | 4.90 | 19.60 | 10 |
| 30 | 100 | 0.62 | 2.49 | 9.99 | 39.99 |
| 60 | 100 | 0.62 | 2.49 | 9.98 | 39.54 |

#### II-E.1.2.2.2 TDD RIT

Table 5

NR TDD UL RIT

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SCS [kHz]** | | **Per CC BW (MHz)** | **Peak data rate per CC SISO (Gbit/s)** | **Number of Layers** | **Peak data rate per CC MIMO (Gbit/s)** | **Number of CC** | **Aggregated peak data rate SISO (Gbit/s)** | **Aggregated peak data rate MIMO (Gbit/s)** | **Req. (Gbit/s)** |
| FR1 | 15 | 50 | 0.19 | 4 | 0.75 | 16 | 3.00 | 12.03 | 10 |
| 30 | 100 | 0.38 | 1.52 | 6.11 | 24.46 |
| 60 | 100 | 0.37 | 1.50 | 6.02 | 24.08 |
| FR2 | 60 | 200 | 0.73 | 2.94 | 11.79 | 47.16 |
| 120 | 400 | 1.47 | 5.91 | 23.64 | 94.57 |

## II-E.1.3 LTE

DL peak data rate is calculated in FDD (Table 6 and Table 8) and TDD modes (Table 7 and Table 9) for the frequency range set between 450 MHz and 6000 MHz. Data rate values have been obtained per component carrier with SISO and MIMO schemes and also with aggregated component carriers for both antenna configurations. Two different modulation orders and PDCCH symbol configurations have been considered for the calculation. The rest of parameters is described in Annex A.

### II-E.1.3.1 Downlink

#### II-E.1.3.1.1 FDD RIT

Table 6

LTE FDD DL RIT

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Modulation  Order | Number of PDCCH symbols | Peak data rate per CC, SISO (Gbit/s) | Peak data rate per CC, MIMO (Gbit/s) | Number of CC | Aggregated peak data rate SISO (Gbit/s | Aggregated peak data rate MIMO (Gbit/s) | Req. (Gbit/s) |
| **256 QAM** | 1 | 0.08 | 0.70 | 32 | 2.83 | 22.73 | 20 |
| 2 | 0.08 | 0.67 | 32 | 2.69 | 21.53 |
| **1024 QAM** | 1 | 0.10 | 0.86 | 32 | 3.47 | 27.82 |
| 2 | 0.10 | 0.82 | 32 | 3.29 | 26.36 |

#### II-E.1.3.1.2 TDD RIT

Table 7

LTE TDD DL RIT

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Modulation**  **Order** | **Number of PDCCH symbols** | **Peak data rate per CC, SISO (Gbit/s)** | **Peak data rate per CC, MIMO (Gbit/s)** | **Number of CC** | **Aggregated peak data rate SISO (Gbit/s** | **Aggregated peak data rate MIMO (Gbit/s)** | **Req. (Gbit/s)** |
| **256 QAM** | 1 | 0.06 | 0.54 | 32 | 2.17 | 17.40 | 20 |
| 2 | 0.06 | 0.51 | 32 | 2.06 | 16.52 |
| **1024 QAM** | 1 | 0.08 | 0.66 | 32 | 2.64 | 21.12 |
| 2 | 0.08 | 0.64 | 32 | 2.52 | 20.65 |

### II-E.1.3.2 Uplink

UL peak data rate is calculated in FDD and TDD modes for the frequency range set between 450 MHz and 6000 MHz. Data rate values have been obtained per component carrier with SISO and MIMO schemes and also with aggregated component carriers for both antenna configurations. Only 256QAM modulation order is allowed in uplink transmissions. The rest of parameter assumptions is described in Annex A.

### II-E.1.3.1.1 FDD RIT

Table 8

LTE FDD UL RIT

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Modulation**  **Order** | **Peak data rate per CC, SISO (Gbit/s)** | **Peak data rate per CC, MIMO (Gbit/s)** | **Number of CC** | **Aggregated peak data rate SISO (Gbit/s)** | **Aggregated peak data rate MIMO (Gbit/s)** | **Req. (Gbit/s)** |
| **256 QAM** | 0.1 | 0.4 | 32 | 3.32 | 13.28 | 10 |

#### II-E.1.3.1.2 TDD RIT

Table 9

LTE TDD UL RIT

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Modulation**  **Order** | **Peak data rate per CC, SISO (Gbit/s)** | **Peak data rate per CC, MIMO (Gbit/s)** | **Number of CC** | **Aggregated peak data rate SISO (Gbit/s)** | **Aggregated peak data rate MIMO (Gbit/s)** | **Req. (Gbit/s)** |
| **256 QAM** | 0.05 | 0.2 | 32 | 1.85 | 7.40 | 10 |

## II-E.1.4 Observations

Observations are summarized in Table 10.

Table 10

Observations

|  |  |  |
| --- | --- | --- |
| **ITU-R requirements** | **NR component RIT** | **LTE component RIT** |
| **Downlink: At least 20 Gbit/s** | **For FDD, one component carrier** is able to provide peak data rate values up to 600 Mbps with SISO antenna configurations and **4.87 Gbps** with 8 layers in MIMO antenna configurations in frequencies between 450 MHz and 6 GHz. Considering **TDD** techniques, peak data rates up to 1.80 Gbps for SISO and **10.85 Gbps** for MIMO 6 layers can be obtained for frequencies between 24.25 GHz and 52.6 GHz.  By **aggregating multiple component carriers**, higher peak data rate values can be reached. Component carriers can be either contiguous or non-contiguous in the frequency domain. The number of component carriers has been set to the maximum, i.e. **16 component carriers**. With this configuration, peak data rates up to 9.75 Gbps and **78.05 Gbps** can be reached for **FDD** SISO and MIMO modes. In **TDD**, values up to 28.9 Gbps and **173.57 Gbps** can be reached with SISO and MIMO configurations, respectively.  The use of **MIMO and carrier aggregation** **allows to meet the ITU-R peak data rate requirement**. With carrier aggregation and SISO configuration, only TDD FR2 case meets the requirement. However, with carrier aggregation and MIMO configuration, all FDD and TDD cases reach peak data rates higher than 20 Gbps. | In **FDD, one component carrier** is able to provide peak data rate values up to **100 Mbps with SISO** antenna configurations and **860 Mbps with 8 layers MIMO** antenna configurations for frequencies between 450 MHz and 6 GHz. **In TDD**, peak data rates get reduced to **80 Mbps in SISO** transmissions **and 660 Mbps in MIMO 8 layers** configurations.  Higher peak data rate values can be reached byaggregating up to **32 component carriers** contiguous or non-contiguous in the frequency domain. In particular, **peak data rate values up to 3.47 Gbps and 27.82 Gbps** can be achieved with **FDD SISO and MIMO** configurations. In TDD, **values up to 2.64 Gbps and 21.12 Gbps** can be reached **if 1024QAM is used in SISO and MIMO** transmissions. LTE cannot meet the data rate requirements when 256QAM modulation is used in TDD.  The use of **MIMO** (up to 8 layers) **and carrier aggregation** (up to 32 component carriers) are keyfactors to enable the **fulfilment of the ITU-R peak data rate requirements**. Additionally, the use of a high modulation order such as **1024QAM** is crucial to meet the 20 Gbps peak data requirement in TDD. Despite these features, **LTE cannot reach peak data rate values as high as 5G NR** due to the **frequency range limitation** from 450 MHz to 6 GHz. |
| **Uplink: At least 10 Gbit/s** | **For FDD, one component carrier** is able to provide peak data rate values up to 620 Mbps with SISO antenna configurations and **2.49 Gbps** with MIMO 4 layers configuration in frequency ranges between 450 MHz and 6 GHz. Considering **TDD** techniques for frequency ranges of 24.25 GHz - 52.6 GHz, peak data rates up to 1.47 Gbps for SISO and **5.91 Gbps** for MIMO 4 layers can be obtained.  By **aggregating multiple component carriers**, higher peak data rate values can also be reached for uplink transmissions. The number of component carriers has also been set to 16 component carriers. With this configuration, peak data rates up to 9.99 Gbps and **39.99 Gbps** can be reached for **FDD** SISO and MIMO modes. In **TDD**, values up to 23.64 Gbps and **94.57 Gbps** can be reached with SISO and MIMO configurations, respectively.  As it can be seen, the use of **MIMO and carrier aggregation** techniques is also the key for uplink since it allows to meet the **10 Gbps ITU-R requirement.** | **In FDD, one component** carrier is able to provide peak data rate values up to **100 Mbps with SISO** and **400 Mbps with 4 layers MIMO** antenna configuration in the range of frequencies between 450 MHz and 6 GHz. For **TDD, peak data rates** get halved to **50 Mbps for SISO** and **200 Mbps for 4 layers MIMO** configurations. The maximum modulation order for both configurations is **256QAM** for the uplink side.  **Higher peak data rate values** can be obtained by aggregating **up to 32 component carriers**. In particular, **peak data rates up to 3.32 Gbps for SISO and 13.28 Gbps for MIMO** can be obtained in FDD mode. On the other hand, **TDD mode** enables values up to 1.85 Gbps and **7.40 Gbps** for SISO and **MIMO** respectively.  The use of **MIMO** (up to 4 layers) and **carrier aggregation** (up to 32 carriers) allows to meet the peak data rate requirement in uplink transmissions for **FDD mode**. Nevertheless, when all resources are **not assigned to the uplink side**, i.e. TDD mode, carrier aggregation and MIMO are **not enough to cover the 10 Gbps** targeted value. |

## II-E.2 Peak spectral efficiency

The ITU-R minimum requirements on peak spectral efficiency are given in [1]. The following requirements and remarks are extracted from [1]:

*Peak spectral efficiency is the maximum data rate under ideal conditions normalised by channel bandwidth (in bit/s/Hz), where the maximum data rate is the received data bits assuming error-free conditions assignable to a single mobile station, when all assignable radio resources for the corresponding link direction are utilized (i.e. excluding radio resources that are used for physical layer synchronization, reference signals or pilots, guard bands and guard times).*

*This requirement is defined for the purpose of evaluation in the eMBB usage scenario.*

*The minimum requirements for peak spectral efficiencies are as follows:*

* *Downlink peak spectral efficiency is 30 bit/s/Hz.*
* *Uplink peak spectral efficiency is 15 bit/s/Hz.*

*These values were defined assuming an antenna configuration to enable eight spatial layers (streams) in the downlink and four spatial layers (streams) in the uplink. However, this does not form part of the requirement and the conditions for evaluation are described in Report ITU-R M.2412-0.*

### II-E.2.1 Basic parameters

Peak spectral efficiency is defined for DL and UL transmissions with FDD and TDD techniques as:

wherein:

* is the peak data rate value obtained for each evaluated configuration.
* is the normalized scaling factor related to the proportion of resources used in the DL/UL ratio for the component carrier j. For FDD DL and ULj=1; and for TDD and other duplexing for DL and UL, j is calculated based on the frame structure and the slot format indicator (SFI).
* is the total bandwidth. It depends on the selected numerology, frequency range and duplexing technique.

### II-E.2.2 5G NR

### II-E.2.2.1 Downlink

DL peak spectral efficiency is calculated for both FDD (Table 11) and TDD techniques (Table 12). For FDD, peak spectral efficiency is only calculated for FR1 while for TDD, both FR1 and FR2 are considered. Peak spectral efficiency has only been calculated per component carrier with MIMO configurations. To enable the calculation, previous peak data rate values have considered. More details about the FDD and TDD frame structure are given in Annex A.

#### II-E.2.2.1.1 FDD RIT

Table 11

NR FDD DL RIT

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SCS [kHz] | | 5  MHz | 10  MHz | 15  MHz | 20 MHz | 25 MHz | 30  MHz | 40 MHz | 50 MHz | 60 MHz | 80 MHz | 90  MHz | 100 MHz | Req. |
| FR1 | 15 | X | X | X | X | X | X | X | 48.1 | - | - | - | - | 30 |
| 30 | X | X | X | X | X | X | X | X | X | X | X | 48.7 | 30 |
| 60 | - | X | X | X | X | X | X | X | X | X | X | 48.8 | 30 |

#### II-E.2.2.1.2 TDD RIT

Table 12

NR TDD DL RIT

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SCS [kHz] | | 5  MHz | 10  MHz | 15  MHz | 30  MHz | 20 MHz | 25 MHz | 40 MHz | 50 MHz | 60 MHz | 80 MHz | 90  MHz | 100 MHz | 200 MHz | 400 MHz | Req. |
| FR1 | 15 | X | X | X | X | X | X | X | 47.3 | - | - | - | - | - | - | 30 |
| 30 | X | X | X | X | X | X | X | X | X | X | X | 47.9 | - | - | 30 |
| 60 | - | X | X | X | X | X | X | X | X | X | X | 47.0 | - | - | 30 |
| FR2 | 60 | - | - | - | - | - | - | - | X | - | - | - | X | 35.2 | - | 30 |
| 120 | - | - | - | - | - | - | - | X | - | - | - | X | X | 35.4 | 30 |

### II-E.2.2.2 Uplink

UL peak spectral efficiency is also calculated for both FDD (Table 13) and TDD (Table 14). Same assumptions about frequency ranges have been made. UL Peak spectral efficiency has only been calculated per component carrier with MIMO configurations. To enable the calculation, previous peak data rate values have considered. More details about the FDD and TDD frame structure are given in Annex A.

#### II-E.2.2.2.1 FDD RIT

Table 13

NR FDD UL RIT

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SCS [kHz] | | 5  MHz | 10  MHz | 15  MHz | 30  MHz | 20 MHz | 25 MHz | 40 MHz | 50 MHz | 60 MHz | 80 MHz | 90  MHz | 100 MHz | Req. |
| FR1 | 15 | X | X | X | X | X | X | X | 24.5 | - | - | - | - | 15 |
| 30 | X | X | X | X | X | X | X | X | X | X | X | 25.0 | 15 |
| 60 | - | X | X | X | X | X | X | X | X | X | X | 24.7 | 15 |

#### II-E.2.2.2.2 TDD RIT

Table 14

NR TDD UL RIT

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| SCS [kHz] | | 5  MHz | 10  MHz | 15  MHz | 30  MHz | 20 MHz | 25 MHz | 40 MHz | 50 MHz | 60 MHz | 80 MHz | 90  MHz | 100 MHz | 200 MHz | 400 MHz | Req. |
| FR1 | 15 | X | X | X | X | X | X | X | 23.6 | - | - | - | - | - | - | 15 |
| 30 | X | X | X | X | X | X | X | X | X | X | X | 24.0 | - | - | 15 |
| 60 | - | X | X | X | X | X | X | X | X | X | X | 23.6 | - | - | 15 |
| FR2 | 60 | - | - | - | - | - | - | - | X | - | - | - | X | 23.1 | - | 15 |
| 120 | - | - | - | - | - | - | - | X | - | - | - | X | X | 23.2 | 15 |

## II-E.2.3 LTE

### II-E.2.2.1 Downlink

DL peak spectral efficiency is calculated for both FDD (Table 15) and TDD techniques (Table 16) in the frequency range set between 450 MHz and 6 GHz. Peak spectral efficiency has been calculated per component carrier with MIMO configuration. To enable the calculation, previous peak data rate values have been considered. More details about the parameter configuration are given in Annex A.

#### II-E.2.2.2.1 FDD RIT

Table 15

LTE FDD DL RIT

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Modulation**  **Order** | **Number of PDCCH symbols** | **1.4 MHz** | **5 MHz** | **10 MHz** | **20 MHz** | **Req. (Bit/s/Hz)** |
| **256 QAM** | 1 | X | X | X | 35.52 | 30 |
| 2 | X | X | X | 33.64 |
| **1024 QAM** | 1 | X | X | X | 43.46 |
| 2 | X | X | X | 41.18 |

#### II-E.2.2.2.2 TDD RIT

Table 16

LTE TDD DL RIT

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Modulation**  **Order** | **Number of PDCCH symbols** | **1.4 MHz** | **5 MHz** | **10 MHz** | **20 MHz** | **Req. (Bit/s/Hz)** |
| **256 QAM** | 1 | X | X | X | 34.79 | 30 |
| 2 | X | X | X | 35.65 |
| **1024 QAM** | 1 | X | X | X | 45.58 |
| 2 | X | X | X | 44.56 |

### II-E.2.2.2 Uplink

UL peak spectral efficiency is calculated for both FDD (Table 17) and TDD techniques (Table 18) in the frequency range set between 450 MHz and 6 GHz. Peak spectral efficiency has been calculated per component carrier with MIMO configuration considering different bandwidth values. To enable the calculation, previous peak data rate values have been considered. More details about the parameter configuration are given in Annex A.

#### II-E.2.2.2.1 FDD RIT

Table 17

LTE FDD UL RIT

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Modulation**  **Order** | **1.4 MHz** | **5 MHz** | **10 MHz** | **20 MHz** | **Req. (Bit/s/Hz)** |
| **256 QAM** | X | X | X | 20.74 | 15 |

#### II-E.2.2.2.2 TDD RIT

Table 18

LTE TDD UL RIT

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Modulation**  **Order** | **1.4 MHz** | **5 MHz** | **10 MHz** | **20 MHz** | **Req. (Bit/s/Hz)** |
| **256 QAM** | X | X | X | 18.81 | 15 |

## II-E.2.4 Observations

Observations are summarized in Table 19.

Table 19

Observations

|  |  |  |
| --- | --- | --- |
| **ITU-R requirements** | **NR component RIT** | **LTE component RIT** |
| **Downlink: At least 30 bits/s/Hz** | **One component carrier** is able toprovide peak spectral efficiency values up to **48.78 bps/Hz** for **FDD** and up to **47.93 bps/Hz** for **TDD** techniques thanks to **the use of MIMO 8 layers configuration in FR1**. In FR2, spectral efficiency gets decreased to values around 35 bps/Hz due to the use of 6 MIMO layers instead of 8. Both configurations are able to **meet the ITU-R requirement** (30 bps/Hz) for all the evaluated bandwidths and numerologies. | **One component carrier** is able to provide peak spectral efficiency values **up to** **35.52 bps/Hz** when 20 MHz bandwidth, MIMO 8 layers and **256QAM** modulation order are configured **in FDD transmissions**. If the modulation order is increased to **1024QAM**, **values up to 43.46 bps/Hz** can be reached. For **TDD**, **35.65 bps/Hz and 45.58 bps/Hz** values can be achieved for 256QAM and 1024QAM respectively. Unlike peak data rate results, all configurations are able to **meet the ITU-R requirement of 30 bps/Hz** thanks to the **bandwidth normalization** done in the spectral efficiency calculation. |
| **Uplink: At least 15 bits/s/Hz** | **One component carrier** is able to provide peak spectral efficiency values up to **24.99 bps/Hz** and **24.05 bps/Hz** for both **FDD** and **TDD** techniques thanks to the use of with MIMO 4 layers configurations. All the numerology and bandwidth combinations are able to provide values above the ITU-R requirement, which is set to 15 bps/Hz. | **One component carrier** is able to provide peak spectral efficiency values up to **20.74 bps/Hz** when 20 MHz bandwidth, MIMO 4 layers and **256QAM** modulation order are configured in FDD transmissions. In **TDD mode**, values up to **18.81 bps/Hz** can be achieved. Both modes meet **the ITU-R requirement**, set to 15 bps/Hz, thanks to the **bandwidth normalization** included in the spectral efficiency calculation. |

## II-E.3 User experienced data rate

The ITU-R minimum requirements on user experienced data rate are given in [1]. The following requirements and remarks are extracted from [1]:

*User experienced data rate is the 5% point of the cumulative distribution function (CDF) of the user throughput. User throughput (during active time) is defined as the number of correctly received bits, i.e. the number of bits contained in the service data units (SDUs) delivered to Layer 3, over a certain period of time.*

*In case of one frequency band and one layer of transmission reception points (TRxP), the user experienced data rate could be derived from the 5th percentile user spectral efficiency through equation (3). Let W denote the channel bandwidth and SEuser denote the 5th percentile user spectral efficiency. Then the user experienced data rate, Ruser is given by:*

*Ruser = W × SEuser*

*In case bandwidth is aggregated across multiple bands (one or more TRxP layers), the user experienced data rate will be summed over the bands.*

*This requirement is defined for the purpose of evaluation in the related eMBB test environment.*

*The target values for the user experienced data rate are as follows in the Dense Urban – eMBB test environment:*

*– Downlink user experienced data rate is 100 Mbit/s.*

*– Uplink user experienced data rate is 50 Mbit/s.*

*These values are defined assuming supportable bandwidth as described in Report ITU-R M.2412-0 for each test environment. However, the bandwidth assumption does not form part of the requirement. The conditions for evaluation are described in Report ITU-R M.2412-0.*

## II-E.3.1 Basic parameters:

As described above, the user experienced data rate is derived from the 5th percentile user spectral efficiency, which is discussed in Section III-4.

## II-E.3.2 5G NR Dense Urban – eMBB

The evaluation of user experienced data rate is conducted for 5G NR TDD in Dense Urban – eMBB test environment. Both, FR1 and FR2 are considered. Detailed evaluation assumptions are based on 5th percentile user spectral efficiency evaluation and can be found in [1], [2].

### II-E.3.2.1 Evaluation configuration A (CF = 4 GHz)

For Configuration A (single-band case), it is assumed that a component carrier of 40 MHz bandwidth is used for frame structure ‘DSUUD’. It is assumed that a component carrier of 40 MHz bandwidth for downlink and 100 MHz bandwidth for uplink is used for frame structure ‘DDDSU’. Additionally, carrier aggregation is applied to achieve the ITU-R requirement. The assumed aggregated system bandwidths in case of downlink and uplink are listed beside the evaluation results for NR TDD in Table 20 and Table 21.

Table 20

User experienced data rate for NR TDD with frame structure ‘DSUUD’  
 in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | System bandwidth [MHz] | User exp. data rate [Mbit/s] | Requirement [Mbit/s] |
| Downlink | 600 | 104.6 | 100 |
| Uplink | 800 | 52.29 | 50 |

Table 21

User experienced data rate for NR TDD with frame structure ‘DDDSU’   
in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | System bandwidth [MHz] | User exp. data rate [Mbit/s] | Requirement [Mbit/s] |
| Downlink | 320 | 111.45 | 100 |
| Uplink | 900 | 54.64 | 50 |

Table 22 and Table 23 show the results for NR FDD from two different contributions.

Table 22

User experienced data rate for NR FDD in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **User exp. data rate [Mbit/s]** | **Requirement [Mbit/s]** |
| **Downlink** | 400 | 103.37 | 100 |
| **Uplink** | 680 | 51.0 | 50 |

Table 23

User experienced data rate for NR FDD in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **User exp. data rate [Mbit/s]** | **Requirement [Mbit/s]** |
| **Downlink** | 240 | 103.2 | 100 |
| **Uplink** | 280 | 103.6 | 50 |

It is observed that NR TDD and FDD meet the downlink and uplink user experienced data rate requirements for Dense Urban – eMBB test environment in Configuration A.

### II-E.3.2.2 Evaluation configuration B (CF = 30 GHz)

For Configuration B, it is assumed that a component carrier of 200 MHz is used. Additionally, carrier aggregation is applied to achieve the ITU-R requirement. The assumed aggregated system bandwidths in case of downlink and uplink are listed beside the evaluation results in Table 24.

Table 24

User experienced data rate for NR TDD with frame structure ‘DSUUD’   
in Dense Urban – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **User exp. data rate [Mbit/s]** | **Requirement [Mbit/s]** |
| **Downlink** | 3200 | 2.0 | 100 |
| **Uplink** | 3200 | 2.13 | 50 |

It is observed that NR TDD neither meets the downlink nor the uplink ITU-R requirements in terms of user experienced data rate for Dense Urban – eMBB test environment in Configuration B. This is due to the fact that already the 5th percentile user requirement is by far not fulfilled, see Section III-4.2.2.2. The reason for this lies in the insufficient outdoor-to-indoor link budget for users in buildings with high penetration loss. Here, inter-cell interference is not the limiting factor, but noise based on a limited transmit power budget of communication devices in both uplink and downlink.

### II-E.3.2.3 Evaluation configuration C

For evaluation configuration C (multi-band), the system-level simulation is employed to evaluate the uplink user experienced data rate, where a TDD band on 30 GHz and a supplementary uplink (SUL) band on 4 GHz are used. In the evaluation, 50 % users with lower reference signal received power on TDD band are offloaded to SUL band. The evaluation results of TDD+SUL bands are provided in Table 25.

In the evaluation, the subcarrier space with 15 kHz and a component carrier with 20 MHz are assumed in SUL band using FDD. In TDD band, the subcarrier space with 60 kHz and a component carrier with 200 MHz are assumed. To meet the required user experienced data rate, multiple component carriers on either TDD band or SUL band are aggregated. The required aggregated system bandwidth is given in Table 25.

Table 25

User experienced data rate in Dense Urban – eMBB Config. C   
(NR TDD+SUL bands and Macro layer only)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Frame structure | Assumed system bandwidth [MHz] | User experienced data rate [Mbps] | ITU Requirements [Mbps] |
| Uplink | 4 GHz: full uplink;  30 GHz: DDDSU with S slot =10DL:2GP:2UL | 4 GHz: 100  (for uplink)  30 GHz: 1200 | 51.39 | 50 |

It is observed that NR can meet the uplink user experienced data rate requirement for Dense Urban – eMBB test environment in evaluation configuration C.

## II-E.4 5th percentile user spectral efficiency

The ITU-R minimum requirements on 5th percentile user spectral efficiency are given in [1]. The following requirements and remarks are extracted from [1]:

*The 5th percentile user spectral efficiency is the 5% point of the CDF of the normalized user throughput. The normalized user throughput is defined as the number of correctly received bits, i.e. the number of bits contained in the SDUs delivered to Layer 3, over a certain period of time, divided by the channel bandwidth and is measured in bit/s/Hz.*

*The channel bandwidth for this purpose is defined as the effective bandwidth times the frequency reuse factor, where the effective bandwidth is the operating bandwidth normalized appropriately considering the uplink/downlink ratio.*

*With Ri (Ti) denoting the number of correctly received bits of user i, Ti the active session time for user i and W the channel bandwidth, the (normalized) user throughput of user i, ri, is defined according to equation (4).*

**

*This requirement is defined for the purpose of evaluation in the eMBB usage scenario.*

*The minimum requirements for 5th percentile user spectral efficiency for various test environments are summarized in 0.*

Table 12 5th percentile user spectral efficiency

|  |  |  |
| --- | --- | --- |
| *Test environment* | *Downlink  (bit/s/Hz)* | *Uplink  (bit/s/Hz)* |
| *Indoor Hotspot – eMBB* | *0.3* | *0.21* |
| *Dense Urban – eMBB (NOTE 1)* | *0.225* | *0.15* |
| *Rural – eMBB* | *0.12* | *0.045* |
| *NOTE 1 – This requirement will be evaluated under Macro TRxP layer of Dense Urban – eMBB test environment as described in Report ITU-R M.2412-0.* | | |

*The performance requirement for Rural-eMBB is not applicable to Rural-eMBB LMLC (low mobility large cell) which is one of the evaluation configurations under the Rural- eMBB test environment.*

*The conditions for evaluation including carrier frequency and antenna configuration are described in Report ITU-R M.2412-0 for each test environment.*

## II-E.4.1 Basic parameters

The 5th percentile user spectral efficiency (SE) is evaluated by system level simulations. The used simulator is calibrated against the results of the calibration which 3GPP performed in the context of self-evaluation, see [13]. System level simulations are performed for TDD technique.

Furthermore, as required in [3], the 5th percentile user spectral efficiency is assessed jointly with the average spectral efficiency using the same simulations.

## II-E.4.2 5G NR

The evaluation of the 5th percentile user spectral efficiency is conducted for the three different test environments of eMBB indoor hotspot, dense urban and rural. The test environments and evaluation configuration parameters are described in [3]. Further evaluation assumptions can be found in Appendix [1], [2].

### II-E.4.2.1 Indoor Hotspot – eMBB

Two modes are considered for the Indoor Hotspot – eMBB test environment, namely operating with one or three sectors per site. For each mode, two configurations are applied. Evaluation configuration A with a carrier frequency of 4 GHz represents FR1, while evaluation configuration B with a carrier frequency of 30 GHz represents FR2.

#### II-E.4.2.1.1 Evaluation configuration A (CF = 4 GHz)

Table 26 and Table 27 show the evaluation results for NR TDD of downlink and uplink 5th percentile user spectral efficiency for Indoor Hotspot – eMBB Configuration A in both operation modes.

Table 26

5th percentile user SE for NR TDD with frame structure ‘DSUUD’ in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | | **Requirement [bit/s/Hz]** |
| **Operation mode** | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 0.36 | 0.34 | 0.3 |
| **Uplink** | 0.49 | 0.31 | 0.21 |

Table 27

5th percentile user SE for NR TDD with frame structure ‘DDDSU’ in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | | **Requirement [bit/s/Hz]** |
| **Operation mode** | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 0.39 | 0.35 | 0.3 |
| **Uplink** | 0.43 | - | 0.21 |

It is observed that NR TDD fulfills downlink and uplink 5th percentile user spectral efficiency requirement for Indoor Hotspot – eMBB test environment in Configuration A in both operation modes.

Table 28 and Table 29 are summarizing the results for NR FDD from different contributions.

Table 28

5th percentile user SE for NR FDD in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | | **Requirement [bit/s/Hz]** |
| **Operation mode** | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 0.37 | 0.31 | 0.3 |
| **Uplink** | 0.48 | 0.28 | 0.21 |

Table 29

5th percentile user SE for NR FDD in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | | **Requirement [bit/s/Hz]** |
| **Operation mode** | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 0.39 | 0.36 | 0.3 |
| **Uplink** | 0.55 | 0.59 | 0.21 |

It is observed that NR FDD fulfils the uplink 5th percentile user spectral efficiency requirement for Indoor Hotspot – eMBB test environment in Configuration A in both operation modes.

#### II-E.4.2.1.2 Evaluation configuration B (CF = 30 GHz)

Table 30 and Table 31 show the evaluation results for NR TDD of downlink and uplink 5th percentile user spectral efficiency for Indoor Hotspot – eMBB Configuration B in both operation modes.

Table 30

5th percentile user SE for NR TDD with frame structure ‘DSUUD’ in Indoor Hotspot – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | | **Requirement [bit/s/Hz]** |
| **Operation mode** | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 0.48 | 0.34 | 0.3 |
| **Uplink** | 0.40 | 0.23 | 0.21 |

Table 31

5th percentile user SE for NR TDD with frame structure ‘DDDSU’ in Indoor Hotspot – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | | **Requirement [bit/s/Hz]** |
| **Operation mode** | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 0.35 | - | 0.3 |
| **Uplink** | 0.41 | - | 0.21 |

Results for NR FDD are shown in Table 32.

Table 32

5th percentile user SE for NR FDD in Indoor Hotspot – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
| **NR FDD are shown in** | **5th percentile user SE [bit/s/Hz]** | | **Requirement [bit/s/Hz]** |
| **Operation mode** | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 0.39 | 0.30 | 0.3 |
| **Uplink** | 0.41 | 0.31 | 0.21 |

It is observed that NR TDD and FDD fulfil downlink and uplink 5th percentile user spectral efficiency requirement for Indoor Hotspot – eMBB test environment in Configuration B in both operation modes.

### II-E.4.2.2 Dense Urban – eMBB

Configuration A (carrier frequency of 4 GHz) and Configuration B (carrier frequency of 30 GHz) are applied for the Dense Urban – eMBB test environment.

In addition to the system bandwidth determined in ITU-R M.2412-0 [3], downlink system-level simulations are performed with a larger component carrier bandwidth. The larger bandwidth provides a more efficient usage of bandwidth and a smaller overhead. The simulation results with the larger bandwidth are used to calculate the user experienced data rate, see Section III-E.3.

#### II-E.4.2.2.1 Evaluation configuration A (CF = 4 GHz)

The downlink and uplink evaluation results for NR TDD for Dense Urban – eMBB Configuration A are provided in Table 33 and Table 34.

Table 33

5th percentile user SE for NR TDD with frame structure ‘DSUUD’ in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **BW [MHz]** | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 20 | 0.30 | 0.225 |
| 40 | 0.32 |
| **Uplink** | 20 | 0.15 | 0.15 |

Table 34

5th percentile user SE for NR TDD with frame structure ‘DDDSU’ in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **BW [MHz]** | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 20 | 0.39 | 0.225 |
| 40 | 0.46 |
| **Uplink** | 20 | 0.25 | 0.15 |

Table 35 and Table 36 are summarizing the NR FDD results from different contributions.

Table 35

5th percentile user SE for NR FDD in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **BW [MHz]** | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 20 | 0.25 | 0.225 |
| **Uplink** | 20 | 0.3 | 0.15 |

Table 36

5th percentile user SE for NR FDD in Dense Urban – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **BW [MHz]** | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 10 | 0.43 | 0.225 |
| **Uplink** | 10 | 0.37 | 0.15 |

It is observed that NR TDD and FDD fulfil the downlink and uplink 5th percentile user spectral efficiency requirement for Dense Urban – eMBB test environment in Configuration A.

#### II-E.4.2.2.2 Evaluation configuration B (CF = 30 GHz)

The downlink and uplink evaluation results for NR TDD for Dense Urban – eMBB Configuration B are provided in Table 37.

Table 37


5th percentile user SE for NR TDD with frame structure ‘DSUUD’ in Dense Urban – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
|  | **BW [MHz]** | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 80 | 0.001 | 0.225 |
| 200 | 0.001 |
| **Uplink** | 80 | 0.004 | 0.15 |

It is observed that NR TDD fulfils neither downlink nor uplink 5th percentile user spectral efficiency requirement for Dense Urban – eMBB test environment in Configuration B. Considering the CDF of geometry received during the calibration process, see Figure 14 in [13], which is also reproduced as Figure 1 herein. This does not seem to be all that surprising because there are geometry values down to -30 dB. Besides, it is general knowledge that for large frequencies the penetration loss and pathloss is significantly higher and therefore it is difficult to achieve high spectral efficiency in scenarios with outdoor-to-indoor coverage.

Figure 1

Distribution of WB-SINR for Urban Config B, see Figure 14 of [13]



### II-E.4.2.3 Rural – eMBB

For Rural – eMBB test environment two configurations in FR1 are applied, namely Configuration A with a carrier frequency of 700 MHz and Configuration B with carrier frequency of 4 GHz.

#### II-E.4.2.3.1 Evaluation configuration A (CF = 700 MHz)

The evaluation results for NR TDD for downlink and uplink in Rural – eMBB Configuration A are provided in Table 38 and Table 39.

Table 38

5th percentile user SE for NR TDD with frame structure ‘DSUUD’ in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.21 | 0.12 |
|
| **Uplink** | 0.06 | 0.045 |

Table 39

5th percentile user SE for NR TDD with frame structure ‘DDDSU’ in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.16 | 0.12 |
|
| **Uplink** | 0.09 | 0.045 |

Table 40 and Table 41 show the results for NR FDD from different contributions.

Table 40

5th percentile user SE for NR FDD in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.19 | 0.12 |
|
| **Uplink** | 0.24 | 0.045 |

Table 41

5th percentile user SE for NR FDD in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.15 | 0.12 |
|
| **Uplink** | 0.13 | 0.045 |

It is observed that NR TDD and FDD fulfil downlink and uplink 5th percentile user spectral efficiency requirement for Rural – eMBB test environment in Configuration A.

#### II-E.4.2.3.2 Evaluation configuration B (CF = 4 GHz)

The evaluation results for NR TDD for downlink and uplink in Rural – eMBB Configuration B are provided in Table 42 and Table 43.

Table 42

5th percentile user SE for NR TDD with frame structure ‘DSUUD’ in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.23 | 0.12 |
| **Uplink** | 0.062 | 0.045 |

Table 43

5th percentile user SE for NR TDD with frame structure ‘DDDSU’ in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.38 | 0.12 |
| **Uplink** | 0.13 | 0.045 |

NR FDD results are shown in Table 44 and Table 45 from different contributions.

Table 44

5th percentile user SE for NR FDD in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.25 | 0.12 |
| **Uplink** | 0.12 | 0.045 |

Table 45

5th percentile user SE for NR FDD in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.39 | 0.12 |
| **Uplink** | 0.21 | 0.045 |

It is observed that NR TDD and FDD fulfil downlink and uplink 5th percentile user spectral efficiency requirement for Rural – eMBB test environment in Configuration B.

#### II-E.4.2.3.3 Evaluation configuration C (CF = 700 MHz)

The evaluation results for downlink and uplink in Rural – eMBB Configuration C are provided in Table 46 to Table 49 from different contributions.

Table 46

5th percentile user SE for NR TDD with frame structure ‘DSUUD’ in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.13 | 0.12 |
| **Uplink** | 0.075 | 0.045 |

Table 47

5th percentile user SE for NR TDD with frame structure ‘DDDSU’ in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.195 | 0.12 |
| **Uplink** | 0.042 | 0.045 |

Table 48

5th percentile user SE for NR FDD in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.13 | 0.12 |
| **Uplink** | 0.071 | 0.045 |

Table 49

5th percentile user SE for NR FDD in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **5th percentile user SE [bit/s/Hz]** | **Requirement [bit/s/Hz]** |
| **Downlink** | 0.182 | 0.12 |
| **Uplink** | 0.075 | 0.045 |

It is observed that NR TDD and FDD fulfil downlink and uplink 5th percentile user spectral efficiency requirement for Rural – eMBB test environment in Configuration C. In the case of Table 47 the performance is slightly below the requirement.

## II-E.5 Average spectral efficiency

The ITU-R minimum requirements on average spectral efficiency are given in [1]. The following requirements and remarks are extracted from [1]:

*Average spectral efficiency[[3]](#footnote-3)**is the aggregate throughput of all users (the number of correctly received bits, i.e. the number of bits contained in the SDUs delivered to Layer 3, over a certain period of time) divided by the channel bandwidth of a specific band divided by the number of TRxPs and is measured in bit/s/Hz/TRxP.*

*The channel bandwidth for this purpose is defined as the effective bandwidth times the frequency reuse factor, where the effective bandwidth is the operating bandwidth normalized appropriately considering the uplink/downlink ratio.*

*Let Ri (T) denote the number of correctly received bits by user i (downlink) or from user i (uplink) in a system comprising a user population of N users and M TRxPs. Furthermore, let W denote the channel bandwidth and T the time over which the data bits are received. The average spectral efficiency, SEavg is then defined according to equation (5).*

**

*This requirement is defined for the purpose of evaluation in the eMBB usage scenario.*

*The minimum requirements for average spectral efficiency for various test environments are summarized in 0.*

Table 13 Average spectral efficiency

|  |  |  |
| --- | --- | --- |
| *Test environment* | *Downlink (bit/s/Hz/TRxP)* | *Uplink (bit/s/Hz/TRxP)* |
| *Indoor Hotspot – eMBB* | *9* | *6.75* |
| *Dense Urban – eMBB (Note 1)* | *7.8* | *5.4* |
| *Rural – eMBB* | *3.3* | *1.6* |
| *NOTE 1 – This requirement applies to Macro TRxP layer of the Dense Urban – eMBB test environment as described in Report ITU-R M.2412-0.* | | |

*The performance requirement for Rural-eMBB is also applicable to Rural-eMBB LMLC which is one of the evaluation configurations under the Rural- eMBB test environment. The details (e.g. 8 km inter-site distance) can be found in Report ITU‑R M.2412-0.*

*The conditions for evaluation including carrier frequency and antenna configuration are described in Report ITU-R M.2412-0 for each test environment.*

## II-E.5.1 Basic parameters

The average spectral efficiency (SE) is evaluated by system level simulations. The used simulator is calibrated against the results of the calibration which 3GPP performed in the context of self-evaluation, see [13]. System level simulations are performed for TDD technique.

Furthermore, as required in [3] and as mentioned in Section III-4.1, the average spectral efficiency is assessed jointly with the 5th percentile user spectral efficiency using the same simulations.

## II-E.5.2 5G NR

The evaluation of the average spectral efficiency is conducted for the three different test environments of eMBB. The test environments and evaluation configuration parameters are described in [3]. Further evaluation assumptions can be found in Appendix [1], [2].

### II-E.5.2.1 Indoor Hotspot – eMBB

Two modes are considered for the Indoor Hotspot – eMBB test environment, namely operating with one or three sectors per site. For each mode, two configurations are applied. Evaluation configuration A with a carrier frequency of 4 GHz represents FR1, while evaluation configuration B with a carrier frequency of 30 GHz represents FR2.

In addition to the system bandwidth determined in ITU-R M.2412-0 [3], downlink system-level simulations are performed with a larger component carrier bandwidth. The larger bandwidth provides a more efficient usage of bandwidth and a smaller overhead. The simulation results with the larger bandwidth are used to calculate the area traffic capacity, see Section III-6.

#### II-E.5.2.1.1 Evaluation configuration A (CF = 4 GHz)

Table 50 and Table 51 provide the evaluation results for NR TDD of downlink and uplink average spectral efficiency for Indoor Hotspot – eMBB Configuration A in both operation modes.

Table 50

Average SE for NR TDD with frame structure ‘DSUUD’ in Indoor Hotspot – eMBB Config. A

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW [MHz]** | **Average SE [bit/s/Hz/TRxP]** | | **Requirement [bit/s/Hz/TRxP]** |
| **Operation mode** |  | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 20 | 13.6 | 12.9 | 9 |
| 40 | 15.5 | 15.3 |
| **Uplink** | 20 | 8.4 | 7.4 | 6.75 |

Table 51

Average SE for NR TDD with frame structure ‘DDDSU’ in Indoor Hotspot – eMBB Config. A

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW [MHz]** | **Average SE [bit/s/Hz/TRxP]** | | **Requirement [bit/s/Hz/TRxP]** |
| **Operation mode** |  | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 20 | 12.94 | 14.25 | 9 |
| 40 | 15.23 | 16.77 |
| **Uplink** | 20 | 7.62 | - | 6.75 |

Table 52 and Table 53 provide the NR FDD results from different contributions.

Table 52

Average SE for NR FDD in Indoor Hotspot – eMBB Config. A

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW [MHz]** | **Average SE [bit/s/Hz/TRxP]** | | **Requirement [bit/s/Hz/TRxP]** |
| **Operation mode** |  | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 20 | 12.14 | 12.17 | 9 |
| **Uplink** | 20 | 8.49 | 7.48 | 6.75 |

Table 53

Average SE for NR FDD in Indoor Hotspot – eMBB Config. A

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW [MHz]** | **Average SE [bit/s/Hz/TRxP]** | | **Requirement [bit/s/Hz/TRxP]** |
| **Operation mode** |  | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 20 | 12.78 | 15.26 | 9 |
| **Uplink** | 10 | 8.87 | 9.44 | 6.75 |

It is observed that NR TDD and FDD fulfil downlink and uplink average spectral efficiency requirement for Indoor Hotspot – eMBB test environment in Configuration A in both operation modes.

#### II-E.5.2.1.2 Evaluation configuration B (CF = 30 GHz)

The Table 54 and Table 55 provide the evaluation results for NR TDD of downlink and uplink average spectral efficiency for Indoor Hotspot – eMBB Configuration B in both operation modes.

Table 54

Average SE for NR TDD with frame structure ‘DSUUD’ in Indoor Hotspot – eMBB Config. B

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW [MHz]** | **Average SE [bit/s/Hz/TRxP]** | | **Requirement [bit/s/Hz/TRxP]** |
| **Operation mode** |  | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 80 | 14.7 | 11.2 | 9 |
| 200 | 15.2 | 12.0 |
| **Uplink** | 80 | 7.4 | 7.33 | 6.75 |

Table 55

Average SE for NR TDD with frame structure ‘DDDSU’ in Indoor Hotspot – eMBB Config. B

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW [MHz]** | **Average SE [bit/s/Hz/TRxP]** | | **Requirement [bit/s/Hz/TRxP]** |
| **Operation mode** |  | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 80 | 11.41 | - | 9 |
| 200 | 13.27 | - |
| **Uplink** | 80 | 7.04 | - | 6.75 |

NR FDD results are available in Table 56.

Table 56

Average SE for NR FDD in Indoor Hotspot – eMBB Config. B

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW [MHz]** | **Average SE [bit/s/Hz/TRxP]** | | **Requirement [bit/s/Hz/TRxP]** |
| **Operation mode** |  | **1 sector per site** | **3 sectors per site** |  |
| **Downlink** | 80 | 13.06 | 10.66 | 9 |
| **Uplink** | 80 | 7.58 | 6.94 | 6.75 |

It is observed that NR TDD and FDD fulfil downlink and uplink average spectral efficiency requirement for Indoor Hotspot – eMBB test environment in Configuration B in both operation modes.

### II-E.5.2.2 Dense Urban – eMBB

Configuration A (carrier frequency of 4 GHz) and Configuration B (carrier frequency 30 GHz) are applied for the Dense Urban – eMBB test environment.

#### II-E.5.2.2.1 Evaluation configuration A (CF = 4 GHz)

The downlink and uplink evaluation results for NR TDD for Dense Urban – eMBB Configuration A are provided in Table 57 and Table 58.

Table 56

Average SE for NR TDD with frame structure ‘DSUUD’ in Dense Urban – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 16.9 | 7.8 |
| **Uplink** | 8.4 | 5.4 |

Table 58

Average SE for NR TDD with frame structure ‘DDDSU’ in Dense Urban – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 12.75 | 7.8 |
| **Uplink** | 6.11 | 5.4 |

Table 59 and Table 60 are summarizing the Nr FDD results from different contributions.

Table 59

Average SE for NR FDD in Dense Urban – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 12.35 | 7.8 |
| **Uplink** | 8.5 | 5.4 |

Table 60

Average SE for NR FDD in Dense Urban – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 12.86 | 7.8 |
| **Uplink** | 8.8 | 5.4 |

It is observed that NR TDD and FDD fulfil the downlink and uplink average spectral efficiency requirement for Dense Urban – eMBB test environment in Configuration A.

#### II-E.5.2.2.2 Evaluation configuration B (CF = 30GHz)

The downlink and uplink evaluation results for NR TDD for Dense Urban – eMBB Configuration B are provided in Table 61.

Table 61

Average SE for NR with frame structure ‘DSUUD’ TDD Dense Urban – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 4.8 | 7.8 |
| **Uplink** | 2.6 | 5.4 |

It is observed that NR TDD fulfil neither downlink nor uplink average spectral efficiency requirement for Dense Urban – eMBB test environment in Configuration B. The reason is the same as explained for the 5th percentile spectral efficiency requirement, see Section III-4.2.2.2. Considering the CDF of geometry received during the calibration process, see Figure 14 in [13] reproduced as Figure 1, this does not seem to be all that surprising because there are geometry values down to -30 dB. Besides, it is general knowledge that for large frequencies the penetration loss and pathloss is significantly higher and therefore it is difficult to achieve high spectral efficiency in scenarios with outdoor-to-indoor coverage.

### II-E.5.2.3 Rural – eMBB

For Rural – eMBB test environment two configurations in FR1 are applied, namely Configuration A with a carrier frequency of 700 MHz and Configuration B with carrier frequency of 4 GHz.

#### II-E.5.2.3.1 Evaluation configuration A (CF = 700 MHz)

The evaluation results for NR TDD for downlink and uplink in Rural – eMBB Configuration A are provided in Table 62 and Table 63.

Table 62

Average SE for NR TDD with frame structure ‘DSUUD’ in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 8.5 | 3.3 |
|
| **Uplink** | 4.7 | 1.6 |

Table 63

Average SE for NR TDD with frame structure ‘DDDSU’ in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 7.54 | 3.3 |
|
| **Uplink** | 5.05 | 1.6 |

NR FDD results are provided in Table 64 and Table 65 from different contributions.

Table 64

Average SE for NR FDD in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 6.24 | 3.3 |
|
| **Uplink** | 4.1 | 1.6 |

Table 65

Average SE for NR FDD in Rural – eMBB Config. A

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 7.30 | 3.3 |
|
| **Uplink** | 4.29 | 1.6 |

It is observed that NR TDD and FDD fulfi downlink and uplink average spectral efficiency requirement for Rural – eMBB test environment in Configuration A.

#### II-E.5.2.3.2 Evaluation configuration B (CF = 4 GHz)

The evaluation results for NR TDD for downlink and uplink in Rural – eMBB Configuration B are provided in Table 66 and Table 67.

Table 66

Average SE for NR TDD with frame structure ‘DSUUD’ in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 16.5 | 3.3 |
| **Uplink** | 7.0 | 1.6 |

Table 67

Average SE for NR TDD with frame structure ‘DDDSU’ in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 15.14 | 3.3 |
| **Uplink** | 5.76 | 1.6 |

FDD results are shown in Table 68 and Table 69.

Table 68

Average SE for NR FDD in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 14.67 | 3.3 |
| **Uplink** | 6.88 | 1.6 |

Table 69

Average SE for NR FDD in Rural – eMBB Config. B

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 15.25 | 3.3 |
| **Uplink** | 7.56 | 1.6 |

It is observed that NR TDD and FDD fulfil downlink and uplink average spectral efficiency requirement for Rural – eMBB test environment in Configuration B.

#### II-E.5.2.3.3 Evaluation configuration C (CF = 700 MHz)

The evaluation results for downlink and uplink in Rural – eMBB Configuration C are provided in Table 70 to Table 73 from different contributions.

Table 70

Average SE for NR TDD with frame structure ‘DSUUD’ in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 6.86 | 3.3 |
| **Uplink** | 3.42 | 1.6 |

Table 71

Average SE for NR TDD with frame structure ‘DDDSU’ in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 7.98 | 3.3 |
| **Uplink** | 3.53 | 1.6 |

Table 72

Average SE for NR FDD in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 5.59 | 3.3 |
| **Uplink** | 3.59 | 1.6 |

Table 73

Average SE for NR FDD in Rural – eMBB Config. C

|  |  |  |
| --- | --- | --- |
|  | **Average SE [bit/s/Hz/TRxP]** | **Requirement [bit/s/Hz/TRxP]** |
| **Downlink** | 7.55 | 3.3 |
| **Uplink** | 4.10 | 1.6 |

It is observed that NR TDD and FDD fulfill downlink and uplink average spectral efficiency requirement for Rural – eMBB test environment in Configuration C.

## II-E.6 Area traffic capacity

The ITU-R minimum requirements on area traffic capacity are given in [1]. The following requirements and remarks are extracted from [1]:

*Area traffic capacity is the total traffic throughput served per geographic area (in Mbit/s/m2). The throughput is the number of correctly received bits, i.e. the number of bits contained in the SDUs delivered to Layer 3, over a certain period of time.*

*This can be derived for a particular use case (or deployment scenario) of one frequency band and one TRxP layer, based on the achievable average spectral efficiency, network deployment (e.g. TRxP (site) density) and bandwidth.*

*Let W denote the channel bandwidth and the TRxP density (TRxP/m2). The area traffic capacity Carea is related to average spectral efficiency SEavg through equation (6).*

*Carea = ρ × W × SEavg*

*In case bandwidth is aggregated across multiple bands, the area traffic capacity will be summed over the bands.*

*This requirement is defined for the purpose of evaluation in the related eMBB test environment.*

*The target value for Area traffic capacity in downlink is 10 Mbit/s/m2 in the Indoor Hotspot – eMBB test environment.*

*The conditions for evaluation including supportable bandwidth are described in Report ITU‑R M.2412-0 for the test environment.*

## II-E.6.1 Basic parameters

As described above, the area traffic capacity is derived from the average spectral efficiency, which is discussed in Section III-5.

## II-E.6.2 5G NR Indoor Hotspot – eMBB

The evaluation of average spectral efficiency is conducted for 5G NR TDD in Indoor Hotspot – eMBB test environment. There are two operation modes considered, namely 1 sector per scenario and 3 sectors per scenario. For each mode, two configurations are applied. Evaluation configuration A with a carrier frequency of 4 GHz represents FR1, while evaluation configuration B with a carrier frequency of 30 GHz represents FR2. Detailed evaluation assumptions are based on average spectral efficiency evaluation and can be found in [1], [2].

### II-E.6.2.1 Evaluation configuration A (CF = 4 GHz)

For Configuration A, it is assumed that a component carrier of 40 MHz bandwidth is used. Additionally, carrier aggregation is applied to achieve the ITU-R requirement. The assumed aggregated system bandwidths are given in Table 74 and Table 75.

Table 74

Area traffic capacity for NR TDD with frame structure ‘DSUUD’ in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **Area traffic capacity [Mbit/s/m2]** | **Requirement [Mbit/s/m2]** |
| **1 sector per site** | 600 | 10.6 | 10 |
| **3 sectors per site** | 200 | 10.04 | 10 |

Table 75

Area traffic capacity for NR TDD with frame structure ‘DDDSU’ in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **Area traffic capacity [Mbit/s/m2]** | **Requirement [Mbit/s/m2]** |
| **1 sector per site** | 440 | 10.15 | 10 |
| **3 sectors per site** | 160 | 12.19 | 10 |

Table 76 and Table 77 show NR FDD results from different contributions.

Table 76

Area traffic capacity for NR FDD in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **Area traffic capacity [Mbit/s/m2]** | **Requirement [Mbit/s/m2]** |
| **1 sector per site** | 400 | 11.77 | 10 |
| **3 sectors per site** | 120 | 12.04 | 10 |

Table 77

Area traffic capacity for NR FDD in Indoor Hotspot – eMBB Config. A

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **Area traffic capacity [Mbit/s/m2]** | **Requirement [Mbit/s/m2]** |
| **1 sector per site** | 400 | 10.22 | 10 |
| **3 sectors per site** | 120 | 10.99 | 10 |

It is observed that NR TDD and FDD meet the ITU-R requirement in terms of area traffic capacity in downlink for Indoor Hotspot – eMBB test environment in Configuration A.

### II-E.6.2.2 Evaluation configuration B (CF = 30 GHz)

For Configuration B, it is assumed that a component carrier of 200 MHz bandwidth is used. Additionally, carrier aggregation is applied to achieve the ITU-R requirement. The assumed aggregated system bandwidths are given in Table 78 and Table 79.

Table 78

Area traffic capacity for NR TDD with frame structure ‘DSUUD’ in Indoor Hotspot – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **Area traffic capacity [Mbit/s/m2]** | **Requirement [Mbit/s/m2]** |
| **1 sector per site** | 600 | 11.4 | 10 |
| **3 sectors per site** | 400 | 17.4 | 10 |

Table 79

Area traffic capacity for NR TDD with frame structure ‘DDDSU’ in Indoor Hotspot – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **Area traffic capacity [Mbit/s/m2]** | **Requirement [Mbit/s/m2]** |
| **1 sector per site** | 600 | 12.06 | 10 |

NR FDD results are shown in Table 80.

Table 80

Area traffic capacity for NR FDD in Indoor Hotspot – eMBB Config. B

|  |  |  |  |
| --- | --- | --- | --- |
|  | **System bandwidth [MHz]** | **Area traffic capacity [Mbit/s/m2]** | **Requirement [Mbit/s/m2]** |
| **1 sector per site** | 400 | 12.63 | 10 |
| **3 sectors per site** | 200 | 15.17 | 10 |

It is observed that NR TDD and FDD meet the ITU-R requirement in terms of area traffic capacity in downlink for Indoor Hotspot – eMBB test environment in Configuration B.

## II-E.7 User plane latency

The ITU-R minimum requirements on user plane latency are given in [1]. The following requirements and remarks are extracted from [1]:

*User plane latency is the contribution of the radio network to the time from when the source sends a packet to when the destination receives it (in ms). It is defined as the one-way time it takes to successfully deliver an application layer packet/message from the radio protocol layer 2/3 SDU ingress point to the radio protocol layer 2/3 SDU egress point of the radio interface in either uplink or downlink in the network for a given service in unloaded conditions, assuming the mobile station is in the active state.*

*This requirement is defined for the purpose of evaluation in the eMBB and URLLC usage scenarios.*

*The minimum requirements for user plane latency are:*

*– 4 ms for eMBB*

*– 1 ms for URLLC*

*assuming unloaded conditions (i.e. a single user) for small IP packets (e.g. 0 byte payload + IP header), for both downlink and uplink.*

## II-E.7.1 Basic parameters / results:

These results will be included in the final Evaluation Report.

## II-E.8 Control plane latency

The ITU-R minimum requirements on control plane are given in [1]. The following requirements and remarks are extracted from [1]:

*Control plane latency refers to the transition time from a most “battery efficient” state (e.g. Idle state) to the start of continuous data transfer (e.g. Active state).*

*This requirement is defined for the purpose of evaluation in the eMBB and URLLC usage scenarios.*

*The minimum requirement for control plane latency is 20 ms. Proponents are encouraged to consider lower control plane latency, e.g. 10 ms.*

## II-E.8.1 Basic parameters – NR Rel-15, control plane latency

For NR Rel-15, control plane latency is evaluated from RRC\_INACTIVE state to RRC\_CONNECTED state. An example control plane flow for NR Rel-15 is given below (Figure 2).

Figure 2

C-plane procedure (Figure 5.7.2.1-1 in TR 37.910)

|  |
| --- |
| UE  gNB  1. Delay for RACH Scheduling Period  3. Processing delay in gNB  5. Processing delay in UE  7. Processing delay in gNB  9. Processing delay in UE  2. RACH Preamble  4. RA response  6. RRC Resume Request  8. RRC Resume  10. RRC Resume Complete  Control plane procedure |

The detailed assumptions of each step are provided in Table 5.7.2.1-1 of TR 37.910 [14] and is rewritten below (Table 81) for convenience. The evaluation is for UL data transfer. It is understood that the evaluation results for DL data transfer can be further reduced because UE processing delay in Step 9 for DL data transfer does not need to handle UL grant receiving, and therefore can be reduced compared to the case of UL data transfer.

Table 81

Assumption of C-plane procedure for NR

|  |  |  |
| --- | --- | --- |
| **Step** | **Description** | **CP Latency for UL data transfer**  **[ms]** |
| 1 | Delay due to RACH scheduling period (1TTI) | 0 |
| 2 | Transmission of RACH Preamble | Length of the preamble according to the PRACH format as specified in [10] |
| 3 | Preamble detection and processing in gNB | Tproc, 2 (assuming d2,1=0) |
| 4 | Transmission of RA response | Ts (the length of 1 slot / non-slot)  NOTE: The length of 1 slot or 1 non-slot include PDCCH and PDSCH (the first OFDM symbol of PDSCH is frequency multiplexed with PDCCH). |
| 5 | UE Processing Delay (decoding of scheduling grant, timing alignment and C-RNTI assignment + L1 encoding of RRC Resume Request) | NT,1+NT,2+0.5 ms |
| 6 | Transmission of RRC Resume Request | Ts (the length of 1 slot / non-slot)  NOTE: The length of 1 slot or 1 non-slot is equal to PUSCH allocation length. |
| 7 | Processing delay in gNB (L2 and RRC) | 3 |
| 8 | Transmission of RRC Resume | Ts (the length of 1 slot / non-slot) |
| 9 | Processing delay in UE of RRC Resume including grant reception | 7 |
| 10 | Transmission of RRC Resume Complete and UP data | 0 |
| **Notes:**   1. For step 1, the procedure for *transition from a most “battery efficient” state* has yet not begun, hence this step is not relevant for the latency of the procedure which is illustrated by a '0' in the above. 2. For step 3, the value of Tproc,2 is used only for evaluation. gNB processing delay may vary depending on implementation. 3. For step 5, the latency of *N*T,1*+N*T,2*+*0.5ms is used according to Section 8.3 of TS 38.213. *N*T,1 is a time duration of *N*1 symbols corresponding to a PDSCH reception time for PDSCH processing capability 1 when additional PDSCH DM-RS is configured; and *N*T,2 is a time duration of *N*2 symbols corresponding to a PUSCH preparation time for PUSCH processing capability 1. The value of *N*1 and *N*2 are shown in Table 5.3-1 and Table 6.4-1 of TS38.214, respectively. 4. For step 7, the processing delay in gNB (L2 and RRC) has been reduced to 3 ms. The delays due to inside-gNB or inter-gNB communication are not included in Step 7. Such delays may exist depending on deployment, but are not within the scope of this evaluation. 5. For step 9 for UL data transfer, the processing delay in the UE (L2 and RRC) is considered, i.e., from reception of RRC Connection Resume to the reception of UL grant. The transmission of UL grant by gNB and processing delay in the UE (processing of UL grant and preparing for UL tx) are also considered. The RRCConnectionResume message only includes MAC and PHY configuration. No DRX, SPS, CA, or MIMO re-configuration will be triggered by this message. Further, the UL grant for transmission of RRC Connection Resume Complete and the data is transmitted over common search space with DCI format 0. 6. For step 10, the beginning of this subframe is considered to be "*the start of continuous data transfer*", hence this step is not relevant for the latency of the procedure which is illustrated by a '0' in the above. 7. For the case of a TDD band (30 kHz SCS) with an SUL band (15 kHz SCS), the sub-carrier spacing of 15 kHz that results in larger delay is used in evaluating the latency for Step 3 and 5. | | |

## II-E.8.2 Evaluation methodology

According to the methodology that was applied to evaluate CP latency, for each step of the C-plane procedure the corresponding time delays were calculated using the parameters mentioned in Table 81.

Especially for step 3, UE PUSCH preparation procedure time is calculated by means of N2 symbols duration while step 5 delay is calculated by means of N2 symbols duration and PDSCH decoding time N1 symbols duration, described in the following two subsections.

### II-E.8.2.1 UE PDSCH processing procedure time for Capability 1 and 2

N1 symbols for UE Capability 1 are given by Table 5.3-1 of TS38.214 [15] which is rewritten below while N1,0 equals to 13 or 14 (Table 82).

Table 82

PDSCH processing time for PDSCH processing capability 1

|  |  |  |
| --- | --- | --- |
|  | PDSCH decoding time *N1* [symbols] | |
| *dmrs-AdditionalPosition* = pos0 in  *DMRS-DownlinkConfig* in both of  *dmrs-DownlinkForPDSCH-MappingTypeA*, *dmrs-DownlinkForPDSCH-MappingTypeB* | *dmrs-AdditionalPosition* ≠ pos0 in  *DMRS-DownlinkConfig* in either of  *dmrs-DownlinkForPDSCH-MappingTypeA*, *dmrs-DownlinkForPDSCH-MappingTypeB*  *or if the higher layer parameter is not configured* |
| 0 | 8 | *N1,0* |
| 1 | 10 | 13 |
| 2 | 17 | 20 |
| 3 | 20 | 24 |

Our calculations were conducted with dmrs-AdditionalPosition = pos0.

For UE Capability 2, N1 symbols are given by Table 5.3-2 of TS38.214 [15] which is rewritten below in Table 83.

Table 83

PDSCH processing time for PDSCH processing capability 2

|  |  |
| --- | --- |
|  | PDSCH decoding time *N1* [symbols] |
| *dmrs-AdditionalPosition* = pos0 in  *DMRS-DownlinkConfig* in both of  *dmrs-DownlinkForPDSCH-MappingTypeA*, *dmrs-DownlinkForPDSCH-MappingTypeB* |
| 0 | 3 |
| 1 | 4.5 |
| 2 | 9 for frequency range 1 |

### II-E.8.2.2 UE PUSCH preparation procedure time for Capability 1 and 2

N2 symbols are given for UE Capability 1 in Table 6.4-1 and for UE Capability 2 in Table 6.4-2 of TS38.214 [15]. Both tables are rewritten below in Table 84 and Table 85.

Table 84

PUSCH preparation time for PUSCH timing capability 1

|  |  |
| --- | --- |
|  | PUSCH preparation time *N2* [symbols] |
| 0 | 10 |
| 1 | 12 |
| 2 | 23 |
| 3 | 36 |

Table 85

PUSCH preparation time for PUSCH timing capability 2

|  |  |
| --- | --- |
|  | PUSCH preparation time *N2* [symbols] |
| 0 | 5 |
| 1 | 5.5 |
| 2 | 11 for frequency range 1 |

Based on the above values, Tproc,2 of step 3, is calculated as follows (section 6.4, TS38.214 [15]):



where,

* *d2,1* = 0, is the basic time unit for NR,
* *Δfmax* = 480∙103 Hz,
* *Nf* = 4096,
* *Ts* is the basic time unit for LTE with and
* *μ* the subcarrier spacing configuration (parameters definition given in section 4.1 of TS 38.211 [10]).
* Moreover, d2,2 is considered equal to zero.

### II-E.8.2.3 Resource mapping type A and B

The type A and type B resource allocation has different constraints that must be taken into account when calculating the control plane latency.

The constraints for the uplink are given in TS 38.214 Table 6.1.2.1-1 [15] (Table 86):

Table 86

Valid S and L combinations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PUSCH mapping type | Normal cyclic prefix | | | Extended cyclic prefix | | |
| *S* | *L* | *S+L* | *S* | *L* | *S+L* |
| Type A | 0 | {4,…,14} | {4,…,14} | 0 | {4,…,12} | {4,…,12} |
| Type B | {0,…,13} | {1,…,14} | {1,…,14} | {0,…, 11} | {1,…,12} | {1,…,12} |

**S** = starting OFDM symbol relative to the start of the slot (numbered from 0 to 13)

**L** = number of consecutive OFDM symbols in scheduled PUSCH resource

For mapping type A the uplink transmission always starts with OFDM symbol 0 in the slot, while the transmission can start at any OFDM symbol for mapping type B. For both mapping type A and B, the whole transmission must fit inside a slot (i.e. it cannot cross the slot boundary).

The constraints for the downlink are given in TS 38.214 Table 5.1.2.1-1 [15] (Table 87):

Table 87

Valid S and L combinations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| PDSCH mapping type | Normal cyclic prefix | | | Extended cyclic prefix | | |
| *S* | *L* | *S+L* | *S* | *L* | *S+L* |
| Type A | {0,1,2,3}  (Note 1) | {3,…,14} | {3,…,14} | {0,1,2,3}  (Note 1) | {3,…,12} | {3,…,12} |
| Type B | {0,…,12} | {2,4,7} | {2,…,14} | {0,…,10} | {2,4,6} | {2,…,12} |
| Note 1: S = 3 is applicable only if *dmrs-TypeA-Position* = 3 | | | | | | |

For mapping type A the downlink transmission can start at OFDM symbol 0, 1 or 2 (and 3 if dmrs-TypeA-Position=3) in the slot. In the calculations only S = 0, 1 or 2 was considered for Type A PDSCH. For mapping type B the transmission can start at any of the first 12 OFDM symbols (i.e. it cannot start at the last symbol) in the slot. For both mapping type A and B, the whole transmission must fit inside a slot (i.e. it cannot cross the slot boundary).

## II-E.8.3 Control plane latency calculations

Based on the above information, our calculations in each step of the procedure are shown in Table 88.

Table 88

Control Plane Latency calculation

|  |  |
| --- | --- |
| **Step** | **Latency contribution** |
| 1 | 0 ms |
| 2 |  |
| 3 | Tproc,2 from the equation on page 35 |
| 4 | Delay due to mapping type constraints + |
| 5 | , with N1, N2 taken from Tables 2,3,4,5 |
| 6 | Delay due to mapping type constraints + |
| 7 | 3 ms |
| 8 | Delay due to mapping type constraints + |
| 9 | 7 ms |
| 10 | 0 ms |

The delays due to mapping type constraints are the delays that must be added in order to satisfy the constraints given in Table 86 and Table 87.

For Step 1 the delay due to RACH scheduling period is not included. However, it should be noted that since the start time for the transition from a most "battery efficient state" is not defined in the ITU-R M.2410 document [1], it is not clear if the delay due to RACH scheduling period should be included in the calculation of the Control Plane latency or not. We have chosen to assume that the transition starts with the transmission of the RACH preamble from the UE, hence the delay due to RACH scheduling period is not included.

For step 7 the gNB processing delay is not specified in the 3GPP standard and depends on implementation. We assume that this delay will be 3 ms or less based on experience from LTE-Advanced.

In TR 37.910 [14] based on the control plane procedure and assumptions given in Table 81, a variety of configurations and UE capabilities are evaluated for NR for UL data transfer. For a specific configuration, the results are the average over the possible start timing of the control plane procedure. For NR FDD, the 3GPP evaluation results of different PRACH lengths are provided in Table 5.7.2.1-2 (TR 37.910 [14]). The evaluation is applied to various non-slot length and sub-carrier spacings.

For the same configurations, 5G PPP IMT2020 Evaluation Group calculated Control Plane Latency according to the methodology described above and the results are given below in Table 89.

Table 89

Control plane latency (ms) for NR FDD

(a) PRACH length = 2 OFDM symbols

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Resource mapping type** | **Non-slot duration** | **UE capability 1** | | | | **UE capability 2** | | |
| **15kHz SCS** | **30kHz SCS** | **60kHz SCS** | **120kHz SCS** | **15kHz SCS** | **30kHz SCS** | **60kHz SCS** |
| Type A | *M* =4  (4OS non-slot) | 15.3 | 12.6 | 12.3 | 11.7 | 15.3 | 12.6 | 12.1 |
| *M* =7  (7OS non-slot) | 15.5 | 13.2 | 12.4 | 11.7 | 15.5 | 13.2 | 12.1 |
| Type B | *M*=2  (2OS non-slot) | 13.1 | 12.0 | 11.8 | 11.4 | 12.7 | 11.8 | 11.6 |
| *M* =4  (4OS non-slot) | 13.6 | 12.3 | 11.9 | 11.4 | 13.3 | 12.0 | 11.7 |
| *M* =7  (7OS non-slot) | 14.5 | 12.8 | 12.1 | 11.6 | 14.0 | 12.8 | 11.9 |

(b) PRACH length = 6 OFDM symbols

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Resource mapping type** | **Non-slot duration** | **UE capability 1** | | | | **UE capability 2** | | |
| **15kHz SCS** | **30kHz SCS** | **60kHz SCS** | **120kHz SCS** | **15kHz SCS** | **30kHz SCS** | **60kHz SCS** |
| Type A | *M* =4  (4OS non-slot) | 15.3 | 13.1 | 12.3 | 11.7 | 15.3 | 12.6 | 12.3 |
| *M* =7  (7OS non-slot) | 15.5 | 13.8 | 12.4 | 11.7 | 15.5 | 13.2 | 12.4 |
| Type B | *M*=2  (2OS non-slot) | 13.4 | 12.1 | 11.8 | 11.4 | 13.0 | 11.9 | 11.6 |
| *M* =4  (4OS non-slot) | 13.8 | 12.4 | 11.9 | 11.5 | 13.6 | 12.3 | 11.7 |
| *M* =7  (7OS non-slot) | 14.5 | 12.8 | 12.1 | 11.6 | 14.5 | 12.8 | 12.0 |

(c) PRACH length=1ms

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Resource mapping type** | **Non-slot duration** | **UE capability 1** | | **UE capability 2** | |
| **15kHz SCS** | **30kHz SCS** | **15kHz SCS** | **30kHz SCS** |
| Type A | *M* =4  (4OS non-slot) | 16.3 | 13.6 | 16.3 | 13.6 |
| *M* =7  (7OS non-slot) | 16.5 | 14.2 | 16.5 | 14.2 |
| *M* =14  (14OS slot) | 17.0 | 14.5 | 17.0 | 14.5 |
| Type B | *M*=2  (2OS non-slot) | 13.9 | 12.9 | 13.6 | 12.7 |
| *M* =4  (4OS non-slot) | 14.6 | 13.3 | 14.0 | 12.9 |
| *M* =7  (7OS non-slot) | 15.5 | 13.8 | 15.0 | 13.2 |

## II-E.8.4 Conclusions

The 5G PPP evaluation results given in Table 89 are quite close to the values provided by 3GPP. The calculated control plane latencies were below the ITU IMT2020 requirement of 20 ms in all cases. The minimum latency value is approaching 11 ms for configurations with 120 kHz subcarrier spacing. No configuration achieved a control plane latency below 10 ms.

## II-E.9 Connection density

The ITU-R minimum requirements on connection density are given in [1]. The following requirements and remarks are extracted from [1]:

*Connection density is the total number of devices fulfilling a specific quality of service (QoS) per unit area (per km2).*

*Connection density should be achieved for a limited bandwidth and number of TRxPs. The target QoS is to support delivery of a message of a certain size within a certain time and with a certain success probability, as specified in Report ITU-R M.2412-0.*

*This requirement is defined for the purpose of evaluation in the mMTC usage scenario.*

*The minimum requirement for connection density is 1 000 000 devices per km2.*

The evaluation methodology is described in [3], Section 7.1.3] and in Section III-9.1. In this report, mainly NR evaluation takes place due to the fact that connection density is one of the main challenges that NR tries to solve compared to previous releases.

## II-E.9.1 Evaluation methodology and KPIs

In mMTC environments, one of the important parameters is the connection density of devices. According to ITU document [1] the connection density is the total number of devices fulfilling a specific quality of service (QoS) per unit area (per km2). Connection density should be achieved for a limited bandwidth and number of connectivity points. The target QoS is to support delivery of a message of a certain size within a certain time and with a certain success probability. This requirement is defined for the purpose of evaluation in the mMTC usage scenario. According to ITU, the minimum requirement for connection density is 1,000,000 devices per km2.

Also, ITU has defined the following steps, for the evaluation of connection density [3]:

• Step 1: Set system user number per TRxP as N.

• Step 2: Generate the user packet according to the traffic model.

• Step 3: Run non-full buffer system-level simulation to obtain the packet outage rate. The outage rate is defined as the ratio of the number of packets that failed to be delivered to the destination receiver within a transmission delay of less than or equal to 10s to the total number of packets generated in Step 2.

• Step 4: Change the value of N and repeat Step 2-3 to obtain the system user number per TRxP N’ satisfying the packet outage rate of 1%.

• Step 5: Calculate connection density by equation C = N’ / A, where the TRxP area A is calculated as A = ISD2 × sqrt(3)/6, and ISD is the inter-site distance.

• The requirement is fulfilled if the connection density C is greater than or equal to 1,000,000  
The simulation bandwidth used to fulfil the requirement should be reported. Additionally, it is encouraged to report the connection efficiency (measured as N’ divided by simulation bandwidth) for the achieved connection density.

The considered traffic model for such an evaluation is message size of 32 bytes with either 1 message/day/device or 1 message/2 hours/device. Packet arrival follows Poisson arrival process for non-full buffer system-level simulation.

## II-E.9.2 Simulation results

System-level simulations have been conducted for the evaluation of connection density in mMTC environments. Narrowband parameters are taken into account in the simulation. As such, considered bandwidth is from 180 kHz up to 1.08 MHz. The success rate (i.e. successful transmission of messages) is calculated in order to check the acceptable level of connection density for meeting the threshold of 99 % of success (1 % of loss). During the evaluation process, the lower number of the considered message generation frequency (e.g. 1 message/day/device) fulfils the requirements of the connection density. The results showed that the 99th percentile of the delay per user was less than 10s for both the 180 kHz and 1.08 MHz tests. Two configurations for ISD (Inter Site Distance) of 500 m and 1732 m were examined during the evaluation. As a result, the focus was given on the investigation and analysis of the higher message frequency of 1 message/2 hours/device which had a different behaviour than the previous.

Figure 3 shows the success rate for different number of devices when bandwidth of 180 kHz is used. According to the results, it is evident that with such bandwidth, up to 2 million devices per km2 assuming messages of 32 bytes and 1 message/2 hours/device can be served. When 3 million devices per km2 were simulated, the success rate dropped below 99 %.

Figure 3

Connection density (nr. of devices per km2)





Figure 4 shows how much bandwidth is needed for serving 1 million devices with 1 message of 32 bytes/2 hours/device as we have seen at Figure 3, but this time by examining at which level the success rate will reach the highest level. The results show that even from 180 kHz, the success rate of 99% is fulfilled and as the bandwidth increases, the success rate is even higher, reaching almost the 100% at 540 kHz.

Figure 4

Success rate depending on bandwidth (ISD 500m)



As a next step we changed the simulation parameters to higher ISD value of 1 732 m and run the same evaluation process as before. Figure 5 shows the success rate for different number of devices when bandwidth of 1.08 MHz is used. According to the results, it is evident that with such bandwidth, up to 40 million devices per km2 can be enabled in the area without serious problems assuming messages of 32 bytes and 1 message/2 hours/device.

Figure 5

Connection density (nr. of devices per km2)





Figure 6 shows how much bandwidth is needed for serving 1 million devices with 1 message of 32 bytes/2 hours/device. The results show that from 500 kHz and above, the success rate of 99 % is met. However, smaller bandwidths (e.g. 180 or 360 kHz) are possible but the success rate is a bit lower than 99 %.

Figure 6

Success rate depending on bandwidth (ISD 1732 m)



## II-E.9.3 Summary

Connection density is an important metric in mMTC environments. Also, the usage of narrowband technologies is encouraged, especially for small and frequent transmissions. As a result, the provided evaluations take into account these assumptions in order to show the number of devices that can be supported with a specific QoS. In cases of 180 kHz of bandwidth the scenarios of ISD at 500 m showed that there were not any major problems for the device density that was considered. In addition, the results for ISD of 1 732 m reveal that there is a need of higher bandwidths to meet the requirements and achieve the proposed success rates, which in many cases more than three times the initial bandwidth had to be used. Also, the results are consistent with the results of vendors in 3GPP [14] who followed the same evaluation process, utilizing the same parameters at their proprietary simulator. For the bandwidth of 1.08 MHz the evaluation process showed that it is possible to handle effectively more than 1 million devices per km2 in every situation.

It can be noted that 1 million devices is the minimum requirement of ITU-R for connection density evaluation.

# II-E.10 Energy efficiency

The ITU-R minimum requirements on energy efficiency are given in [1]. The following requirements and remarks are extracted from [1]:

*Network energy efficiency is the capability of a RIT/SRIT to minimize the radio access network energy consumption in relation to the traffic capacity provided. Device energy efficiency is the capability of the RIT/SRIT to minimize the power consumed by the device modem in relation to the traffic characteristics.*

*Energy efficiency of the network and the device can relate to the support for the following two aspects:*

*a) Efficient data transmission in a loaded case;*

*b) Low energy consumption when there is no data.*

*Efficient data transmission in a loaded case is demonstrated by the average spectral efficiency (see § 4.5,* also look at Section III-5 of this report*).*

*Low energy consumption when there is no data can be estimated by the sleep ratio. The sleep ratio is the fraction of unoccupied time resources (for the network) or sleeping time (for the device) in a period of time corresponding to the cycle of the control signaling (for the network) or the cycle of discontinuous reception (for the device) when no user data transfer takes place. Furthermore, the sleep duration, i.e. the continuous period of time with no transmission (for network and device) and reception (for the device), should be sufficiently long.*

*This requirement is defined for the purpose of evaluation in the eMBB usage scenario.*

*The RIT/SRIT shall have the capability to support a high sleep ratio and long sleep duration. Proponents are encouraged to describe other mechanisms of the RIT/SRIT that improve the support of energy efficient operation for both network and device.*

Guidelines for the evaluation methodology is given in [3] (M.2412). The following is extracted from [3]:

*The energy efficiency for both network and device is verified by inspection by demonstrating that the candidate RITs/SRITs can support high sleep ratio and long sleep duration as defined in Report ITU-R M.2410-0 when there is no data.*

*Inspection can also be used to describe other mechanisms of the candidate RITs/SRITs that improve energy efficient operation for both network and device.*

Hence, only the energy efficiency in the unloaded case is evaluated in this section. The energy efficiency in the loaded case is evaluated in Section II-5 of this report.

## II-E.10.1 Different technical concepts to improve energy efficiency in the system description as submitted by 3GPP

According to [1] and [3] there are no quantative requirements on energy efficiency. Therefore, only a qualitative evaluation of different proposed technical concepts for the improvement of energy efficiency can be evaluated.

### II-E.10.1.1 NR RIT of “5G” [7], Section 5.2.3.2.25

**Network energy efficiency**

The fundamental always-on transmission that must take place is the periodic SS/PBCH block. The SS/PBCH block is used for the UE to detect the cell, obtain basic information of it on PBCH, and maintain synchronization to it. The duration, number and frequency of the SS/PBCH block transmission depends on the network setup. For the purposes of blind initial access the UE may assume that there is an SS/PBCH block once every 20 ms. If the network is configured to transmit the SS/PBCH block less frequently, that will improve the network energy efficiency at the cost of increased initial cell detection time. But after the initial connection has been established, the UE may be informed of the configured SS/PBCH block periodicity in the cell from the set of {5, 10, 20, 40, 80, 160} ms. If the cell set up uses analogue beamformer component, it may provide several SS/PBCH blocks multiplexed in time-domain fashion within one SS/PBCH block period.

Remaining minimum system information carried over SIB1 needs to be broadcast at least in the cells in which the UEs are expected to be able to set up the connection to the network. There is no specific rate at which the SIB1 needs to be repeated in the cell, and once the UE acquires the SIB1, it does not need to read it again. SIB1 could be time or frequency multiplexed with the SS/PBCH block. In the frequency multiplexing case, there would be no additional on-time for the gNB transmitter. In the time multiplexing case, having a lower rate for SIB1 than for SS/PBCH block would suffice at least for higher SS/PBCH repetition frequencies.

The sleep ratio under the above mechanism is evaluated in [14].

**Device energy efficiency**

Multiple features facilitating device energy efficiency have been specified for NR Rel-15.

**Discontinuous reception (DRX) in RRC\_CONNECTED, RRC\_INACTIVE and RRC\_IDLE**. When DRX is configured, the UE does not have to continuously monitor PDCCH for scheduling or paging messages, but it can remain sleeping. DRX is characterized by the following:

**– on-duration**: duration that the UE waits for, after waking up, to receive PDCCHs. If the UE successfully decodes a PDCCH, the UE stays awake and starts the inactivity timer;

**– inactivity-timer**: duration that the UE waits to successfully decode a PDCCH, from the last successful decoding of a PDCCH, failing which it can go back to sleep. The UE shall restart the inactivity timer following a single successful decoding of a PDCCH for a first transmission only (i.e. not for retransmissions);

**– retransmission-timer**: duration until a retransmission can be expected;

**– DRX cycle**: specifies the periodic repetition of the on-duration followed by a possible period of inactivity (see Figure 7).

Figure 7

DRX Cycle



Bandwidth part (BWP) adaptation

With dynamic bandwidth part adaptation, the UE can fall-back to monitoring the downlink and transmitting the uplink over a narrower bandwidth than the nominal carrier bandwidth used for high data rate transactions. This allows the UEs BB-RF interface to operate with a much lower clock rate and thus reduce energy consumption. Lower data rate exchange can still take place so that there is no need to resume full bandwidth operation just for exchanging network signalling messages or always-on packets of applications. The UE can be moved to the narrow BWP by gNBs transmitting a BWP switch bit on the scheduling DCI on the PDCCH or based on an inactivity timer. UE can be moved back to the full bandwidth operation at any time by the gNB with the BWP switch bit.

RRC\_INACTIVE state

The introduction of RRC-inactive state to the RRC state machine (Figure 8) allows for the UE to maintain RRC connection in an inactive state while having the battery saving characteristics of the Idle mode. This allows for maintaining the RRC connection also when the UE is inactive for longer time durations and avoid the signalling overhead and related energy consumption needed when the RRC connection is re-established from Idle mode.

Figure 8

NR RRC state machine



Pipelining frame structure enabling micro-sleep within slots in which the UE is not scheduled

The fact that the typical data transmission employs a control channel in the beginning of the slot, and the absence of the continuous reference signal to receive for channel estimate maintenance allows for the UE to determine early on in the slot whether there is a transmission to it, and if there is no data for it to decode, it may turn off its receiver until the end of the slot.

Additional power saving mechanisms for NR are under study for 3GPP Release 16.

### II-E.10.1.2 SRIT of “5G” [7], Section 5.2.3.2.25

**For NR component RIT:**

**Network energy efficiency**

The fundamental always-on transmission that must take place is the periodic SS/PBCH block. The SS/PBCK block is used for the UE to detect the cell, obtain basic information of it on PBCH, and maintain synchronization to it. The duration, number and frequency of the SS/PBCH block transmission depends on the network setup. For the purposes of blind initial access the UE may assume that there is an SS/PBCH block once every 20 ms. If the network is configured to transmit the SS/PBCH block less frequently, that will improve the network energy efficiency at the cost of increased the initial cell detection time, but after the initial connection has been established, the UE may be informed of the configured SS/PBCH block periodicity in the cell from set of {5, 10, 20, 40, 80, 160} ms. If the cell set up uses analogue beamformer component, it may provide several SS/PBCH blocks multiplexed in time-domain fashion within one SS/PBCH block period.

Remaining minimum system information carried over SIB1 needs to be broadcast at least in the cells in which the UEs are expected to be able to set up the connection to the network. There is no specific rate at which the SIB1 needs to be repeated in the cell, and once the UE acquires the SIB1, it does not need to read it again. SIB1 could be time or frequency multiplexed with the SS/PBCH block. In the frequency multiplexing case, there would be no additional on-time for the gNB transmitter. In the time multiplexing case, having a lower rate for SIB1 than for SS/PBCH block would suffice at least for higher SS/PBCH repetition frequencies.

The sleep ratio under the above mechanism is evaluated in [14].

**Device energy efficiency**

Multiple features facilitating device energy efficiency have been specified for NR Rel-15.

**Discontinuous reception (DRX) in RRC\_CONNECTED, RRC\_INACTIVE and RRC\_IDLE**. When DRX is configured, the UE does not have to continuously monitor PDCCH for scheduling or paging messages, but it can remain sleeping. DRX is characterized by the following:

**– on-duration**: duration that the UE waits for, after waking up, to receive PDCCHs. If the UE successfully decodes a PDCCH, the UE stays awake and starts the inactivity timer;

**– inactivity-timer**: duration that the UE waits to successfully decode a PDCCH, from the last successful decoding of a PDCCH, failing which it can go back to sleep. The UE shall restart the inactivity timer following a single successful decoding of a PDCCH for a first transmission only (i.e. not for retransmissions);

**– retransmission-timer**: duration until a retransmission can be expected;

**– DRX cycle**: specifies the periodic repetition of the on-duration followed by a possible period of inactivity (see Figure 9).

Figure 9

DRX Cycle



Bandwidth part (BWP) adaptation

With dynamic bandwidth part adaptation, the UE can fall-back to monitoring the downlink and transmitting the uplink over a narrower bandwidth than the nominal carrier bandwidth used for high data rate transactions. This allows the UEs BB-RF interface to operate with a much lower clock rate and thus reduce energy consumption. Lower data rate exchange can still take place so that there is no need to resume full bandwidth operation just for exchanging network signalling messages or always-on packets of applications. The UE can be moved to the narrow BWP by gNBs transmitting a BWP switch bit on the scheduling DCI on the PDCCH, or based on an inactivity timer. UE can be moved back to the full bandwidth operation at any time by the gNB with the BWP switch bit.

RRC\_INACTIVE state

The introduction of RRC-inactive state to the RRC state machine (Figure 10) allows for the UE to maintain RRC connection in an inactive state while having the battery saving characteristics of the Idle mode. This allows for maintaining the RRC connection also when the UE is inactive for longer time durations, and avoid the signalling overhead and related energy consumption needed when the RRC connection is re-established from Idle mode.

Figure 10

NR RRC state machine



Pipelining frame structure enabling micro-sleep within slots in which the UE is not scheduled

The fact that the typical data transmission employs a control channel in the beginning of the slot, and the absence of the continuous reference signal to receive for channel estimate maintenance allows for the UE to determine early on in the slot whether there is a transmission to it, and if there is no data for it to decode, it may turn off its receiver until the end of the slot.

Additional power saving mechanisms for NR are under study for 3GPP Release 16.

**For LTE component RIT:**

**Network energy efficiency**

In the LTE system the capacity boosting cells can be distinguished from cells providing basic coverage. This can be used to enhance network energy efficiency by switching off LTE or EN-DC cells providing additional capacity when its capacity is not needed and re-activate the cells on a need basis.

The eNB owning a capacity booster cell can autonomously decide to switch-off such a cell to lower energy consumption (dormant state). The decision is typically based on cell load information, consistently with configured information. The switch-off decision may also be taken by O&M. The eNB may initiate handover actions in order to off-load the cell being switched off and may indicate the reason for handover with an appropriate cause value to support the target node in taking subsequent actions, e.g. when selecting the target cell for subsequent handovers. All peer eNBs are informed by the eNB owning the concerned cell about the switch-off actions over the X2 interface with the eNB Configuration Update procedure. The eNB indicates the switch-off action to a GERAN and/or UTRAN node with the eNB Direct Information Transfer procedure over S1. All informed nodes maintain the cell configuration data, e.g., neighbour relationship configuration, also when a certain cell is dormant. If basic coverage is ensured by E-UTRAN cells, eNBs owning non-capacity boosting cells may request a re-activation over the X2 interface if capacity needs in such cells demand to do so. This is achieved via the Cell Activation procedure. If basic coverage is ensured by UTRAN or GERAN cells, the eNB owning the capacity booster cell may receive a re-activation request from a GERAN or UTRAN node with the MME Direct Information Transfer procedure over S1. The eNB owning the capacity booster cell may also receive from the sending GERAN or UTRAN node the minimum time before that cell switches off; during this time, the same eNB may prevent idle mode UEs from camping on the cell and may prevent incoming handovers to the same cell.

**Device energy efficiency**

Multiple features facilitating device energy efficiency have been specified for LTE Rel-15.

Discontinuous reception (DRX) in RRC connected mode

When DRX is configured, the UE does not have to continuously monitor PDCCH for scheduling or paging messages, but it can remain sleeping. DRX is characterized by the following:

**– on-duration**: duration that the UE waits for, after waking up, to receive PDCCHs. If the UE successfully decodes a PDCCH, the UE stays awake and starts the inactivity timer;

**– i nactivity-timer**: duration that the UE waits to successfully decode a PDCCH, from the last successful decoding of a PDCCH, failing which it can go back to sleep. The UE shall restart the inactivity timer following a single successful decoding of a PDCCH for a first transmission only (i.e. not for retransmissions);

**– retransmission-timer**: duration until a retransmission can be expected;

**– DRX cycle**: specifies the periodic repetition of the on-duration followed by a possible period of inactivity (see Figure 11).

Figure 11

DRX Cycle



Discontinuous reception (DRX) in RRC idle mode

The UE may use discontinuous reception (DRX) to reduce power consumption in idle mode. When DRX is used, the UE wakes up and listens to PDCCH only on specific paging occasion defined in-terms of paging frame and subframe within period of N radio frames defined by the DRX cycle of the cell. The UE can remain in sleep mode for remaining duration within DRX cycle.

The UE listens to PDCCH on the paging occasion and decodes the PDCCH based on P-RNTI and if the PDCCH decoding is success, UE decodes the PDSCH indicated in the PDCCH. The UE enters into sleep mode if the PDCCH decoding is not successful or if the UE does not find any page for its UE-ID in the paging message.

The paging occasion of UE within DRX cycle is determined based on the UE-ID, DRX cycle and nB. n is the number of paging occasions per DRX cycle. Higher the value of nB indicates lesser the paging occasions within DRX cycle and vice versa.

For higher sleep ratio, higher DRX cycle needs to be configured at the cell.

Extended discontinuous reception (DRX) in RRC idle mode

To support higher sleep duration upto several hours for low complexity mMTC devices, extended DRX functionality can be configured in LTE.

When eDRX is configured for UE, the UE wakes up periodically in every longer DRX cycle defined as eDRX cycle for short duration called paging window to monitor the PDCCH for reception of paging message. The eDRX cycle length is configured in terms of number of hyper-frames (1 hyper frame =1024 radio frames) by higher layers. Maximum value of eDRX cycle is 256 hyper frames for LTE and 1024 for NB-IoT devices.

During the paging window, the UE monitors the PDCCH using the DRX cycle configured for the cell. The paging window duration will be longer than DRX cycle so that UE monitors for paging message in more than one paging occasion within paging window. (See Figure 12).

Figure 12

Paging window



The PTW is UE specific and defined in terms of PH (paging hyper frame) and starting and end position of the paging window within the paging hyper-frame.

The paging hyper frame is selected based on UE-ID and the extended DRX-cycle value. The length of extended DRX-cycle value can be configured as multiples of hyper-frame (1024 radio frames). Maximum eDRX length can be 1024 hyper frames (approximately) 3hours.

The paging occasions where UE should monitor PDCCH for the UE configured with eDRX is given in terms of paging window within eDRX cycle. The start of paging window is aligned to the paging hyper frame calculated based on eDRX cycle and UE-ID. Within paging hyper frame, the paging window starts at radio frames in multiples of 256. The actual starting radio frame is determined based on UE-ID. From start of paging window UE monitors all the paging occasions until the end of paging window which is calculated based paging window length configured by upper layers.

The UE enters into sleep mode at the end of PTW or if it has received a valid page for its UE ID within PTW whichever happens earlier and wake up only during next occurrence of PTW in next eDRX cycle.

Paging with wake-up signal in idle mode

When UE supports WUS and the cell is configured to support WUS transmission, UE shall monitor WUS prior to paging reception on the PO. If DRX is used and if UE detects WUS it reads the PDCCH in the following PO. If eDRX is configured and if the UE detects WUS within its paging window, it monitors N paging occasions configured by higher layers. If the UE does not detect WUS it need not monitor the following paging occasions.

Power saving mode operation in idle mode (PSM)

The UE may be configured by higher layers to enter into indefinite sleep after configurable timer duration from last successful uplink transmission. The UE exit the sleep mode when it needs to send next uplink transmission for sending tracking area update or for application data transmission. The UE is not expected to listen to any downlink channels including PDCCH for paging when it is in sleep mode. Any network-initiated downlink data transmission towards the UE needs to be delayed until UE access the network for next uplink transmission.

For EN-DC operation:

In EN-DC operation, the en-gNB may autonomously decide to switch-off NR cells to lower energy consumption. MeNBs are informed by the en-gNB owning the concerned cell about the switch-off actions over the X2 interface with the EN-DC Configuration Update procedure. The en-gNB may initiate dual connectivity procedures towards the MeNB in order to off-load the cell being switched off, and may indicate the reason for release or modification with an appropriate cause value to support the master node in taking subsequent actions. The MeNB may request a re-activation over the X2 interface if capacity needs demand to do so. This is achieved via the EN-DC Cell Activation procedure. The switch-on decision may also be taken by O&M. All peer eNBs are informed by the en-gNB owning the concerned NR cell about the re-activation by an indication on the X2 interface.

## II-E.10.2 Evaluation of sleep ratio and sleep duration

## II-E.10.2.1 5G NR

#### II-E.10.2.1.1 NR network side

The sleep ratio for NR on the network side is given in [14], and the following Table 90 and Table 91 for the sleep ratio is taken from there:

Table 90

NR network sleep ratio in slot level (from [14])

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **SSB configuration** | | **SSB set periodicity** *P*SSB | | | | | |
| **SCS [kHz]** | **Number of SS/PBCH block per SSB set,** *L* | 5ms | 10ms | 20ms | 40ms | 80ms | 160ms |
| 15kHz | 1 | 80.00% | 90.00% | 95.00% | 97.50% | 98.75% | 99.38% |
| 2 | 80.00% | 90.00% | 95.00% | 97.50% | 98.75% | 99.38% |
| 30kHz | 1 | 95.00% | 97.50% | 98.75% | 99.38% | 99.69% | 99.84% |
| 4 | 80.00% | 90.00% | 95.00% | 97.50% | 98.75% | 99.38% |
| 120kHz | 8 | 90.00% | 95.00% | 97.50% | 98.75% | 99.38% | 99.69% |
| 16 | 80.00% | 90.00% | 95.00% | 97.50% | 98.75% | 99.38% |
| 240kHz | 16 | 90.00% | 95.00% | 97.50% | 98.75% | 99.38% | 99.69% |
| 32 | 80.00% | 90.00% | 95.00% | 97.50% | 98.75% | 99.38% |

Table 91

NR network sleep ratio in symbol level (from [14])

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **SSB configuration** | | **SSB set periodicity** *P*SSB | | | | | |
| **SCS [kHz]** | **Number of SS/PBCH block per SSB set,** *L* | 5ms | 10ms | 20ms | 40ms | 80ms | 160ms |
| 15kHz | 1 | 93.57% | 96.43% | 97.86% | 98.93% | 99.46% | 99.73% |
| 2 | 87.14% | 92.86% | 95.71% | 97.86% | 98.93% | 99.46% |
| 30kHz | 1 | 96.79% | 98.21% | 98.93% | 99.46% | 99.73% | 99.87% |
| 4 | 87.14% | 92.86% | 95.71% | 97.86% | 98.93% | 99.46% |
| 120kHz | 8 | 94.29% | 97.14% | 98.57% | 99.29% | 99.64% | 99.82% |
| 16 | 88.57% | 94.29% | 97.14% | 98.57% | 99.29% | 99.64% |
| 240kHz | 16 | 94.29% | 97.14% | 98.57% | 99.29% | 99.64% | 99.82% |
| 32 | 88.57% | 94.29% | 97.14% | 98.57% | 99.29% | 99.64% |

From Table 90 it can be seen that with SSB set period of 5 ms, more than 80% of sleep ratio can be obtained, and with SSB set period larger than 10 ms more than 90% of sleep ratio can be obtained.

Table 91 shows that the sleep ratio is higher with finer sleep granularity (symbol level).

Therefore, it can be concluded that 5G NR networks can achieve high sleep ratio in the unloaded case.

The sleep duration for NR on the network side is given in [14], and Table 92 for the sleep duration is taken from there.

Table 92

NR network sleep duration (ms) in slot level (from [14])

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **SSB configuration** | | **SSB set periodicity** *P*SSB | | | | | |
| **SCS [kHz]** | **Number of SS/PBCH block per SSB set,** *L* | 5ms | 10ms | 20ms | 40ms | 80ms | 160ms |
| 15kHz | 1 | 4.00 | 9.00 | 19.00 | 39.00 | 79.00 | 159.00 |
| 2 | 4.00 | 9.00 | 19.00 | 39.00 | 79.00 | 159.00 |
| 30kHz | 1 | 4.50 | 9.50 | 19.50 | 39.50 | 79.50 | 159.50 |
| 4 | 4.00 | 9.00 | 19.00 | 39.00 | 79.00 | 159.00 |
| 120kHz | 8 | 4.50 | 9.72 | 18.92 | 39.03 | 78.97 | 158.99 |
| 16 | 4.00 | 9.88 | 18.77 | 39.05 | 78.96 | 158.99 |
| 240kHz | 16 | 4.50 | 9.86 | 18.90 | 39.04 | 78.97 | 158.99 |
| 32 | 4.00 | 9.94 | 18.76 | 39.06 | 78.96 | 158.99 |

From Table 92 it can be seen that with SSB set period of 160 ms, more than 150 ms sleep duration can be obtained. It can therefore be concluded that NR networks can achieve long sleep duration in unloaded case.

Since NR both support high sleep ratios and long sleep durations, NR meets the energy efficiency requirement in the unloaded case for the network side.

#### II-E.10.2.1.1 NR device side

The sleep ratio for NR on the device side is given in [14], Table 93 and Table 94 for the sleep ratio is taken from there

Table 93

NR device sleep ratio in slot level (for idle / inactive mode)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Paging cycle *N*PC\_RF \*10 (ms)** | **SCS(kHz)** | **SSB L** | **SSB reception time(ms)** | **SSB cycle (ms)** | **Number of SSB burst set** | **RRM measurement time per DRX (ms)** | **Transition time(ms)** | **Sleep ratio** |
| RRC-Idle/Inactive | 320 | 240 | 32 | 1 | -- | 1 | 3.5 | 10 | 95.5% |
| 2560 | 15 | 2 | 1 | -- | 1 | 3 | 10 | 99.5% |
| 2560 | 15 | 2 | 1 | 160 | 2 | 3 | 10 | 93.2% |

From Table 93 it can be seen that sleep ratios of more than 90% is achieved in idle mode by NR devices.

Table 94

NR device sleep ratio in slot level (for connected mode)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **DRX cycle *T*SC\_ms \* *M*SC (ms)** | **Number of SSB burst set** | **DRX-onDurationTimer(ms)** | **RRM measurement time per DRX (ms)** | **Transition time(ms)** | **Sleep ratio** |
| RRC-Connected | 320 | 1 | 2 | 3.5 | 10 | 95.2% |
| 320 | 1 | 10 | 3 | 10 | 92.8% |
| 2560 | 1 | 100 | 3 | 10 | 95.6% |
| 10240 | 1 | 1600 | 3 | 10 | 84.2% |

From Table 94 it can be seen that sleep ratios of more than 90% can be achieved in connected mode by NR devices.

It can therefore be concluded that NR devices can achieve high sleep ratio for both idle/inactive state and connected state in unloaded case.

The sleep duration for NR on the device side is given in [14], and the following is an extract of the text:

*The sleep duration for NR UE in idle mode is 2546 ms for paging cycle of 2560 ms with the assumed parameters. The sleep duration of NR UE in connected state is 8627 ms for paging cycle of 10240 ms with the assumed parameters.*

Consequently, NR devices can achieve very long sleep duration in both idle mode and connected mode.

It can therefore be concluded that NR meets the device side energy efficiency requirement.

### II-E.10.2.2 LTE

#### II-E.10.2.2.1 LTE network side

The sleep ratio for LTE on the network side is given in [14], and Table 95 for the sleep ratio is taken from there.

Table 95

LTE network sleep ratio in subframe level (from [14])

|  |  |
| --- | --- |
| Cell type | Sleep ratio |
| FeMBMS/Unicast-mixed cell | 80% |
| MBMS-dedicated cell | 93.75% |

From Table 95 it can be seen that LTE networks can achieve high sleep ratio for FeMBMS/Unicast-mixed cell and MBMS-dedicated cell in unloaded case.

The sleep duration for LTE is given in [14], and Table 96 for the sleep duration is taken from there:

Table 96

LTE network sleep duration (ms) in subframe level (from [14])

|  |  |
| --- | --- |
| Cell type | Sleep duration (ms) |
| FeMBMS/Unicast-mixed cell | 4.00 |
| MBMS-dedicated cell | 39.00 |

From Table 96 it can be seen that MBMS-dedicated cells can achieve a sleep duration of 39 ms in the unloaded case.

Therefore, LTE meets network side energy efficiency requirement for FeMBMS/Unicast-mixed cell and MBMS-dedicated cell.

#### II-E.10.2.2.1 LTE device side

The sleep ratio for LTE on the device side is given in [14], and Table 97 and Table 98 for the sleep ratio is taken from there:

Table 97

LTE device sleep ratio in subframe level (for idle mode)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Paging cycle *N*PC\_RF \*10 (ms) | Synchronization reception time per cycle(ms) | Synchronization cycle(ms) | Number of  synchronization | RRM measurement time per DRX (ms) | Transition time (ms) | DL/UL subframe ratio | Sleep ratio |
| RRC-Idle | 320 | 2 | 10\* | 1 | 6 | 10 | 1 | 93.1% |
| 320 | 2 | 10\* | 2 | 6 | 10 | 1 | 90.0% |
| 2560 | 2 | 10\* | 1 | 6 | 10 | 1 | 99.1% |
| 2560 | 2 | 10\* | 2 | 6 | 10 | 1 | 98.8% |

From Table 97 it can be seen that more than 90% sleep ratio can be achieved in idle mode by LTE devices.

Table 98

LTE device sleep ratio in subframe level (for connected mode)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | DRX cycle *T*CYCLE\_SF (ms) | Synchronization reception time(ms) | Synchronization cycle(ms) | Number of synchronization | PDCCH reception time(ms) | RRM measurement time per DRX (ms) | DL/UL subframe ratio | Sleep ratio |
| RRC-Connected | 320 | 2 | -- | 1 | 10 | 6 | 1 | 91.9% |
| 320 | 2 | 10 | 2 | 10 | 6 | 0.5 | 85.6% |
| 2560 | 2 | -- | 1 | 100 | 6 | 1 | 95.5% |
| 2560 | 2 | 10 | 2 | 100 | 6 | 0.5 | 91.2% |
| 10240 | 2 | -- | 1 | 1600 | 6 | 1 | 84.2% |

From Table 98 it can be seen that high sleep ratios can be achieved for different DRX cycles.

It can therefore be concluded that LTE devices can achieve high sleep ratio for both idle/inactive state and connected state in the unloaded case.

The sleep duration for NR on the device side is given in [14], and the following is an extract of the text:

*Based on LTE DRX mechanism for idle mode and connected mode, the sleep duration for idle mode is 2538 ms for paging cycle of 2560 ms with the assumed parameters, and for connected mode, it is 8624 ms for paging cycle of 10240 ms with the assumed parameters.*

Consequently, the LTE device can achieve very long sleep duration in both idle mode and connected mode.

It can therefore be concluded that LTE meets the device side energy efficiency requirement.

## II-E.11 Reliability

The ITU-R minimum requirements on reliability are given in [1]. The following requirements and remarks are extracted from [1]:

*Reliability relates to the capability of transmitting a given amount of traffic within a predetermined time duration with high success probability.*

*Reliability is the success probability of transmitting a layer 2/3 packet within a required maximum time, which is the time it takes to deliver a small data packet from the radio protocol layer 2/3 SDU ingress point to the radio protocol layer 2/3 SDU egress point of the radio interface at a certain channel quality.*

*This requirement is defined for the purpose of evaluation in the URLLC usage scenario.*

*The minimum requirement for the reliability is 1-10−5 success probability of transmitting a layer 2 PDU (protocol data unit) of 32 bytes within 1 ms in channel quality of coverage edge for the Urban Macro-URLLC test environment, assuming small application data (e.g. 20 bytes application data + protocol overhead).*

*Proponents are encouraged to consider larger packet sizes, e.g. layer 2 PDU size of up to 100 bytes.*

## II-E.11.1 Evaluation methodology and KPIs

The ITU-R minimum requirements on reliability are given in [1]. Specifically, reliability relates to the capability of transmitting a given amount of traffic within a predetermined time duration with high success probability. Reliability is the success probability of transmitting a layer 2/3 packet within a required maximum time, which is the time it takes to deliver a small data packet from the radio protocol layer 2/3 SDU ingress point to the radio protocol layer 2/3 SDU egress point of the radio interface at a certain channel quality. This requirement is defined for the purpose of evaluation in the URLLC usage scenario.

The minimum requirement for the reliability is 1-10−5 success probability of transmitting a layer 2 PDU (protocol data unit) of 32 bytes within 1 ms in channel quality of coverage edge for the Urban Macro-URLLC test environment, assuming small application data   
(e.g. 20 bytes application data + protocol overhead).

## II-E.11.2 Simulation results

The basic evaluation parameters for downlink in Urban – URLLC are provided Table 99:

Table 99

Evaluation parameters

|  |  |
| --- | --- |
|  | **Value** |
| **Inter-site distance** | 500 m |
| **Macro BSs**  **(3 TRxP each)** | 3 |
| **Bandwidth (MHz)** | 10 |
| **Packet size (bytes)** | 50 |

Two scenarios have been examined (Table 100) to determine the reliability metric for the evaluation configurations A and B (CF equals to 700 MHz and 4 GHz respectively). The first one considers a fixed amount of UEs and variable session periods (Figure 13) while the second one uses a fixed session period for every UE and varies the UE density in the area (Figure 14).

Table 100

Scenario configuration

|  |  |  |
| --- | --- | --- |
|  | **UE density** | **Session period** |
| **Scenario 1** | 10 UEs/TRxP | variable |
| **Scenario 2** | variable | 1000 sessions/hour/UE |

Figure 13

Reliability for variable session periods





Figure 14

Reliability for variable UE densities



For uplink reliability, both evaluation configuration A and evaluation configuration B are evaluated. In the evaluation, one-shot PUSCH transmission with 14 OFDM symbols is assumed. The evaluation results are provided in Table 101.

Table 101

Uplink reliability evaluation results for evaluation configuration A and configuration B

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Evaluation configuration | Antenna configuration | Sub-carrier spacing [kHz] | ITU  Requirement | Channel model A | | Channel model B | |
| Channel condition | Reliability | Channel condition | Reliability |
| Evaluation configuration A | 1T8R | 60 | 99.999% | NLOS | 99.999995% | NLOS | 99.9999997% |
| Evaluation configuration B | 1T16R | 60 | NLOS | 99.99989% | NLOS | 99.999992% |

It can be observed that NR can meet the reliability requirement in evaluation configuration A and configuration B.

## II-E.11.2 Summary

The provided results from the conducted system-level simulation show that NR fulfils the reliability constraint for several setups. Frequencies of 700 MHz and 4 GHz have been checked according to the ITU requirements. As it is expected, configuration B (as indicated by ITU) achieves lower reliability values than configuration A almost all the times due to the higher loss it faces. In general, it is shown that the minimum requirement for the reliability is 1-10−5 success probability of transmitting a layer 2 PDU (protocol data unit) of 32 bytes is achieved for up to almost 12,000 sessions/hour at 700 MHz and up to almost 5,000 sessions/hour at 4 GHz. Similarly, reliability is 1-10−5 success probability for UE densities for up to almost 250 UEs/TRx at 700 MHz and up to almost 120 UEs/TRx at 4 GHz.

## II-E.12 Mobility

The ITU-R minimum requirements on mobility are given in [1]. The following requirements and remarks are extracted from [1]:

*Mobility is the maximum mobile station speed at which a defined QoS can be achieved (in km/h).*

*The following classes of mobility are defined:*

*– Stationary: 0 km/h*

*– Pedestrian: 0 km/h to 10 km/h*

*– Vehicular: 10 km/h to 120 km/h*

*– High speed vehicular: 120 km/h to 500 km/h.*

*High speed vehicular up to 500 km/h is mainly envisioned for high speed trains. Table 1 defines the mobility classes that shall be supported in the respective test environments.*

1. Mobility classes

|  |  |  |  |
| --- | --- | --- | --- |
|  | *Test environments for eMBB* | | |
| *Indoor Hotspot – eMBB* | *Dense Urban – eMBB* | *Rural – eMBB* |
| *Mobility classes supported* | *Stationary, Pedestrian* | *Stationary, Pedestrian,*  *Vehicular (up to 30 km/h)* | *Pedestrian, Vehicular, High speed vehicular* |

*A mobility class is supported if the traffic channel link data rate on the uplink, normalized by bandwidth, is as shown in Table 2. This assumes the user is moving at the maximum speed in that mobility class in each of the test environments.*

*This requirement is defined for the purpose of evaluation in the eMBB usage scenario.*

1. Traffic channel link data rates normalized by bandwidth

|  |  |  |
| --- | --- | --- |
| *Test environment* | *Normalized traffic channel link data rate (bit/s/Hz)* | *Mobility (km/h)* |
| *Indoor Hotspot – eMBB* | *1.5* | *10* |
| *Dense Urban – eMBB* | *1.12* | *30* |
| *Rural – eMBB* | *0.8* | *120* |
| *0.45* | *500* |

*These values were defined assuming an antenna configuration as described in Report ITU-R M.2412-0.*

*Proponents are encouraged to consider higher normalized channel link data rates in the uplink. In addition, proponents are encouraged to consider the downlink mobility performance.*

## II-E.12.1 Evaluation methodology

The general evaluation method and procedure for mobility evaluation is defined in Report ITU-R M.2412. This procedure includes system-level simulation (SLS) part and link-level simulation (LLS) part. The following evaluation steps are extracted from Report ITU-R M.2412.

*Step 1:* Run uplink system-level simulations, identical to those for average spectral efficiency, and 5th percentile user spectral efficiency except for speeds taken from Table 4 of Report ITU-R M.2410-0, using link-level simulations and a link-to-system interface appropriate for these speed values, for the set of selected test environment(s) associated with the candidate RITs/SRITs and collect overall statistics for uplink *SINR* values, and construct CDF over these values for each test environment.

*Step 2:* Use the CDF for the test environment(s) to save the respective 50th-percentile *SINR* value.

*Step 3:* Run new uplink link-level simulations for the selected test environment(s) for either NLOS or LOS channel conditions using the associated speeds in Table 4 of Report ITU‑R M.2410‑0, as input parameters, to obtain link data rate and residual packet error ratio as a function of *SINR*. The link-level simulation shall use air interface configuration(s) supported by the proposal and take into account retransmission, channel estimation and phase noise impact.

*Step 4:* Compare the uplink spectral efficiency values (link data rate normalized by channel bandwidth) obtained from *Step 3* using the associated *SINR* value obtained from *Step 2* for selected test environments, with the corresponding threshold values in the Table 4 of Report ITU-R M.2410-0.

*Step 5:* The proposal fulfils the mobility requirement if the spectral efficiency value is larger than or equal to the corresponding threshold value and if also the residual decoded packet error ratio is less than 1%, for all selected test environments. For the selected test environment it is sufficient if one of the spectral efficiency values (using either NLOS or LOS channel conditions) fulfils the threshold.

For SLS part, the pre-processing SINR is used. The pre-processing SINR is defined on an Rx antenna port with respect to a Tx antenna port.

## II-E.12.2 Results

Actual available evaluation results are provided in Table 102. Further details will be provided in the final Evaluation Report.

Table 102

Mobility evaluation results for different test environments

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test environment | ITU requirement (bit/s/Hz) | Evaluation configuration | Channel Model | 50%-ile point of SINR CDF (dB) | Uplink SE (bit/s/Hz) | | | |
| FDD | | TDD | |
| NLOS | LOS | NLOS | LOS |
| Indoor Hotspot –eMBB  (12 TRxP) | 1.5 | Config. A  (4 GHz) | Channel model A | 3.90 | 1.75 | 2.05 | 1.59 | 1.94 |
| Channel model B | 3.95 | 1.75 | 2.07 | 1.60 | 1.95 |
| Dense Urban – eMBB | 1.12 | Config. A  (4 GHz) | Channel model A | 5.52 | 1.92 | 2.22 | 1.82 | 2.17 |
| Channel model B | 5.32 | 1.89 | 2.19 | 1.79 | 2.06 |
| Rural –eMBB  (120 km/h) | 0.8 | Config. A  (700 MHz) | Channel model A | 10.21 | 2.32 | 2.90 | 2.10 | 2.63 |
| Channel model B | 10.14 | 2.31 | 2.90 | 2.09 | 2.63 |
| Config. B  (4 GHz) | Channel model A | 4.66 | 1.30 | 1.74 | 1.18 | 1.57 |
| Channel model B | 4.50 | 1.28 | 1.68 | 1.16 | 1.52 |
| Rural –eMBB  (500 km/h) | 0.45 | Config. A  (700 MHz) | Channel model A | 9.67 | 2.07 | 2.64 | 1.88 | 2.39 |
| Channel model B | 9.65 | 2.07 | 2.64 | 1.87 | 2.39 |
| Config. B  (4 GHz) | Channel model A | 2.90 | 0.92 | 1.33 | 0.84 | 1.22 |
| Channel model B | 2.72 | 0.91 | 1.33 | 0.83 | 1.22 |

It is observed that NR meets the mobility requirements in the test environments for eMBB.

## II-E.13 Mobility interruption time

The ITU-R minimum requirements on mobility interruption time are given in [1]. The following requirements and remarks are extracted from [1]:

*Mobility interruption time is the shortest time duration supported by the system during which a user terminal cannot exchange user plane packets with any base station during transitions.*

*The mobility interruption time includes the time required to execute any radio access network procedure, radio resource control signalling protocol, or other message exchanges between the mobile station and the radio access network, as applicable to the candidate RIT/SRIT.*

*This requirement is defined for the purpose of evaluation in the eMBB and URLLC usage scenarios.*

*The minimum requirement for mobility interruption time is 0 ms.*

The ITU-R Guidelines for Evaluation report [3] is requesting in addition:

*The procedure of exchanging user plane packets with base stations during transitions shall be described based on the proposed technology including the functions and the timing involved.*

## II-E.13.1 Mobility interruption time in NR and LTE

A typical mobility handover procedure includes procedures in the radio access network (RAN) as well as procedures in the core network (CN). Figure 15 shows a handover procedure in NR. It can be observed that there a handover preparation step and a handover execution step in the RAN network between the source next generation RAN (NG-RAN) and the target NG-RAN. During the handover execution procedure, the source NG-RAN needs to forward user plane data to the target NG-RAN using the Xn interface in NR. Next, a number of messaging steps occur between CN functions to modify the user plane data path for the user. Although LTE has a different system architecture, LTE is using similar procedures in LTE RAN and CN.

Figure 15

Mobility handover procedure in NR (intra NR)



Depending on the types of the source cell and the target cell, handover scenarios can additionally include handover between intra-3GPP cells, and handover between 3GPP and non-3GPP cells. Intra-3GPP handover may include intra-NR cells, intra-LTE cells, NR and LTE cells, NR and UTRAN. In this case, the user only needs to ensure its synchronization to the target cell. Handover between 3GPP and non-3GPP cells may include NR- HRPD handover and NR- cdma2000 1X handover. In this case, there is an additional registration process to the target cell. The RAN procedure can result in delays in the order of a few milliseconds while the CN procedure can result in delays in the order of tens of milliseconds.

## II-E.13.2 Means to minimize mobility interruption

In order to satisfy the requirement of 0 ms proposed by ITU-R, a number of means, which are based on the “Make-before-break Handover” and “Dual Connectivity” (DC) principle, have been proposed in Section 5.2.3.2.5 in [16] and Section 5.10 in [20]. With DC, before the handover procedure starts, DC in the master base station (MeNB) will be configured and a secondary base station (SeNB) will be added to the UE.

The SeNB addition procedure and SeNB release procedures are shown in Figure 16, Figure 17, and Figure 18. The SeNB addition procedure is initiated by the MeNB and is used to establish a UE context at the SeNB in order to provide radio resources from the SeNB to the UE. This procedure is used to add at least the first cell (PSCell) of the SCG. Figure 5.10.2.2-1 shows the SeNB addition procedure. The detailed description of each step is found in Section 10.1.2.8.1 in 3GPP TS36.300.

Figure 16

SeNB Addition procedure

**

The SeNB Release procedure may be initiated either by the MeNB or by the SeNB and is used to initiate the release of the UE context at the SeNB. It does not necessarily need to involve signalling towards the UE, e.g., RRC connection re-establishment due to Radio Link Failure in MeNB.

Figure 17

SeNB Release procedure – MeNB initiated

**

Figure 18

SeNB Release procedure – SeNB initiated

**

The DC principle can be applied to intra-NR handover, intra-LTE handover, inter-RAT handover, and inter-system handover. It is observed that during these procedures, the UE can always exchange user plane packets with MeNB during transitions. Therefore, 0ms mobility interruption time is achieved by LTE for the DC mobility scenario.

### II-E.13.2.1 Intra-NR handover

Network controlled mobility applies to UEs in RRC\_CONNECTED and is categorized into two types of mobility.

The first type is cell-level mobility, which requires explicit RRC signalling to be triggered, i.e. handover. For inter-gNB handover, handover request, handover acknowledgement, handover command, handover complete procedure are supported between source gNB and target gNB. Using the “Make-before-break Handover” and DC principle, the release of the resources at the source gNB during the handover completion phase is triggered by the target gNB. The second type is beam-level mobility, which does not require explicit RRC signalling to be triggered. Beam-level mobility is handled by lower layers and RRC is not required to know which beam is being used at a given point in time.

In both types, a UE needs to perform measurement to assist the mobility procedure. In RRC\_CONNECTED, the UE measures multiple beams (at least one) of a cell and the measurements results (power values) are averaged to derive the cell quality. In doing so, the UE is configured to consider a subset of the detected beams: the N best beams above an absolute threshold. Filtering takes place at two different levels: at the physical layer to derive beam quality and then at RRC level to derive cell quality from multiple beams. Cell quality from beam measurements is derived in the same way for the serving cell(s) and for the non-serving cell(s). Measurement reports may contain the measurement results of the X best beams if the UE is configured to do so by the gNB. In addition, data forwarding, in-sequence delivery and duplication avoidance at handover can be guaranteed between target gNB and source gNB. For more details, refer to [17] sub-clauses 9.2.3 & 9.3.

### II-E.13.2.2 Intra-LTE handover

In E-UTRAN RRC\_CONNECTED state, network-controlled UE-assisted handovers and DC specific activities are performed and various DRX cycles are supported. Handover procedures, like processes that precede the final handover decision on the source network side (control and evaluation of UE and eNB measurements taking into account certain UE specific roaming and access restrictions), preparation of resources on the target network side, commanding the UE to the new radio resources and finally releasing resources on the (old) source network side with the DC principle. It contains mechanisms to transfer context data between evolved nodes, and to update node relations on C-plane and U-plane.

Measurements to be performed by a UE for intra/inter-frequency mobility can be controlled by E-UTRAN, using broadcast or dedicated control. In RRC\_IDLE state, a UE shall follow the measurement parameters defined for cell reselection specified by the E-UTRAN broadcast. The use of dedicated measurement control for RRC\_IDLE state is possible through the provision of UE specific priorities. In RRC\_CONNECTED state, a UE shall follow the measurement configurations specified by RRC directed from the E-UTRAN (e.g. as in UTRAN MEASUREMENT\_CONTROL). In RRC\_IDLE and RRC\_CONNECTED the UE may be configured to monitor some UTRA or E-UTRA carriers according to reduced performance requirements as specified in [18]. For more details, refer to [19] sub-clauses 10.1 & 10.2.

### II-E.13.2.3 Inter-RAT handover

Intra 5GC inter RAT mobility is supported between NR and E-UTRA. Inter RAT measurements in NR are limited to E-UTRA and the source RAT should be able to support and configure target RAT measurement and reporting. The in-sequence and lossless handover is supported for the handover between gNB and ng-eNB. Both Xn and NG based inter-RAT handover between NG-RAN nodes is supported. Whether the handover is over Xn or CN is transparent to the UE. The target RAT receives the UE NG-C context information and based on this information configures the UE with a complete RRC message and full configuration (not delta).

## II-E.13.2.4 Inter-System handover

Inter-system handover is supported between 5G Core Network (5GC) and EPC. Handover between NR in 5GC and E-UTRA in EPC is supported via inter-RAT handover. Handover between E-UTRA in 5GC and E-UTRA in EPC is supported via intra-E-UTRA handover with change of CN type. The source eNB/ng-eNB decides handover procedure to trigger (e.g. via the same CN type or to the other CN type). UE has to know the target CN type from the handover command during intra-LTE inter-system handover, intra-LTE intra-system handover.

## II-E.13.3 Evaluation of the proposal

The proposal is using means like “Make-before-break Handover” and DC to mitigate Mobility interruption time. This ensures that the minimum ITU-R requirement above of 0 ms mobility interruption time is fulfilled.

## II-E.14 Bandwidth

The ITU-R minimum requirements on supported bandwidth is given in [1]. The following requirements and additional remarks are following from [1]:

*Bandwidth is the maximum aggregated system bandwidth. The bandwidth may be supported by single or multiple radio frequency (RF) carriers. The bandwidth capability of the RIT/SRIT is defined for the purpose of IMT-2020 evaluation.*

*The requirement for bandwidth is at least 100 MHz.*

*The RIT/SRIT shall support bandwidths up to 1 GHz for operation in higher frequency bands (e.g. above 6 GHz).*

*Proponents are encouraged to consider extensions to support operation in wider bandwidths considering the research targets expressed in Recommendation ITU-R M.2083.*

*The RIT/SRIT shall support scalable bandwidth. Scalable bandwidth is the ability of the candidate RIT/SRIT to operate with different bandwidths.*

The Table 103 and Table 104 are summarizing the characteristics of the SRIT and the NR RIT of 5G.

Table 103

Characteristics template for SRIT of “5G” (Release 15 and beyond)

|  |  |  |
| --- | --- | --- |
| **ITU-R requirements** | **NR component RIT** | **LTE component RIT** |
| Below 6 GHz: at least 100 MHz | [4], [7], Section 5.2.3.2.8.2  **One component carrier** supports a scalable bandwidth, **5, 10, 15, 20, 25, 40, 50, 60, 80, 100MHz** for frequency range 450 MHz to 6000 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 20% to 2%; and a scalable bandwidth, 50, 100, 200, 400 MHz for frequency range 24250 – 52600 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 8% to 5%.  By **aggregating multiple component carriers**, transmission bandwidths **up to 6.4 GHz** are supported to provide high data rates. Component carriers can be either contiguous or non-contiguous in the frequency domain. The number of component carriers transmitted and/or received by a mobile terminal can vary over time depending on the instantaneous data rate.  [4], [7], Section 5.2.3.2.8.5  The 3 dB bandwidth is not part of the specifications, however:   * The **minimum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + 5 MHz for frequency range 450 – 6000 MHz; * **The maximum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + **100 MHz** for frequency range 450 – 6000 MHz; * **Multiple component carriers** can be aggregated to achieve **up to 6.4 GHz** of transmission bandwidth. | [4], [7], Section 5.2.3.2.8.2  **One component carrier** supports a scalable bandwidth, **1.4, 3, 5, 10, 15 and 20 MHz**, with guard band ratio from 23% to 10% (see [12] sub-clause 5.6 for more details).  By **aggregating multiple component carriers**, transmission bandwidths **up to 640 MHz** are supported to provide the high data rates. Component carriers can be either contiguous or non-contiguous in the frequency domain. The number of component carriers transmitted and/or received by a mobile terminal can vary over time depending on the instantaneous data rate.  For NB-IoT, the channel bandwidth is not scalable. There is not aggregation of multiple NB-IoT carriers – see item [4], [7] Section 5.2.3.2.8.1 for more details.  For **eMTC**, the above scalable bandwidth from **1.4 to 20 MHz** is supported. The eMTC UE can have a narrower RF bandwidth than the cell is configured with. Category M1 UE has a bandwidth of 1.4 MHz, and category M2 UE has 5 MHz bandwidth.  [4], [7], Section 5.2.3.2.8.5  The 3 dB bandwidth is not part of the specifications, however:   * The **minimum 99% channel bandwidth** (occupied bandwidth of single component carrier) is 1.4 MHz. * The **maximum 99% channel bandwidth** (occupied bandwidth of single component carrier) is **20 MHz**. * **Multiple component carriers** can be aggregated to achieve **up to 640 MHz** of transmission bandwidth.   For NB-IoT, the 99% channel bandwidth is **0.2 MHz**. |
| Above 6 GHz: up to 1 GHz | [4], [7], Section 5.2.3.2.8.2  **One component carrier** supports a scalable bandwidth, **5, 10, 15, 20, 25, 40, 50, 60, 80, 100 MHz** for frequency range 450 MHz to 6000 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 20% to 2%; and a scalable bandwidth, 50, 100, 200, 400 MHz for frequency range 24250 – 52600 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 8% to 5%.  By **aggregating multiple component carriers**, transmission bandwidths **up to 6.4 GHz** are supported to provide high data rates. Component carriers can be either contiguous or non-contiguous in the frequency domain. The number of component carriers transmitted and/or received by a mobile terminal can vary over time depending on the instantaneous data rate.  [4], [7], Section 5.2.3.2.8.5  The 3 dB bandwidth is not part of the specifications, however:   * The **minimum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + 50 MHz for frequency range 24250 – 52600 MHz * **The maximum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + **400 MHz** for frequency range 24250 – 52600 MHz. * **Multiple component carriers** can be aggregated to achieve **up to 6.4 GHz** of transmission bandwidth. | [4], [7], Section 5.2.3.2.8.2  No higher frequency bands above 6 GHz are supported by the LTE component. |
| Minimum amount of spectrum | [4], [7], Section 5.2.3.2.8.4   * The minimum amount of paired spectrum is **2 x 5 MHz**. * The minimum amount of unpaired spectrum is **5 MHz**. | [4], [7], Section 5.2.3.2.8.4   * The minimum amount of paired spectrum is **2 x 1.4 MHz**, and the minimum amount of unpaired spectrum is **1.4 MHz**, except for NB-IoT. * For NB-IoT, the minimum amount of unpaired spectrum is **0.2 MHz**. |

Table 104

Characteristics template for NR RIT of “5G” (Release 15 and beyond)

|  |  |
| --- | --- |
| **ITU-R requirements** | **NR RIT** |
| Below 6 GHz: at least 100 MHz | [4], [7], Section 5.2.3.2.8.2  **One component carrier** supports a scalable bandwidth, **5, 10, 15, 20, 25, 40, 50, 60, 80, 100MHz** for frequency range 450 MHz to 6000 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 20% to 2%; and a scalable bandwidth, 50, 100, 200, 400MHz for frequency range 24250 – 52600 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 8% to 5%.  By **aggregating multiple component carriers**, transmission bandwidths **up to 6.4 GHz** are supported to provide high data rates. Component carriers can be either contiguous or non-contiguous in the frequency domain. The number of component carriers transmitted and/or received by a mobile terminal can vary over time depending on the instantaneous data rate.  [4], [7], Section 5.2.3.2.8.5  The 3 dB bandwidth is not part of the specifications, however:   * The **minimum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + **5 MHz** for frequency range 450 – 6000 MHz; * The **maximum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + **100 MHz** for frequency range 450 – 6000 MHz;   **Multiple component carriers** can be aggregated to achieve **up to 6.4 GHz** of transmission bandwidth. |
| Above 6 GHz: up to 1 GHz | [4], [7], Section 5.2.3.2.8.2  **One component carrier** supports a scalable bandwidth, **5, 10, 15, 20, 25, 40, 50, 60, 80, 100MHz** for frequency range 450 MHz to 6000 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 20% to 2%; and a scalable bandwidth, 50, 100, 200, 400MHz for frequency range 24250 – 52600 MHz (see [11] for the actual support of bandwidth for each band), with guard band ratio from 8% to 5%.  By **aggregating multiple component carriers**, transmission bandwidths **up to 6.4 GHz** are supported to provide high data rates. Component carriers can be either contiguous or non-contiguous in the frequency domain. The number of component carriers transmitted and/or received by a mobile terminal can vary over time depending on the instantaneous data rate.  [4], [7], Section 5.2.3.2.8.5  The 3 dB bandwidth is not part of the specifications, however:   * The **minimum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + **50 MHz** for frequency range 24250 – 52600 MHz * **The maximum 99% channel bandwidth** (occupied bandwidth of single component carrier) is   + **400 MHz** for frequency range 24250 – 52600 MHz.   **Multiple component carriers** can be aggregated to achieve **up to 6.4 GHz** of transmission bandwidth. |
| Minimum amount of spectrum | [4], [7], Section 5.2.3.2.8.4   * The minimum amount of paired spectrum is **2 x 5 MHz**. * The minimum amount of unpaired spectrum is **5 MHz**. |

The combination of the 3GPP submissions on

• SRIT of “5G” (Release 15 and beyond) including NR component RIT and LTE component RIT and

• NR RIT of “5G” (Release 15 and beyond)

is supporting the minimum requirements on bandwidth of

• at least 100 MHz for frequency bands below 6 GHz

• and up to 1 GHz for higher frequency bands e.g., above 6 GHz.

By means of carrier aggregation higher bandwidth up to 6.4 GHz are possible.

The bandwidth is scalable in several steps.

The 3GPP submission is fulfilling the minimum requirements according to [1].

## II-E.15 Support of wide range of services

The ITU-R requirements on “support of wide range of services” are given in [2] and specifically section 3.1 Services:

*Recommendation ITU-R M.2083 – IMT Vision – Framework and overall objectives of the future development of IMT for 2020 and beyond, envisaged three usage scenarios for IMT-2020:*

*– Enhanced Mobile Broadband (eMBB).*

*– Ultra-reliable and low latency communications (URLLC).*

*– Massive machine type communications (mMTC).*

*Diverse services and applications for the three usage scenarios are envisaged, as shown in Fig. 2 in Recommendation ITU-R M.2083.*

*IMT-2020 RIT/SRIT shall support a wide range of services across different usage scenarios, for which the evaluation methodology is found in § 7.3.3 of Report ITU-R M.2412-0.*

These results will be provided in the final Evaluation Report after all other characteristics have been available.

## II-E.16 Supported spectrum bands

The ITU-R minimum requirements on supported spectrum bands are given in [2]. The following requirements and additional remarks are following from [2]:

*The following frequency bands have been identified for* *IMT in the ITU Radio Regulations by WARC-92, WRC-2000, WRC-07, WRC-12 and WRC-15.*

*450-470 MHz (see No.* ***5.286AA*** *of the Radio Regulations (RR))*

*470-698 MHz (see RR Nos.* ***5.295****,* ***5.308****,* ***5.296A****)*

*694/698-960 MHz (see RR Nos.* ***5.313A****,* ***5.317A****)*

*1 427-1 518 MHz (see RR Nos.* ***5.341A****,* ***5.346****,* ***5.341B****,* ***5.341C****,* ***5.346A****)*

*1 710-2 025 MHz (see RR Nos.* ***5.384A****,* ***5.388****)*

*2 110-2 200 MHz (see RR No.* ***5.388****)*

*2 300-2 400 MHz (see RR No.* ***5.384A****)*

*2 500-2 690 MHz (see RR No.* ***5.384A****)*

*3 300-3 400 MHz (see RR Nos.* ***5.429B****,* ***5.429D****,* ***5.429F****)*

*3 400-3 600 MHz (see RR Nos.* ***5.430A****,* ***5.431B****,* ***5.432A****,* ***5.432B****,* ***5.433A****)*

*3 600-3 700 MHz (see RR No.* ***5.434****)*

*4 800-4 990 MHz (see RR Nos.* ***5.441A****,* ***5.441B****)*

*Frequency arrangements for these bands identified before WRC-15 are incorporated in Recommendation ITU-R M.1036-5. Work on frequency arrangements for the frequency bands that were identified by WRC-15 is currently ongoing in ITU-R.*

*Administrations would endeavour to make spectrum available from the frequency bands listed above.*

*Recommendation ITU-R M.2083 indicates a need of higher frequency bands to support the different usage scenarios with a requirement of several hundred MHz up to at least 1 GHz bandwidth corresponding wider and contiguous spectrum ability. Further, the development of IMT‑2020 is expected to enable new use cases and applications associated with radio traffic growth.*

*Taking into account the IMT-2020 deployment to be expected from the year 2020 onwards, Administrations would endeavour to make spectrum available from the higher frequency bands in a timely manner.*

*The requirements related to spectrum are in the compliance templates in* *§ 5.2.4.2.*

The Table 105 and Table 106 show the supported bands compared to the minimum requirements.

Table 105

Characteristics template for SRIT of “5G” (Release 15 and beyond)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ITU-R [2]  [MHz] | ***For NR component RIT:***[4], [7], Section 5.2.3.2.8.3  *The following frequency bands will be supported, in accordance with spectrum requirements defined by Report ITU-R M.2411-0. Introduction of other ITU-R IMT identified bands are not precluded in the future. 3GPP technologies are also defined as appropriate to operate in other frequency arrangements and bands.* | | | ***For LTE component RIT:***[4], [7], Section 5.2.3.2.8.3  *The following frequency bands are currently specified, in accordance with spectrum requirements defined by Report ITU-R M.2411-0. Introduction of other ITU-R IMT identified bands are not precluded in the future. 3GPP technologies are also defined as appropriate to operate in other frequency arrangements and bands. Detailed information on the following bands can be found in [12] sub-clause 5.5.* | | |
| **Band number** | **UL operating band** | **DL operating band** | **Band number** | **UL operating band** | **DL operating band** |
| 450 – 470 MHz | - | - | - | n73  n72  n31 | 450 – 455 MHz  451 – 456 MHz  452.5 – 457.5 MHz | 460 – 465 MHz  461 – 466 MHz  462.5 – 467.5 MHz |
| 470 – 698 MHz | n71 | 663 – 698 MHz | 617 – 652 MHz | n71 | 663 – 698 MHz | 617 – 652 MHz |
| 694/698 – 960 MHz | n12  n28  n83  n5  n20  n82  n8  n81 | 699 – 716 MHz  703 – 748 MHz  703 – 748 MHz  824 – 849 MHz  832 – 862 MHz  832 – 862 MHz  880 – 915 MHz  880 – 915 MHz | 729 – 746 MHz  758 – 803 MHz  N/A  869 – 894 MHz  791– 821 MHz  N/A  925 – 960 MHz  N/A | n85  n12  n28  n5  n19  n20  n8  n68  n44  n29  n17  n67  n13  n14  n27  n26  n18  n6 | 698 – 716 MHz  699 – 716 MHz  703 – 748 MHz  824 – 849 MHz  830 – 845 MHz  832 – 862 MHz  880 – 915 MHz  698 – 728 MHz  703 – 803 MHz  N/A  704 – 716 MHz  N/A  777 – 787 MHz  788 – 798 MHz  807 – 824 MHz  814 – 849 MHz  815 – 830 MHz  830 – 840 MHz | 728 – 746 MHz  729 – 746 MHz  758 – 803 MHz  869 – 894 MHz  875 – 890 MHz  791– 821 MHz  925 – 960 MHz  753 – 783 MHz  703 – 803 MHz  717 – 728 MHz  734 – 746 MHz  738 – 758 MHz  746 – 756 MHz  758 – 768 MHz  852 – 869 MHz  859 – 894 MHz  860 – 875 MHz  875 – 885 MHz |
| 1427 – 1518 MHz | n51  n76  n75  n74  n50 | 1427 – 1432 MHz  N/A  N/A  1427 – 1470 MHz  1432 – 1517 MHz | 1427 – 1432 MHz  1427 – 1432 MHz  1432 – 1517 MHz  1475 – 1518 MHz  1432 – 1517 MHz | n51  n76  n75  n74  n50  n32  n11  n45  n21  n24 | 1427 – 1432 MHz  N/A  N/A  1427 –1470 MHz  1432 – 1517 MHz  N/A  1427.9 – 1447.9 MHz  1447 – 1467 MHz  1447.9 – 1462.9 MHz  1626.5 – 1660.5 MHz | 1427 – 1432 MHz  1427 – 1432 MHz  1432 – 1517 MHz  1475 – 1518 MHz  1432 – 1517 MHz  1452 – 1496 MHz  1475.9 – 1495.9 MHz  1447 – 1467 MHz  495.9 – 1510.9 MHz  1525 – 1559 MHz |
| 1710 – 2025 MHz  2110 – 2200 MHz | n70  n66  n86  n3  n80  n2  n25  n39  n1  n84  n34 | 1695 – 1710 MHz  1710 – 1780 MHz  1710 – 1780 MHz  1710 – 1785 MHz  1710 – 1785 MHz  1850 – 1910 MHz  1850 – 1915 MHz  1880 – 1920 MHz  1920 – 1980 MHz  1920 – 1980 MHz  2010 – 2025 MHz | 1995– 2020 MHz  2110 – 2200 MHz  N/A  1805 – 1880 MHz  N/A  1930 – 1990 MHz  1930 – 1995 MHz  1880 – 1920 MHz  2110 – 2170 MHz  N/A  2010 – 2025 MHz | n70  n66  n3  n2  n1  n4  n10  n9  n35  n25  n39  n33  n37  n65  n36  n23  n34 | 1695 – 1710 MHz  1710 – 1780 MHz  1710 – 1785 MHz  1850 – 1910 MHz  1920 – 1980 MHz  1710 – 1755 MHz  1710 – 1770 MHz  1749.9 – 1784.9 MHz  1850 – 1910 MHz  1850 – 1915 MHz  1880 – 1920 MHz  1900 33 – 1920 MHz  1910 – 1930 MHz  1920 – 2010 MHz  1930 – 1990 MHz  2000 – 2020 MHz  2010 – 2025 MHz | 1995– 2020 MHz  2110 – 2200 MHz  1805 – 1880 MHz  1930 – 1990 MHz  2110 – 2170 MHz  2110 – 2155 MHz  2110 – 2170 MHz  1844.9 – 1879.9 MHz  1850 – 1910 MHz  1930 – 1995 MHz  1880 – 1920 MHz  1900 33 – 1920 MHz  1910 – 1930 MHz  2110 – 2200 MHz  1930 – 1990 MHz  2180 – 2200 MHz  2010 – 2025 MHz |
| 2300 – 2400 MHz | n40 | 2300 – 2400 MHz | 2300 – 2400 MHz | n40  n30 | 2300 – 2400 MHz  2305 – 2315 MHz | 2300 – 2400 MHz  2350 – 2360 MHz |
| 2500 – 2690 MHz | n41  n7  n38 | 2496 – 2690 MHz  2500 – 2570 MHz  2570 – 2620 MHz | 2496 – 2690 MHz  2620 – 2690 MHz  2570 – 2620 MHz | n41  n7  n38  n69 | 2496 – 2690 MHz  2500 – 2570 MHz  2570 – 2620 MHz  N/A | 2496 – 2690 MHz  2620 – 2690 MHz  2570 – 2620 MHz  2570 – 2570 MHz |
| 3300 – 3400 MHz  3400 – 3600 MHz  3600 – 3700 MHz  4800 – 4990 MHz | n78  n77  n79 | 3.3 – 3.8 GHz  3.3 – 4.2 GHz  4.4 – 5.0 GHz | 3.3 – 3.8 GHz  3.3 – 4.2 GHz  4.4 – 5.0 GHz | n52  n42  n22  n48 / n49  n43  n46  n47 | 3300 – 3400 MHz  3400 – 3600 MHz  3410 – 3490 MHz  3550 – 3700 MHz  3600 – 3800 MHz  5150 – 5925 MHz  5855 – 5925 MHz | 3300 – 3400 MHz  3400 – 3600 MHz  3510 – 3590 MHz  3550 – 3700 MHz  3600 – 3800 MHz  5150 – 5925 MHz  5855 – 5925 MHz |
|  |  |  |  |  |  |  |
| Higher frequency bands are subject of WRC 2019 | n258 | 24.25 – 27.5 GHz | 24.25 – 27.5 GHz | - | - | - |
| n257 | 26.5 –29.5 GHz | 26.5 – 29.5 GHz |  |  |  |
| n261 | 27.5 – 28.35 GHz | 27.5 – 28.35 GHz | - | - | - |
| n260 | 37 – 40 GHz | 37 – 40 GHz | - | - | - |
|  |  |  |  |  |  |  |
|  | **Remark by 3GPP** [4], [7], Section 5.2.3.2.8.3  *For NB-IoT, Category NB1 and NB2 are designed to operate in band 1, 2, 3, 4, 5, 8, 11, 12, 13, 17, 18, 19, 20, 21, 25, 26, 28, 31, 41, 66, 70, 71, 72 and 74 in the above table. See more details in [12] sub-clause 5.5F.*  *For eMTC, UE category M1 and M2 is designed to operate in band 1, 2, 3, 4, 5, 7, 8, 11, 12, 13, 14, 18, 19, 20, 21, 25, 26, 27, 28, 31, 39, 40, 41, 66, 71, 72 and 74 in the above table. See more details in [12] sub-clause 5.5E.*  *For V2X communication, the bands can be found in [12] sub-clause 5.5G.* | | | | | |

Table 106

Characteristics template for NR RIT of “5G” (Release 15 and beyond)

|  |  |  |  |
| --- | --- | --- | --- |
| ITU-R [2]  [MHz] | ***For NR component RIT:***[4], [7], Section 5.2.3.2.8.3  *The following frequency bands will be supported, in accordance with spectrum requirements defined by Report ITU-R M.2411-0. Introduction of other ITU-R IMT identified bands are not precluded in the future. 3GPP technologies are also defined as appropriate to operate in other frequency arrangements and bands.* | | |
| **Band number** | **UL operating band** | **DL operating band** |
| 450 – 470 MHz | - | - | - |
| 470 – 698 MHz | n71 | 663 – 698 MHz | 617 – 652 MHz |
| 694/698 – 960 MHz | n12  n28  n83  n5  n20  n82  n8  n81 | 699 – 716 MHz  703 – 748 MHz  703 – 748 MHz  824 – 849 MHz  832 – 862 MHz  832 – 862 MHz  880 – 915 MHz  880 – 915 MHz | 729 – 746 MHz  758 – 803 MHz  N/A  869 – 894 MHz  791– 821 MHz  N/A  925 – 960 MHz  N/A |
| 1427 – 1518 MHz | n51  n76  n75  n74  n50 | 1427 – 1432 MHz  N/A  N/A  1427 –1470 MHz  1432 – 1517 MHz | 1427 – 1432 MHz  1427 – 1432 MHz  1432 – 1517 MHz  1475 – 1518 MHz  1432 – 1517 MHz |
| 1710 – 2025 MHz  2110 – 2200 MHz | n70  n66  n86  n3  n80  n2  n25  n39  n1  n84  n34 | 1695 – 1710 MHz  1710 – 1780 MHz  1710 – 1780 MHz  1710 – 1785 MHz  1710 – 1785 MHz  1850 – 1910 MHz  1850 – 1915 MHz  1880 – 1920 MHz  1920 – 1980 MHz  1920 – 1980 MHz  2010 – 2025 MHz | 1995– 2020 MHz  2110 – 2200 MHz  N/A  1805 – 1880 MHz  N/A  1930 – 1990 MHz  1930 – 1995 MHz  1880 – 1920 MHz  2110 – 2170 MHz  N/A  2010 – 2025 MHz |
| 2300 – 2400 MHz | n40 | 2300 – 2400 MHz | 2300 – 2400 MHz |
| 2500 – 2690 MHz | n41  n7  n38 | 2496 – 2690 MHz  2500 – 2570 MHz  2570 – 2620 MHz | 2496 – 2690 MHz  2620 – 2690 MHz  2570 – 2620 MHz |
| 3300 – 3400 MHz  3400 – 3600 MHz  3600 – 3700 MHz  4800 – 4990 MHz | n78  n77  n79 | 3.3 – 3.8 GHz  3.3 – 4.2 GHz  4.4 – 5.0 GHz | 3.3 – 3.8 GHz  3.3 – 4.2 GHz  4.4 – 5.0 GHz |
|  |  |  |  |
| Higher frequency bands are subject of WRC 2019 | n258 | 24.25 – 27.5 GHz | 24.25 – 27.5 GHz |
| n257 | 26.5 –29.5 GHz | 26.5 – 29.5 GHz |
| n261 | 27.5 – 28.35 GHz | 27.5 – 28.35 GHz |
| n260 | 37 – 40 GHz | 37 – 40 GHz |
|  |  |  |  |

The combination of the 3GPP submissions on

• SRIT of “5G” (Release 15 and beyond) including NR component RIT and LTE component RIT and

• NR RIT of “5G” (Release 15 and beyond)

is supporting all frequency bands, which are identified for IMT in the ITU Radio Regulations by WARC-92, WRC-2000, WRC-07, WRC-12 and WRC-15.

In addition, the 3GPP submissions are also including higher frequency bands to support the different usage scenarios with a requirement of several hundred MHz up to at least 1 GHz bandwidth corresponding wider and contiguous spectrum ability (c.f. Section 14 on Bandwidth).

The 3GPP submission is fulfilling the minimum requirements according to [2].

## II-E.17 Analysis of submitted link budgets

In Report ITU-R M.2133 Section 4.2.3.3, link budget templates are given.

For a given deployment scenario many of the parameter values called out in the link budget templates are given in or are given constraints in Report ITU-R M.2135, § 8. The corresponding parameter entries in the link budget templates follow those sets of values or constraints.

The parameter entries for which there is no guidance in the template should be provided by the proponent. There is no specific requirement associated with how these input parameters have been chosen by the proponent. Furthermore, there is no specific requirement associated with the *results* of the link budget calculations.

In that sense, the link budgets are only informative, but they should be filled in and calculated correctly.

For each of the FDD RIT and TDD RIT, the proponent has supplied link budgets for the LoS and NLOS propagation case (and in the microcellular case also the Outdoor-to-Indoor propagation case) for all mandatory scenarios for all four test environments. For the base coverage urban test environment also link budgets for the optional suburban macro-cell deployment are given.

In a note after each link budget, the proponent states that “*it was necessary to provide separate values for the data channel and the control channel in the following entries: cell area reliability, items 15, 16, 17, 18 and 25 for the reason that the control channel link budget is based on a set of different parameters from those for the data channel, e.g. the bandwidth, cell area reliability, receiver interference density, shadow fading margin, etc.”*

This is a more detailed approach than what Report ITU-R M.2133 requires and provides more information on the balance between control and data link budgets.

*As a conclusion, 5G Infrastructure Association finds that the proponent has supplied all required information for both the TDD and FDD RIT in all test environments. Furthermore, it has been verified that all these link budgets are filled in and that the calculations has been performed correctly.*

The Table 107, Table 108 and Table 109 summarize available results to the three radio environments. Further elaborated results will pe provided in the final Evaluation Report.

Table 107

Indoor Hotspot – eMBB

|  |  |  |
| --- | --- | --- |
| **Item** | **Downlink** | **Uplink** |
| **System configuration** | | |
| Carrier frequency (GHz) | 4/30 | 4/30 |
| BS antenna heights (m) | 3 | 3 |
| UT antenna heights (m) | 1.5 | 1.5 |
| Cell area reliability(1) (%) (Please specify how it is calculated.) |  |  |
| Transmission bit rate for control channel (bit/s) |  |  |
| Transmission bit rate for data channel (bit/s) |  |  |
| Target packet error rate for the required SNR in item (19a) for control channel |  |  |
| Target packet error rate for the required SNR in item (19b) for data channel |  |  |
| Spectral efficiency(2) (bit/s/Hz) |  |  |
| Pathloss model(3) (select from LoS or NLoS) | Mixed | Mixed |
| Mobile speed (km/h) | 3 | 3 |
| Feeder loss (dB) | 0 | 0 |
| **Transmitter** | | |
| (1) Number of transmit antennas. (The number shall be within the indicated range in Table 6 of Report ITU-R M.2135) | 32 | 4 |
| (2) Maximal transmit power per antenna (dBm) | 6/9 | 17 |
| (3) Total transmit power = function of (1) and (2) (dBm)  (The value shall not exceed the indicated value in Table 6 of Report  ITU-R M.2135) | 21/24 | 23 |
| (4) Transmitter antenna gain (dBi) | 5 | 5 |
| (5) Transmitter array gain (depends on transmitter array configurations and technologies such as adaptive beam forming, CDD (cyclic delay diversity), etc.) (dB) | Maximum 15 | Maximum 6 |
| (6) Control channel power boosting gain (dB) | 0 | 0 |
| (7) Data channel power loss due to pilot/control boosting (dB) | 0 | 0 |
| (8) Cable, connector, combiner, body losses, etc. (enumerate sources) (dB) (feeder loss must be included for and only for downlink) | 0 | 0 |
| (9a) Control channel EIRP = (3) + (4) + (5) + (6) – (8) dBm | 41/44 | 34 |
| (9b) Data channel EIRP = (3) + (4) + (5) – (7) – (8) dBm | 41/44 | 34 |
| **Receiver** | | |
| (10) Number of receive antennas (The number shall be within the indicated range in Table 6 of Report ITU-R M.2135) | 4 | 32 |
| (11) Receiver antenna gain (dBi) | 0/5 | 0 |
| (12) Cable, connector, combiner, body losses, etc. (enumerate sources) (dB) (feeder loss must be included for and only for uplink) | 0 | 0 |
| (13) Receiver noise figure (dB) | 7 | 5 |
|  |  |  |
|  |  |  |
| **Item** | **Downlink** | **Uplink** |
| **Receiver (*cont.*)** |  |  |
| (14) Thermal noise density (dBm/Hz) | –174 | –174 |
| (15) Receiver interference density (dBm/Hz) |  |  |
| (16) Total noise plus interference density  = 10 log (10^(((13) + (14))/10) + 10^((15)/10)) dBm/Hz |  |  |
| (17) Occupied channel bandwidth (for meeting the requirements of the traffic type) (Hz) | 20M/80M | 20M/80M |
| (18) Effective noise power = (16) + 10 log((17)) dBm |  |  |
| (19a) Required SNR for the control channel (dB) |  |  |
| (19b) Required SNR for the data channel (dB) |  |  |
| (20) Receiver implementation margin (dB) |  |  |
| (21a) H-ARQ gain for control channel (dB) |  |  |
| (21b) H-ARQ gain for data channel (dB) |  |  |
| (22a) Receiver sensitivity for control channel  = (18) + (19a) + (20) – (21a) dBm |  |  |
| (22b) Receiver sensitivity for data channel  = (18) + (19b) + (20) – (21b) dBm |  |  |
| (23a) Hardware link budget for control channel  = (9a) + (11) − (22a) dB |  |  |
| (23b) Hardware link budget for data channel  = (9b) + (11) − (22b) dB |  |  |
| **Calculation of available pathloss** | | |
| (24) Lognormal shadow fading std deviation (dB) | 3(LOS)/8(NLOS) | 3(LOS)/8(NLOS) |
| (25) Shadow fading margin (function of the cell area reliability and (24)) (dB) |  |  |
| (26) BS selection/macro-diversity gain (dB) | 0 | 0 |
| (27) Penetration margin (dB) | 0 | 0 |
| (28) Other gains (dB) (if any please specify) | 0 | 0 |
| (29a) Available path loss for control channel  = (23a) – (25) + (26) – (27) + (28) – (12) dB |  |  |
| (29b) Available path loss for data channel  = (23b) – (25) + (26) – (27) + (28) – (12) dB |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | | **Downlink** | | **Uplink** |
| **Range/coverage efficiency calculation** | | | | |
| (30a) Maximum range for control channel (based on (29a) and according to the system configuration section of the link budget) (m) |  | |  | |
| (30b) Maximum range for data channel (based on (29b) and according to the system configuration section of the link budget) (m) |  | |  | |
| (31a) Coverage Area for control channel = (π (30a)2) (m2/site) |  | |  | |
| (31b) Coverage Area for data channel = (π (30b)2) (m2/site) |  | |  | |

Table 108

UMa – eMBB

|  |  |  |
| --- | --- | --- |
| **Item** | **Downlink** | **Uplink** |
| **System configuration** | | |
| Carrier frequency (GHz) | 4/30 | 4/30 |
| BS antenna heights (m) | 25 | 25 |
| UT antenna heights (m) | Outdoor UEs: 1.5 m  Indoor UTs: 3(n – 1) + 1.5; n~uniform(1,N) where N~ uniform(4,8) | Outdoor UEs: 1.5 m  Indoor UTs: 3(n – 1) + 1.5; n~uniform(1,N) where N~ uniform(4,8) |
| Cell area reliability(1) (%) (Please specify how it is calculated.) |  |  |
| Transmission bit rate for control channel (bit/s) |  |  |
| Transmission bit rate for data channel (bit/s) |  |  |
| Target packet error rate for the required SNR in item (19a) for control channel |  |  |
| Target packet error rate for the required SNR in item (19b) for data channel |  |  |
| Spectral efficiency(2) (bit/s/Hz) |  |  |
| Pathloss model(3) (select from LoS or NLoS) | Mixed | Mixed |
| Mobile speed (km/h) | 3 | 3 |
| Feeder loss (dB) | 0 | 0 |
| **Transmitter** | | |
| (1) Number of transmit antennas. (The number shall be within the indicated range in Table 6 of Report ITU-R M.2135) | 32/256 | 2/32 |
| (2) Maximal transmit power per antenna (dBm) | 29/20 | 30/8 |
| (3) Total transmit power = function of (1) and (2) (dBm)  (The value shall not exceed the indicated value in Table 6 of Report  ITU-R M.2135) | 44 | 23 |
| (4) Transmitter antenna gain (dBi) | 8 | 0 |
| (5) Transmitter array gain (depends on transmitter array configurations and technologies such as adaptive beam forming, CDD (cyclic delay diversity), etc.) (dB) | Maximum 15/24 | Maximum 3/15 |
| (6) Control channel power boosting gain (dB) | 0 | 0 |
| (7) Data channel power loss due to pilot/control boosting (dB) | 0 | 0 |
| (8) Cable, connector, combiner, body losses, etc. (enumerate sources) (dB) (feeder loss must be included for and only for downlink) | 0 | 0 |
| (9a) Control channel EIRP = (3) + (4) + (5) + (6) – (8) dBm | 67/76 | 26/38 |
| (9b) Data channel EIRP = (3) + (4) + (5) – (7) – (8) dBm | 67/76 | 26/38 |
| **Receiver** | | |
| (10) Number of receive antennas (The number shall be within the indicated range in Table 6 of Report ITU-R M.2135) | 4 | 32 |
| (11) Receiver antenna gain (dBi) | 0 | 8 |
| (12) Cable, connector, combiner, body losses, etc. (enumerate sources) (dB) (feeder loss must be included for and only for uplink) | 0 | 0 |
| (13) Receiver noise figure (dB) | 7 | 5 |
|  |  |  |
|  |  |  |
| **Item** | **Downlink** | **Uplink** |
| **Receiver (*cont.*)** |  |  |
| (14) Thermal noise density (dBm/Hz) | –174 | –174 |
| (15) Receiver interference density (dBm/Hz) |  |  |
| (16) Total noise plus interference density  = 10 log (10^(((13) + (14))/10) + 10^((15)/10)) dBm/Hz |  |  |
| (17) Occupied channel bandwidth (for meeting the requirements of the traffic type) (Hz) | 20M/80M | 10M/80M |
| (18) Effective noise power = (16) + 10 log((17)) dBm |  |  |
| (19a) Required SNR for the control channel (dB) |  |  |
| (19b) Required SNR for the data channel (dB) |  |  |
| (20) Receiver implementation margin (dB) |  |  |
| (21a) H-ARQ gain for control channel (dB) |  |  |
| (21b) H-ARQ gain for data channel (dB) |  |  |
| (22a) Receiver sensitivity for control channel  = (18) + (19a) + (20) – (21a) dBm |  |  |
| (22b) Receiver sensitivity for data channel  = (18) + (19b) + (20) – (21b) dBm |  |  |
| (23a) Hardware link budget for control channel  = (9a) + (11) − (22a) dB |  |  |
| (23b) Hardware link budget for data channel  = (9b) + (11) − (22b) dB |  |  |
| **Calculation of available pathloss** | | |
| (24) Lognormal shadow fading std deviation (dB) | 4/6 | 4/6 |
| (25) Shadow fading margin (function of the cell area reliability and (24)) (dB) | 0 | 0 |
| (26) BS selection/macro-diversity gain (dB) | 0 | 0 |
| (27) Penetration margin (dB) | 0 for ourdoor user, 31 for indoor user | 0 for ourdoor user, 31 for indoor user |
| (28) Other gains (dB) (if any please specify) | 0 | 0 |
| (29a) Available path loss for control channel  = (23a) – (25) + (26) – (27) + (28) – (12) dB |  |  |
| (29b) Available path loss for data channel  = (23b) – (25) + (26) – (27) + (28) – (12) dB |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | | **Downlink** | | **Uplink** |
| **Range/coverage efficiency calculation** | | | | |
| (30a) Maximum range for control channel (based on (29a) and according to the system configuration section of the link budget) (m) |  | |  | |
| (30b) Maximum range for data channel (based on (29b) and according to the system configuration section of the link budget) (m) |  | |  | |
| (31a) Coverage Area for control channel = (π (30a)2) (m2/site) |  | |  | |
| (31b) Coverage Area for data channel = (π (30b)2) (m2/site) |  | |  | |

Table 109

Rural – eMBB

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Downlink** | | **Uplink** | |
| **System configuration** | | | | |
| Carrier frequency (GHz) | 0.7/4 | | 0.7/4 | |
| BS antenna heights (m) | 35 | | 35 | |
| UT antenna heights (m) | 1.5 | | 1.5 | |
| Cell area reliability(1) (%) (Please specify how it is calculated.) |  | |  | |
| Transmission bit rate for control channel (bit/s) |  | |  | |
| Transmission bit rate for data channel (bit/s) |  | |  | |
| Target packet error rate for the required SNR in item (19a) for control channel |  | |  | |
| Target packet error rate for the required SNR in item (19b) for data channel |  | |  | |
| Spectral efficiency(2) (bit/s/Hz) |  | |  | |
| Pathloss model(3) (select from LoS or NLoS) | Mixed | | Mixed | |
| Mobile speed (km/h) | 3 | | 3 | |
| Feeder loss (dB) | 0 | | 0 | |
| **Transmitter** | | | | |
| (1) Number of transmit antennas. (The number shall be within the indicated range in Table 6 of Report ITU-R M.2135) | 8/32 | | 2/4 | |
| (2) Maximal transmit power per antenna (dBm) | 37/31 | | 20/17 | |
| (3) Total transmit power = function of (1) and (2) (dBm)  (The value shall not exceed the indicated value in Table 6 of Report  ITU-R M.2135) | 46 | | 23 | |
| (4) Transmitter antenna gain (dBi) | 8 | | 0 | |
| (5) Transmitter array gain (depends on transmitter array configurations and technologies such as adaptive beam forming, CDD (cyclic delay diversity), etc.) (dB) | Maximum 9/15 | | Maximum 3/6 | |
| (6) Control channel power boosting gain (dB) | 0 | | 0 | |
| (7) Data channel power loss due to pilot/control boosting (dB) | 0 | | 0 | |
| (8) Cable, connector, combiner, body losses, etc. (enumerate sources) (dB) (feeder loss must be included for and only for downlink) | 0 | | 0 | |
| (9a) Control channel EIRP = (3) + (4) + (5) + (6) – (8) dBm | 63/69 | | 26/33 | |
| (9b) Data channel EIRP = (3) + (4) + (5) – (7) – (8) dBm | 63/69 | | 26/33 | |
| **Receiver** | | | | |
| (10) Number of receive antennas (The number shall be within the indicated range in Table 6 of Report ITU-R M.2135) | 4 | | 8/32 | |
| (11) Receiver antenna gain (dBi) | 0 | | 8 | |
| (12) Cable, connector, combiner, body losses, etc. (enumerate sources) (dB) (feeder loss must be included for and only for uplink) | 0 | | 0 | |
| (13) Receiver noise figure (dB) | 7 | | 5 | |
|  |  | |  | |
|  |  | |  | |
| **Item** | **Downlink** | | **Uplink** | |
| **Receiver (*cont.*)** |  | |  | |
| (14) Thermal noise density (dBm/Hz) | –174 | | –174 | |
| (15) Receiver interference density (dBm/Hz) |  | |  | |
| (16) Total noise plus interference density  = 10 log (10^(((13) + (14))/10) + 10^((15)/10)) dBm/Hz |  | |  | |
| (17) Occupied channel bandwidth (for meeting the requirements of the traffic type) (Hz) | 20M/80M | | 10M/80M | |
| (18) Effective noise power = (16) + 10 log((17)) dBm |  | |  | |
| (19a) Required SNR for the control channel (dB) |  | |  | |
| (19b) Required SNR for the data channel (dB) |  | |  | |
| (20) Receiver implementation margin (dB) |  | |  | |
| (21a) H-ARQ gain for control channel (dB) |  | |  | |
| (21b) H-ARQ gain for data channel (dB) |  | |  | |
| (22a) Receiver sensitivity for control channel  = (18) + (19a) + (20) – (21a) dBm |  | |  | |
| (22b) Receiver sensitivity for data channel  = (18) + (19b) + (20) – (21b) dBm |  | |  | |
| (23a) Hardware link budget for control channel  = (9a) + (11) − (22a) dB |  | |  | |
| (23b) Hardware link budget for data channel  = (9b) + (11) − (22b) dB |  | |  | |
| **Calculation of available pathloss** | | | | |
| (24) Lognormal shadow fading std deviation (dB) | 4/6 | | 4/6 | |
| (25) Shadow fading margin (function of the cell area reliability and (24)) (dB) | 0 | | 0 | |
| (26) BS selection/macro-diversity gain (dB) | 0 | | 0 | |
| (27) Penetration margin (dB) | 0 | | 0 | |
| (28) Other gains (dB) (if any please specify) | 0 | | 0 | |
| (29a) Available path loss for control channel  = (23a) – (25) + (26) – (27) + (28) – (12) dB |  | |  | |
| (29b) Available path loss for data channel  = (23b) – (25) + (26) – (27) + (28) – (12) dB |  | |  | |
| **Item** | | **Downlink** | | **Uplink** |
| **Range/coverage efficiency calculation** | | | | |
| (30a) Maximum range for control channel (based on (29a) and according to the system configuration section of the link budget) (m) |  | |  | |
| (30b) Maximum range for data channel (based on (29b) and according to the system configuration section of the link budget) (m) |  | |  | |
| (31a) Coverage Area for control channel = (π (30a)2) (m2/site) |  | |  | |
| (31b) Coverage Area for data channel = (π (30b)2) (m2/site) |  | |  | |

# II-F Questions and feedback to WP 5D and/or the proponents or other IEGs

The minimum requirements on Dense Urban for 30 GHz cannot be realized due to a too high path loss.

# II-G In the inhjterim report, kindly provide the proposed next steps towards the final report to be sent to WP 5D for the February 2020 meeting

Some aspects of the system evaluation are still under preparation and will be provided in the final Evaluation Report:

• Link budget calculation are work in progress.

• User Plane Latency evaluation is work in progress.

• Control Plane Latency for the LTE component is work in progress.

• Mobility: Further details will be provided in the final Evaluation Report.

• Support of Wide Range of Services can only be evaluated after all other characteristics have been evaluated.

The 5G Infrastructure Association Evaluation Group will finalize the missing evaluation characteristics and results before submitting the final Evaluation Report in February 2020.

Potentially, detailed interactions with other evaluation groups will take place after the ITU-R Evaluation Workshop on December 10 and 11, 2019.

# Part III: Conclusion

# III-1 Completeness of submission

5G Infrastructure Association finds that the submission in [4], [5], [6], [7] and [8] are ‘complete’ according to [2].

# III-2 Compliance with requirements

These are the main conclusions on the 5G Infrastructure Association evaluation of the evaluated proposal. In Table 110 below, it is shown whether or not 5G Infrastructure Association has confirmed the proponent’s claims relating to IMT-Advanced requirements.

The phrase ‘Requirements fulfilled’ in the tables below indicates that 5G Infrastructure Association Evaluation Group assessment confirms the associated claim from the proponent that the requirement is fulfilled.

In Section III-2.1 the detailed compliance templates are summarized.

## III-2.1 Overall compliance

Table 110

5G Infrastructure Association assessment of compliance with requirements

| Characteristic for evaluation | RIT NR:  5G IA assessment | RIT LTE:  5G IA assessment | Section |
| --- | --- | --- | --- |
| Peak data rate | Requirements fulfilled | Requirements fulfilled | Part II-E.1 |
| Peak spectral efficiency | Requirements fulfilled | Requirements fulfilled | Part II-E.2 |
| User experienced data rate | Requirements fulfilled except II-E.3.2.2 for dense urban TDD at 30 GHz | Not applicable | Part II-E.3 |
| 5th percentile user spectral efficiency | Requirements fulfilled except II-E.4.2.2.2 for dense urban at 30 GHz | Not applicable | Part II-E.4 |
| Average spectral efficiency | Requirements fulfilled except II-E.5.2.2.2 for dense urban at 30 GHz | Not applicable | Part II-E.5 |
| Area traffic capacity | Requirements fulfilled | Not applicable | Part II-E.6 |
| User plane latency | Results provided in final Evaluation Report | Results provided in final Evaluation Report | Part II-E.7 |
| Control plane latency | Requirements fulfilled | Results provided in final Evaluation Report | Part II-E.8 |
| Connection density | Requirements fulfilled | Results provided in final Evaluation Report | Part II-E.9 |
| Energy efficiency | Requirements fulfilled | Requirements fulfilled | Part II-E.10 |
| Reliability | Requirements fulfilled | Requirements fulfilled | Part II-E.11 |
| Mobility | Requirements fulfilled | Requirements fulfilled | Part II-E.12 |
| Mobility interruption time | Requirements fulfilled | Requirements fulfilled | Part II-E.13 |
| Bandwidth | Requirements fulfilled | Requirements fulfilled | Part II-E.14 |
| Support of wide range of services | Will be provided in the final Evaluation Report after all other characteristics are evaluated | Will be provided in the final Evaluation Report after all other characteristics are evaluated | Part II-E.15 |
| Supported spectrum band(s)/range(s) | Requirements fulfilled | Requirements fulfilled | Part II-E.16 |

It should be noted that the analysis behind the analytical and inspection results is not limited by properties of the test environment; hence all these conclusions are valid for all test environments.

## III-2.2 Detailed compliance templates

### III-2-2.1 Compliance template **for** services[[4]](#footnote-4)

|  |  |  |
| --- | --- | --- |
|  | Service capability requirements | Evaluator’s comments |
| **5.2.4.1.1** | **Support for wide range of services**  Is the proposal able to support a range of services across different usage scenarios (eMBB, URLLC, and mMTC)?: YES / NO  Specify which usage scenarios (eMBB, URLLC, and mMTC) the candidate RIT or candidate SRIT can support.(1) | These details will be provided in the final Evaluation Report after all evaluation characteristics have been evaluated. |
| (1) Refer to the process requirements in IMT-2020/2. | | |

### III-2-2.2 Compliance template for spectrum3

|  |  |
| --- | --- |
|  | Spectrum capability requirements |
| **5.2.4.2.1** | **Frequency bands identified for IMT**  Is the proposal able to utilize at least one frequency band identified for IMT in the ITU Radio Regulations?: X YES / NO  Specify in which band(s) the candidate RIT or candidate SRIT can be deployed. |
| **5.2.4.2.2** | **Higher Frequency range/band(s)**  Is the proposal able to utilize the higher frequency range/band(s) above 24.25 GHz?: X YES / NO  Specify in which band(s) the candidate RIT or candidate SRIT can be deployed.  Details are provided in Section II-E.16.  NOTE 1 – In the case of the candidate SRIT, at least one of the component RITs need to fulfil this requirement. |

### III-2-2.3 Compliance template for **technical** performance3

| Minimum technical performance requirements item (5.2.4.3.x), units, and Report ITU-R M.2410-0 section reference(1) | Category | | | Required value | Value(2) | Requirement met? | Comments (3) |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Usage scenario | Test environment | Downlink or uplink |  |  |  |  |
| **5.2.4.3.1** Peak data rate (Gbit/s) *(4.1)* | eMBB | Not applicable | Downlink | 20 |  | X Yes  No | c.f.  II-E.1 |
| Uplink | 10 |  | X Yes  No |
| **5.2.4.3.2** Peak spectral efficiency (bit/s/Hz) *(4.2)* | eMBB | Not applicable | Downlink | 30 |  | X Yes  No | c.f.  II-E.2 |
| Uplink | 15 |  | X Yes  No |
| **5.2.4.3.3** User experienced data rate (Mbit/s) *(4.3)* | eMBB | Dense Urban – eMBB | Downlink | 100 |  | X Yes  No | c.f.  II-E.3  Not fulfilled in config-B, c.f. explanation |
| Uplink | 50 |  | X Yes  No |
| **5.2.4.3.4** 5th percentile user spectral efficiency (bit/s/Hz) *(4.4)* | eMBB | Indoor Hotspot – eMBB | Downlink | 0.3 |  | X Yes  No | c.f.  II-E.4 |
| Uplink | 0.21 |  | X Yes  No |
| eMBB | Dense Urban – eMBB | Downlink | 0.225 |  | X Yes  No | c.f.  II-E.4  Not fulfilled in config-B, c.f. explanation |
| Uplink | 0.15 |  | X Yes  No |
| eMBB | Rural – eMBB | Downlink | 0.12 |  | X Yes  No | c.f.  II-E.4 |
| Uplink | 0.045 |  | X Yes  No |
| **5.2.4.3.5** Average spectral efficiency (bit/s/Hz/ TRxP) *(4.5)* | eMBB | Indoor Hotspot – eMBB | Downlink | 9 |  | X Yes  No | c.f.  II-E.5 |
| Uplink | 6.75 |  | X Yes  No |
| eMBB | Dense Urban – eMBB | Downlink | 7.8 |  | X Yes  No | c.f.  E-II.5  Not fulfilled in Config-B, c.f. explanation |
| Uplink | 5.4 |  | X Yes  No |
| eMBB | Rural – eMBB | Downlink | 3.3 |  | X Yes  No | c.f.  E-II.5 |
| Uplink | 1.6 |  | X Yes  No | c.f.  E-II.5 |
| **5.2.4.3.6** Area traffic capacity (Mbit/s/m2) *(4.6)* | eMBB | Indoor-Hotspot – eMBB | Downlink | 10 |  | X Yes  No | c.f.  E-II.6 |
| **5.2.4.3.7** User plane latency (ms) *(4.7.1)* | eMBB | Not applicable | Uplink and Downlink | 4 |  | Yes  No | c.f.  E-II.7 |
| URLLC | Not applicable | Uplink and Downlink | 1 |  | Yes  No | c.f.  E-II.7 |
| **5.2.4.3.8** Control plane latency (ms) *(4.7.2)* | eMBB | Not applicable | Not applicable | 20 |  | X Yes  No | c.f.  E-II.8 |
| URLLC | Not applicable | Not applicable | 20 |  | X Yes  No | c.f.  E-II.8 |
| **5.2.4.3.9** Connection density (devices/km2) *(4.8)* | mMTC | Urban Macro – mMTC | Uplink | 1 000 000 |  | X Yes  No | c.f.  E-II.9 |
| **5.2.4.3.10** Energy efficiency *(4.9)* | eMBB | Not applicable | Not applicable | Capability to support a high sleep ratio and long sleep duration |  | X Yes  No | c.f.  E-II.10 |
| **5.2.4.3.11** Reliability *(4.10)* | URLLC | Urban Macro –URLLC | Uplink or Downlink | 1-10−5 success probability of transmitting a layer 2 PDU (protocol data unit) of size 32 bytes within 1 ms in channel quality of coverage edge |  | X Yes  No | c.f.  E-II.11 |
| **5.2.4.3.12** Mobility classes *(4.11)* | eMBB | Indoor Hotspot – eMBB | Uplink | Stationary, Pedestrian |  | X Yes  No | c.f.  E-II.12 |
| eMBB | Dense Urban – eMBB | Uplink | Stationary, Pedestrian,  Vehicular (up to 30 km/h) |  | X Yes  No | c.f.  E-II.12 |
| eMBB | Rural – eMBB | Uplink | Pedestrian, Vehicular, High speed vehicular |  | X Yes  No | c.f.  E-II.12 |
| **5.2.4.3.13**  Mobility Traffic channel link data rates (bit/s/Hz) *(4.11)* | eMBB | Indoor Hotspot – eMBB | Uplink | 1.5 (10 km/h) |  | X Yes  No | c.f.  E-II.13 |
| eMBB | Dense Urban – eMBB | Uplink | 1.12 (30 km/h) |  | X Yes  No | c.f.  E-II.13 |
| eMBB | Rural – eMBB | Uplink | 0.8 (120 km/h) |  | X Yes  No | c.f.  E-II.13 |
| 0.45 (500 km/h) |  | X Yes  No | c.f.  E-II.13 |
| **5.2.4.3.14** Mobility interruption time (ms)  *(4.12)* | eMBB and URLLC | Not applicable | Not applicable | 0 |  | X Yes  No | c.f.  E-II.14 |
| **5.2.4.3.15** Bandwidth and Scalability *(4.13)* | Not applicable | Not applicable | Not applicable | At least 100 MHz |  | X Yes  No | c.f.  II-E.16 |
| Up to 1 GHz |  | X Yes  No | c.f.  II-E.16 |
| Support of multiple different bandwidth values(4) |  | X Yes  No | c.f.  II-E.16 |
| (1) As defined in Report ITU-R M.2410-0.  (2) According to the evaluation methodology specified in Report ITU-R M.2412-0.  (3) Proponents should report their selected evaluation methodology of the Connection density, the channel model variant used, and evaluation configuration(s) with their exact values (e.g. antenna element number, bandwidth, etc.) per test environment, and could provide other relevant information as well. For details, refer to Report ITU-R M.2412-0, in particular, § 7.1.3 for the evaluation methodologies, § 8.4 for the evaluation configurations per each test environment, and Annex 1 on the channel model variants.  (4) Refer to § 7.3.1 of Report ITU-R M.2412-0. | | | | | | | |

## III-3: Number of test environments meeting all IMT-2020 requirements

This section is a place holder for the final report since no conclusions can be drawn until all relevant simulation-based evaluations have been made.

## III-4: Conclusion of link budget analysis

Link budget calculations are work in progress Details will be provided in the final Evaluation Report.5G Infrastructure Association concludes that the proponent has provided the required information relating to link budgets for all four test environments for both the TDD RIT and the FDD RIT.

Annex A: Detailed assumptions on DL and UL peak data rate and peak spectral efficiency calculations for 5G NR and LTE

5G NR Downlink

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Parameters** | **Downlink Configuration** | | | **Details** |
| **FDD FR1** | **TDD FR1** | **TDD FR2** |
| Total number of aggregated carriers  *J* | 16 | | | Maximum allowed value |
|  | 1 | 0.7643 | 0.7643 | **Note 1** |
| Max. number of layers | 8 (FR1), 6 (FR2) | | | **Note 2** |
| Highest modulation order | 8 | | | 256 QAM |
| Scaling factor of modulation | 1 | | | No capability mismatch between baseband and RF. |
| Max. coding rate  *Rmax* | 984/1024 = 0.9258 | | | Maximum CR |
|  | 0,1,2,3 | | | According to [10] |
|  |  | | | Depending on the numerology. |
|  | - 270 for BW 50 MHz, SCS 15 kHz  - 273 for BW 100 MHz, SCS 30 kHz  - 135 for BW 100 MHz, SCS 60 kHz | | - 264 for BW 200 MHz, SCS 60 kHz  - 264 for BW 400 MHz, SCS 120 kHz | Depending on the available bandwidth [9] and the numerology. |
|  | - 0.1037 for BW 50 MHz, SCS 15 kHz  - 0.1036 for BW 100 MHz, SCS 30 kHz  - 0.1076 for BW 100 MHz, SCS 60 kHz | - 0.1192 for BW 50 MHz, SCS 15 kHz  - 0.1193 for BW 100 MHz, SCS 30 kHz  - 0.1235 for BW 100 MHz, SCS 60 kHz | - 0.1855 for BW 200 MHz, SCS 60 kHz  - 0.1827 for BW 400 MHz, SCS 120 kHz | **Note 3** |
| **Note 1: FDD/TDD Frame Structure**  **-** For FDD DL, all subframes, slots and OFDM symbols in the 5G NR frame are assigned to DL ---------- ---------- transmissions.  - For TDD DL, frame structure: DDDSUDDDSU (6D: Downlink, 2U: Uplink, 2S: Mixed Downlink and ---------- Uplink) and SFI = 31 with a slot structure allocating 14 OFDM symbols as: 11 DL, 1 GP and 2 UL. Half ----------of the GP symbols are considered as DL resources.  **Note 2: Maximum number of layers**  **-** In FR1, the maximum number of layers is equal to the maximum value allowed for DL, i.e. 8 layers.  **-** In FR2, the maximum number of layers is set to 6 since 8 layers cannot be configured due to complexity ----------issues related to the operation in high frequency bands.  **Note 3: Overhead Assumptions**  **-**  For FDD FR1:  **· Total REs:** 10 subframes with 14 OFDM symbols per slot assigned to DL transmissions.  **· SS/PBCH:** 1 block transmitted each 20 slots. Each block is composed of 240 subcarriers x 4 OFDM ---- symbols.  **· PDCCH:** 1 CORESET per slot with 2 CCEs (12 RB) in all subframes with DL content (All the ----------subframes).  **· PDSCH:**   * DMRS: 16 RE/RB/slot in all RBs in all slots in all subframes. * CSI-RS NZP: 8 RE/RB/slot in all RBs each 20 slots. * CSI – IM: 4 RE/RB/slot in all RBs each 20 slots. * CSI-RS (TRS): 12 RE/RB/slot in 52 RBs each 20 slots.   **-**  For TDD FR1:  **· Total REs:** 6 DL subframes with 14 OFDM symbols per slot, 1 Mixed subframe with ---------- ----------12 OFDM symbols (11 DL and 1 GP) per slot and 1 Mixed subframe with 12 OFDM symbols (11 ---------- DL) assigned to DL transmissions.  **· GP:** 1 OFDM symbol in each slot in 1 Mixed UL/DL subframe.  **· SS/PBCH:** 1 block transmitted each 20 slots. Each block is composed of 240 subcarriers x 4 OFDM ---- symbols.  **· PDCCH:** 1 CORESET per slot with 2 CCEs (12 RB) in all subframes with DL content (8 out of 10---------- subframes).  **· PDSCH:**   * DMRS: 16 RE/RB/slot in all RBs in all slots in 8 out of 10 subframes. * CSI-RS NZP: 8 RE/RB/slot in all RBs each 20 slots. * CSI – IM: 4 RE/RB/slot in all RBs each 20 slots. * CSI-RS (TRS): 12 RE/RB/slot in 52 RBs each 20 slots.   **-**  For TDD FR2:  **· Total REs:** 6 DL subframes with 14 OFDM symbols per slot, 1 Mixed subframe with ---------- ----------12 OFDM symbols (11 DL and 1 GP) per slot and 1 Mixed subframe with 12 OFDM symbols (11 ------------DL) assigned to DL transmissions.  **· GP:** 1 OFDM symbol in each slot in 1 Mixed UL/DL subframe.  **· SS/PBCH:** 8 blocks transmitted each 20 slots. Each block 240 subcarriers x 4 OFDM symbols.  **· PDCCH:** 1 CORESET per slot with 4 CCEs (24 RB) in all subframes with DL content (8 out of 10------- subframes).  **· PDSCH:**   * DMRS: 12 RE/RB/slot in all RBs in all slots in 8 out of 10 subframes. * CSI-RS NZP: 8 RE/RB/slot in all RBs each 20 slots. * CSI – IM: 4 RE/RB/slot in all RBs each 20 slots. * CSI-RS (TRS): 12 RE/RB/slot in 52 RBs each 20 slots. * PT-RS: 4 RB in 1 OFDM symbol in all slots in 8 out of 10 subframes. | | | | |

**5G NR Uplink**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Parameters** | **Uplink Configuration** | | | **Details** |
| **FDD FR1** | **TDD FR1** | **TDD FR2** |
| Total number of aggregated carriers  *J* | 16 | | | Maximum value allowed |
|  | 1 | 0.6375 | 0.6375 | **Note 1** |
| Max. number of layers | 4 | | | Maximum value allowed for UL |
| Highest modulation order | 8 | | | 256 QAM |
| Scaling factor of modulation | 1 | | | No capability mismatch between baseband and RF. |
| Max. coding rate  *Rmax* | 984/1024 = 0.9258 | | | Maximum CR |
|  | 0,1,2,3 | | | According to [10] |
|  |  | | | Depending on the numerology. |
|  | - 270 for BW 50 MHz, SCS 15 kHz  - 273 for BW 100 MHz, SCS 30 kHz  - 135 for BW 100 MHz, SCS 60 kHz | | - 264 for BW 200 MHz, SCS 60 kHz  - 264 for BW 400 MHz, SCS 120 kHz | Depending on the available bandwidth [9] and the numerology. |
|  | - 0.0834 for BW 50 MHz, SCS 15 kHz  - 0.0815 for BW 100 MHz, SCS 30 kHz  -0.0826 for BW 100 MHz, SCS 60 kHz | - 0.1194 for BW 50 MHz, SCS 15 kHz  - 0.1163 for BW 100 MHz, SCS 30 kHz  - 0.1174 for BW 100 MHz, SCS 60 kHz | - 0.1163 for BW 200 MHz, SCS 60 kHz  - 0.1155 for BW 400 MHz, SCS 120 kHz | **Note 2** |
| **Note 1: FDD/TDD Frame Structure**  **-** For FDD UL, all subframes, slots and OFDM symbols in the 5G NR frame are assigned to UL ---------- ---------- transmissions.  - For TDD UL, frame structure: UUUSDUUUSD (6U: Uplink, 2D: Downlink, 2S: Mixed Downlink and ---------- Uplink) and SFI = 31 with a slot structure allocating 14 OFDM symbols as: 11 DL, 1 GP and 2 UL.  **Note 2: Overhead Assumptions**  **-**  For FDD FR1:  **· Total REs:** 10 subframes where all slots convey 14 OFDM symbols for UL transmissions.  **· PRACH:** Preamble #71, 12 RB in 6 OFDM symbols in each slot in 2 out of 10 subframes.  **· PUCCH:** Format 3 to convey CSI, HARQ ACK/NACK and SR. 2 RB in 4 OFDM Symbols in each ---------- slot in all subframes.  **· PUSCH:**   * DMRS: 12 RE/RB/slot in all RBs in all slots in all subframes. * SRS: 12 RE/RB in all RBs of 1 OFDM symbol each 10 slots.   **-**  For TDD FR1:  **· Total REs:** 6 UL subframes with 14 OFDM symbols per slot, 1 Mixed subframes with 2 OFDM --------- -symbols per slot assigned to UL transmissions, and 1 Mixed subframe with 3 OFDM symbols per slot ---- assigned to UL transmissions.  **· PRACH:** Preamble #71, 12 RB in 6 OFDM symbols in 2 out of 10 subframes.  **· PUCCH:** Format 3 to convey CSI, HARQ ACK/NACK and SR. 2 RB in 2 OFDM symbols in each ---------- slot in 6 out of 10 subframes.  **· PUSCH:**   * DMRS: 12 RE/RB/slot in all RBs in all slots in all subframes. * SRS: 12 RE/RB in all RBs of 1 OFDM symbol each 10 slots.   **-**  For TDD FR2:  **· Total REs:** 6 UL subframes with 14 OFDM symbols per slot, 1 Mixed subframes with 2 OFDM --------- -symbols per slot assigned to UL transmissions, and 1 Mixed subframe with 3 OFDM symbols per slot ---- assigned to UL transmissions.  **· PRACH:** Preamble #71, 12 RB in 6 OFDM symbols in 2 out of 10 subframes.  **· PUCCH:** Format 3 to convey CSI, HARQ ACK/NACK and SR. 2 RB in 2 OFDM symbols in each ---------- slot in 6 out of 10 subframes.  **· PUSCH:**   * DMRS: 12 RE/RB/slot in all RBs in all slots in 8 out of 10 subframes. * SRS: 12 RE/RB in all RBs of 1 OFDM symbol each 10 slots. * PT-RS: 4 RB in 1 OFDM symbol in all slots in 8 out of 10 subframes. | | | | |

LTE Downlink

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameters** | **Downlink Configuration** | | **Details** |
| **FDD** | **TDD** |
| Total number of aggregated carriers  *J* | 32 | | Maximum allowed value |
|  | 1 | 0.7429 | **Note 1** |
| Max. number of layers | 8 | | Maximum value allowed for DL |
| Highest modulation order | 8, 10 | | 256 QAM  1024 QAM |
| Scaling factor of modulation | 1 | | No capability mismatch between baseband and RF. |
| Max. coding rate  *Rmax* | *Rmax* ≤ 0.93 | | Depending on the maximum Transport block size (TBS) defined in [10] and the number of useful data bits. |
| Subcarrier Spacing (kHz) | 15 | | According to [10] for unicast subframes |
|  |  | | OFDM symbol duration |
|  | 100 for BW 20 MHz, SCS 15 kHz | | Depending on the available bandwidth and the subcarrier spacing [10] |
|  | 0.327 for BW 20 MHz, SCS 15 kHz | 0.304 for BW 20 MHz, SCS 15 kHz | **Note 2** |
| **Note 1: FDD/TDD Frame Structure**  **-** For FDD DL, all subframes, slots and OFDM symbols in the LTE frame are assigned to DL ---------- ---------- transmissions.  - For TDD DL, frame structure: DSUDDDSUDD (6D: Downlink, 2U: Uplink, 2S: Mixed Downlink and ---------- Uplink) and TDD Special subframe configuration of 10 OFDM symbols for DL, 1 for UL and 3 for GP.  **Note 2: Overhead Assumptions**  **-**  For FDD:  **· Total REs:** 10 subframes with 14 OFDM symbols per subframe assigned to DL transmissions.  **· PBCH:** 1 transmitted each 20 slots. Each block is composed of 240 REs excluding CRS.  **· PSS/SSS + Null Cells:** 288 REs each 10 ms.  **· PDCCH:** 1 or 2 full OFDM symbols in all subframes with DL content.  **· PDSCH:**   * CRS: 8 RE/RB/subframe in all RBs in all subframes. * DMRS: 24 RE/RB/subframe in all RBs in all subframes. * CSI-RS: 8 RE/RB in all RBs each 20 ms.   **-**  For TDD:  **· Total REs:** 6 DL subframes with 14 OFDM symbols and 2 Mixed DL/UL subframes with 13 OFDM --------symbols assigned to DL or GP transmissions.  **· GP:** 3 full OFDM symbols in each slot in 2 Mixed UL/DL subframes in each 5G NR frame.  **· PBCH:** 1 transmitted each 20 slots. Each block is composed of 240 REs excluding CRS.  **· PSS/SSS + Null Cells:** 288 REs per subframe. Each block is composed of 240 REs excluding CRS.  **· PDCCH:** 1 or 2 full OFDM symbols in all subframes with DL and mixed DL/UL content.  **· PDSCH:**   * CRS: 4 RE/RB/slot in all RBs in all slots in all subframes. * DMRS: 12 RE/RB/subframe in all RBs in all subframes. * CSI-RS: 8 RE/RB in all RBs each 20 ms. | | | |

LTE Uplink

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameters** | **Downlink Configuration** | | **Details** |
| **FDD** | **TDD** |
| Total number of aggregated carriers  *J* | 32 | | Maximum allowed value |
|  | 1 | 0.6143 | **Note 1** |
| Max. number of layers | 4 | | Maximum value allowed for UL |
| Highest modulation order | 8 | | 256QAM |
| Scaling factor of modulation | 1 | | No capability mismatch between baseband and RF. |
| Max. coding rate  *Rmax* | *Rmax* ≤ 0.93 | | Depending on the maximum Transport block size (TBS) defined in [10] and the number of useful data bits. |
| Subcarrier Spacing (kHz) | 15 | | According to [10] for unicast subframes |
|  |  | | OFDM symbol duration |
|  | 100 for BW 20 MHz, SCS 15 kHz | | Depending on the available bandwidth and the subcarrier spacing [10] |
|  | 0.1701 for BW 20 MHz, SCS 15 kHz | 0.2472 for BW 20 MHz, SCS 15 kHz | **Note 2** |
| **Note 1: FDD/TDD Frame Structure**  **-** For FDD UL, all subframes, slots and OFDM symbols in LTE frames are assigned to UL transmission.  - For TDD UL, frame structure: DSUUUDSUUU (2D: Downlink, 6U: Uplink, 2S: Mixed Downlink and ---------- Uplink) and TDD Special subframe configuration of 10 OFDM symbols for DL, 1 for UL and 3 for GP.  **Note 2: Overhead Assumptions**  **-**  For FDD:  **· Total REs:** 10 subframes with 14 OFDM symbols per subframe assigned to UL transmissions.  **· PRACH:** 72 REs in 1 subframe each 10 ms  **· PUCCH:** 336 REs per subframe in all UL subframes.  **· PUSCH:**   * DMRS: 2 full OFDM symbols per subframe in all UL subframes * SRS: 96 RBs in 1 OFDM symbol in 1 subframe each 10 ms.   **-**  For TDD:  **· Total REs:** 6 DL subframes with 14 OFDM symbols and 2 Mixed DL/UL subframes with 1 OFDM --------symbols assigned to UL transmissions.  **· GP:** 3 OFDM symbols in each slot in 2 Mixed UL/DL subframes in each 5G NR frame.  **· PRACH:** 72 REs in 1 subframe each 10 ms.  **· PUCCH:** 336 REs per subframe in all UL and mixed DL/UL subframes.  **· PUSCH:**   * DMRS: 2 OFDM per subframe in all UL subframes. * SRS: 96 RBs in 1 OFDM symbol in 1 subframe each 10 ms. | | | |

References

1. ITU-R: Minimum requirements related to technical performance for IMT-2020 radio interface(s). Report ITU-R M.2410-0, (11/2017).
2. ITU-R: Requirements, evaluation criteria and submission templates for the development of IMT-2020. Report ITU-R M.2411-0, (11/2017).
3. ITU-R: Guidelines for evaluation of radio interface technologies for IMT-2020. Report ITU-R M.2412-0, (10/2017).
4. 3GPP: Initial Description template of 3GPP 5G candidate for inclusion in IMT-2020.   
   ITU-R WP 5D, Document 5D/817-E, 23 January 2018.
5. China (People’s Republic of): Initial submission of candidate technology for IMT-2020 radio interface. ITU-R WP 5D, Document 5D/838-E, 24 January 2018.
6. Korea (Republic of): Submission of a candidate technology of IMT-2020. ITU-R WP 5D, Document 5D/819-E, 23 January 2018.
7. ITU-R WP 5D: Submission received for proposals of candidate Radio Interface Technologies from proponent ‘3GPP’ under step 3 of the IMT-2020 process. Document 5D/TEMP/653, Revision 2 to Document IMT-2020/3-E, 19 October 2018.
8. ITU-R WP 5D: Revision 3 to Submission received for proposals of candidate Radio Interface Technologies from proponent ‘3GPP’ under step 3 of the IMT-2020 process. Document 5D/TEMP/701, 14 February 2019.
9. ITU-R WP 5D: Information of the evaluation for the terrestrial components of the radio interface(s) for IMT-2020. Liaison statement to registered Independent Evaluation Groups. Document 5D/TEMP/769(Rev 1), 16 July 2019.
10. 3GPP: TS38.211v15.2.0 “NR; Physical channels and modulation (Release 15)”.
11. 3GPP: [38.101]: TS38.101v15.2.0 “NR; User Equipment (UE) radio transmission and reception”.
12. 3GPP: [36.101]: TS36.101v15.3.0 “Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio transmission and reception”.
13. L. Yu, C. Dietrich, V. Pauli, “IMT- 2020 Evaluation: Calibration of NOMOR’s System Simulator“, Nomor White Paper, November 2018.
14. 3GPP TR 37.910 V1.0.0 (2018-09): Study on Self Evaluation towards IMT-2020 Submission (Release 15).
15. 3GPP: TS38.214 v15.4.0 (2018-12) “Physical layer procedures for data (Release 15)”.
16. ITU-R WP 5D: Preliminary Description Template and Self-Evaluation of 3GPP 5G candidate for inclusion in IMT-2020 from proponent ‘3GPP’ under step 3 of the IMT-2020 process – Characteristics Template. Document 5D/TEMP/1050, 1 October 2018.
17. 3GPP: TS38.300 V15.6.0 (2019-06) “Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access Network (E-UTRAN), Overall description, Stage 2 (Release 15)”.
18. 3GPP: TS36.133 V16.2.0 (2019-06) “Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements for support of radio resource management (Release 16)”.
19. 3GPP: TS36.300 V15.6.0 (2019-06) “Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access Network (E-UTRAN);Overall description;Stage 2(Release 15)”.
20. 3GPP: TR37.910 V1.0.0 (2018-09) “Technical Specification Group Radio Access Network**,** Study on Self Evaluation towards IMT-2020 Submission (Release 15)”.
21. 3GPP: [22.261]: TS22.261v16.4.0 “Service requirements for next generation new services and markets”.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Submitted on behalf of the Independent Evaluation Group 5G Infrastructure Association. [↑](#footnote-ref-1)
2. This contribution is based on work underway within the research in 5G PPP and 5G Infrastructure Association, see <https://5g-ppp.eu/>. The views expressed in this contribution do not necessarily represent the 5G PPP. [↑](#footnote-ref-2)
3. Average spectral efficiency corresponds to “spectrum efficiency” in Recommendation ITU‑R M.2083. [↑](#footnote-ref-3)
4. If a proponent determines that a specific question does not apply, the proponent should indicate that this is the case and provide a rationale for why it does not apply. [↑](#footnote-ref-4)