|  |  |  |
| --- | --- | --- |
|  | **Radiocommunication Study Groups** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| Source: Document 5A/TEMP/29 | **Annex 14 to****Document 5A/114-E** |
| **23 May 2016** |
| **English only** |
| Annex 14 to Working Party 5A Chairman’s Report |
| PRELIMINARY DRAFT REVISION TO RECOMMENDATION ITU‑R M.1732‑1[[1]](#footnote-1)\* |
| Characteristics of systems operating in the amateurand amateur-satellite services for use in sharing studies |

(Question ITU-R 48-6/5)

(2005-2012)

Scope

This Recommendation documents the technical and operational characteristics of systems used in the amateur service and amateur-satellite services for the purposes of carrying out sharing studies. The systems and their characteristics described in this Recommendation are considered representative of those operating in the frequency bands available to these services ranging from 135.7 kHz through 250 GHz.

Keywords

The ITU Radiocommunication Assembly,

considering

*a)* that the Radio Regulations (RR) defines an amateur service and an amateur-satellite service and allocates frequencies to them on an exclusive or shared basis;

*b)* that systems in the amateur and amateur-satellite services operate over a wide range of frequencies;

*c)* that the technical characteristics of systems operating in the amateur and amateur‑satellite services may vary within a band;

*d)* that some ITU-R technical groups are considering the potential for the introduction of new types of systems or services in bands used by systems operating in the amateur and amateur‑satellite services;

*e)* that representative technical and operational characteristics of systems operating in the amateur and amateur-satellite services are required to determine the feasibility of introducing new types of systems into frequency bands in which the amateur and amateur-satellite services operate,

recommends

1 that the technical and operational characteristics of systems operating in the amateur and amateur-satellite services described in Annex 1 should be considered representative of those operating in the frequency bands allocated to the amateur and amateur-satellite services;

2 that Recommendation ITU-R M.1044 should be used as a guide in studies of the compatibility between systems operating in the amateur and amateur-satellite services and systems operating in other services.

Annex 1

Characteristics of systems operating in the amateur
and amateur-satellite services for use in sharing studies

# 1 Introduction

A number of frequency bands are allocated to the amateur and amateur-satellite services throughout the spectrum. These bands have been selected to provide different propagation conditions.

Amateur and amateur-satellite stations perform a variety of functions, such as:

– training, intercommunication between amateur stations and technical investigations by duly authorized persons interested in radio technique solely with a personal aim and without pecuniary interest (RR Nos. **1.56** and **1.57**);

– disaster relief communications as elaborated in Recommendation ITU-R M.1042.

To achieve these aims amateurs make use of existing mature and leading edge technology to advance their self-education, technical interests and service to the wider community including providing communications for disaster relief. Amateur operators often apply communications technology in new and innovative ways to meet their needs in an increasingly crowded and noisy electromagnetic spectrum. As new technology becomes available it is applied by amateurs to extending the range and capability of their amateur stations, and this feeds back into new ideas and uses that might have application in the wider community through commercial non-amateur providers.

The bands and modes listed in this recommendation are those currently used by the amateur and amateur satellite services; as band allocations and technology changes, this recommendation will be updated to reflect the most recent developments.

# 2 Operational characteristics

Amateur stations and amateur-satellite earth stations generally do not have assigned frequencies but dynamically select frequencies within an allocated band using listen-before-talk techniques. Terrestrial repeaters, digital relay stations and amateur satellites use frequencies selected on the basis of voluntary coordination within the amateur services.

Some amateur frequency allocations are exclusive to the amateur and amateur-satellite services. Many of the allocations are shared with other radio services and amateur operators are aware of the sharing limitations.

Communications may be initiated on prearranged schedule or by one station initiating a general or specific call. One or more stations may respond. Formal and informal nets may be initiated as needed. Contacts may last from about 1 min to about 1 h, depending on traffic to be transmitted. In specific applications including, e.g., emergency and disaster-relief, amateur radio voice networks may utilize automatic link establishment[[2]](#footnote-2) employing a variation of the 2G ALE protocol (sometimes referred to as 2.5G ALE) typically utilizing an outboard PC controller.

Operating protocols vary according to communication requirements and propagation:

– LF and MF bands typically use ground wave propagation and sky wave propagation over medium distance paths;

– HF bands are used for near-vertical-incidence-sky wave and low angle sky wave propagation paths for regional and global paths;

– VHF, UHF and SHF bands are generally used for short-range communications, however, there are times when suitable propagation conditions allow beyond line‑of‑sight communications;

– Amateur satellites afford an opportunity to use frequencies above HF for long-distance communications; and

– Signals bounced off the moon offer worldwide communication paths.

# 3 Technical characteristics

Tables 1 to 8 contain technical characteristics of representative systems operating in the amateur and amateur-satellite services. This information is sufficient for general calculation to assess the compatibility between these systems and systems operating in other services. The upper frequency boundaries shown in Tables 1 to 8 represent the current state of deployment of most amateur radio systems. As amateur usage of the 135.7–137.8 kHz and 472-kHz frequency bands is restricted to maximum radiated power of 1 W (e.i.r.p.)[[3]](#footnote-3) and electrically short antennas in a high noise environment, operation on these bands is generally different to higher frequency bands. To establish communications with distant stations weak-signal techniques and operating protocols have been developed for use in this difficult environment and representative characteristics are shown in Table 4. These techniques utilize digital signal processing, forward error correction and bandwidth limitation to minimize the effects of high levels of natural and man-made noise.

Tables 1 through 8 contain data on transmitter power, antenna gain and radiated power (e.i.r.p.) and it should be noted that the values shown are notional and operational characteristics and any given amateur service station may deviate from specific values given in the following tables. This particularly applies to transmitter power which is often more likely to be determined by the licence conditions of individual countries, equipment availability and the need/interest of the individual amateur station, so the actual transmitter power used is very likely to be significantly less than the maximum values shown in the tables.

Another factor to consider is that various transmissions modes have significantly different duty cycles and this affects the average power that is actually radiated. For continuous-carrier modes, e.g., F3E (FM), the power shown is constant for the duration of the transmission. For duty-cycle transmission modes, e.g., A1A (CW), the power shown is during key-down and the average power during a transmission is approximately 45% of the value shown. For single-sideband (SSB) voice, Emission Class J3E, the power shown is expressed as Peak Envelope Power (PEP). The average power per transmission is approximately 33% of the value shown. For emission class A3E (AM), the power shown is PEP and the average power per transmission is about 80% of the value shown. Narrow-bandwidth digital modes, e.g., J2B (PSK31), typically operate at far less than the maximum power authorized.

Similarly for antenna gain and feed loss, the maximum values shown are also notional and the actual antenna gain and feed loss at any amateur station will be affected by near field effects, cost considerations, equipment availability and individual operator needs.

To improve the usability of the data in tables 1 through 8 the frequency ranges in the tables have been arranged to group, as far as possible, frequency bands that use similar techniques and equipment, noting that the techniques used by the amateur service continues to evolve over time as technology, equipment availability and the regulatory environment changes, so individual characteristics for any particular band or mode of transmission may be different to the values in the tables.

Users of this document should consider these features of the amateur service when using the data contained in tables 1 through 8 when undertaking sharing and compatibility studies.

TABLE 1a

Characteristics of amateur systems for Morse on-off keying, PSK31, NBDP and Weak Signal modes below 900 MHz

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 1.8‑7.3 MHz | 10.1-29.7 MHz | 50-54 MHz | 144-225 MHz | 420-450 MHz |
| Necessary bandwidth and class of emission (emission designator) | 150HA1A150HJ2A60H0J2B250HF1D1H00A1D(2)1H00F1D(2) | 150HA1A150HJ2A60H0J2B250HF1D1H00A1D1H00F1D | 150HA1A150HJ2A60H0J2B250HF1D1H00A1D1H00F1D | 150HA1A150HJ2A60H0J2B250HF1D1H00A1D1H00F1D | 150HA1A150HJ2A60H0J2B250HF1D1H00A1D1H00F1D |
| Transmitter power (dBW)(3) | 3‑31.7 | 3‑31.7 | 3‑31.7 | 3-31.7 | 3‑31.7 |
| Feeder loss (dB) | 0.2 | 0.3‑0.9 | 1-2 | 1-2 | 1-2 |
| Transmitting antenna gain (dBi) | −20 to 6 | −10 to 12 | -6 to 12 | -6 to 18 | -3 to 23 |
| Typical e.i.r.p. (dBW) (4) | −17 to 23 | −7 to 26 | 2-26 | 2-34 | 2-36 |
| Antenna polarization | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical  | Horizontal, vertical |
| Receiver IF bandwidth (kHz) | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 |
| Receiver noise figure (dB)(5) | 13 | 7-13 | 0.5-6 | 0.5-2 | 0.5-1 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) “Weak Signal Modes” are structured for very basic communication with low data and narrow bandwidth for weak signal performance. Well known and commonly used weak modes include WSPR, JT65 and Opera.

(3) Maximum powers are determined by each administration.

(4) May be limited by RR Article **5** in some cases.

(5) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

TABLE 1B

Characteristics of amateur systems for Morse on-off keying, PSK31 and NBDP above 900 MHz

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 0.902-3.5 GHz | 5.65-10.5 GHz | 24-47.2 GHz | 76-250 GHz |
| Necessary bandwidth and class of emission (emission designator) | 150HA1A150HJ2A60H0J2B250HF1B | 150HA1A150HJ2A60H0J2B250HF1B | 150HA1A150HJ2A60H0J2B250HF1B | 150HA1A150HJ2A60H0J2B250HF1B |
| Transmitter power (dBW)(2) | 3‑31.7 | 3‑20 | -10 to 10 | -10 to 10 |
| Feeder loss (dB) | 1-6 | 1-6 | 0-6 | 0-6 |
| Transmitting antenna gain (dBi) | 10-42 | 10-42 | 10-42 | 10-52 |
| Typical e.i.r.p. (dBW) (3) | 1-45 | 1-45 | 1-45 | 1-45 |
| Antenna polarization | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical |
| Receiver IF bandwidth (kHz) | 0.5 | 0.5 | 0.5 | 0.5 |
| Receiver noise figure (dB)(4) | 0.5 - 1 | 0.5 - 1 | 3 - 7 | 3 - 7 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Maximum powers at 24-250 GHz are usually limited by available equipment and less than the administration maximum.

(3) May be limited by RR Article **5** in some cases.

(4) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

|  |  |
| --- | --- |
|  |  |
|  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |

TABLE 2a

Characteristics of amateur analogue voice systems below 900 MHz

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 1.8‑7.3 MHz | 10.1-29.7 MHz | 50-54 MHz | 144-225 MHz | 420-450 MHz |
| Necessary bandwidth and class of SSBemission (emission designator) FM | 2K70J3E11K0F3E16K0F3E20K0F3E | 2K70J3E11K0F3E16K0F3E20K0F3E | 2K70J3E11K0F3E16K0F3E20K0F3E | 2K70J3E11K0F3E16K0F3E20K0F3E | 2K70J3E11K0F3E16K0F3E20K0F3E |
| Transmitter power (dBW)(2) | 3‑31.7 | 3‑31.7 | 3‑31.7 | 3-31.7 | 3‑31.7 |
| Feeder loss (dB) | 0.2 | 0.3‑0.9 | 1-2 | 1-  | 1-2 |
| Transmitting antenna gain (dBi) | −20 to 6 | −10 to 12 | -6 to 12 | –-6 to 18 | –-3 to 23 |
| Typical e.i.r.p. (dBW) (3) | −17 to 23 | −7 to 26 | 2-26 | 2-34 | 2-36 |
| Antenna polarization | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical  | Horizontal, vertical |
| Receiver IF bandwidth (kHz) SSB FM  | 2.791216 | 2.791216 | 2.791216 | 2.791216 | 2.791216 |
| Receiver noise figure (dB)(4) | 13 | 7 - 13 | 0.5 - 6 | 0.5 - 2 | 0.5 - 1 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. For single-sideband (SSB) voice (Class of Emission 2K70J3E) these power limits are expressed as Peak Envelope Power (PEP) which value is typically about three times the average power.

(3) May be limited by RR Article **5** in some cases.

(4) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

TABLE 2B

Characteristics of amateur analogue voice systems above 900 MHz

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 0.902-3.5 GHz | 5.65-10.5 GHz | 24-47.2 GHz | 76-250 GHz |
| Necessary bandwidth and class of SSBemission (emission designator) FM | 2K70J3E11K0F3E16K0F3E20K0F3E | 2K70J3E11K0F3E16K0F3E20K0F3E | 2K70J3E11K0F3E16K0F3E20K0F3E | 2K70J3E11K0F3E16K0F3E20K0F3E |
| Transmitter power (dBW)(2) | 3‑31.7 | 3‑20 | -10 to 10 | -10 to 10 |
| Feeder loss (dB) | 1-6 | 1-6 | –0-6 | –0-6 |
| Transmitting antenna gain (dBi) | 10-42 | 10-42 | 10-42 | 10-52 |
| Typical e.i.r.p. (dBW) (3) | 1-45 | 1-45 | 1-45 | 1-45 |
| Antenna polarization | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical |
| Receiver IF bandwidth (kHz) SSB FM  | 2.791216 | 2.791216 | 2.791216 | 2.791216 |
| Receiver noise figure (dB)(4) | 0.5 - 1 | 0,5 - 1 | 3 - 7 | 3 - 7 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Maximum powers at 24-250 GHz are usually limited by available equipment and less than the administration maximum.

(3) May be limited by RR Article **5** in some cases.

(4) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

|  |  |
| --- | --- |
|  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |

|  |  |
| --- | --- |
|  |  |
|  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |

TABLE 3a

Characteristics of amateur data, digital voice and multimedia systems below 900 MHz

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 1.8‑7.3 MHz | 10.1-29.7 MHz | 50-54 MHz | 144-225 MHz | 420-450 MHz |
| Necessary bandwidth and class of emission (emission designator) | 2K70J2E | 2K70J2E | 2K70J2E5K76G1E8K10F1E | 2K70J2E5K76G1E8K10F1E | 2K70G1D6K00F7D16K0D1D150KF1W2M00G7W |
| Transmitter power (dBW)(2) | 3‑31.7 | 3‑31.7 | 3-31.7 | 3-31.7 | 3-31.7 |
| Feeder loss (dB) | 0.2 | 0.3‑0.9 | 1-2 | 1-2 | 1-2 |
| Transmitting antenna gain (dBi) | −20 to 6 | −10 to 12 | -6 to 12 | –-6 to 18 | -3 to 23 |
| Typical e.i.r.p. (dBW) (3) | −17 to 17 | −7 to 20 | 2-20 | 2-28 | 2-30 |
| Antenna polarization | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical  | Horizontal, vertical |
| Receiver IF bandwidth (kHz) | 2.7 | 2.7 | 2.7, 6, 9  | 2.7, 6, 9 | 2.7, 6, 16, 1502 000 |
| Receiver noise figure (dB)(4) | 13 | 7 - 13 | 0.5 - 6 | 0.5 - 2 | 0.5 - 1 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Duty cycle limitations affect the transmitter power used.

(3) May be limited by RR Article **5** in some cases.

(4) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

TABLE 3B

Characteristics of amateur data, digital voice and multimedia systems above 900 MHz

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 0.902-3.5 GHz | 5.65-10.5 GHz | 24-47.2 GHz | 76-250 GHz |
| Necessary bandwidth and class of emission (emission designator) | 2K70G1D6K00F7D16K0D1D150KF1W2M50G7W | 2K70G1D6K00F7D16K0D1D150KF1W10M5G7W  | 2K70G1D6K00F7D16K0D1D150KF1W10M5G7W | 2K70G1D6K00F7D16K0D1D150KF1W10M5G7W |
| Transmitter power (dBW)(2) | 3-31.7 | 3-20 | -10 to 10 | -10 to 10 |
| Feeder loss (dB) | 1-6 | 1-6 | 0-6 | 0-6 |
| Transmitting antenna gain (dBi) | 10-42 | 10-42 | 10-42 | 10-52 |
| Typical e.i.r.p. (dBW) (3) | 1-45 | 1-45 | 1-45 | 1-45 |
| Antenna polarization | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical | Horizontal, vertical |
| Receiver IF bandwidth (kHz) | 2.7, 6, 16, 1502 500 | 2.7, 6, 16, 150, 10 500 | 2.7, 6, 16, 150, 10 500 | 2.7, 6, 16, 150, 10 500 |
| Receiver noise figure (dB)(4) | 0.5 - 1 | 0.5 - 1 | 3 -7 | 3 -7 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Maximum powers at 24-250 GHz are usually limited by available equipment and less than the administration maximum.. Duty cycle limitations affect the transmitter power used.

(3) May be limited by RR Article **5** in some cases.

(4) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

|  |  |
| --- | --- |
|  |  |
|  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |

TABLE 4

Characteristics of amateur operation in the 135.7-137.8 kHz and 472–479 KHz frequency bands

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Mode of operation | Continuous wave (CW)Morse 10‑50 Bd | Slow Morse≤ 1 Bd CW | Weak signal modes:(1) |
| Necessary bandwidth and class of emission (emission designator) | 150H00A1A, 150H00J2A | 1H00A1B, 1H00J2B | 2H00A1D, 2H00F1D 2H00J2D |
| Typical transmitter power (dBW) | 20 |
| Feeder loss (dB) | Negligible |
| Transmitting antenna gain (dBi) | -40 to -10 |
| Maximum e.i.r.p (dBW)  | 0(2) |
| Antenna polarization | Vertical |
| Receiver IF bandwidth (kHz) | 0.4(3) |
| Receiver noise figure (dB) | 13 |

(1) These modes are highly structured for weak signal performance and only send enough information to confirm a radio contact. Further information about these modes of operation can be obtained from the ARRL Handbook for Radio Communications (2012 Ed.), American Radio Relay League, ISBN: 978-0-87259-677-1, published 2011 and from the ARRL HF Digital Handbook (4th Ed.), American Radio Relay League, ISBN: 0‑87259‑103-4, published 2008. Well known and commonly used weak modes include WSPR, JT65 and Opera.

(2) In the frequency range 472-479 kHz, administrations may increase this limit to 5 W e.i.r.p in accordance with RR No. **5.80A**.

(3) Digital signal processing techniques can narrow the IF bandwidth to a fraction of a Hertz if needed.

TABLE 5

Characteristics of Earth-Moon-Earth (EME) systems

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 144-438 MHz | 1.24-3.5 GHz | 5.65-10.5 GHz | 24-47.2 GHz | 76-250 GHz |
| Necessary bandwidth and class of emission (emission designator) | 50H0A1A50H0J2A1K80F1B | 50H0A1A50H0J2A1K80F1B | 50H0A1A50H0J2A1K80F1B1K50J2D | 50H0A1A50H0J2A1K80F1B2K00J2D | 50H0A1A50H0J2A1K80F1B2K40J2D |
| Transmitter power (dBW)(2) | 17-31.7 | 17-31.7 | 13-20 | 13-20 | 10-20 |
| Feeder loss (dB) | 1-2 | 1-4 | 1-4  | 1-4 | 1-4 |
| Transmitting antenna gain (dBi) | 15-24 | 25-40 | 25-46 | 25-53 | 25-53 |
| Typical e.i.r.p. (dBW) | 30-40 | 40-68 | 68 | 68 | 68 |
| Antenna polarization | Horizontal, vertical, LHCP,RHCP | Horizontal, vertical, LHCP,RHCP | Horizontal, vertical, LHCP,RHCP | Horizontal, vertical, LHCP,RHCP | Horizontal, vertical, LHCP,RHCP |
| Receiver IF bandwidth (kHz) | 0.4 | 1 | 1.5 | 2 | 2.4 |
| Receiver noise figure (dB)(3) | 0.5 | 0.5 | 1 | 3-7 | 3-7 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Maximum powers at 24-250 GHz are usually limited by available equipment and less than the administration maximum.

(3) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers.

Usage Note: Main antenna beam direction can be assumed to be pointing above the horizon.

Emission Note: EME increasingly employs digital “Weak Signal Modes” which are structured for very basic communication with low data rates and narrow bandwidth for weak signal performance.

TABLE 6

Characteristics of amateur~~-~~satellite systems in the Earth-to-space direction

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) |  7 - 28 MHz  | 144-438 MHz | 1.24-3.5 GHz | 5.65-10.5 GHz | 24-47.2 GHz | 76-250 GHz |
| Necessary bandwidth and class of CW Morseemission (emission designator) 10 - Bd | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A |
| Necessary bandwidth and class of SSB voiceemission (emission designator) digital voice FM voice dataDigital multimedia | 2K70J3E2K70J2E16KF3E | 2K70J3E2K70J2E5K76G1E8K10F1E16K0F3E | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D2M50G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W |
| Transmitter power (dBW)(2) | 3-31.7 | 3-31.7 | 3-31.7 | 3-20 | -10 to 10 | -10 to 10 |
| Feeder loss (dB) | 0.3-0.9 | 1-2 | 1-2 | 1-10 | 1-10 | 1-10 |
| Transmitting antenna gain (dBi) | -10 to 12 | 0-26 | 10-42 | 10-42 | 10-42 | 10-52 |
| Typical e.i.r.p. (dBW) | 7-43 | 2-55 | 3-45 | 3-45 | 3-45 | 3-45 |
| Antenna polarization | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP |
| Satellite receiver IF bandwidth (kHz) | 2.75,768.116 | 2.716 | 16501004002 500 | 165010040010 000 | 165010040010 000 | 165010040010 000 |
| Satellite receiver noise figure (dB)(3) | 3-10 | 1-3 | 1-3 | 1-3 | 3-7 | 3-7 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Maximum powers at 24-250 GHz are usually limited by available equipment and less than the administration maximum.

(3) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

TABLE 7

Characteristics of amateur~~-~~satellite systems in the space-to-Earth direction for LEOs

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 28 MHz  | 144-438 MHz | 1.24-3.5 GHz | 5.65-10.5 GHz | 24-47.2 GHz | 76-250 GHz |
| Necessary bandwidth and class of CW Morseemission (emission designator) 10 – 50 Bd | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A |
| Necessary bandwidth and class of SSB voiceemission (emission designator) digital voice FM voice dataDigital multimedia | 2K70J3E2K70J2E16KF3E | 2K70J3E2K70J2E16K0F3E | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D2M50G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W |
| Transmitter power (dBW)(2) | -10 to 10 | -10 to 10 | -10 to 10 | -10 to 10 | -10 to 10 | -10 to 10 |
| Feeder loss (dB) | 0.2-1 | 0.2-1 | 0.2-1 | 0.2-1 | 0.2-2 | 0.2-2 |
| Transmitting antenna gain (dBi) | 0-3 | 0-6 | 0-10 | 0-23 | 0-23 | 0-23 |
| Typical e.i.r.p. (dBW) | -7 to 9 | -7 to 15 | -7 to 15 | 0-15 | 0-15 | 0-15 |
| Antenna polarization | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP |
| Receiver IF bandwidth (kHz) CW Morse 10-50 Bd | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 |
| Receiver IF bandwidth (kHz) SSB voice digital voice FM voice dataDigital multimedia | 2.716 | 2.716 | 2.71650100400 2,500 | 2.7165010040010,000 | 2.7165010040010,000 | 2.7165010040010,000 |
| Receiver noise figure (dB)(3) | 3-10 | 1-3 | 1-7 | 1-7 | 3-7 | 3-7 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Maximum powers at 24-250 GHz are usually limited by available equipment and less than the administration maximum.

(3) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

TABLE 8

Characteristics of amateur~~-~~satellite systems in the space-to-Earth direction for GEOs and higher orbit satellites

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Frequency range(1) | 28 MHz  | 144-438 MHz | 1.24-3.5 GHz | 5.65-10.5 GHz | 24-47.2 GHz | 76-250 GHz |
| Necessary bandwidth and class of CW Morseemission (emission designator) 10 - Bd | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A | 150HA1A150HJ2A |
| Necessary bandwidth and class of SSB voiceemission (emission designator) digital voice FM voice dataDigital multimedia | 2K70J3E2K70J2E16KF3E | 2K70J3E2K70J2E16K0F3E | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D2M50G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W | 2K70J3E2K70J2E16K0F3E44K2F1D88K3F1D350KF1D10M0G7W |
| Transmitter power (dBW)(2) | 0-10 | 0-20 | 0-20 | 0-20 | 0-17 | -3 to 10 |
| Feeder loss (dB) | 0.2-1 | 0.2-1 | 0.2-1 | 0.2-1 | 0.2-2 | 0.2-2 |
| Transmitting antenna gain (dBi) | 0-3 | 0-6 | 0-20 | 0-20 | 0-30 | 0-30 |
| Typical e.i.r.p. (dBW) | 9 | 9-15 | 9-25 | 9-30 | 6-30 | 3-30 |
| Antenna polarization | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP | Horizontal, vertical, RHCP, LHCP |
| Receiver IF bandwidth (kHz) CW Morse 10-0 Bd  | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4 |
| Receiver IF bandwidth (kHz) SSB voice digital voice FM voice dataDigital multimedia | 2.716 | 2.716 | 2.716501004002,500 | 2.7165010040010,000 | 2.7165010040010,000 | 2.7165010040010,000 |
| Receiver noise figure (dB)(3) | 3-10 | 1-3 | 1-7 | 1-7 | 3-7 | 3-7 |

(1) Amateur bands within the frequency ranges shown conform to RR Article **5**.

(2) Maximum powers are determined by each administration. Maximum powers at 24-250 GHz are usually limited by available equipment and less than the administration maximum.

(3) Receiver noise figures for bands above 50 MHz assume the use of low-noise preamplifiers. Below 29.7 MHz the external noise level is the dominant factor and typically higher than the equipment noise level.

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \* This Recommendation should be brought to the attention of Radiocommunication Study Group 1. [↑](#footnote-ref-1)
2. “Frequency-Adaptive Communications Systems and Networks in the MF/HF Bands”, ITU Radiocommunication Bureau, 2002. <https://www.itu.int/pub/R-HDB-40>. [↑](#footnote-ref-2)
3. Administrations may increase this limit to 5 W e.i.r.p. in accordance with RR No. **5.80A**. [↑](#footnote-ref-3)