|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Revision 1 toDocument 28(Add.6)(Add.1)-E** |
|  | **13 October 2015** |
|  | **Original: English** |
|  |
| African Common Proposals |
| Proposals for the work of the conference |
|  |
| Agenda item 1.6.1 |

1.6 to consider possible additional primary allocations:

1.6.1 to the fixed-satellite service (Earth-to-space and space-to-Earth) of 250 MHz in the range between 10 GHz and 17 GHz in Region 1;

and review the regulatory provisions on the current allocations to the fixed-satellite service within each range, taking into account the results of ITU‑R studies, in accordance with Resolutions **151 (WRC‑12)** and **152 (WRC‑12)**, respectively;

Part A: All bands except for 13.4-13.75 GHz for FSS (space-to-Earth). See part B for 13.4‑13.75 GHz for FSS (space-to-Earth)

NOC AFCP/28A6A1/1

Radio Regulations

**Reasons:** To protect existing services.

NOTE – This proposal applies to both directions for all bands except for 13.4-13.75 GHz as shown: See Part B for proposals regarding the special case of 13.4-13.75 GHz for FSS (space-to-Earth)

A) 10-10.5 GHz,

B) 10.5-10.6 GHz,

C) 10.6-10.68 GHz,

D) 13.25-13.40 GHz,

E) 13.4-13.75 GHz (Earth-to-space only),

F) 14.5-14.8 GHz,

G) 14.8-15.35 GHz,

H) 15.35-15.4 GHz,

I) 15.4-15.7 GHz,

J) 15.7-16.6 GHz and

K) 16.6-17 GHz.

Part B: The special case of 13.4-13.75 GHz for FSS (space-to-Earth)

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD AFCP/28A6A1/2

11.7-14 GHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 13.4-13.65EARTH EXPLORATION-SATELLITE (active)FIXED-SATELLITE (space-to-Earth) ADD 5.C161 ADD 5.X161 ADD 5.C161*bis*RADIOLOCATIONSPACE RESEARCH ADD 5.L161Standard frequency and time signal-satellite (Earth-to-space)5.499 5.500 5.501 5.501B | 13.4-13.65EARTH EXPLORATION-SATELLITE (active)RADIOLOCATIONSPACE RESEARCH ADD 5.L161Standard frequency and time signal-satellite (Earth-to-space)5.499 5.500 5.501 5.501B |
| 13.65-13.75 EARTH EXPLORATION-SATELLITE (active) RADIOLOCATION SPACE RESEARCH MOD 5.501A Standard frequency and time signal-satellite (Earth-to-space) 5.499 5.500 5.501 5.501B |

**Reasons:** To allocate the band 13.4-13.65 GHz to the FSS (space-to-Earth) in Region 1.

ADD AFCP/28A6A1/3

5.C161 The use of the band 13.4-13.65 GHz by the fixed-satellite service (space-to-Earth) is limited to geostationary-satellite systems and is subject to agreement obtained under No. **9.21** with respect to satellite systems, operating in the space research service (space-to-space) to relay data from space stations in the geostationary satellite orbit to associated space stations in the non-geostationary satellite orbit, for which information for advance publication has been received by the Bureau prior to 27 November 2015.     (WRC‑15)

**Reasons:** To limit use of the new FSS allocation (space-to-Earth) in Region 1 to GSO FSS, and to specify the terms and conditions for sharing between newly filed GSO FSS networks and SRS systems already notified to the Bureau, operating on space-to-space link to relay data from GSO space station to non-GSO user space station. There is understanding, that coordination of newly filed GSO FSS networks and already notified to the Bureau SRS (space-to-Earth) systems is subject to RR No. 9.7.

ADD AFCP/28A6A1/4

5.C161*bis* In the band 13.4-13.65 GHz, geostationary-satellite networks in the fixed-satellite service (space-to-Earth) shall not claim protection from space stations in the Earth exploration-satellite service (active) operating in accordance with these Regulations. No. **5.43A** and No. **22.2** do not apply.     (WRC‑15)

ADD AFCP/28A6A1/5

5.L161 The allocation of the band 13.4-13.65 GHz to the space research service on a primary basis is limited to active spaceborne sensors, as well as satellite systems, operating in the space research service (space-to-Earth and space-to-space) to relay data from space stations in the geostationary-satellite orbit to associated earth stations and space stations in the non-geostationary-satellite orbit, for which information for advance publication has been received by the Bureau prior to 27 November 2015. Satellite systems in the space research service (space-to-Earth and space-to-space) shall not cause harmful interference to nor claim protection from stations in the fixed, mobile, radiolocation and Earth exploration-satellite (active) services. Other uses of the band by the space research service are on a secondary basis.     (WRC‑15)

**Reasons:** Since only the frequency assignments having allocation of the considered frequency band on an equal basis are taken into account in the coordination under RR Article 9 it is proposed to modify footnote No. 5.501А and to add a new footnote under which the status of the ITU BR notified frequency assignments of DRS in SRS (s-E and s-s) will be increased up to the primary with regard to FSS. With respect to FSS stations in Region 1 in any case it is required to seek the agreement of other administrations (under RR No. 9.21) operating DRS in SRS (space-to-space) in Region 1, with NGSO user which can be potentially located over the territories of Regions 2 and 3. The direction of the DRS SRS links (space-to-Earth and space-to-space) is defined by the relevant Recommendations therefore it is not specified in RR Article 5 footnotes.

ADD AFCP/28A6A1/6

5.X161 Administrations shall not preclude the deployment and operation of transmitting earth stations in the standard frequency and time signal-satellite (Earth-to-space) allocated on a secondary basis in the band 13.4-13.65 GHz, due to the primary allocation to FSS (space-to-Earth).

**Reasons:** To ensure the deployment of transmitting Earth stations for the European ACES system in the band 13.4-13.75 GHz operating under the standard frequency and time signal-satellite.

MOD AFCP/28A6A1/7

5.501A The allocation of the band 13.65-13.75 GHz to the space research service on a primary basis is limited to active spaceborne sensors. Other uses of the band by the space research service are on a secondary basis.     (WRC‑15)

**Reasons:** To ensure operation of notified SRS systems to the Bureau on space-to-Earth and space-to-space links on an equal basis with newly filed stations in the fixed-satellite service (space-to-Earth).

ARTICLE 21

Terrestrial and space services sharing frequency bands above 1 GHz

Section I − Choice of sites and frequencies

MOD AFCP/28A6A1/8

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1 21.2.1 For their own protection receiving stations in the fixed or mobile service operating in bands shared with space radiocommunication services (space-to-Earth) should also avoid directing their antennas towards the geostationary-satellite orbit if their sensitivity is sufficiently high that interference from space station transmissions may be significant. In particular, in the bands 13.4‑13.65 GHz and 21.4-22 GHz, it is recommended to maintain a minimum separation angle of 1.5° with respect to the direction of the geostationary-satellite orbit.    (WRC‑15)

Section V − Limits of power flux-density from space stations

MOD AFCP/28A6A1/9

TABLE **21-4**  (*continued*)     (Rev.WRC‑15)

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency band | Service\* | Limit in dB(W/m2) for anglesof arrival (δ) above the horizontal plane | Reference bandwidth |
| 0°-5° | 5°-25° | 25°-90° |
| 12.2-12.75 GHz 7(Region 3)12.5‑12.75 GHz 7(Region 1 countries listed in Nos. 5.494 and 5.496) | Fixed-satellite(space-to-Earth)(geostationary-satellite orbit) | −148 | −148 + 0.5(δ − 5) | −138 | 4 kHz |
| 13.4-13.65 GHz(Region 1) | Fixed-satellite(space-to-Earth)(geostationary-satellite orbit) | **0°-0.6°**−137.5 | **0.6°-1.25°**−136.5 | **1.25°-21.25°**−130.5 | **21.25°-70°**−127.5 | **70°-90°**−122 | 1 MHz |

**Reasons:** To insert pfd limits for GSO FSS (space-to-Earth) into RR Article 21 in order to protect allocations to terrestrial services (FS, MS) and RLS.

APPENDIX 5 (REV.WRC‑12)

Identification of administrations with which coordination is to be effected or
agreement sought under the provisions of Article 9

MOD AFCP/28A6A1/10

TABLE 5-1     (Rev.WRC‑15)

Technical conditions for coordination

(see Article 9)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO | A station in a satellite network using the geostationary-satellite orbit (GSO), in any space radiocommunication service, in a frequency band and in a Region where this service is not subject to a Plan, in respect of any other satellite network using that orbit, in any space radiocommunication service in a frequency band and in a Region where this service is not subject to a Plan, with the exception of the coordination between earth stations operating in the opposite direction of transmission | 1) 3 400-4 200 MHz5 725-5 850 MHz (Region 1) and5 850-6 725 MHz7 025-7 075 MHz | i) Bandwidth overlap, andii) any network in the fixed-satellite service (FSS) and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS |  | With respect to the space services listed in the threshold/condition column in the bands in 1), 2), 3), 4), 5), 6), 7) and 8), an administration may request, pursuant to No. **9.41**, to be included in requests for coordination, indicating the networks for which the value of Δ*T*/*T* calculated by the method in § 2.2.1.2 and 3.2 of Appendix **8** exceeds 6%. When the Bureau, on request by an affected administration, studies this information pursuant to No. **9.42**, the calculation method given in § 2.2.1.2 and 3.2 of Appendix **8** shall be used |
| 2) 10.95-11.2 GHz11.45‑11.7 GHz 11.7-12.2 GHz (Region 2)12.2-12.5 GHz (Region 3)12.5‑12.75 GHz (Regions 1 and 3) 12.7‑12.75 GHz (Region 2) and 13.75‑14.5 GHz2*bis*) 13.4-13.65 GHz (Region 1) | i) Bandwidth overlap, andii) any network in the FSS or broadcasting-satellite service (BSS), not subject to a Plan, and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±7° of the nominal orbital position of a proposed network in the FSS or BSS, not subject to a Plani) Bandwidth overlap, andii) any network in the space research service (SRS) or any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±7° of the nominal orbital position of a proposed network in the FSS |

**Reasons:** To specify the order and mechanism of coordination in accordance with provisions of RR No 9.7 between newly notifying networks of the FSS and SRS (space-to-Earth).

MOD AFCP/28A6A1/11

TABLE 5-1 (*end*)     (Rev.WRC‑15)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Reference ofArticle 9 | Case | Frequency bands (and Region) of the service for which coordination is sought | Threshold/condition | Calculation method | Remarks |
| No. **9.21**Terrestrial, GSO, non‑GSO/ terrestrial, GSO, non‑GSO | A station of a service for which the requirement to obtain the agreement of other administrations is included in a footnote to the Table of Frequency Allocations referring to No. **9.21** | Band(s) indicated in the relevant footnote except 13.4‑13.65 GHz in Region 113.4-13.65 GHz in Region 1 | Incompatibility established by the use of Appendices **7**, **8**, technical Annexes of Appendices **30** or **30A**, pfd values specified in some of the footnotes, other technical provisions of the Radio Regulations or ITU‑R Recommendations, as appropriateAny network in the space research service (SRS) within an orbital arc of ±(24)° of the nominal orbital position of a proposed network in the FSS | Methods specified in, or adapted from, Appendices **7**, **8**, **30**, **30A**, other technical provisions of the Radio Regulations or ITU‑R Recommendations |  |

**Reasons:** To define the procedure for coordination under the provisions of RR No. 9.21 between the newly notified FSS networks and SRS networks.

APPENDIX 7 (REV.WRC‑12)

Methods for the determination of the coordination area around an earth
station in frequency bands between 100 MHz and 105 GHz

ANNEX 7

System parameters and predetermined coordination distances for determination of the coordination area around an earth station

# 3 Horizon antenna gain for a receiving earth station with respect to a transmitting earth station

MOD AFCP/28A6A1/12

TABLE 8c    (Rev.WRC‑15)

Parameters required for the determination of coordination distance for a receiving earth station

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiving spaceradiocommunicationservice designation | Fixed-satellite | Fixed-satellite,radio-determinationsatellite | Fixed-satellite | Fixed-satellite | Meteorological-satellite7, 8 | Meteorological-satellite9 | Earth exploration-satellite7 | Earth exploration-satellite9 | Spaceresearch10 | Fixed-satellite | Broadcasting-satellite | Fixed-satellite9 | Broadcasting-satellite | Fixed-satellite7 |
|  |  |  |  |  |  |  |  |  | Deep space |  |  |  |  |  |  |
| Frequency bands (GHz) | 4.500-4.800 | 5.150-5.216 | 6.700-7.075 | 7.250-7.750 | 7.450-7.550 | 7.750-7.900 | 8.025-8.400 | 8.025-8.400 | 8.400-8.450 | 8.450-8.500 | 10.7-12.7513.4-13.657 | 12.5-12.7512 | 15.4-15.7 | 17.7-17.8 | 17.7-18.819.3-19.7 |
| Transmitting terrestrial service designations | Fixed, mobile | Aeronautical radionavigation | Fixed, mobile | Fixed, mobile | Fixed, mobile | Fixed, mobile | Fixed, mobile | Fixed, mobile | Fixed, mobile | Fixed, mobile | Fixed, mobile | Aeronau-tical radio-navigation | Fixed | Fixed, mobile |
| Method to be used | § 2.1 | § 2.1 | § 2.2 | § 2.1 | § 2.1, § 2.2 | § 2.2 | § 2.1 | § 2.2 | § 2.2 | § 2.1, § 2.2 | § 1.4.5 |  | § 1.4.5 | § 2.1 |
| Modulation at earth station1 | A | N |  | N | A | N | N | N | N | N | N | N | A | N | A | N | – |  | N |
| Earth stationinterferenceparametersand criteria | *p*0 (%) | 0.03 | 0.005 |  | 0.005 | 0.03 | 0.005 | 0.002 | 0.001 | 0.083 | 0.011 | 0.001 | 0.1 | 0.03 | 0.003 | 0.03 | 0.003 | 0.003 |  | 0.003 |
| *n* | 3 | 3 |  | 3 | 3 | 3 | 2 | 2 | 2 | 2 | 1 | 2 | 2 | 2 | 1 | 1 | 2 |  | 2 |
| *p* (%) | 0.01 | 0.0017 |  | 0.0017 | 0.01 | 0.0017 | 0.001 | 0.0005 | 0.0415 | 0.0055 | 0.001 | 0.05 | 0.015 | 0.0015 | 0.03 | 0.003 | 0.0015 |  | 0.0015 |
| *NL* (dB) | 1 | 1 |  | 1 | 1 | 1 | – | – | 1 | 0 | 0 | 0 | 1 | 1 | 1 | 1 | 1 |  | 1 |
| *Ms* (dB) | 7 | 2 |  | 2 | 7 | 2 | – | – | 2 | 4.7 | 0.5 | 1 | 7 | 4 | 7 | 4 | 4 |  | 6 |
| *W* (dB) | 4 | 0 |  | 0 | 4 | 0 | – | – | 0 | 0 | 0 | 0 | 4 | 0 | 4 | 0 | 0 |  | 0 |
| Terrestrial station parameters | *E* (dBW)in *B*2 | A | 923 | 923 |  | 55 | 55 | 55 | 55 | 55 | 55 | 55 | 25 5 | 255 | 40 | 40 | 55 | 55 |  |  | 35 |
| N | 424 | 424 |  | 42 | 42 | 42 | 42 | 42 | 42 | 42 | −18 | −18 | 43 | 43 | 42 | 42 |  | 40 | 40 |
| *Pt* (dBW) in *B* | A | 403 | 403 |  | 13 | 13 | 13 | 13 | 13 | 13 | 13 | −175 | −175 | −5 | −5 | 10 | 10 |  |  | −10 |
| N | 0 | 0 |  | 0 | 0 | 0 | 0 | 0 | 0 | 0 | −60 | −60 | −2 | −2 | −3 | −3 |  | −7 | −5 |
| *Gx* (dBi) | 523, 4 | 523, 4 |  | 42 | 42 | 42 | 42 | 42 | 42 | 42 | 42 | 42 | 45 | 45 | 45 | 45 |  | 47 | 45 |
| Reference band-width6 | *B* (Hz) | 106 | 106 |  | 106 | 106 | 106 | 107 | 107 | 106 | 106 | 1 | 1 | 106 | 106 | 27 × 106 | 27 × 106 |  |  | 106 |
| Permissible interference power | *Pr*( *p*) (dBW)in *B* |  |  |  | −151.2 |  |  | −125 | −125 | −15411 | −142 | −220 | −216 |  |  | −131 | −131 |  |  |  |

**Reasons:** To specify coordination distances for the FSS receiving earth station in order to protect it from interferences produced by terrestrial FS and MS stations, based on the allowable interference criterion *I*/*N* = 6%, see Recommendation ITU-R S.1432.

SUP AFCP/28A6A1/13

RESOLUTION 151 (WRC‑12)

Additional primary allocations to the fixed-satellite service
in frequency bands between 10 and 17 GHz in Region 1

**Reasons:** If the Conference agrees to the proposals above, Resolution 151 may no longer be necessary.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_