|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 2 toDocument 58(Add.23)(Add.1)-E** |
|  | **9 October 2015** |
|  | **Original: English** |
|  |
| Indonesia (Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 9.1(9.1.2) |

9 to consider and approve the Report of the Director of the Radiocommunication Bureau, in accordance with Article 7 of the Convention:

9.1 on the activities of the Radiocommunication Sector since WRC‑12;

9.1(9.1.2) Resolution **756 (WRC-12)** − Studies on possible reduction of the coordination arc and technical criteria used in application of No. **9.41** in respect of coordination under No. **9.7**

Introduction

In respect of *resolves* 1 of Resolution 756 (WRC-12), Indonesia is of the view that the current mechanism in the RR has been applied without any constraint. Hence Indonesia supports Option 1D which proposes no change to the RR.

In respect of *resolves* 2 of Resolution 756 (WRC-12), Indonesia is of the view that a reduction to the coordination arc may be possible while concurrently ensuring adequate protection to other existing and proposed satellite networks. Hence, Indonesia supports Option 2B which proposes as follow.

• In the frequency bands under item 1) of Table 5-1 of RR Appendix 5, reduce the coordination arc from ±8º to ±6º;

• In the frequency bands under item 2) of Table 5-1 of RR Appendix 5, reduce the coordination arc from ±7º to ±5º;

• In the frequency bands under items 3) and 7) of Table 5-1 of RR Appendix 5, reduce the coordination arc from ±8º to ±6º;

In the frequency bands under items 4), 5), 6) and 8) of Table 5-1 of RR Appendix 5, no change.

Proposals

NOC INS/58A23A1A2/1

ARTICLE 9

Procedure for effecting coordination with or obtaining agreement of other administrations1, 2, 3, 4, 5, 6, 7, 8, 8*bis*    (WRC‑12)

NOC INS/58A23A1A2/2

ARTICLE 11

Notification and recording of frequency
assignments1, 2, 3, 4, 5, 6, 7, 7*bis*    (WRC‑12)

APPENDIX 5 (REV.WRC-12)

Identification of administrations with which coordination is to be effected or
agreement sought under the provisions of Article 9

МОD INS/58A23A1A2/3

TABLE 5-1     (Rev.WRC‑15)

Technical conditions for coordination
(see Article 9)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO | A station in a satellite network using the geostationary-satellite orbit (GSO), in any space radiocommunication service, in a frequency band and in a Region where this service is not subject to a Plan, in respect of any other satellite network using that orbit, in any space radiocommunication service in a frequency band and in a Region where this service is not subject to a Plan, with the exception of the coordination between earth stations operating in the opposite direction of transmission | 1) 3 400-4 200 MHz5 725-5 850 MHz (Region 1) and5 850-6 725 MHz7 025-7 075 MHz | i) Bandwidth overlap, andii) any network in the fixed-satellite service (FSS) and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±6° of the nominal orbital position of a proposed network in the FSS |  | With respect to the space services listed in the threshold/condition column in the bands in 1), 2), 3), 4), 5), 6), 7) and 8), an administration may request, pursuant to No. **9.41**, to be included in requests for coordination, indicating the networks for which the value of Δ*T*/*T* calculated by the method in § 2.2.1.2 and 3.2 of Appendix **8** exceeds 6%. When the Bureau, on request by an affected administration, studies this information pursuant to No. **9.42**, the calculation method given in § 2.2.1.2 and 3.2 of Appendix **8** shall be used |
| 2) 10.95-11.2 GHz11.45‑11.7 GHz 11.7-12.2 GHz (Region 2)12.2-12.5 GHz (Region 3)12.5‑12.75 GHz (Regions 1 and 3) 12.7‑12.75 GHz (Region 2) and 13.75‑14.5 GHz | i) Bandwidth overlap, andii) any network in the FSS or broadcasting-satellite service (BSS), not subject to a Plan, and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±5° of the nominal orbital position of a proposed network in the FSS or BSS, not subject to a Plan |

TABLE 5-1 (*continued*)     (REV.WRC‑15)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO(*cont.*) |  | 3) 17.7‑20.2 GHz,(Regions 2 and 3), 17.3-20.2 GHz (Region 1) and27.5‑30 GHz | i) Bandwidth overlap, andii) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±6° of the nominal orbital position of a proposed network in the FSS |  |  |
|  |  | 4) 17.3‑17.7 GHz (Regions 1 and 2) | i) Bandwidth overlap, andii) a) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the BSS, or b) any network in the BSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS |  |  |

TABLE 5-1 (*continued*)     (REV.WRC‑15)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO(*cont.*) |  | 5) 17.7‑17.8 GHz | i) Bandwidth overlap, andii) a) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the BSS, or b) any network in the BSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSSNOTE – No. **5.517** applies in Region 2. |  |  |
|  |  | 6) 18.0-18.3 GHz (Region 2) 18.1-18.4 GHz (Regions 1 and 3) | i) Bandwidth overlap, andii) any network in the FSS or meteorological-satellite service and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS or the meteorological-satellite service |  |  |

TABLE 5-1 (*continued*)     (REV.WRC‑15)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO(*cont.*) |  | 6*bis*) 21.4-22 GHz (Regions 1 and 3)7) Bands above 17.3 GHz, except those defined in § 3) and 6) | i) Bandwidth overlap; andii) any network in the BSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±12° of the nominal orbital position of a proposed network in the BSS (see also Resolutions **554 (WRC‑12)** and **553 (WRC‑12)**).i) Bandwidth overlap, andii) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±6° of the nominal orbital position of a proposed network in the FSS (see alsoResolution **901 (Rev.WRC‑07)**) |  | No. **9.41** does not apply. |
|  |  | 8) Bands above 17.3 GHz except those defined in § 4), 5) and 6*bis*) | i) Bandwidth overlap, andii) any network in the FSS or BSS, not subject to a Plan, and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±16° of the nominal orbital position of a proposed network in the FSS or BSS, not subject to a Plan, except in the case of a network in the FSS with respect to a network in the FSS (see also Resolution **901 (Rev.WRC‑07)**) |  |  |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_