|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 6 toDocument 85(Add.21)-E** |
|  | **16 October 2015** |
|  | **Original: English** |
|  |
| Burundi (Republic of)/Kenya (Republic of)/Uganda (Republic of)/Rwanda (Republic of)/Tanzania (United Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 7(F) |

7 to consider possible changes, and other options, in response to Resolution 86 (Rev. Marrakesh, 2002) of the Plenipotentiary Conference, an advance publication, coordination, notification and recording procedures for frequency assignments pertaining to satellite networks, in accordance with Resolution **86 (Rev.WRC‑07)** to facilitate rational, efficient, and economical use of radio frequencies and any associated orbits, including the geostationary‑satellite orbit;

7(F) Issue F – Modifications to RR Appendix **30B** in relation to the suspension of use of a frequency assignment recorded in the MIFR

Introduction

Under this issue, modifications are considered to RR Appendix 30B in order to align the allowed period of suspension of use of a frequency assignment recorded in the MIFR and brought into use with the suspension period applied for assignments of services in non-Planned bands in RR Article 11 and for Planned BSS in RR Appendices 30 and 30A.

EACO member countries (BDI/KEN/UGA/RRW/TZA) support the proposed method in the CPM Report.

Proposal

BDI/KEN/UGA/RRW/TZA (EACO member countries) propose the following.

APPENDIX 30B (REV.WRC‑12)

Provisions and associated Plan for the fixed-satellite service
in the frequency bands 4 500-4 800 MHz, 6 725-7 025 MHz,
10.70-10.95 GHz, 11.2-11.45 GHz and 12.75-13.25 GHz

MOD BDI/KEN/UGA/RRW/TZA/85A21A6/1

ARTICLE 6     (REV.WRC‑12)

Procedures for the conversion of an allotment into an assignment, for
the introduction of an additional system or for the modification of
an assignment in the List1, 2     (WRC‑07)

6.33

When:

i) an assignment is no longer required; *or*

ii) an assignment recorded in the List and brought into use has been suspended for a period exceeding three years and ending after the expiry date specified in § 6.31; *or*

iii) an assignment recorded in the List has not been brought into use within the eight-year period following the receipt by the Bureau of the relevant complete information under § 6.1 (or within the extended period in the event of an extension under § 6.31*bis*), with the exception of assignments submitted by new Member States where § 6.35 and 7.7 apply,

the Bureau shall:

*a)* publish in a Special Section of its BR IFIC the cancellation of the related Special Sections and the assignments recorded in the Appendix **30B** List;

*b)* if the cancelled assignment is the result of a conversion of an allotment without modification, reinstate the allotment in the Appendix **30B** Plan;

*c)* if the cancelled assignment is the result of the conversion of an allotment with modifications, reinstate the allotment with the same orbital location and technical parameters of the cancelled assignment except for its service area, which shall be the national territory of the administration whose allotment is being reinstated; *and*

*d)* update the reference situation for the allotments of the Plan and the assignments of the List.     (WRC‑15)

MOD BDI/KEN/UGA/RRW/TZA/85A21A6/2

ARTICLE 8     (REV.WRC‑12)

Procedure for notification and recording in the Master Register
of assignments in the planned bands for the
fixed-satellite service11, 12     (WRC‑07)

8.17 Wherever the use of a frequency assignment to a space station recorded in the Master Register is suspended for a period exceeding six months, the notifying administration shall, as soon as possible, but not later than six months from the date on which the use was suspended, inform the Bureau of the date on which such use was suspended. When the recorded assignment is brought back into use, the notifying administration shall so inform the Bureau, as soon as possible. The date on which the recorded assignment is brought back into use ADD 14*bis* shall be no later than three years from the date of suspension. If a recorded frequency assignment is not brought back into use within three years from the date of suspension, the Bureau shall cancel the assignment from the Master Register and apply the provisions of § 6.33.     (WRC‑15)

ADD BDI/KEN/UGA/RRW/TZA/85A21A6/3

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

14*bis* The date of bringing back into use of a frequency assignment to a space station in the geostationary-satellite orbit shall be the date of the commencement of the ninety-day period defined below. A frequency assignment to a space station in the geostationary-satellite orbit shall be considered as having been brought back into use when a space station in the geostationary-satellite orbit with the capability of transmitting or receiving that frequency assignment has been deployed and maintained at the notified orbital position for a continuous period of ninety days. The notifying administration shall so inform the Bureau within thirty days from the end of the ninety-day period. (WRC 15).

\_\_\_\_\_\_\_\_\_\_\_\_\_\_