|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| COMMITTEE 6 | **Addendum 22 toDocument 85-E** |
|  | **6 November 2015** |
|  | **Original: English** |
|  |
| Burundi (Republic of)/Kenya (Republic of)/Uganda (Republic of)/ Rwanda (Republic of)/Tanzania (United Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 8 |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC‑07)**;

Proposal

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD BDI/KEN/UGA/RRW/TZA/85A22/1

5.296 *Additional allocation:* in Albania, Germany, Saudi Arabia, Austria, Bahrain, Belgium, Benin, Bosnia and Herzegovina, Burkina Faso, Burundi, Cameroon, Congo (Rep. of the), Côte d'Ivoire, Croatia, Denmark, Djibouti, Egypt, United Arab Emirates, Spain, Estonia, Finland, France, Gabon, Ghana, Iraq, Ireland, Iceland, Israel, Italy, Jordan, Kenya, Kuwait, Latvia, The Former Yugoslav Republic of Macedonia, Libya, Liechtenstein, Lithuania, Luxembourg, Mali, Malta, Morocco, Moldova, Monaco, Niger, Norway, Oman, the Netherlands, Poland, Portugal, Qatar, the Syrian Arab Republic, Slovakia, the Czech Republic, the United Kingdom, Sudan, Sweden, Switzerland, Swaziland, Chad, Togo, Tunisia and Turkey, Angola, Botswana, Lesotho, Malawi, Mauritius, Mozambique, Namibia, Nigeria, Uganda, Rwanda, South Africa, Tanzania, Zambia and Zimbabwe, the band 470-694 MHz is also allocated on a secondary basis to the land mobile service, intended for applications ancillary to broadcasting and programme-making. Stations of the land mobile service in the countries listed in this footnote shall not cause harmful interference to existing or planned stations operating in accordance with the Table in countries other than those listed in this footnote.     (WRC‑15)

**Reasons:** Applications ancillary to broadcasting and programme-making will be accommodated in the band 470-694 MHz allocated to broadcasting.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_