|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 2 toDocument 85(Add.9)-E** |
|  | **16 October 2015** |
|  | **Original: English** |
|  |
| Burundi (Republic of)/Kenya (Republic of)/Uganda (Republic of)/ Rwanda (Republic of)/Tanzania (United Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 1.9.2 |

1.9 to consider, in accordance with Resolution **758 (WRC‑12)**:

1.9.2 the possibility of allocating the bands 7 375-7 750 MHz and 8 025-8 400 MHz to the maritime-mobile satellite service and additional regulatory measures, depending on the results of appropriate studies;

Introduction

This agenda item calls for allocation to MMSS in frequency bands 7 375-7 750 MHz and 8 025‑8 400 MHz. These bands are extensively used by Fixed Services in EACO member countries (BDI/KEN/UGA/RRW/TZA). Allocation to MMSS in these bands would affect Fixed Services in this band. **Method A** proposed in CPM report is supported.

Proposal

BDI/KEN/UGA/RRW/TZA (EACO member countries) propose the following:

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

NOC BDI/KEN/UGA/RRW/TZA/85A9A2/1

7 250-8 500 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 7 450-7 550 FIXED FIXED-SATELLITE (space-to-Earth) METEOROLOGICAL-SATELLITE (space-to-Earth) MOBILE except aeronautical mobile 5.461A |
| 7 550-7 750 FIXED FIXED-SATELLITE (space-to-Earth) MOBILE except aeronautical mobile |

**Reasons:** Allocation to MMSS in this band would affect Fixed Services.

NOC BDI/KEN/UGA/RRW/TZA/85A9A2/2

7 250-8 500 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 8 025-8 175 EARTH EXPLORATION-SATELLITE (space-to-Earth) FIXED FIXED-SATELLITE (Earth-to-space) MOBILE 5.463 5.462A |
| 8 175-8 215 EARTH EXPLORATION-SATELLITE (space-to-Earth) FIXED FIXED-SATELLITE (Earth-to-space) METEOROLOGICAL-SATELLITE (Earth-to-space) MOBILE 5.463 5.462A |
| 8 215-8 400 EARTH EXPLORATION-SATELLITE (space-to-Earth) FIXED FIXED-SATELLITE (Earth-to-space) MOBILE 5.463 5.462A |

**Reasons:** Allocation to MMSS in this band would affect Fixed Services.

SUP BDI/KEN/UGA/RRW/TZA/85A9A2/3

RESOLUTION 758 (WRC‑12)

Allocation to the fixed-satellite service and the maritime-
mobile satellite service in the 7/8 GHz range

**Reasons:** This resolution should consequently be suppressed.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_