|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-15)Geneva, 2–27 November 2015** |  |
| **INTERNATIONAL TELECOMMUNICATION UNION** |  |
|  |  |
| PLENARY MEETING | **Addendum 1 toDocument 91-E** |
|  | **19 October 2015** |
|  | **Original: English** |
|  |
| Australia |
| Proposals for the work of the conference |
| **Proposal to add Australia’s name to RR Nos. 5.432B and 5.433A** |
| Agenda item 1.1 |

1.1 to consider additional spectrum allocations to the mobile service on a primary basis and identification of additional frequency bands for International Mobile Telecommunications (IMT) and related regulatory provisions, to facilitate the development of terrestrial mobile broadband applications, in accordance with Resolution **233 (WRC‑12)**;

Introduction

Australia supports the allocation of the frequency band 3 400-3 600 MHz to the mobile service, except aeronautical mobile, on a primary basis and the identification for IMT in response to WRC‑15 agenda item 1.1. Australia notes that RR Nos. 5.430A, 5.432A, 5.432B and 5.433A already identify, in a number of countries, the frequency band 3 400-3 600 MHz (or parts of it) for IMT.

Australia proposes to add its name to RR footnotes 5.432B and 5.433A, which are the footnotes relevant to Region 3, in accordance with Methods B Option B4 and C Option C4 described in section 1/1.1/5.10 of the CPM Report. These methods allow for the addition of country names to existing footnotes without any further modification of the footnotes.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD AUS/91A1/1

2 700-4 800 MHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 3 400-3 600FIXEDFIXED-SATELLITE(space-to-Earth)Mobile 5.430ARadiolocation5.431 | 3 400-3 500FIXEDFIXED-SATELLITE (space-to-Earth)AmateurMobile 5.431ARadiolocation 5.4335.282 | 3 400-3 500FIXEDFIXED-SATELLITE (space-to-Earth)AmateurMobile MOD 5.432BRadiolocation 5.4335.282 5.432 5.432A |
| 3 500-3 700FIXEDFIXED-SATELLITE (space-to-Earth)MOBILE except aeronautical mobileRadiolocation 5.433 | 3 500-3 600FIXEDFIXED-SATELLITE (space-to-Earth)MOBILE except aeronautical mobile MOD 5.433ARadiolocation 5.433 |

MOD AUS/91A1/2

5.432B *Different category of service:*  in Australia, Bangladesh, China, French overseas communities of Region 3, India, Iran (Islamic Republic of), New Zealand and Singapore, the band 3 400-3 500 MHz is allocated to the mobile, except aeronautical mobile, service on a primary basis, subject to agreement obtained under No. **9.21** with other administrations and is identified for International Mobile Telecommunications (IMT). This identification does not preclude the use of this band by any application of the services to which it is allocated and does not establish priority in the Radio Regulations. At the stage of coordination the provisions of Nos. **9.17** and **9.18** also apply. Before an administration brings into use a (base or mobile) station of the mobile service in this band it shall ensure that the power flux-density (pfd) produced at 3 m above ground does not exceed −154.5 dB(W/(m2 ⋅ 4 kHz)) for more than 20% of time at the border of the territory of any other administration. This limit may be exceeded on the territory of any country whose administration has so agreed. In order to ensure that the pfd limit at the border of the territory of any other administration is met, the calculations and verification shall be made, taking into account all relevant information, with the mutual agreement of both administrations (the administration responsible for the terrestrial station and the administration responsible for the earth station) with the assistance of the Bureau if so requested. In case of disagreement, the calculation and verification of the pfd shall be made by the Bureau, taking into account the information referred to above. Stations of the mobile service in the band 3 400-3 500 MHz shall not claim more protection from space stations than that provided in Table **21‑4** of the Radio Regulations (Edition of 2004). This allocation is effective from 17 November 2010.     (WRC‑15)

**Reasons:** To allocate the band 3 400-3 500 MHz to the mobile service, except aeronautical mobile, on a primary basis and identify for IMT in Australia by including Australia in the list of countries in RR No. 5.432B.

MOD AUS/91A1/3

5.433A In Australia, Bangladesh, China, French overseas communities of Region 3, Korea (Rep. of), India, Iran (Islamic Republic of), Japan, New Zealand and Pakistan, the band 3 500-3 600 MHz is identified for International Mobile Telecommunications (IMT). This identification does not preclude the use of this band by any application of the services to which it is allocated and does not establish priority in the Radio Regulations. At the stage of coordination the provisions of Nos.**9.17** and **9.18** also apply. Before an administration brings into use a (base or mobile) station of the mobile service in this band it shall ensure that the power flux-density (pfd) produced at 3 m above ground does not exceed −154.5 dB(W/(m2 ⋅ 4 kHz)) for more than 20% of time at the border of the territory of any other administration. This limit may be exceeded on the territory of any country whose administration has so agreed. In order to ensure that the pfd limit at the border of the territory of any other administration is met, the calculations and verification shall be made, taking into account all relevant information, with the mutual agreement of both administrations (the administration responsible for the terrestrial station and the administration responsible for the earth station), with the assistance of the Bureau if so requested. In case of disagreement, the calculation and verification of the pfd shall be made by the Bureau, taking into account the information referred to above. Stations of the mobile service in the band 3 500-3 600 MHz shall not claim more protection from space stations than that provided in Table **21‑4** of the Radio Regulations (Edition of 2004).     (WRC‑15)

**Reasons:** To identify the frequency band 3 500-3 600 MHz for IMT in Australia by including Australia in the list of countries in RR No. 5.433A.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_