|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 2 toDocument 12(Add.19)-E** |
|  | **24 June 2019** |
|  | **Original: Russian** |
|  |
| Regional Commonwealth in the field of Communications Common Proposals |
| proposals for the work of the conference |
|  |
| Agenda item 7(B) |

7 to consider possible changes, and other options, in response to Resolution 86 (Rev. Marrakesh, 2002) of the Plenipotentiary Conference, an advance publication, coordination, notification and recording procedures for frequency assignments pertaining to satellite networks, in accordance with Resolution **86 (Rev.WRC-07)**, in order to facilitate rational, efficient and economical use of radio frequencies and any associated orbits, including the geostationary-satellite orbit;

7(B) Issue B - Application of coordination arc in the Ka-band, to determine coordination requirements between the FSS and other satellite services

Introduction

The RCC Administrations support the implementation of the coordination arc mechanism in the Ka‑band to determine the need for coordination between geostationary-satellite networks in the mobile-satellite service (MSS) and the fixed-satellite service (FSS), as well as between MSS geostationary-satellite networks, with the possibility of applying RR No. **9.41**, in accordance with the only method put forward in the CPM Report.

APPENDIX 5 (REV.WRC‑15)

Identification of administrations with which coordination is to be effected or
agreement sought under the provisions of Article 9

MOD RCC/12A19A2/1

TABLE 5-1     (Rev.WRC‑19)

Technical conditions for coordination

(see Article 9)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO | A station in a satellite network using the geostationary-satellite orbit (GSO), in any space radiocommunication service, in a frequency band and in a Region where this service is not subject to a Plan, in respect of any other satellite network using that orbit, in any space radiocommunication service in a frequency band and in a Region where this service is not subject to a Plan, with the exception of the coordination between earth stations operating in the opposite direction of transmission | 1) 3 400-4 200 MHz5 725-5 850 MHz (Region 1) and5 850-6 725 MHz7 025-7 075 MHz | i) Bandwidth overlap, andii) any network in the fixed-satellite service (FSS) and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±7° of the nominal orbital position of a proposed network in the FSS |  | With respect to the space services listed in the threshold/condition column in the frequency bands in 1), 2), 2*bis*), 3), 3*bis)*, 4), 5), 6), 7) and 8), an administration may request, pursuant to No. **9.41**, to be included in requests for coordination, indicating the networks for which the value of Δ*T*/*T* calculated by the method in § 2.2.1.2 and 3.2 of Appendix **8** exceeds 6%. When the Bureau, on request by an affected administration, studies this information pursuant to No. **9.42**, the calculation method given in § 2.2.1.2 and 3.2 of Appendix **8** shall be used |
| 2) 10.95-11.2 GHz11.45‑11.7 GHz 11.7-12.2 GHz (Region 2)12.2-12.5 GHz (Region 3)12.5‑12.75 GHz (Regions 1 and 3) 12.7‑12.75 GHz (Region 2) and 13.75‑14.8 GHz | i) Bandwidth overlap, andii) any network in the FSS or broadcasting-satellite service (BSS), not subject to a Plan, and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±6° of the nominal orbital position of a proposed network in the FSS or BSS, not subject to a Planiii) in the band 14.5-14.8 GHz any network in the space research service (SRS) or FSS not subject to a Plan and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±6° of the nominal orbital position of a proposed network in the SRS or FSS not subject to a Plan |

TABLE 5-1 (*continued*)     (Rev.WRC‑19)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO(*cont.*) |  | 2*bis*) 13.4-13.65 GHz (Region 1) | i) Bandwidth overlap, andii) any network in the space research service (SRS) or any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±6° of the nominal orbital position of a proposed network in the FSS or SRS |  |  |
|  | 3) 17.7‑19.7 GHz,(Regions 2 and 3), 17.3-19.7 GHz (Region 1) and27.5‑29.5 GHz | i) Bandwidth overlap, andii) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS |  |  |
|  |  | 3*bis*)19.7-20.2 GHz and29.5-30 GHz | i) Bandwidth overlap, andii) any network in the FSS or in the MSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS or in the MSS. |  |  |
|  |  | 4) 17.3‑17.7 GHz (Regions 1 and 2) | i) Bandwidth overlap, andii) a) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the BSS, or b) any network in the BSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS |  |  |

TABLE 5-1 (*continued*)     (Rev.WRC‑19)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO(*cont.*) |  | 5) 17.7‑17.8 GHz | i) Bandwidth overlap, andii) a) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the BSS, or b) any network in the BSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSSNOTE – No. **5.517** applies in Region 2. |  |  |
|  |  | 6) 18.0-18.3 GHz (Region 2) 18.1-18.4 GHz (Regions 1 and 3)  | i) Bandwidth overlap, andii) any network in the FSS or meteorological-satellite service and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS or the meteorological-satellite service |  |  |

TABLE 5-1 (*continued*)     (Rev.WRC‑19)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO(*cont.*) |  | 6*bis*) 21.4-22 GHz (Regions 1 and 3) | i) Bandwidth overlap; andii) any network in the BSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±12° of the nominal orbital position of a proposed network in the BSS (see also Resolutions **554 (WRC‑12)** and **553 (WRC‑12)**). |  | No. **9.41** does not apply. |
|  |  | 7) Bands above 17.3 GHz, except those defined in § 3), 3*bis*) and 6) | i) Bandwidth overlap, andii) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS (see alsoResolution **901 (Rev.WRC‑07)**) |  |  |
|  |  | 8) Bands above 17.3 GHz except those defined in § 4), 5) and 6*bis*) | i) Bandwidth overlap, andii) any network in the FSS or BSS, not subject to a Plan, and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±16° of the nominal orbital position of a proposed network in the FSS or BSS, not subject to a Plan, except in the case of a network in the FSS with respect to a network in the FSS (see also Resolution **901 (Rev.WRC‑07)**) |  |  |

TABLE 5-1 (*continued*)     (Rev.WRC‑19)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
| No. **9.7**GSO/GSO(*cont.*) |  | 9) All frequency bands, other than those in 1), 2), 2*bis*), 3), 3*bis*), 4), 5), 6), 6*bis)*, 7) and 8), allocated to a space service, and the bands in 1), 2), 2*bis*), 3), 3*bis*), 4), 5), 6), 6*bis*), 7) and 8) where the radio service of the proposed network or affected networks is other than the space services listed in the threshold/ condition column, or in the case of coordination of space stations operating in the opposite direction of transmission | i) Bandwidth overlap, andii) Value of ∆*T/T* exceeds 6% | Appendix **8** | In application of Article 2A of Appendix **30** for the space operation functions using the guardbands defined in § 3.9 of Annex 5 of Appendix **30**, the threshold/condition specified for the FSS in the bands in 2) applies.In application of Article 2A of Appendix**30A** for the space operation functions using the guardbands defined in § 3.1 and 4.1 of Annex 3 of Appendix**30A**, the threshold/condition specified for the FSS in the bands in 7) applies |

**Reasons:** Extend the coordination arc to consider MSS in the frequency bands 29.5-30 GHz and 19.7-20.2 GHz.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_