|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 2 toDocument 49(Add.13)-E** |
|  | **4 October 2019** |
|  | **Original: English** |
|  |
| Viet Nam (Socialist Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 1.13 |

1.13 to consider identification of frequency bands for the future development of International Mobile Telecommunications (IMT), including possible additional allocations to the mobile service on a primary basis, in accordance with Resolution **238 (WRC-15)**;

# 1 Introduction

This contribution provides views and proposals for WRC-19 agenda item 1.13 in terms of Condition A2a of the CPM Report for the frequency range 24.25-27.5 GHz.

# 2 Considerations

## 2.1 Importance to identify IMT spectrum bands above 24.25 GHz

From Recommendation ITU-R M.2083 for IMT-2020 vision and study results on spectrum needs conducted by ITU-R Task Group 5/1 (TG 5/1), tens of GHz bandwidth would be required to realize IMT-2020 vision and to facilitate global momentum for developments and rollout timely.

## 2.2 Urgency for identified IMT spectrum above 24.25 GHz

Recently, many countries are establishing their policies to make available bands above 24.25 GHz for their IMT-2020 services around 2020 recommended by Recommendation ITU-R M.2083. There are plenty of global demands to use bands above 24.25 GHz for IMT-2020 around 2020. Taking into account these global demands, timely identification and technically harmonized IMT bands above 24.25 GHz at WRC-19 is significant.

## 2.3 Reasonable conditions to facilitate IMT-2020 using bands above 24.25 GHz

IMT-2020 supporting bands above 24.25 GHz is totally new technology using advanced technologies such as beam array antenna, beam tracking and RFIC. These new technical paradigms controlling interference issues can support co-existence between IMT-2020 and other services. From this aspect, not only protection of other services but also promotion of new services by IMT‑2020 should be considered with reasonable balance, under co-primary basis.

Unwanted emission levels for BS and UE of IMT-2020 in the 24.2-27.5 GHz to protect EESS (passive) in the 23.6-24 GHz is one of the key discussion items under Condition A2a in [CPM Report](https://www.itu.int/md/R15-CPM19.02-R-0001/en). From administrations’ regulatory point of view, some countries have already been decided their regulations addressing −20 dB(W/200 MHz) for BS and UE, which is totally same with the unwanted emission limit defined by 3GPP. Also several regional preparatory groups for WRC-19 have been decided their positions to support unwanted emission limits for base and mobile stations based on balance between facilitation of IMT-2020 service and protection of near adjacent band service.

# 3 Proposal

Taking into account above, followings are proposed for unwanted emission limits:

– To revise No. **5.338A**

– To revise Resolution **750 (Rev.WRC-15)**

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD VTN/49A13A2/1#49841

5.338AIn the frequency bands 1 350-1 400 MHz, 1 427-1 452 MHz, 22.55-23.55 GHz, 24.25-24.75 GHz, 30-31.3 GHz, 49.7‑50.2 GHz, 50.4-50.9 GHz, 51.4-52.6 GHz, 81-86 GHz and 92-94 GHz, Resolution **750 (Rev.WRC‑19)** applies.     (WRC‑19)

**Reasons:** The identification of the band 24.25-27.5 GHz to IMT will require limits in Resolution **750 (Rev. WRC-15)** to ensure near adjacent band compatibility with EESS (passive) in the band 23.6-24.0 GHz.

MOD VTN/49A13A2/2#49845

RESOLUTION 750 (Rev.WRC‑19)

Compatibility between the Earth exploration-satellite service (passive) and relevant active services

The World Radiocommunication Conference (Sharm el-Sheikh, 2019),

…

resolves

1 that unwanted emissions of stations brought into use in the frequency bands and services listed in Table 1‑1 below shall not exceed the corresponding limits in that table, subject to the specified conditions;

…

TABLE 1-1

|  |  |  |  |
| --- | --- | --- | --- |
| EESS (passive) band | Activeservice band | Active service | Limits of unwanted emission power fromactive service stations in a specified bandwidthwithin the EESS (passive) band1 |
| … | … | … | … |
| 23.6-24 GHz | 24.25-24.75 GHz | Mobile | −33.5 dBW in any 200 MHz in the EESS (passive) band for IMT base stations−29.7 dBW in any 200 MHz in the EESS (passive) band for IMT mobile stations |

**Reasons:** The identification of the band 24.25-27.5 GHz to IMT will require limits in Resolution **750 (Rev. WRC-15)** to ensure near adjacent band compatibility with EESS (passive) in the band 23.6-24.0 GHz.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_