|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19)Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 10 toDocument 49(Add.19)-E** |
|  | **9 October 2019** |
|  | **Original: English** |
|  |
| Viet Nam (Socialist Republic of) |
| Proposals for the work of the conference |
|  |
| Agenda item 7(J) |

7 to consider possible changes, and other options, in response to Resolution 86 (Rev. Marrakesh, 2002) of the Plenipotentiary Conference, an advance publication, coordination, notification and recording procedures for frequency assignments pertaining to satellite networks, in accordance with Resolution **86 (Rev.WRC-07)**, in order to facilitate rational, efficient and economical use of radio frequencies and any associated orbits, including the geostationary-satellite orbit;

7(J) Issue J - Pfd limit in Section 1, Annex 1 of RR Appendix **30**

Introduction

Viet Nam is of the view that the pfd limit referred to in the first paragraph of Section 1 of Annex 1 to RR Appendix **30** is a hard limit that shall not be exceeded in order to protect BSS assignments from interference that may be caused by BSS networks located outside an arc of 9around a wanted BSS network.

In particular, Method F1 of the CPM Report could not apply for narrow countries. Therefore, Viet Nam supports Method F2 of the CPM Report.

Proposals

APPENDIX 30 (REV.WRC‑15)[[1]](#footnote-1)\*

Provisions for all services and associated Plans and List[[2]](#footnote-2)1 for
the broadcasting-satellite service in the frequency bands
11.7-12.2 GHz (in Region 3), 11.7-12.5 GHz (in Region 1)
         and 12.2-12.7 GHz (in Region 2)    (WRC‑03)

ANNEX 1     (REV.WRC‑15)

Limits for determining whether a service of an administration is affected
by a proposed modification to the Region 2 Plan or by a proposed
new or modified assignment in the Regions 1 and 3 List
or when it is necessary under this Appendix to seek
the agreement of any other administration[[3]](#footnote-3)25

NOC VTN/49A19A10/1#50132

# 1 Limits for the interference into frequency assignments in conformity with the Regions 1 and 3 Plan or with the Regions 1 and 3 List or into new or modified assignments in the Regions 1 and 3 List

**Reasons:** Because it would be very hard, technically in practice, to comply with the pfd limit referred to in the first paragraph of Section 1 of Annex 1 to RR Appendix **30** on the territory of other administrations that is geographically close to that of the notifying administration whenexceedance of the limit is allowed within the national territory of the notifying administration, current regulatory provisions for the hard limit should not be changed.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \* The expression “frequency assignment to a space station”, wherever it appears in this Appendix, shall be understood to refer to a frequency assignment associated with a given orbital position. See also Annex 7 for the orbital limitations.     (WRC‑2000) [↑](#footnote-ref-1)
2. 1 The Regions 1 and 3 List of additional uses is annexed to the Master International Frequency Register (see Resolution **542 (WRC‑2000)**\*\*).     (WRC‑03)

 \*\* *Note by the Secretariat*: This Resolution was abrogated by WRC‑03.

*Note by the Secretariat*: Reference to an Article with the number in roman is referring to an Article in this Appendix. [↑](#footnote-ref-2)
3. 25 With respect to this Annex, except for Section 2, the limits relate to the power flux‑density which would be obtained assuming free-space propagation conditions.

 With respect to Section 2 of this Annex, the limit specified relates to the overall equivalent protection margin calculated in accordance with § 2.2.4 of Annex 5. [↑](#footnote-ref-3)