|  |  |
| --- | --- |
| **World Radiocommunication Conference (WRC-19) Sharm el-Sheikh, Egypt, 28 October – 22 November 2019** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 20 to Document 51-E** |
|  | **4 October 2019** |
|  | **Original: English** |
|  | |
| Azerbaijan (Republic of) | |
| Proposals for the work of the conference | |
|  | |
| Agenda item 8 | |

8 to consider and take appropriate action on requests from administrations to delete their country footnotes or to have their country name deleted from footnotes, if no longer required, taking into account Resolution **26 (Rev.WRC-07)**;

In accordance with Resolution **26 (Rev.WRC-07)**, the Communication Administration of the Republic of Azerbaijan has reviewed footnotes to the Table of Frequency Allocations and proposes to delete country name of Azerbaijan from footnotes Nos. **5.128**, **5.194**, **5.312**, **5.350**, **5.428**, **5.430** and **5.448** of the Radio Regulations.

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations  
(See No. 2.1)

MOD AZE/51A20/1

5.128 Frequencies in the bands 4 063-4 123 kHz and 4 130-4 438 kHz may be used exceptionally by stations in the fixed service, communicating only within the boundary of the country in which they are located, with a mean power not exceeding 50 W, on condition that harmful interference is not caused to the maritime mobile service. In addition, in Afghanistan, Argentina, Armenia, Belarus, Botswana, Burkina Faso, the Central African Rep., China, the Russian Federation, Georgia, India, Kazakhstan, Mali, Niger, Pakistan, Kyrgyzstan, Tajikistan, Chad, Turkmenistan and Ukraine, in the bands 4 063-4 123 kHz, 4 130-4 133 kHz and 4 408-4 438 kHz, stations in the fixed service, with a mean power not exceeding 1 kW, can be operated on condition that they are situated at least 600 km from the coast and that harmful interference is not caused to the maritime mobile service.    (WRC‑19)

**Reasons:** The reference to Azerbaijan is no longer necessary in this footnote.

MOD AZE/51A20/2

5.194 *Additional allocation:*in Kyrgyzstan, Somalia and Turkmenistan, the band 104-108 MHz is also allocated to the mobile, except aeronautical mobile (R), service on a secondary basis.     (WRC-19)

**Reasons:** The reference to Azerbaijan is no longer necessary in this footnote.

MOD AZE/51A20/3

5.312 *Additional allocation*:  in Armenia, Belarus, the Russian Federation, Georgia, Kazakhstan, Uzbekistan, Kyrgyzstan, Tajikistan, Turkmenistan and Ukraine, the frequency band 645-862 MHz, in Bulgaria the frequency bands 646-686 MHz, 726-758 MHz, 766-814 MHz and 822‑862 MHz, and in Poland the frequency band 860‑862 MHz until 31 December 2017, are also allocated to the aeronautical radionavigation service on a primary basis.     (WRC‑19)

**Reasons:** The reference to Azerbaijan is no longer necessary in this footnote.

MOD AZE/51A20/4

5.350 *Additional allocation:*in Kyrgyzstan and Turkmenistan, the band 1 525-1 530 MHz is also allocated to the aeronautical mobile service on a primary basis.     (WRC‑19)

**Reasons:** The reference to Azerbaijan is no longer necessary in this footnote.

MOD AZE/51A20/5

5.428 *Additional allocation:*in Kyrgyzstan and Turkmenistan, the frequency band 3 100-3 300 MHz is also allocated to the radionavigation service on a primary basis.     (WRC‑19)

**Reasons:** The reference to Azerbaijan is no longer necessary in this footnote.

MOD AZE/51A20/6

5.430 *Additional allocation:*in Kyrgyzstan and Turkmenistan, the frequency band 3 300-3 400 MHz is also allocated to the radionavigation service on a primary basis.     (WRC‑19)

**Reasons:** The reference to Azerbaijan is no longer necessary in this footnote.

MOD AZE/51A20/7

5.448 *Additional allocation:* in Kyrgyzstan, Romania and Turkmenistan, the band 5 250-5 350 MHz is also allocated to the radionavigation service on a primary basis.    (WRC‑19)

**Reasons:** The reference to Azerbaijan is no longer necessary in this footnote.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_