|  |  |  |
| --- | --- | --- |
| A close up of a sign  Description automatically generated | **World Radiocommunication Conference (WRC-23)Dubai, 20 November - 15 December 2023** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 2 toDocument 65(Add.2)-E** |
|  | **29 September 2023** |
|  | **Original: English** |
|  |
| European Common Proposals |
| Proposals for the work of the conference |
|  |
| Agenda item 1.2 |

1.2 to consider identification of the frequency bands 3 300-3 400 MHz, 3 600‑3 800 MHz, 6 425-7 025 MHz, 7 025-7 125 MHz and 10.0-10.5 GHz for International Mobile Telecommunications (IMT), including possible additional allocations to the mobile service on a primary basis, in accordance with Resolution **245 (WRC‑19)**;

**Part 2 – Frequency band 3 300-3 400 MHz in Region 2**

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

NOC EUR/65A2A2/1

5.429C *Different category of service*: in Argentina, Belize, Brazil, Chile, Colombia, Costa Rica, the Dominican Republic, El Salvador, Ecuador, Guatemala, Mexico, Paraguay and Uruguay, the frequency band 3 300-3 400 MHz is allocated to the mobile, except aeronautical mobile, service on a primary basis. In Argentina, Brazil, the Dominican Republic, Guatemala, Mexico, Paraguay and Uruguay, the frequency band 3 300-3 400 MHz is also allocated to the fixed service on a primary basis. Stations in the fixed and mobile services operating in the frequency band 3 300-3 400 MHz shall not cause harmful interference to, or claim protection from, stations operating in the radiolocation service.     (WRC‑19)

NOC EUR/65A2A2/2

5.429D In the following countries in Region 2: Argentina, Belize, Brazil, Chile, Colombia, Costa Rica, the Dominican Republic, El Salvador, Ecuador, Guatemala, Mexico, Paraguay and Uruguay, the use of the frequency band 3 300-3 400 MHz is identified for the implementation of International Mobile Telecommunications (IMT). Such use shall be in accordance with Resolution **223 (Rev.WRC‑19)**. This use in Argentina, Paraguay and Uruguay is subject to the application of No. **9.21**. The use of the frequency band 3 300-3 400 MHz by IMT stations in the mobile service shall not cause harmful interference to, or claim protection from, systems in the radiolocation service, and administrations wishing to implement IMT shall obtain the agreement of neighbouring countries to protect operations within the radiolocation service. This identification does not preclude the use of this frequency band by any application of the services to which it is allocated and does not establish priority in the Radio Regulations.     (WRC‑19)

**Reasons:** CEPT supports maintaining the regulatory provisions in RR Nos. **5.429C** and **5.429D** applicable to IMT stations in this band. In particular, IMT stations shall not cause harmful interference to, or claim protection from, systems in the radiolocation service in various national and international operational environments and shall meet unwanted emission levels specified in the relevant ITU-R Recommendations.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_