|  |  |  |
| --- | --- | --- |
| A close up of a sign  Description automatically generated | **World Radiocommunication Conference (WRC-23)Dubai, 20 November - 15 December 2023** |  |
|  |  |
|  |  |
| PLENARY MEETING | **Addendum 19 toDocument 85-E** |
|  | **22 October 2023** |
|  | **Original: Russian** |
|  |
| Regional Commonwealth in the field of Communications Common Proposals |
| proposals for the work of the conference |
|  |
| Agenda item 1.19 |

1.19to consider a new primary allocation to the fixed-satellite service in the space-to-Earth direction in the frequency band 17.3-17.7 GHz in Region 2, while protecting existing primary services in the band, in accordance with Resolution **174 (WRC‑19)**;

Introduction

The RCC Administrations do not object to the new primary allocation to the fixed-satellite service in the space-to-Earth direction in the frequency band 17.3-17.7 GHz in Region 2, while protecting the existing services in Region 1 within this and adjacent frequency bands without imposing any additional constraints on these services.

The RCC Administrations support Method C to satisfy this agenda item.

Proposals

ARTICLE 5

Frequency allocations

Section IV – Table of Frequency Allocations
(See No. 2.1)

MOD RCC/85A19/1#1941

15.4-18.4 GHz

|  |
| --- |
| Allocation to services |
| Region 1 | Region 2 | Region 3 |
| 17.3-17.7FIXED-SATELLITE(Earth-to-space) 5.516(space-to-Earth) MOD 5.516A 5.516BRadiolocation | 17.3-17.7FIXED-SATELLITE(Earth-to-space) 5.516(space-to-Earth)  ADD 5.XXX MOD 5.516A MOD 5.517BROADCASTING-SATELLITERadiolocation | 17.3-17.7FIXED-SATELLITE(Earth-to-space) 5.516Radiolocation |
| 5.514 | 5.514 5.515 | 5.514 |

**Reasons**: Introduce an FSS (space-to-Earth) allocation in the frequency band 17.3-17.7 GHz in Region 2 and apply RR Nos. **5.516A** and **5.517** to this new allocation. Also, add new footnote RR No. **5.XXX** to address the fact that the FSS (space-to-Earth) allocation in the frequency band 17.3-17.7 GHz in Region 2 is limited to geostationary satellites.

ADD RCC/85A19/2

5.XXX The use of the band 17.3-17.7 GHz in Region 2 by systems in the fixed-satellite service (space-to-Earth) is limited to geostationary satellites.     (WRC‑23)

**Reasons:** As the frequency band 17.3-17.7 GHz is not allocated globally to FSS (space-to-Earth), its use in Region 2 shall be limited to geostationary-satellite systems.

MOD RCC/85A19/3#1944

5.516A In the band 17.3-17.7 GHz, earth stations of the fixed-satellite service (space-to-Earth) in Regions 1 and 2 shall not claim protection from the broadcasting-satellite service feeder-link earth stations operating under Appendix 30A, nor put any limitations or restrictions on the locations of the broadcasting-satellite service feeder-link earth stations anywhere within the service area of the feeder link. In Region 2, the use of the fixed-satellite service in the band 17.3-17.7 GHz (space-to-Earth) shall not cause unacceptable interference to the space station receivers of the broadcasting-satellite service feeder link in Regions 1 and 3 operating and those to be operated in the future under Appendix **30A**; upon receipt of a report of unacceptable interference, the notifying administration of the fixed-satellite service shall immediately eliminate or reduce interference to an acceptable level.     (WRC‑23)

**Reasons:** Extend the applicability of this footnote to Region 2 and ensure the protection of receiving space stations operating under RR Appendix **30A**.

MOD RCC/85A19/4

5.517 In Region 2, use of the fixed-satellite (space-to-Earth) service in the band 17.3-17.8 GHz shall not cause harmful interference to nor claim protection from assignments in the broadcasting-satellite service operating in conformity with the Radio Regulations.     (WRC‑23)

**Reasons:** Extend the applicability of the frequency ranges in this footnote to Region 2.

MOD RCC/85A19/5

APPENDIX 5 (REV.WRC‑23)

Identification of administrations with which coordination is to be effected or
agreement sought under the provisions of Article 9

MOD RCC/85A19/6#1939

TABLE 5-1     (Rev.WRC‑23)

Technical conditions for coordination

(see Article 9)

...

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ReferenceofArticle 9 | Case | Frequency bands(and Region) of the service for which coordinationis sought | Threshold/condition | Calculation method | Remarks |
|  |  |  |  |  |  |
| No. **9.7**GSO/GSO(*cont.*) |  | 2*bis*) 13.4-13.65 GHz(Region 1) | i) Bandwidth overlap, andii) any network in the space research service (SRS) or any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±6° of the nominal orbital position of a proposed network in the FSS or SRS |  |  |
|  | 3) 17.7‑19.7 GHz,(Region 3), 17.3-19.7 GHz (Regions 1 and 2) and27.5‑29.5 GHz | i) Bandwidth overlap, andii) any network in the FSS and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS |  |  |
|  | 3*bis*)19.7-20.2 GHz and29.5-30 GHz | i) Bandwidth overlap, andii) any network in the FSS or in the mobile-satellite service (MSS) and any associated space operation functions (see No. **1.23**) with a space station within an orbital arc of ±8° of the nominal orbital position of a proposed network in the FSS or in the MSS. |  |  |

...

**Reasons:** Covers the coordination of two GSO networks of the FSS (except earth stations operating in opposite directions of transmission) under RR No. **9.7**.

APPENDIX 30A (REV.WRC‑19)[[1]](#footnote-1)\*

Provisions and associated Plans and List[[2]](#footnote-2)1 for feeder links for the broadcasting-satellite service (11.7-12.5 GHz in Region 1, 12.2-12.7 GHz
in Region 2 and 11.7-12.2 GHz in Region 3) in the frequency bands
14.5-14.8 GHz[[3]](#footnote-3)2 and 17.3-18.1 GHz in Regions 1 and 3,
and 17.3-17.8 GHz in Region 2     (WRC‑03)

MOD RCC/85A19/7

ARTICLE 7     (Rev.WRC‑23)

Coordination, notification and recording in the Master International
Frequency Register of frequency assignments to stations in the fixed-satellite service (space-to-Earth) in Regions 1 and 2 in the frequency band 17.3-18.1 GHz and in Region 3 in the frequency band 17.7-18.1 GHz, to stations in the fixed‑satellite service (Earth-to-space) in Region 2 in the frequency bands 14.5‑14.8 GHz and 17.8‑18.1 GHz, to stations in the fixed-satellite service (Earth-to-space) in countries listed in Resolution 163 (WRC‑15) in the frequency band 14.5‑14.75 GHz and in countries listed in Resolution 164 (WRC‑15) in the frequency band 14.5-14.8 GHz where those stations are not for feeder links for the broadcasting-satellite service, and to stations in the broadcasting-satellite service in Region 2 in the frequency band 17.3-17.8 GHz when frequency assignments to feeder links for broadcasting-satellite stations in the frequency bands 14.5-14.8 GHz and 17.3-18.1 GHz in Regions 1 and 3 or in the
frequency band 17.3-17.8 GHz in Region 2 are involved[[4]](#footnote-4)28     (Rev.WRC‑23)

Section I – Coordination of transmitting space or earth stations in the fixed-satellite
service or transmitting space stations in the broadcasting-satellite service
with assignments to broadcasting-satellite service feeder links

MOD RCC/85A19/8

7.1 The provisions of No. 9.7[[5]](#footnote-5)29 and the associated provisions under Articles 9 and 11 are applicable to transmitting space stations in the fixed-satellite service in Regions 1 and 2 in the frequency band 17.3-18.1 GHz, to transmitting space stations in the fixed-satellite service in Region 3 in the frequency band 17.7-18.1 GHz, to transmitting earth stations in the fixed-satellite service in Region 2 in the frequency bands 14.5-14.8 GHz and 17.8‑18.1 GHz, to transmitting earth stations in the fixed-satellite service in countries listed in Resolution **163 (WRC‑15)** in the frequency band 14.5-14.75 GHz and in countries listed in Resolution **164 (WRC‑15)** in the frequency band 14.5-14.8 GHz where those stations are not for feeder links for the broadcasting-satellite service, and to transmitting space stations in the broadcasting-satellite service in Region 2 in the frequency band 17.3-17.8 GHz.     (WRC‑23)

SUP RCC/85A19/9

RESOLUTION 174 (WRC‑19)

Primary allocation to the fixed-satellite service in the space-to-Earth direction in the frequency band 17.3-17.7 GHz in Region 2

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. \* The expression “frequency assignment to a space station”, wherever it appears in this Appendix, shall be understood to refer to a frequency assignment associated with a given orbital position.     (WRC‑03) [↑](#footnote-ref-1)
2. 1 The Regions 1 and 3 feeder-link List of additional uses is annexed to the Master International Frequency Register (see Resolution **542 (WRC‑2000**)\*\*).     (WRC‑03)

 \*\* *Note by the Secretariat*: This Resolution was abrogated by WRC‑03. [↑](#footnote-ref-2)
3. 2 This use of the band 14.5-14.8 GHz is reserved for countries outside Europe.

*Note by the Secretariat*: Reference to an Article with the number in roman is referring to an Article in this Appendix. [↑](#footnote-ref-3)
4. 28 These provisions do not replace the procedures prescribed in Articles **9** and **11** when stations other than those for feeder links in the broadcasting-satellite service subject to a Plan are involved.     (WRC‑03) [↑](#footnote-ref-4)
5. 29 (SUP – WRC-19) [↑](#footnote-ref-5)