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QUESTION ITU-R 234-1/7
[bookmark: dtitle2]Frequency sharing between active sensor systems in the
Earth exploration-satellite service and systems operating in
other services in the 1 215-1 300 MHz band
(2000-2026)
The ITU Radiocommunication Assembly,
considering
a)	that the characteristics of Earth exploration-satellite systems (EESS)(active), frequencies and bandwidths, and performance, interference and frequency sharing criteria are given in Recommendations ITU-R RS.577, ITU-R RS.1166 and ITU-R RS.2105;
b)	that WRC-2000 allocated the frequency band 1 215-1 300 MHz to the EESS (active) on a primary basis for use by spaceborne active sensors subject to RR Nos. 5.332, 5.335 and 5.335A;
c)	that ITU-R studies show that sharing between spaceborne synthetic aperture radars and terrestrial radars is feasible except for frequency-modulated pulsed radar;
d)	that mitigation techniques may be applied to the spaceborne active sensors if required to improve sharing feasibility between spaceborne active sensors and radiolocation radar systems operating in the band 1 215-1 300 MHz,
decides that the following Questions should be studied
1	What are the possibilities and conditions for frequency sharing between spaceborne active sensor systems in the EESS and systems operating in other services in the 1 215-1 300 MHz band?
2	What are the possible interference mitigation techniques that could be used by spaceborne active sensors to facilitate sharing in the 1 215-1 300 MHz band?
further decides
1	that the results of the above studies should be included in (a) Recommendation(s);
2	that the above studies should be completed by 2031.
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