|  |
| --- |
| **Report ITU-R BS.2214-5**  **(10/2020)** |
| **Planning parameters for terrestrial digital sound broadcasting systems in VHF bands** |
| **BS Series**  **Broadcasting service (sound)** |

Foreword

The role of the Radiocommunication Sector is to ensure the rational, equitable, efficient and economical use of the radio-frequency spectrum by all radiocommunication services, including satellite services, and carry out studies without limit of frequency range on the basis of which Recommendations are adopted.

The regulatory and policy functions of the Radiocommunication Sector are performed by World and Regional Radiocommunication Conferences and Radiocommunication Assemblies supported by Study Groups.

# Policy on Intellectual Property Right (IPR)

ITU-R policy on IPR is described in the Common Patent Policy for ITU-T/ITU-R/ISO/IEC referenced in Resolution ITU‑R 1. Forms to be used for the submission of patent statements and licensing declarations by patent holders are available from <http://www.itu.int/ITU-R/go/patents/en> where the Guidelines for Implementation of the Common Patent Policy for ITU‑T/ITU‑R/ISO/IEC and the ITU-R patent information database can also be found.

|  |  |
| --- | --- |
| Series of ITU-R Reports  (Also available online at <http://www.itu.int/publ/R-REP/en>) | |
| **Series** | Title |
| **BO** | Satellite delivery |
| **BR** | Recording for production, archival and play-out; film for television |
| **BS** | Broadcasting service (sound) |
| **BT** | Broadcasting service (television) |
| **F** | Fixed service |
| **M** | Mobile, radiodetermination, amateur and related satellite services |
| **P** | Radiowave propagation |
| **RA** | Radio astronomy |
| **RS** | Remote sensing systems |
| **S** | Fixed-satellite service |
| **SA** | Space applications and meteorology |
| **SF** | Frequency sharing and coordination between fixed-satellite and fixed service systems |
| **SM** | Spectrum management |

|  |
| --- |
|  |

|  |
| --- |
| ***Note****: This ITU-R Report was approved in English by the Study Group under the procedure detailed in Resolution ITU-R 1.* |

*Electronic Publication*

Geneva, 2020

© ITU 2020

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without written permission of ITU.

REPORT ITU-R BS.2214-5

Planning parameters for terrestrial digital sound  
broadcasting systems in VHF bands

(Question ITU-R 56/6)

(2011-2015-2016-04/2019-09/2019-2020)

TABLE OF CONTENTS

Page

[Policy on Intellectual Property Right (IPR) ii](#_Toc54790051)

[1 Introduction 4](#_Toc54790052)

[2 Reception modes 4](#_Toc54790053)

[2.1 Fixed reception 4](#_Toc54790054)

[2.2 Portable reception 5](#_Toc54790055)

[2.3 Mobile reception 6](#_Toc54790056)

[3 Correction factors for field-strength predictions 6](#_Toc54790057)

[3.1 Reference frequencies 7](#_Toc54790058)

[3.2 Antenna gain 7](#_Toc54790059)

[3.3 Feeder loss 8](#_Toc54790060)

[3.4 Height loss correction factor 9](#_Toc54790061)

[3.5 Building entry loss 10](#_Toc54790062)

[3.6 Allowance for man-made noise 11](#_Toc54790063)

[3.7 Implementation loss factor 15](#_Toc54790064)

[3.8 Correction factors for location variability 15](#_Toc54790065)

[3.9 Polarization discrimination 19](#_Toc54790066)

[3.10 Calculation of minimum median field-strength level 19](#_Toc54790067)

[3.11 Calculation of minimum median field-strength level – integrated method for 100 MHz band 20](#_Toc54790068)

[4 Planning parameters for digital terrestrial broadcasting system DRM robustness mode E in VHF Bands I, II and III 24](#_Toc54790069)

[4.1 DRM system parameters 25](#_Toc54790070)

[4.2 DRM receiver parameters 27](#_Toc54790071)

[4.3 DRM planning parameters 29](#_Toc54790072)

[5 Planning parameters for digital terrestrial broadcasting system RAVIS in VHF Bands I and II 44](#_Toc54790073)

[5.1 System parameters of RAVIS 44](#_Toc54790074)

[5.2 RAVIS radio receiver related parameters 45](#_Toc54790075)

[5.3 RAVIS planning parameters 47](#_Toc54790076)

[6 Planning parameters for Digital System C (HD Radio) in VHF Band II 69](#_Toc54790077)

[6.1 HD Radio system parameters 69](#_Toc54790078)

[6.2 HD Radio receiver parameters 76](#_Toc54790079)

[6.3 HD Radio planning parameters 78](#_Toc54790080)

[7 Planning parameters for Digital System A (DAB) in VHF Band III 81](#_Toc54790081)

[7.1 System parameters of DAB 81](#_Toc54790082)

[7.2 Receiver parameters 91](#_Toc54790083)

[7.3 Additional considerations for DAB planning 92](#_Toc54790084)

[7.4 Planning parameters 98](#_Toc54790085)

[8 Planning parameters for digital terrestrial broadcasting system ISDB-TSB in VHF bands II and III 106](#_Toc54790086)

[8.1 System parameters of ISDB-TSB 106](#_Toc54790087)

[8.2 Receiver parameters 107](#_Toc54790088)

[8.3 ISDB-TSB planning parameters 107](#_Toc54790089)

[9 Planning parameters for digital terrestrial broadcasting system CDR in VHF 107](#_Toc54790090)

[9.1 System parameters of CDR 107](#_Toc54790091)

[9.2 Minimum receiver input power level 109](#_Toc54790092)

[9.3 Minimum median field-strength for planning 110](#_Toc54790093)

[Annex 1 Symbols and abbreviations 115](#_Toc54790094)

[Annex 2 Technical references 118](#_Toc54790095)

[1 Position of DRM frequencies 118](#_Toc54790096)

[1.1 VHF Band II 118](#_Toc54790097)

[1.2 VHF Band III 120](#_Toc54790098)

[2 Computations of correction factors 122](#_Toc54790099)

[2.1 Computation of the antenna gain for portable handheld reception 122](#_Toc54790100)

[2.2 Computation of man-made noise allowance from the antenna noise factor 123](#_Toc54790101)

[References 125](#_Toc54790102)

# 1 Introduction

Recommendation ITU-R BS.1114 describes the following systems for terrestrial digital sound broadcasting to vehicular, portable and fixed receivers in the frequency range 30-3 000 MHz:

– Digital System A (also known as DAB and designed for use in VHF Band III);

– Digital System F (also known as ISDB-TSB);

– Digital System G (also known as DRM+ and designed for use in VHF Bands I, II and III);

– Digital System C (also known as HD Radio and designed for use in VHF Band II);

– Digital System I (also known as RAVIS and designed for use in VHF Bands I and II); and

– Digital System H (also known as CDR and designed for use in VHF Bands II).

Recommendation ITU-R BS.1660 describes the planning criteria for terrestrial digital sound broadcasting in the VHF band, for Digital Systems A, F, G and C of Recommendation ITU-R BS.1114.

This Report defines a framework for calculating all relevant network planning parameters that are very similar for the systems and provides planning parameters for Digital Systems C, G, A, I, F and H.

Framework for evaluation of planning parameters is given in §§ 2 to 3.

Section 4 gives planning parameter for DRM+.

Section 5 gives planning parameter for RAVIS.

Section 6 gives planning parameters for HD Radio.

Section 7 gives planning parameters for DAB.

Section 8 gives planning parameters for ISDB-TSB.

Section 9 gives planning parameters for CDR.

Normative and technical references are given in Annexes 1 and 2 respectively.

To calculate the relevant planning parameters minimum median field strength and protection ratios, firstly receiver and transmitter characteristics, system parameters as well as transmission aspects as common basis for concrete digital broadcasting transmission network planning are determined. All parameters are either derived or the reference to the source of origin is given. Various typical reception scenarios are taken into account to match as much as possible planning and prediction scenarios.

# 2 Reception modes

A total of seven reception modes can be distinguished and include fixed, portable and mobile, where portable and mobile receptions are further sub-divided.

Reception availability as addressed by ITU in [[15]](#ITU_RBS412_9) and [[18]](#ITU_RP1546) considers certain percentile ranges over time and locations but does not attempt to address the practical modes or usage scenario with specific percentile or minimum requirements. Therefore, the analysis derives availability requirements from other related broadcasting areas and broadcasting technologies, and best practices, as broadly recognized.

## 2.1 Fixed reception

Fixed reception (FX) is defined as reception where a receiving antenna mounted at roof level is used. It is assumed that near-optimal reception conditions (within a relatively small volume on the roof) are found when the antenna is installed. In calculating the field-strength levels for fixed antenna reception, a receiving antenna height of 10 m above ground level is considered to be representative for the broadcasting service [1].

A location probability of 70% is assumed to obtain a good reception situation.

Fixed roof top reception is generally not considered a reception scenario for the planning of DAB networks. DAB networks in most cases are planned for portable or mobile reception and within the service area of the portable or mobile service fixed roof top reception is guaranteed. Therefore, in this Report, fixed roof top reception is not considered for the DAB system.

## 2.2 Portable reception

In general, portable reception means a reception where a portable receiver with an attached or built‑in antenna is used outdoors or indoors at no less than 1.5 m above ground level.

A location probability of 95% is assumed to obtain a good reception situation.

Two receiving locations will be distinguished:

– **Indoor reception** with a reception place in a building.

– **Outdoor reception** with a reception place outside a building.

Within these receiving locations two opposed receiving conditions will be distinguished additionally due to the great variability of portable reception situations with different receiver‑/antenna-types and also different reception conditions:

– **Portable reception**:This situation models the reception situation with good reception conditions for both situations indoor and outdoor, resp., and a receiver with an omnidirectional VHF antenna pattern as given in GE06 [1].

– **Portable handheld reception**: This situation models the reception situation with bad reception conditions and a receiver with an external antenna (for example telescopic antennas or the cable of wired headsets) as given in EBU-3317 [2].

### 2.2.1 Portable indoor reception

Portableindoor (PI) reception is defined by a portable receiver with stationary power supply and a built-in (folded)-antenna or with a plug for an external antenna. The receiver is used indoors at no less than 1.5 m above floor level in rooms on the ground floor and with a window in an external wall. It is assumed that optimal receiving conditions will be found by moving the antenna up to 0.5 m in any direction and the portable receiver is not moved during reception and large objects near the receiver are also not moved [1]. A suburban area is assumed.

### 2.2.2 Portable outdoor reception

Portable outdoor (PO) reception is defined as reception by a portable receiver with battery supply and an attached or built-in antenna which is used outdoors at no less than 1.5 m above ground level [1]. A suburban area is assumed in this case.

### 2.2.3 Portable indoor/outdoor handheld reception (PI-H, PO-H)

Portable reception is defined as reception by a portable handheld receiver with battery supply and an external antenna as given in EBU-3317 [2] for both reception situations indoor and outdoor, respectively. An urban area is assumed in this case.

## 2.3 Mobile reception

Mobile reception (MO) is defined as reception by a receiver in motion, at speeds ranging from approximately two km/h and up to 300 km/h. Speeds in the range of 50 km/h to 60 km/h are of particular interest, as they may represent urban vehicular motion. For this reception category, the antenna is considered matched and situated 1.5 m or more above ground level [1]. While not specifically addressed in [[18]](#ITU_RP1546) but yet allowed along with providing valid guidance for calculations, a reception location probability of 99% is assumed, in order to guarantee ‘good’ reception. Such choice is further supported in [[1]](#GE_06) and [[2]](#EBU_TECH_3317).

### 2.3.1 Mobile handheld reception (MO-H)

This situation corresponds to the reception scenario inside a moving vehicle at no less than 1.5 m above ground level at high speed with a handheld receiver without connection to the external antenna of the vehicle but with its own external antenna (for example, telescopic antennas or the cable of wired headsets). This reception scenario is used in DAB system, mainly because this system is developed for integrated outdoor antennas. The main difference between MO and MO-H reception modes is that in MO mode the receiver can be mounted inside the car and connected to the car antenna, while in MO-H scenario the handheld device is located inside the car but not connected to the car antenna.

In order to cover all of the indicated combinations by using as few cases as possible while providing realistic reception scenarios, only seven reception modes are analysed, as indicated in Table 1.

TABLE 1

Definition of reception modes for performance analysis

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Reception mode | FX | MO | PO | PI | PO-H | PI-H | MO-H |
| Antenna type | Fixed | Mounted | External | External | Integrated (see Note 1) | Integrated  (see Note 1) | Integrated |
| Location | Outdoor | Outdoor | Outdoor | Indoor | Outdoor | Indoor | Outdoor |
| Speed [km/h] | 0  (static) | 2-150 | 2  (walking) | 0  (quasi static) | 2  (walking) | 0  (quasi static) | 2-150 |
| Reception percentage | 70% | 99% | 95% | 95% | 95% | 95% | 99% |
| Note 1: For the DAB system in handheld reception (PO-H, PI-H) it is assumed that a built-in (folded or telescopic) antenna is used. | | | | | | | |

# 3 Correction factors for field-strength predictions

Recommendation [ITU-R P.1546](https://www.itu.int/rec/R-REC-P.1546/en) [18] forms the basis of a field-strength prediction method applicable for the broadcasting services amongst other services. Predictions can be made from 30 MHz up to 3 000 MHz within a path distance of 1 to 1 000 km, percentage of time of 1 to 50%, and for various transmitting antenna heights. The method draws a distinction between paths over land, cold seas and warm seas, makes due allowance for location variability for land area-service predictions and takes account of local clutter surrounding the receiving location. It also provides procedures for handling negative effective transmitting antenna heights and mixed-path propagation (i.e. with combinations of land and sea).

The wanted field-strength level values predicted [18] refer always to the median value at a receiving location with a receiving antenna in 10 m height above ground level. This antenna height is a generic value, used as stated only in rural or suburban areas, with constructions or vegetation below 10 m height. For the DAB system the wanted field-strength level values are provided at a receiving location with a receiving antenna at 1.5 m height above ground level. Otherwise the wanted field-strength values are predicted at the average construction or vegetation height at the receiving location. The true receiving antenna height influences the height loss correction factor (see § ‎3.4).

To take into account different receiving modes and circumstances into network planning correction factors have to be included to carry the minimum receiver input power level or the minimum field‑strength level over to the median minimum field-strength level for predictions [18].

## 3.1 Reference frequencies

The planning parameters and correction factors in this Report are calculated for the reference frequencies given in Table 2.

TABLE 2

Reference frequencies for calculations

|  |  |  |  |
| --- | --- | --- | --- |
| VHF band (frequency range) | I (47-68 MHz) | II (87.5-108 MHz) | III (174-230 MHz) |
| Reference frequency (MHz) | 65 | 100 | 200 |

## 3.2 Antenna gain

The antenna gain *GD* (dBd) references to a half-wave dipole.

### 3.2.1 Antenna gain for fixed reception

In Recommendation ITU-R BS.599 [25] and GE06 [1], the antenna pattern for fixed reception are given for both VHF Band II (4 dB) and VHF Band III (7 dB). In ETSI-DVB [3] the antenna pattern for fixed reception is given for VHF Band I (3 dB).

Taking into account the current use of roof-top antenna systems with omnidirectional dipole antennas or ground plane antennas for future planning it is recommended that an omnidirectional antenna pattern with a gain of 0 dBd is used (see Table 3).

TABLE 3

Antenna gain *GD* for fixed reception

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Antenna gain *GD* (dBd) | 0 | 0 | 0 |

### 3.2.2 Antenna gain for portable reception

GE06 [1] assumes an omnidirectional VHF antenna pattern with an antenna gain of −2.2 dBd for standard portable receiver planning. From this reference, the antenna gains *GD* for portable reception are assumed to −2.2 dBd as given in Table 4.

TABLE 4

Antenna gain *GD* for portable reception (1)

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Antenna gain *GD* (dBd) | −2.2 | −2.2 | −2.2 |
| (1) The antenna gain values for DAB portable reception (PI, PO) is assumed –8 dBd – –10 dBd (further information can be found in EBU Report Tech 3391 [45]). | | | |

### 3.2.3 Antenna gain for portable and mobile handheld reception

Antenna gains *GD* for portable and mobile handheld reception in VHF Band III (200 MHz) are given by EBU‑3317 [2]:

– Receiver integrated antenna: *GD* = −17 dBd

– External antenna (telescopic or wired headsets): *GD =*−13 dBd

– Adapted antenna (for mobile reception): *GD* = −2.2 dBd

The antenna gain for portable and mobile handheld reception in VHF Band I and VHF Band II can be calculated by the computation given in Annex 2 [4]. From it the antenna gains *GD* (dB) for portable handheld reception modes with an external antenna are given in Table 5.

TABLE 5

Antenna gains *GD* for portable and mobile handheld reception

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Gain variation Δ*G* referenced to 200 MHz (dB) | −9.76 | −6.02 | 0.00 |
| Antenna gain *GD* for receiver integrated antenna (dBd) | −26.76 | −23.02 | −17.00 |
| Antenna gain *GD* for portable handheld reception (external antenna, telescopic or wired headsets) (dBd) | −22.76 | −19.02 | −13.00 |

### 3.2.4 Antenna gain for mobile reception

For mobile reception an omnidirectional VHF antenna pattern with an antenna gain *GD* of −2.2 dBd [1] is assumed, see Table 6.

TABLE 6

Antenna gains *GD* for mobile reception (1)

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Antenna gain *GD* for adapted antenna (mobile reception) (dBd) | −2.2 | −2.2 | −2.2 |
| (1) The antenna gain values for DAB mobile reception (MO) is assumed ‑5 dBd – ‑10 dBd (further information can be found in EBU Report Tech 3391 [45]). | | | |

## 3.3 Feeder loss

The feeder loss *Lf* expresses the signal attenuation from the receiving antenna to the receiver’s RF input. The feeder loss *Lf* for fixed reception at 200 MHz is given in GE06 [1] with 2 dB for 10 m cable length. The frequency dependent cable attenuation per unit length *L′f* is assumed to be equal to:

 (1)

with *f* the frequency (MHz). The feeder loss values per unit length *L′f* are given in Table 7.

TABLE 7

Feeder loss *L′f* per unit length

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Feeder loss *L*′*f* (dB/m) | 0.11 | 0.14 | 0.2 |

The feeder loss *Lf* is given by:

 (2)

with *l* the length of the feeder cable (m).

The cable length *l* for the different reception modes are given in Table 8, and the feeder losses *Lf*for different frequencies and reception modes are given in Table 9.

TABLE 8

Cable length *l* for reception modes

|  |  |  |  |
| --- | --- | --- | --- |
| Reception mode | Fixed reception  (FX) | Portable and mobile  handheld reception  (PO, PI, PO-H, PI-H, MO-H) | Mobile reception  (MO) |
| Cable length *l* (m) | 10 | 0 | 2 |

TABLE 9

Feeder loss *Lf* for different reception modes (1)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency (MHz) | | 65 | 100 | 200 |
| Feeder loss *Lf* | for fixed reception (FX) (dB) | 1.1 | 1.4 | 2.0 |
|  | for portable and mobile handheld reception (PO, PI, PO-H, PI-H, MO-H) (dB) | 0.0 | 0.0 | 0.0 |
|  | for mobile reception (MO) (dB) | 0.22 | 0.28 | 0.4 |
| (1) For the DAB system a feeder loss of 0 dB has been assumed for all reception modes. | | | | |

## 3.4 Height loss correction factor

For portable reception a receiving antenna height of 1.5 m above ground level (outdoor and mobile) or above floor level (indoor) is assumed. The propagation prediction method usually provides field‑strength values at 10 m. To correct the predicted value from 10 m to 1.5 m above ground level a height loss factor *Lh* (dB) has to be applied.

The height loss correction factor *Lh* for an antenna height of 1.5 m is given in GE06 [1] as follows:

*Lh =*12 dB at 200 MHz

*Lh* = 16 dB at 500 MHz

*Lh* = 18 dB at 800 MHz

Therefore, the height loss correction factor *Lh* (dB) at 100 MHz is assumed to 10 dB, and at 65 MHz to 8 dB, for portable and mobile reception modes The height loss correction factor *Lh* for handheld reception with external antenna is given in EBU-3317 [2] for VHF Band III as 19 dB in urban areas and is assumed to 17 dB at 100 MHz and to 15 dB at 65 MHz.

The height loss correction factor *Lh* for different reception modes is given in Table 10.

TABLE 10

Height loss correction factor *Lh* for different reception modes (1)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency (MHz) | | 65 | 100 | 200 |
| Height loss correction factor *Lh* | for fixed reception (FX) (dB) | 0 | 0 | 0 |
| for portable and mobile reception (PO, PI, MO) (dB) | 8 | 10 | 12 |
| for portable handheld reception (PO-H, PI-H) (dB) | 15 | 17 | 19 |
| (1) For the DAB system the height loss is provided for different environment classes and typical clutter heights, see § 7.3.1. | | | | |

## 3.5 Building entry loss

Traditionally the loss associated with the RF signal entering a building or vehicle was referred to as the ‘penetration’ loss [44]. In the latest ITU Recommendation on this subject [42], the term ‘entry’ has replaced ‘penetration’.

The ratio between the mean field strength inside a building at a given height above ground level and the mean field strength outside the same building at the same height above ground level expressed in (dB) is the mean building entry loss (BEL).

Historically, the mean building entry loss *Lb* in VHF Band III was given in GE06 [1] and EBU-3317 [2] as 9 dB, which was proposed to be used for VHF Band II, too. The mean building entry loss for VHF Band I was given in ETSI-DVB [3] as 8 dB. The standard deviation of the building entry loss σ*b* was always given by 3 dB.

Recently, the topic of building entry loss has been revisited and ITU has issued two documents: Report ITU-R P.2346 [43] and Recommendation ITU-R P.2109 [42].

A major finding of recent investigations is the observation that a principal distinction is to be made between buildings equipped with metalized windows and other measures to provide thermal efficiency and those which are not.

In accordance with Recommendation ITU-R P.2109 [42], the mean building entry loss *Lb* and the standard deviation σ*b* are calculated as follow:

*Lb* = *Lh*+ *Le*

σ*b* = 𝑢 + 𝑣 log(𝑓)

where:

*Lh:* median loss for horizontal paths, given by:

𝐿ℎ = 𝑟 + 𝑠 log(𝑓) + 𝑡 (log(𝑓))2

*Le:* correction for elevation angle of the path at the building faсade:

𝐿𝑒 = 0.212 |θ|

and:

*f* : frequency (GHz)

θ : elevation angle of the path at the building faсade (degrees),

and the coefficients *r*, *s*, *t*, *u* and *v*, depending on the building type, listed in Table 11.

TABLE 11

Coefficients for the calculation of building entry loss

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Building type | *r* | *s* | *t* | *u* | *v* |
| Traditional | 12.64 | 3.72 | 0.96 | 9.6 | 2.0 |
| Thermally-efficient | 28.19 | −3.00 | 8.48 | 13.5 | 3.8 |

In § 7.3.2.1 there is an example of the calculation of building entry loss where *f* = 0.2 GHz.

## 3.6 Allowance for man-made noise

The allowance for man-made noise (MMN) (dB), takes into account the effect of the MMN received by the antenna on the system performance. The system equivalent noise figure *Fs* (dB) to be used for coverage calculations is calculated from the receiver noise figure *Fr* (dB) and MMN (dB) (for details see Annex 2, § 2.2):

 (3)

The allowance for man-made noise is calculated from an antenna noise factor *fa*, which takes into account the man-made noise received by the antenna:

 (4)

where:

*fr* : the receiver noise factor:

 (5)

*fa* : the antenna noise factor:

 (6)

where:

*Fa* : antenna noise figure.

### 3.6.1 Allowance for man-made noise for fixed, portable and mobile reception

Recommendation ITU-R P.372 [26] gives the legal values to calculate the allowance of man-man noise in different areas and frequencies with the definitions of the antenna noise figure, its mean values *Fa,med* and the values of decile variations (10% and 90%) measured in different regions as a function of the frequency. The equation to calculate the antenna noise figure is given in [26] by:

 (7)

For all reception modes the residential area (Curve B in [26]) is assumed. In this case the values for the variables *c* and *d* are given by:

*c =*72.5                *d =*27.7

Herewith the values of the medium antenna noise figure *Fa,med* (dB) can be computed. The results are shown in Table 12.

TABLE 12

Medium antenna noise figure *Fa,med*

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Medium antenna noise figure *Fa,med* for residential area (curve B) (dB) | 22.28 | 17.10 (1) | 8.76 |
| (1) For HD Radio *Fa*value is equal to 21 dB. | | | |

Herewith the MMN (dB), taking into account a receiver noise figure *Fr* of 7 dB, can be computed. The results are shown in Table 13.

TABLE 13

Allowance for man-made noise (MMN) for fixed, portable and mobile reception

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Allowance for man-made noise for fixed, portable and mobile reception (*Fr*= 7 dB) (dB)(1) | 15.38 | 10.43 (2) | 3.62 |
| (1) For DAB a *Fr* of6 dB needs to be used.  (2) For HD Radio *Fa*value is equal to 21 dB, which results in the MMN value of 14.1 dB. | | | |

However, the listed results are based on measurements taken in 1974, under completely different RF environments and different antenna system implementation approaches. More recent studies (2001‑2003) by OFCOM, as indicated in [[27]](#AY3952) and [[28]](#AY4119), and by others in [[29]](#Rantakko) show that the realistic noise may be substantially higher. For example, for the purpose of calculating MMN allowance, a reference Fa value of 21 dB (equivalent to a noise temperature of approximately 360 000 K) for 100 MHz is derived from OFCOM [[28]](#AY4119) and corresponds to a ‘quiet’ rural environment. The measurements for that environment resulted in the lowest standard deviation and may be considered the most repetitive. The use of that higher and much more realistic value has been extended to reception modes. A similar approach of adjusting the man-made noise allowance for cases with noticeable antenna losses (i.e. high integrated NF) is used in [[2]](#EBU_TECH_3317) and shows the result of 14.1 dB for the 100 MHz system with antenna gain higher than −2.2 dBd.

The IRT carried out indoor-measurements of man-made noise in 2005 [32]. SRG carried out indoor measurements of man-made noise in 2017 according to [33]. From these measurements, the extrapolated value of *Fam* for 200 MHz is shown in the last three lines of Table 14*.* The values of IRT and SRG are considerably higher than the values given in [26]. The ITU values were measured many years ago outside buildings when there were few PCs, no DSL-connections and no widespread mobile and WLAN telecommunication systems as found nowadays and which contribute significantly to man-made noise level. Today, especially in buildings, and in proximity to many noise sources, the antenna external noise figure *Fam* can have higher values than the values measured many years ago outside buildings.

TABLE 14

*Fa,med* and *Pmmn* values in dB for 0 dBi antenna gain for 200 MHz band and different areas

|  |  |  |
| --- | --- | --- |
| Values for 200 MHz | *Fa,med*  (dB) | *Pmmn*  (dB) |
| ITU Rural | 3.5 | 1.6 |
| ITU Residential/suburban | 8.8 | 4.0 |
| ITU City (Business)/urban | 13.1 | 7.0 |
| IRT Urban indoor [32] 2005 | 16.5 | 10.0 |
| SRG Urban indoor 2017 @ 3 m [33] | 21.1 | 14.3 |
| SRG Urban indoor 2017 @ 1 m [33] | 30.6 | 23.6 |

Antenna gain values for in‑home and in‑car receivers are generally much less than 0 dBi (−2.2 dBd) [44]. The negative antenna gains can be traced back to a lack of efficiency caused by mismatches between antenna and receiver, and between antenna and the received signal, often due to antenna size relative to the wanted signal wavelength. Therefore, the man‑made noise received by the antenna is attenuated as is the wanted signal. Consequently, a negative antenna gain induces a modification of the man‑made noise allowance value. Based upon the values in Table 14 the value of *Pmmn* for planning can be calculated for different antenna gains. Calculations are based upon [56][[1]](#footnote-1).

The results are presented in Table 15. The calculations are based on the *Fam* values in Table 14 for different values of the antenna gain.

TABLE 15

*Pmmn* in dB as function of antenna gain (*Fr* = 6 dB, *f* = 200 MHz)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Antenna gain (dBd) | −2.2 | −5 | −8 | −10 | −13 | −17 |
| ITU Rural | 1.6 | 0.9 | **0.5** | 0.3 | 0.2 | 0.1 |
| ITU Residential/suburban | 4.0 | 2.5 | **1.5** | 1.0 | 0.5 | 0.2 |
| ITU City (Business)/urban | 7.0 | 5.0 | **3.2** | 2.2 | 1.3 | 0.5 |
| IRT Urban indoor [EBU\_9] 2005 [32] | 10.0 | 7.6 | **5.3** | 4.0 | 2.4 | 1.1 |
| SRG urban indoor 2017 @3 m to interferer[33] | 14.3 | 11.6 | **8.9** | 7.2 | 5.0 | 2.7 |
| SRG Urban Indoor 2017 @1 m to interferer [33] | 23.6 | 20.9 | **17.9** | 15.9 | 13.0 | 9.4 |

Field strength targets are usually focused on vehicles in rural areas and table top radios for in‑building reception in suburban and urban grade areas. For a typical antenna gain value for planning of *Ga* = −8 dBd the resulting MMN adjustment value *Pmmn* to be used in coverage field strength planning is highlighted in Table 15.

Whilst witnessing an increase in man‑made noise, further increases can be expected as new electronic devices, in particular LED lights, are introduced. As a consequence of these ongoing changes, levels of MMN need to be monitored; studies and measurements of MMN should continue.

Recommendation ITU-R P.372 [26] gives the value of decile location variations (10% and 90%) in residential area by 5.8 dB. For 90% location probability the distribution factor μ = 1.28. Therefore, the standard deviation of MMN for fixed, portable and mobile reception σ*MMN* = 4.53 dB, see Table 16.

TABLE 16

Standard deviation of MMN σ*MMN*for fixed, portable and mobile reception

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Standard deviation of MMN σ*MMN* (dB) | 4.53 | 4.53 | 4.53 |

The standard deviation of MMN has to be considered in the calculation of the combined standard deviation for the wanted field-strength level (see § 3.8.2).

### 3.6.2 Allowance for man-made noise for portable handheld reception

The antenna gain is the product of directivity and efficiency. The lowest realistic directivity is the one of a short dipole (length l << λ) and it has the value 1.5 (1.8 dBi). Any gain lower than 1.8 dBi (−0.4 dBd) is due to an antenna efficiency η lower than 1. The interference power at the receiver input is reduced accordingly and the MMN equation is (see Annex 2, § 2.2):

 (8)

The efficiency η can be calculated from the antenna gain *GD* (dB) for gains lower than −0.4 dBd:

 (9)

The MMN for portable handheld reception, taking the receiver noise figure as 7 dB, are given in Table 17.

TABLE 17

Allowance for man-made noise for portable handheld reception (external antenna)

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Handheld antenna gain *GD* (dBd) | −22.8 | −19 | −13 |
| Efficiency η | 0.0058 | 0.0138 | 0.055 |
| Calculated MMN allowance (dB) | 0.42 | 0.30 | 0.14 |
| **Allowance for man-made noise for portable handheld reception (dB)** | **0.0** | **0.0** | **0.0 (1)** |
| (1) For DAB the allowance for man-made noise for portable handheld reception (dB) for an antenna gain of −13 dB is provided in Table 15. | | | |

In the further calculations the allowance for man-made noise is specified to 0 dB due to the very low calculated values.

## 3.7 Implementation loss factor

Implementation loss, as indicated in this document, reflects the correction factor to the minimum input power in order to compensate for the non-ideal receiver. Choosing such a factor may be subjective. For receivers that are internally spacious (i.e. reception circuitry not significantly limited by device size) and non-power-restricted (i.e. have constant or frequent access to durable power source), it is often considered to be 3 dB.

Advanced and highly integrated small receivers, such as handheld devices and particularly inclusion in smart phones, may experience additional higher implementation losses. Such losses may be due to the small physical dimensions, limited battery capacity, and co-existence with several additional hardware and radio wave-based functions. Therefore, the implementation loss, *Lim*, for such receivers are considered to be 5 dB. The implementation losses per reception mode are provided in Table 18.

TABLE 18

Implementation loss factor *Li* for different reception modes (1)

|  |  |  |
| --- | --- | --- |
|  | FX, MO, PO, PI | PO-H, PI-H |
| Implementation loss, *Li* (dB) | 3 | 5 |
| (1) For the DAB system, no implementation loss factor is considered. | | |

## 3.8 Correction factors for location variability

The random variation of the received signal field strength with location due to terrain irregularities and the effect of obstacles in the near vicinity of the receiver location is modelled by a statistical distribution (typically log normal) over a specified macro-scale area (typically a square with edge lengths of 100 m to 500 m). Considering the received signal field-strength level *E* (dB(μV/m)), the lognormal distribution is transformed in a Gaussian distribution with mean (and median) *Emed* (dB) and standard deviation σ (dB).

The field-strength level *E*(*p*)(dB(μV/m)), used for coverage and interference predictions in the different reception modes, which will be exceeded for *p*(%) of locations for a land receiving/mobile antenna location, is given by:

 for 50% ≤ *p* ≤ 99% (10)

with:

*C*1(*p*) (dB) : location correction factor

*Emed* (dB(μV/m) : field-strength value for 50% of locations and 50% of time.

The location correction factor *C*l(*p*) (dB) depends on the so called combined standard deviation σ*c* (dB) of the wanted field-strength level that sums the single standard deviations of all relevant signal parts that have to be taken into account and the so-called distribution factor μ(*p*), namely:

 (11)

with:

: distribution factor and  (standard normal Gaussian CDF)

σ*C* : combined standard deviation of the wanted field-strength level (dB).

### 3.8.1 Distribution factor

The distribution factors μ(*p*) of the different location probabilities taking into account the different receiving modes (see § 2) are given in Table 19.

TABLE 19

Distribution factor μ

|  |  |  |  |
| --- | --- | --- | --- |
| Percentage of receiving locations p (%) | 70 | 95 | 99 |
| Reception mode | fixed | portable | mobile |
| Distribution factor μ | 0.524 | 1.645 | 2.326 |

### 3.8.2 Combined standard deviation

The combined standard deviation σ*c* (dB) takes into account the standard deviation of the wanted field-strength level σ*m* (dB), the standard deviation of the MMNσ*MMN* (dB), and, in the case of indoor reception, the standard deviation of the building entry loss, σ*b*(dB), respectively.

Since the statistics of the received wanted field-strength level for macro-scale, the statistics of the MMNσ*MMN* (dB), and the statistics of the building attenuation can be assumed to be statistically uncorrelated, the combined standard deviation σ*c* (dB) is calculated by:

 (12)

The values of the standard deviations of the building entry loss σ*b*(dB) and of the MMNσ*MMN* (dB) are given in §§ 3.5 and ‎3.6, respectively.

The values of standard deviation σ*m* (dB) of the wanted field-strength level *E* are dependent on frequency and environment, and empirical studies have shown a considerable spread. Representative values for areas of 500 m × 500 m are given by Recommendation ITU-R P.1546 as well as the expression to calculate the standard deviation σ*m* (dB):

 (13)

where:

*K* = 1.2, for receivers with antennas below clutter height in urban or suburban environments for mobile systems with omnidirectional antennas at car-roof height

*K*  1.0, for receivers with rooftop antennas near the clutter height

*K*  0.5, for receivers in rural areas

*f*: required frequency (MHz).

The standard deviations σ*m* (dB) for DRM, RAVIS and HD Radio in urban and suburban areas as well as in rural areas are given in Table 20.

TABLE 20

Standard deviation for DRM, HD Radio and RAVIS σ*m* (1)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency (MHz) | | 65 | 100 | 200 |
| Standard deviation for DRM, RAVIS and HD Radio σ*m* | in urban and suburban areas (dB) | 3.56 | 3.80 | 4.19 |
| in rural areas (dB) | 2.86 | 3.10 | 3.49 |
| (1)For the DAB system σ*m* is equal to 4.0 dB. | | | | |

These values of the standard deviation take into account only the effects of slow fading, but not the effects of fast fading. Therefore it must be ensured that the determination of the minimum *C*/*N* value consider the effects of the fast fading. Otherwise a margin depending to the bandwidth of the signal of 1.6 dB at 8 MHz, 2.3 dB at 1.5 MHz and 4.6 dB at 120 kHz has to be added.

For DRM and RAVIS the effects of fast fading are included into the measurement method and therefore they do not have to be added.

For the different reception modes more or less parts of the given particular standard deviations have to be taken into account, see Table 21.

Due to these differences the combined standard deviation σ*c* (dB) for the respective reception modes are given in Table 22.

TABLE 21

Allowance for the particular standard deviations for the different reception modes

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Particular standard deviations | | σ*m* | σ*m* | σ*m* | σ*MMN* | σ*b* |
| Frequency (MHz) | | 65 | 100 | 200 | all | all |
| Reception modes | fixed (FX) and portable outdoor (PO) (dB) | 3.56 | 3.80 | 4.19 | 4.53 | 0.00 |
| portable handheld outdoor (PO‑H) (dB) | 3.56 | 3.80 | 4.19 | 0.00 | 0.00 |
| mobile (MO) (dB) | 2.86 | 3.10 | 3.49 | 4.53 | 0.00 |
| portable indoor (PI) (dB) | 3.56 | 3.80 | 4.19 | 4.53 | 3.00 |
| portable handheld indoor (PI-H) (dB) | 3.56 | 3.80 | 4.19 | 0.00 | 3.00 |
| mobile handheld (MO-H) | n/a | n/a | 4.19 | 0.00 | 2.00 |

TABLE 22

Combined standard deviation σ*c* for the different reception modes (1)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency (MHz) | | 65 | 100 | 200 |
| Combined standard deviation σ*c*for reception mode | fixed (FX) and portable outdoor (PO) (dB) | 5.76 | 5.91 | 6.17 |
| portable handheld outdoor (PO-H) (dB) | 3.56 | 3.80 | 4.19 |
| mobile (MO) (dB) | 5.36 | 5.49 | 5.72 |
| portable indoor (PI) (dB) | 6.49 | 6.63 | 6.86 |
| portable handheld indoor (PI‑H) (dB) | 4.65 | 4.84 | 5.15 |
| mobile handheld (MO-H) | n/a | n/a | 4.64 |
| (1)For the DAB system the combined standard deviation and location correction factor for different reception modes and service qualities, see § 7.3.3. | | | | |

### 3.8.3 Combined location correction factor for protection ratios

The needed protection of a wanted signal against an interfering signal is given as the basic protection ratio *PRbasic* (dB) for 50% of location probability.

In the case of higher location probability as given for all reception modes a so called combined location correction factor *CF* (dB) is used as a margin that has to be added to the basic protection ratio *PRbasic*, valid for the wanted field-strength level and the nuisance field-strength level, to the protection ratio *PR*(*p*) corresponding to the needed percentage *p* (%) of locations for the wanted service [1].

 for 50% ≤ *p* ≤ 99% (14)

with:

 (15)

where σ*w* and σ*n*, both in (dB), denote the standard deviation of location variation for the wanted signal for the nuisance signal, respectively. The values for σ*w* and σ*n*are given in § 3.8.2 for the different broadcasting systems as σ*m*.

## 3.9 Polarization discrimination

In principal it is possible to take advantage of polarization discrimination for fixed reception. GE84 [5] does not take into account polarization discrimination in the planning procedure for VHF Band II, except in specific cases with the agreement of administrations concerned. In such cases, a value of 10 dB was used for orthogonal polarization discrimination.

GE06 [1] gives that in VHF Band III polarization discrimination shall not be taken into account in the DAB planning procedures.

For the planning procedures of digital sound broadcasting systems in the VHF bands no polarization discrimination will be taken into account for all reception modes.

## 3.10 Calculation of minimum median field-strength level

The calculation of the minimum median field-strength level at 10 m above ground level for 50% of time and for 50% of locations is given in GE06 [1] by the following steps (for the DAB system as described in § 7, the minimum median field-strength levels are calculated at 1.5 m above ground level):

*Step 1*:Determine the receiver noise input power level *Pn*:

 (16)

where:

*F* : receiver noise figure (dB)

*k* : Boltzmann’s constant, *k* = 1.38 10−23 (J/K)

*T*0 : absolute temperature (K)

*B* : receiver noise bandwidth (Hz).

*Step 2*:Determine the minimum receiver input power level *Ps,min*:

 (17)

where:

(*C*/*N*)*min* : minimum carrier-to-noise ratio at the digital broadcasting decoder input (dB).

*Step 3*: Determine the minimum power flux-density (i.e. the magnitude of the Poynting vector) at receiving place ϕ*min*:

 (18)

where:

*Lf* : feeder loss (dB)

*Aa* : effective antenna aperture (dBm2).

 (19)

*Step* *4*: Determine the minimum RMS field-strength level at the location of the receiving antenna *Emin*:

 (20)

with:

 , the characteristic impedance in free space (21)

resulting in:

 (22)

*Step 5*: Determine the minimum median RMS field-strength level *Emed*:

For the different receiving scenarios the minimum median RMS field strength is calculated as follows:

– for fixed reception:

*Emed* = *Emin* + *Pmmn* + *Cl*(23)

– for portable outdoor and mobile reception:

*Emed* = *Emin* + *Pmmn* + *Cl* + *Lh*(24)

– for portable indoor reception:

*Emed* = *Emin* + *Pmmn* + *Cl* + *Lh* + *Lb*(25)

## 3.11 Calculation of minimum median field-strength level – integrated method for 100 MHz band

For the purpose of sensitivity calculations, antennas are often represented by gains, and then attached to receivers with separately calculated noise figure. Several legacy design and analysis approaches, as well as certain measurements, refer to the entire gain by a single factor. Then, only the low noise amplifier (LNA) noise figure (referred to as receiver noise figure) is applied to the overall gain and noise calculations. However, an antenna gain consists of fixed physical structure gain, which can be calculated, and additional gain (typically attenuation) component that depends on attached circuitry. While the physical positive gain higher than 0 dBi (−2.2 dBd) corresponds to radiation patterns, negative gains are related to impaired antenna efficiency, which is caused typically by mismatch between the antenna and the receiver, as described in [[2]](#EBU_TECH_3317).

Advanced receiver implementation techniques, may employ dynamically adjustable circuitry that may improve the matching of the receiver input network, including the LNA. Therefore, for such implementations it may be useful to calculate the combined receiver system noise figure, as resulting from the receiver input network, while separating it from the physical antenna gain. Then, a reference physical antenna gain (typically the lowest realistic gain) is used, and any further antenna attenuation is expressed by a combined noise figure. When a higher physical antenna gain is available, it may then be used to adjust the calculations, without affecting the combined noise figure calculations.

The effect of the matching circuitry on the overall noise, or otherwise on the integrated antenna gain is described further. Required adjustments for the physical antenna gain are further described in this section.

Antenna gain adjustment

The sensitivity (required field strength) based on the overall receiver system NF, already assumed antenna gain of 1.5 (‘net physical’ isotropic element of 1.8 dBi / −0.4 dBd, separate of matching loss), as indicated further. Therefore, antenna gain correction factor Δ*AG* is applied where the physical element is different (noticeably larger). For fixed reception, an antenna gain of 4 dBd is used, as recommended in [[26]](#ITU_RP372). In all other reception modes, no physical antenna gains are available, and therefore are assumed to have no gain over the reference antenna.

The applicable antenna gain correction for all reception modes is provided in Table 23.

TABLE 23

Antenna physical gain correction

|  |  |  |
| --- | --- | --- |
|  | FX | MO, PO, PI, PO-H, PI-H |
| Antenna gain correction. Δ*AG* (dB) | 4.4 | 0 |

Background for calculating the reference minimum field strength

Receiver sensitivity, being the minimum required signal field strength at the receiver antenna (*E*) is expressed as a function of the required pre-detection *C*/*N*0, the noise, the effective length he of the antenna (*he* is a function of radiation resistance), and the antenna matching circuit *Ha*(*f*). For a given signal field strength *E* (µV/m) impinging upon the antenna, *C*/*N*0 is expressed as a function of the field strength, the antenna effective length *he*(*f*), the transfer function of the antenna circuit (matched) filter *Ha*(*f*), and the sum of noise sources comprising *N*0.

NOTE – The expression is provided for the lowest realistic directivity antenna, which is the one of a short dipole (length, l << λ) and it has the gain value of 1.5 (1.76 dBi; −0.4 dBd). Any gain higher than −0.4 dBd has to be separately applied to the link budget calculations. Any gain lower than −0.4 dBd is assumed to result from reduced efficiency that is caused by a mismatched network, and is already included in the calculations, as provided in this section.

The signal power *C* (*V*2) applied to the LNA input is given by:

 (26)

The noise power spectral density (PSD) at the LNA input (for a conjugately matched antenna) as a function of the ambient noise and the LNA noise figure (NFLNA) is given by:

 (27)

For reference temperature (*T*0) discussion, *Tamb* = *T*0 is assumed. In addition, the LNA input is frequency dependent and may not be conjugately matched to the antenna. The combined noise PSD is given by:

 (28)

where *Zin* is the input impedance seen at the LNA input, including the LNA input impedance, and NFLNA is the noise figure of the LNA. The receiver system NF is the ratio (in dB) of the overall noise to the noise produced by the antenna’s radiation resistance:

 (29)

or equivalently:

 (30)

*C*/*N*0 at the output of the LNA is given by:

 (31)

This is expressed in dB as:

 (32)

or equivalently:

 (33)

Then the required field strength *E* (dBu) as a function of the required CNR:

 (34)

Using the antenna’s effective length *he* as related to its radiation resistance *Ra* is given by:

 (35)

where , , and *G* = 1.5 (1.8 dBi; −0.4 dBd) is the constant directivity for small antennas (*he* << λ):

 (36)

Then the required field strength, as a function of λ and receiver system *NF* is given by:

 (37)

Determining the minimum required field strength

For each system configuration and for each reception mode, the applicable *CNR* and the applicable *NF* where:

*NF* receiver system integrated noise figure (dB)

*C*/*N*0 carrier-to-noise density ratio (dB-Hz).

The following relationship may be used for convenience:

 (38)

where *BWn* is the receiver noise bandwidth (ideally the signal bandwidth).

When using λ = 3 m for 100 MHz, the minimum required field strength *Er* is given by:

 (39)

Physical antenna gain adjustment

Since the reference calculation in equation (39) is using the minimum realistic gain, of −0.4 dBd, then the difference should be calculated for any other higher indicated physical gain as follows:

Δ*AG* [dB] = *Ag* [dB] + 0.4 (40)

where Δ*AG* is antenna gain correction in dB.

Determining the minimum median required field strength

The minimum median field strength is calculated as follows:

*Emed* = *Er* + *MMN* − Δ*AG* + *Lrl* + *Li* (41)

or otherwise:

*Emed* = *C/N*0 – 58.5 + *NF* + *MMN* – Δ*AG* + *Lrl* + *Li*(42)

where:

*Lrl =* µ*∙*σ*m + Lh + Lf + Lb*: reception location loss (dB);

*Li* : implementation loss (dB).

MMN is man-made noise allowance, calculated according to the recommended method in [[12]](#GOSTR55688), but based on integrated *NF* rather than on antenna gain.

IBOC conversion of *C*/*N*0 to *S*/*N*

The carrier-to-noise ratio, often written *CNR* or *C*/*N*, is the signal-to-noise ratio (*S*/*N*) of a modulated signal. The noise power *N* is typically defined in the signal’s processing (reception) bandwidth.

The carrier-to-noise-density ratio (*C*/*N*0) is similar to carrier-to-noise ratio, except that the noise *N*0 is defined per unit Hz bandwidth.

For analysis, the digital modulation power of the signal *Cd* is often distinguished from the total signal power *C*. This is used in, for example, an FM Hybrid IBOC signal where the digital-only power *Cd* is distinguished from the FM analogue power *C*.

IBOC FM conversion of *Cd*/*N*0 to digital *C*/*N* or *S*/*N* example

For a single 70-kHz digital signal bandwidth system configuration:

 (43)

then:

 (44)

# 4 Planning parameters for digital terrestrial broadcasting system DRM robustness mode E in VHF Bands I, II and III

Digital Radio MondialeTM (DRM) was originally designed by the DRM Consortium as a digital broadcasting system for the radio bands below 30 MHz and it is standardized as ETSI ES 201 980 [6]. In 2009, DRM was extended by a mode E – called “DRM+” – to use DRM in radio bands up to 174 MHz.

The University of Applied Sciences in Kaiserslautern[[2]](#footnote-2) (Germany) and the University of Hannover[[3]](#footnote-3) (Germany) successfully conducted laboratory measurements and field trials with DRM in VHF Band II and in VHF Band III, respectively. Demonstrations were also given successfully in Paris in VHF Band I by the University of Applied Sciences in Kaiserslautern. Other field trials all over the world, especially in Brazil, Italy, Sri Lanka, the United Kingdom and in the Republic of Korea, have completed the tests.

The measurements and field trials have confirmed the technical parameters, and comparisons of coverage area have been performed between FM in VHF Band II and DRM also as with DAB in VHF Band III and DRM. In addition, protection ratio measurements have been performed and planning models have been used to predict coverage. The results from both German sites show that DRM works well in all VHF bands including VHF Band III.

From these results and based on relevant ITU Recommendations, this Report defines a framework for calculating all relevant DRM network planning parameters in all VHF bands. The focus lies on VHF Band II (87.5-108 MHz) and VHF Band III (174-230 MHz) in ITU Region 1, however where the values for the VHF Band I (47-68 MHz) are available, they are given.

Other frequency allocations in VHF bands assigned to broadcasting services are not exhaustively covered yet, e.g. areas in ITU Region 1 where allocations of the Wiesbaden T-DAB Agreement 1995 are still used (230-240 MHz) or in some Southern African countries, where the VHF Band III is allocated to the broadcasting services up to 254 MHz, or the broadcasting bands in ITU Regions 2 and 3, perhaps the OIRT FM band (65.8-74 MHz) or the Japanese FM band (76‑90 MHz), respectively, that can later be adapted. Planning parameters for these unconsidered cases can be derived or taken from the given values, considering 254 MHz as the international top boundary of the VHF broadcasting spectrum[[4]](#footnote-4).

## 4.1 DRM system parameters

The description of the DRM system parameters refers to Mode E of the DRM system [6].

### 4.1.1 Modes and code rates

#### 4.1.1.1 Overview of SDC and MSC code rates

ETSI-DRM [6] defines the SDC code rates summarized in Table 24 and the MSC modes with code rates *R* given in Table 25.

TABLE 24

SDC code rates

|  |  |  |  |
| --- | --- | --- | --- |
| MSC-mode 11  (4-QAM) | | MSC-mode 00  (16-QAM) | |
| SDC-mode | Code rate *R* | SDC-mode | Code rate *R* |
| 0 | 0.5 | 0 | 0.5 |
| 1 | 0.25 | 1 | 0.25 |

TABLE 25

MSC code rates

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Protection level | Code rate R for  MSC mode 11: 4-QAM | | Code rate R combinations for  MSC mode 00: 16-QAM | | | |
| *Rall* | *R*0 | *Rall* | *R*0 | *R*1 | *RYlcm* |
| 0 | 0.25 | 1/4 | 0.33 | 1/6 | 1/2 | 6 |
| 1 | 0.33 | 1/3 | 0.41 | 1/4 | 4/7 | 28 |
| 2 | 0.4 | 2/5 | 0.5 | 1/3 | 2/3 | 3 |
| 3 | 0.5 | 1/2 | 0.62 | 1/2 | 3/4 | 4 |

The net bit rate of the MSC varies from 37 kbit/s to 186 kbit/s depending of the used parameter set.

#### 4.1.1.2 SDC and MSC code rates for calculations

Several of the derived parameters depend on the characteristic of the transmitted DRM signal. To limit the amount of tests two typical parameters sets were chosen as basic sets, see Table 26:

–DRM with 4-QAM as a high protected signal with a lower data rate which is suited for a robust audio signal with a low data rate data service.

–DRM with 16-QAM as a low protected signal with a high data rate which is suited for several audio signals or for an audio signal with a high data rate data service.

TABLE 26

MSC code rates for calculations

|  |  |  |
| --- | --- | --- |
| MSC mode | 11-4-QAM | 00-16-QAM |
| MSC protection level | 1 | 2 |
| MSC code rate *R* | 1/3 | 1/2 |
| SDC mode | 1 | 1 |
| SDC code rate *R* | 0.25 | 0.25 |
| Bit rate approx. | 49.7 kbit/s | 149.1 kbit/s |

### 4.1.2 Propagation-related OFDM parameters

The propagation-related OFDM parameters of DRM are given in Table 27.

TABLE 27

OFDM parameters

|  |  |
| --- | --- |
| Elementary time period *T* | 83 1/3 μs |
| Duration of useful (orthogonal) part *Tu*= 27 · *T* | 2.25 ms |
| Duration of guard interval *Tg*= 3 · *T* | 0.25 ms |
| Duration of symbol *Ts = Tu + Tg* | 2.5 ms |
| *Tg*/*Tu* | 1/9 |
| Duration of transmission frame *Tf* | 100 ms |
| Number of symbols per frame *Ns* | 40 |
| Channel bandwidth *B* | 96 kHz |
| Carrier spacing 1/*Tu* | 444 4/9 Hz |
| Carrier number space | *Kmin* = −106;  *Kmax*= 106 |
| Unused carriers | none |

### 4.1.3 Single frequency operation capability

DRM transmitter can be operating in single frequency networks (SFN). The maximum transmitter distance that has to go below to prevent self-interferences depends on the length of the OFDM guard interval.

The maximum transmitter distance is calculated with the maximum echo delay which is given by:

*Decho*(*max*) (km) = *Tg* · *c*0 (45)

where:

*c*0 = 300 · 103 (km/s)

*Tg* = 0.25 (s).

Since the length *Tg* of the DRM guard interval is 0.25 ms, see Table 27, the maximum echo delay, and, therefore, the maximum transmitter distance, yields 75 km.

### 4.1.4 Channel models

Radio wave propagation in VHF bands is characterized by diffraction, scattering and reflection of the electromagnetic waves on their way between the transmitter and the receiver. Typically the waves arrive at different times and different angles at the receiver (multipath propagation) resulting in more or less strong frequency-selective fading (dependent on system bandwidth). In addition movements of the receiver or surrounding objects cause a time variation of the channel characteristic and can result in Doppler shift.

For calculation of the different reception modes, the channel models given in Table 28 [6] have been assumed and investigated. These channel models are considering the fading characteristics for different reception environments. For receivers with higher frequencies the fading in time direction is normally short, so the interleaving and error correction algorithms can work. With slow receiver velocities flat fading over a time, longer than the interleaver (600 ms) can result in signal drop outs.

TABLE 28

Channel models in the ETSI standard for DRM

|  |  |  |
| --- | --- | --- |
| Channel model (name) | Velocity | Remark |
| Channel 7 (AWGN) | 0 km/h | no time variation |
| Channel 8 (urban) | 2 km/h and 60 km/h | pedestrian and vehicle speed |
| Channel 9 (rural) | 150 km/h | vehicle speed on highways |
| Channel 10 (terrain obstructed) | 60 km/h | vehicle speed within built-in areas |
| Channel 11 (hilly terrain) | 100 km/h | vehicle speed along country roads |
| Channel 12 (SFN) | 150 km/h | vehicle speed on highways |

## 4.2 DRM receiver parameters

### 4.2.1 General characteristics

A DRM receiver is intended to receive and decode programmes transmitted according to the DRM system specification Mode E (DRM+) [6].

The parameters relevant for determining the required minimum field-strength levels are:

–noise figure *Fr* (dB), measured from the antenna input to the I/Q base band DRM decoder input (including down conversion and A/D conversion);

–receiver noise input power *Pn* (dBW);

–minimum carrier-to-noise ratio (*C*/*N*)*min* (dB) at the DRM decoder input;

–minimum receiver input power level *Ps,min* (dBW).

### 4.2.2 Receiver noise figure

In GE06 a receiver noise figure of 7 dB is been used for DVB-T. For having cost effective DRM receiver solutions, the receiver noise figure *F* is assumed to be *Fr* = 7 dB too for all VHF bands, see Table 29.

TABLE 29

Receiver noise figure *Fr*

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency (MHz) | 65 | 100 | 200 |
| Receiver noise figure *Fr* (dB) | 7 | 7 | 7 |

### 4.2.3 Receiver noise input power

With *B* = 100 kHz and *T* = 290 K, the thermal receiver noise input power level *Pn* for DRM Mode E yields:

 (46)

### 4.2.4 Minimum carrier to noise ratio

On basis of the channel models in the respective reception mode the required minimum values of the (*C*/*N*)*min* had been calculated. Therefore effects of the narrow-band system like fast fading are included in the calculated values of the (*C*/*N*)*min*.

ETSI-DRM [6] gives a required (*C*/*N*)*min* for a transmission in VHF Band II to achieve an average coded bit error ratio BER = 1 ⋅ 10–4 (bit) after the channel decoder for different channel models, see Table 30.

TABLE 30

(*C*/*N*)*min* with different channel models

|  |  |  |  |
| --- | --- | --- | --- |
|  | | (*C*/*N*)*min* (dB) for | |
| Reception mode | Channel model | 4-QAM, *R* = 1/3 | 16-QAM, *R* = 1/2 |
| Fixed reception | Channel 7 (AWGN) | 1.3 | 7.9 |
| Portable reception | Channel 8 (urban@60 km/h) | 7.3 | 15.4 |
|  | Channel 9 (rural) | 5.6 | 13.1 |
|  | Channel 10 (terrain obstructed) | 5.4 | 12.6 |
| Mobile reception | Channel 11 (hilly terrain) | 5.5 | 12.8 |
|  | Channel 12 (SFN) | 5.4 | 12.3 |

### 4.2.5 Minimum receiver input power level

Based on the above equations and including the implementation loss factor, the minimum receiver input power level at the receiving location can be calculated for both 16-QAM and 4‑QAM, see Table 31 and Table 32.

TABLE 31

Minimum receiver input power level *Ps,min* for 4-QAM, R = 1/3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reception mode | | Fixed | Portable | Mobile |
| Receiver noise figure | *Fr* (dB) | 7 | 7 | 7 |
| Receiver noise input power level | *Pn* (dBW) | −146.98 | −146.98 | −146.98 |
| Representative minimum *C*/*N* | (*C*/*N*)*min* (dB) | 1.3 | 7.3 | 5.5 |
| Implementation loss factor | *Li* (dB) | 3 | 3 | 3 |
| **Minimum receiver input power level** | ***Ps*,*min*** (**dBW**) | **−142.68** | **−136.68** | **−138.48** |

TABLE 32

Minimum receiver input power level *Ps,min* for 16-QAM, *R* = 1/2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reception mode | | Fixed | Portable | Mobile |
| Receiver noise figure | *Fr* (dB) | 7 | 7 | 7 |
| Receiver noise input power level | *Pn* (dBW) | −146.98 | −146.98 | −146.98 |
| Representative minimum *C*/*N* | (*C*/*N*)*min* (dB) | 7.9 | 15.4 | 12.8 |
| Implementation loss factor | *Li* (dB) | 3 | 3 | 3 |
| **Minimum receiver input power level** | ***Ps*,*min*** (**dBW**) | **−136.08** | **−128.58** | **−131.18** |

## 4.3 DRM planning parameters

### 4.3.1 Minimum median field-strength level

Based on the equations in § 3, the minimum median field-strength level for the respective reception modes had been calculated for both 16-QAM and 4-QAM, for VHF Bands I, II and III, see Table 33 to Table 38.

#### 4.3.1.1 VHF Band I

TABLE 33

Minimum median field-strength level *Emed* for 4-QAM, *R =*1/3 in VHF Band I

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DRM modulation | | | 4-QAM. *R* = 1/3 | | | | |
| Receiving situation | | FX | PI | PI-H | PO | PO-H | MO |
| Minimum receiver input power level | *Ps,min* (dBW) | −142.68 | −136.68 | −136.68 | −136.68 | −136.68 | −138.48 |
| Antenna gain | *GD* (dBd) | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lc* dB | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | φ*min* (dBW/m2) | −146.02 | −138.92 | −118.36 | −138.92 | −118.36 | −140.50 |
| Minimum field‑strength level at receiving antenna | *Emin* (dB(μV/m)) | −0.25 | 6.85 | 27.41 | 6.85 | 27.41 | 5.27 |
| Allowance for man‑made noise | *Pmmn* (dB) | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Antenna height loss | *Lh* (dB) | 0.00 | 8.00 | 15.00 | 8.00 | 15.00 | 8.00 |
| Building penetration loss | *Lb* (dB) | 0.00 | 8.00 | 8.00 | 0.00 | 0.00 | 0.00 |

TABLE 33 (*end*)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Location probability |  | 70% | 95% | 95% | 95% | 95% | 99% |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 1.64 | 1.64 | 2.33 |
| Standard deviation of DRM field strength | σ*m* (dB) | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of MMN | σ*MMN* (dB) | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Location correction factor | *Cl* (dB) | 3.02 | 10.68 | 7.65 | 9.47 | 5.85 | 12.46 |
| **Minimum median field‑strength level** | ***Emed* (dB(μV/m))** | **18.15** | **48.91** | **58.06** | **39.71** | **48.26** | **41.11** |

TABLE 34

Minimum median field-strength level *Emed* for 16 QAM, *R* = 1/2 in VHF Band I

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DRM modulation | | 16-QAM. *R* = 1/2 | | | | | |
| Receiving situation | | FX | PI | PI-H | PO | PO-H | MO |
| Minimum receiver input power level | *Ps,min* (dBW) | −136.08 | −128.58 | −128.58 | −128.58 | −128.58 | −131.18 |
| Antenna gain | *GD* (dBd) | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lc* (dB) | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux-density at receiving place | ϕ*min* (dBW/m2) | −139.42 | −130.82 | −110.26 | −130.82 | −110.26 | −133.20 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | 6.35 | 14.95 | 35.51 | 14.95 | 35.51 | 12.57 |
| Allowance for man-made noise | *Pmmn* (dB) | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Antenna height loss | *Lh* (dB) | 0.00 | 8.00 | 15.00 | 8.00 | 15.00 | 8.00 |
| Building penetration loss | *Lb* (dB) | 0.00 | 8.00 | 8.00 | 0.00 | 0.00 | 0.00 |
| Location probability |  | 70% | 95% | 95% | 95% | 95% | 99% |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 1.64 | 1.64 | 2.33 |
| Standard deviation of DRM field strength | σ*m* (dB) | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of MMN | σ*MMN* (dB) | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Location correction factor | *Cl*(dB) | 3.02 | 10.68 | 7.65 | 9.47 | 5.85 | 12.46 |
| **Minimum median field-strength level** | ***Emed*** (**dB(μV/m))** | **24.75** | **57.01** | **66.16** | **47.81** | **56.36** | **48.41** |

#### 

#### 4.3.1.2 VHF Band II

TABLE 35

Minimum median field-strength level *Emed* for 4-QAM, *R* = 1/3 in VHF Band II

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DRM modulation | | 4-QAM. *R* = 1/3 | | | | | |
| Receiving situation | | FX | PI | PI-H | PO | PO-H | MO |
| Minimum receiver input power level | *Ps*,*min* (dBW) | −142.68 | −136.68 | −136.68 | −136.68 | −136.68 | −138.48 |
| Antenna gain | *GD* (dBd) | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lc* (dB) | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | φ*min* (dBW/m2) | −141.97 | −135.17 | −118.35 | −135.17 | −118.35 | −136.69 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | 3.79 | 10.59 | 27.41 | 10.59 | 27.41 | 9.07 |
| Allowance for man-made noise | *Pmmn* (dB) | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Antenna height loss | *Lh* (dB) | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Location probability |  | 70% | 95% | 95% | 95% | 95% | 99% |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 1.64 | 1.64 | 2.33 |
| Standard deviation of DRM field strength | σ*m* (dB) | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of MMN | σ*MMN* (dB) | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Location correction factor | *Cl*(dB) | 3.10 | 10.91 | 7.96 | 9.73 | 6.25 | 12.77 |
| **Minimum median field‑strength level** | ***Emed*** (**dB(μV/m))** | **17.32** | **50.92** | **61.37** | **40.74** | **50.66** | **42.27** |

TABLE 36

Minimum median field-strength level *Emed* for 16-QAM, *R* = 1/2 in VHF Band II

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DRM modulation | | 16-QAM *R* = 1/2 | | | | | |
| Receiving situation | | FX | PI | PI-H | PO | PO-H | MO |
| Minimum receiver input power level | *Ps,min* (dBW) | −136.08 | −128.58 | −128.58 | −128.58 | −128.58 | −131.18 |
| Antenna gain | *GD* (dBd) | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lc* (dB) | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | φ*min* (dBW/m2) | −135.37 | −127.07 | −110.25 | −127.07 | −110.25 | −129.39 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | 10.39 | 18.69 | 35.51 | 18.69 | 35.51 | 16.37 |
| Allowance for man-made noise | *Pmmn* (dB) | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Antenna height loss | *Lh* (dB) | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Location probability |  | 70% | 95% | 95% | 95% | 95% | 99% |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 1.64 | 1.64 | 2.33 |
| Standard deviation of DRM field strength | σ*m* (dB) | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of MMN | σ*MMN* (dB) | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Location correction factor | *Cl*(dB) | 3.10 | 10.91 | 7.96 | 9.73 | 6.25 | 12.77 |
| **Minimum median field‑strength level** | ***Emed* (dB(μV/m))** | **23.92** | **59.02** | **69.47** | **48.84** | **58.76** | **49.57** |

#### 4.3.1.3 VHF Band III

TABLE 37

Minimum median field-strength level *Emed* for 4-QAM, *R* = 1/3 in VHF Band III

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DRM modulation | | 4-QAM. *R* = 1/3 | | | | | |
| Receiving situation | | FX | PI | PI-H | PO | PO-H | MO |
| Minimum receiver input power level | *Ps,min* (dBW) | −142.68 | −136.68 | −136.68 | −136.68 | −136.68 | −138.48 |
| Antenna gain | *GD* (dBd) | 0.00 | −2.20 | −13.00 | −2.20 | −13.00 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) | −5.32 | −7.52 | −18.32 | −7.52 | −18.32 | −7.52 |
| Feeder-loss | *Lc* (dB) | 2.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.40 |

TABLE 37 (*end*)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Minimum power flux‑density at receiving place | ϕ*min* (dBW/m2) | −135.35 | −129.15 | −118.35 | −129.15 | −118.35 | −130.55 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | 10.41 | 16.61 | 27.41 | 16.61 | 27.41 | 15.21 |
| Allowance for man-made noise | *Pmmn* (dB) | 3.62 | 3.62 | 0.00 | 3.62 | 0.00 | 3.62 |
| Antenna height loss | *Lh* (dB) | 0.00 | 12.00 | 19.00 | 12.00 | 19.00 | 12.00 |
| Building penetration loss | *Lb* (dB) | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Location probability |  | 70% | 95% | 95% | 95% | 95% | 99% |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 1.64 | 1.64 | 2.33 |
| Standard deviation of DRM field strength | σ*m* (dB) | 4.19 | 4.19 | 4.19 | 4.19 | 4.19 | 3.49 |
| Standard deviation of MMN | σ*MMN* (dB) | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Location correction factor | *Cl*(dB) | 3.24 | 11.29 | 8.48 | 10.15 | 6.89 | 13.31 |
| **Minimum median field‑strength level** | ***Emed* (dB(μV/m))** | **17.26** | **52.52** | **63.89** | **42.38** | **53.30** | **44.13** |

TABLE 38

Minimum median field-strength level *Emed* for 16-QAM, *R* = 1/2 in VHF Band III

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DRM modulation | | 16-QAM. R = ½ | | | | | |
| Receiving situation | | FX | PI | PI-H | PO | PO-H | MO |
| Minimum receiver input power level | *Ps*,*min* (dBW) | −136.08 | −128.58 | −128.58 | −128.58 | −128.58 | −131.18 |
| Antenna gain | *GD* (dBd) | 0.00 | −2.20 | −13.00 | −2.20 | −13.00 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) | −5.32 | −7.52 | −18.32 | −7.52 | −18.32 | −7.52 |
| Feeder-loss | *Lc* (dB) | 2.00 | 0.00 | 0.00 | 0.00 | 0.00 | 0.40 |
| Minimum power flux‑density at receiving place | φ*min* (dBW/m2) | −128.75 | −121.05 | −110.25 | −121.05 | −110.25 | −123.25 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | 17.01 | 24.71 | 35.51 | 24.71 | 35.51 | 22.51 |
| Allowance for man-made noise | *Pmmn* (dB) | 3.62 | 3.62 | 0.00 | 3.62 | 0.00 | 3.62 |
| Antenna height loss | *Lh* (dB) | 0.00 | 12.00 | 19.00 | 12.00 | 19.00 | 12.00 |
| Building penetration loss | *Lb* (dB) | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Location probability |  | 70% | 95% | 95% | 95% | 95% | 99% |

TABLE 38 (*end*)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 1.64 | 1.64 | 2.33 |
| Standard deviation of DRM field strength | σ*m* (dB) | 4.19 | 4.19 | 4.19 | 4.19 | 4.19 | 3.49 |
| Standard deviation of MMN | σ*MMN*(dB) | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Location correction factor | *Cl* (dB) | 3.24 | 11.29 | 8.48 | 10.15 | 6.89 | 13.31 |
| **Minimum median field-strength level** | ***Emed* (dB(μV/m))** | **23.86** | **60.62** | **71.99** | **50.48** | **61.40** | **51.43** |

### 4.3.2 Position of DRM frequencies

The DRM system is designed to be used at any frequency with variable channelization constraints and propagation conditions throughout these bands [6].

Referring to the legal frequency plans in ITU Region 1 this Report covers DRM:

–in VHF Band I as well as in VHF Band II regarding to GE84 [5];

–in VHF Band III regarding to GE06 [1].

Other areas in the VHF bands assigned for sound broadcasting services, e.g. areas in ITU Region 1 where allocations of the Wiesbaden T-DAB Agreement 1995 are still used (230-240 MHz) or in southern Africa, where the VHF Band III is allocated to the broadcasting services up to 254 MHz, or the broadcasting bands in ITU Region 2 and 3, perhaps the OIRT FM band (65.8-74 MHz) or the Japanese FM band (76-90 MHz), respectively, are not yet covered in this section and can be adapted later.

#### 4.3.2.1 VHF Band I and VHF Band II

The DRM centre frequencies are positioned in 100 kHz distance according to the FM frequency grid in VHF Band II. The nominal carrier frequencies are, in principle, integral multiples of 100 kHz [5]. The DRM system is designed to be used with this raster [6].

The table of centre frequencies of DRM in VHF Band II is given in Annex 2.

On the other hand it has to be considered to allow a spacing of 50 kHz in VHF Band II to achieve the full potential of the DRM hybrid mode and to alleviate the deployment of new DRM transmitters in the overcrowded FM band.

#### 4.3.2.2 VHF Band III

The DRM centre frequencies are positioned in 100 kHz distance beginning by 174.05 MHz and integral multiples of 100 kHz up to the end of VHF Band III.

The table of the centre frequencies of DRM in VHF Band III in the range from 174 to 230 MHz is given in Annex 2.

### 4.3.3 Out-of-band spectrum mask

The power density spectrum at the transmitter output is important to determine the adjacent channel interference.

The spectrum characteristics of an OFDM system are given in Recommendation ITU-R SM.328, Annex 6, § 5.

#### 4.3.3.1 VHF Band I and VHF Band II

An out-of-band spectrum mask for DRM in VHF Band I and VHF Band II, respectively, as minimum transmitter requirement is proposed in Fig. 1 and Table 39. The vertices of the symmetric out-of-band spectrum mask for FM transmitters are given in ETSI-FM [7].

Note that the out-of-band spectrum masks are defined for a resolution bandwidth (RBW) of 1 kHz.

Figure 1

Out-of-band spectrum masks for FM in VHF Band II and DRM in VHF Bands I and II




TABLE 39

Out-of-band spectrum masks for FM in VHF Band II and DRM in VHF Bands I and II

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Spectrum mask  (100 kHz channel)/ relative level for FM | |  | Spectrum mask  (100 kHz channel)/ relative level for DRM | |
| Frequency offset (kHz) | Level  (dBc)/(1 kHz) |  | Frequency offset (kHz) | Level  (dBc)/(1 kHz) |
| **0** | 0 |  | **0** | −20 |
| **±50** | 0 |  | **±50** | −20 |
| **±70** | 0 |  | **±70** | −50 |
| **±100** | 0 |  | **±100** | −70 |
| **±200** | −80 |  | **±200** | −80 |
| **±300** | −85 |  | **±300** | −85 |
| **±400** | −85 |  | **±400** | −85 |

#### 4.3.3.2 VHF Band III

The vertices of the symmetric out-of-band spectrum masks for DAB transmitters are given in Recommendation ITU‑R BS.1660 [44]. An out-of-band spectrum mask for DRM is proposed that fits into the DAB masks, see Fig. 2 and Table 40.

Note that the out-of-band spectrum masks are defined for a resolution bandwidth (RBW) of 4 kHz. Thus the value of −14 dBr results for DRM.

Figure 2

Out-of-band spectrum masks for DAB and DRM in VHF Band III




TABLE 40

Out-of-band spectrum masks for DRM in VHF Band III

|  |  |
| --- | --- |
| Spectrum mask (100 kHz channel)  relative level for DRM | |
| Frequency offset (kHz) | Level (dBc) |
| **0** | −14 |
| **±50** | −14 |
| **±60** | −44 |
| **±181.25** | −59 |
| **±200** | −74 |
| **±300** | −79 |
| **±500** | −84 |

### 4.3.4 Protection ratios

The minimum acceptable ratio between a wanted signal and interfering signals to protect the reception of the wanted signal is defined as the protection ratio *PR* (dB). The values of protection ratios are given as:

–Basic protection ratio *PRbasic* for a wanted signal interfered with by an unwanted signal at 50% location probability. These values are determined in accordance with Recommendation ITU‑R BS.641.

–Combined location correction factor *CF* (dB) as a margin that has to be added to the basic protection ratio for a wanted signal interfered with by an unwanted signal for the calculation of protection ratios at location probability greater as 50%. The equation for the calculation is given in § 3.8.3.

–Corresponding protection ratio *PR*(*p*) for a wanted digital signal interfered with by an unwanted signal at location probability greater than 50% taking into account the respective location probability of the corresponding reception modes that have higher protection requirements due to the higher location probability to be protected.

#### 4.3.4.1 Protection ratios for DRM

The DRM signal parameters are given in § 4.1.

##### 4.3.4.1.1 DRM interfered with by DRM

The basic protection ratio *PRbasic* for DRM is valid for all VHF bands, see Table 41. For the standard deviation of DRM differs in the respective VHF bands the combined location correction factors CF, see Table 42, are different in the respective VHF bands as well as the corresponding protection ratios *PR*(*p*), see Table 43 for 4-QAM and Table 44 for 16-QAM.

TABLE 41

Basic protection ratios *PRbasic* for DRM interfered with by DRM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| DRM (4-QAM, *R* = 1/3) | *PRbasic* (dB) | 4 | −16 | −40 |
| DRM (16-QAM, *R* = 1/2) | *PRbasic* (dB) | 10 | −10 | −34 |

TABLE 42

Combined location correction factor *CF* for DRM interfered with by DRM

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Reference frequency band (MHz) | | 65 MHz VHF Band I | | | 100 MHz VHF Band II | | | 200 MHz VHF Band III | | |
| Location probability *p* (%) | | 70 | 95 | 99 | 70 | 95 | 99 | 70 | 95 | 99 |
| Combined location correction factor in urban and suburban area for fixed and portable reception | *CF* (dB) | 2.64 | 8.27 | 11.70 | 2.82 | 8.84 | 12.50 | 3.11 | 9.75 | 13.79 |
| Combined location correction factor in rural area for mobile reception | *CF* (dB) | 2.12 | 6.65 | 9.40 | 2.30 | 7.21 | 10.20 | 2.59 | 8.12 | 11.49 |

TABLE 43

Corresponding protection ratios *PR*(*p*) to reception modes for DRM (4-QAM. *R* = 1/3) interfered with by DRM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reference frequency band (MHz) | | 65 MHz VHF Band I | | |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 6.64 | −13.36 | −37.36 |
| Portable reception (PO, PI, PO-H, PI-H) | *PR*(*p*) (dB) | 12.27 | −7.73 | −31.73 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 13.40 | −6.60 | −30.60 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reference frequency band (MHz) | | 100 MHz  VHF Band II | | |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 6.82 | −13.18 | −37.18 |
| Portable reception (PO, PI, PO-H, PI-H) | *PR*(*p*) (dB) | 12.84 | −7.16 | −31.16 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 14.20 | −5.80 | −29.80 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reference frequency band (MHz) | | 200 MHz VHF Band III | | |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 7.11 | −12.89 | −36.89 |
| Portable reception (PO. PI. PO-H. PI-H) | *PR*(*p*) (dB) | 13.75 | −6.25 | −30.25 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 15.49 | −4.51 | −28.51 |

TABLE 44

Corresponding protection ratios *PR*(*p*) to reception modes for DRM (16-QAM. *R* = 1/2) interfered with by DRM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reference frequency band (MHz) | | 65 MHz VHF Band I | | |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 12.64 | −7.36 | −31.36 |
| Portable reception (PO. PI. PO-H. PI-H) | *PR*(*p*) (dB) | 18.27 | −1.73 | −25.73 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 19.40 | −0.60 | −24.60 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reference frequency band (MHz) | | 100 MHz  VHF Band II | | |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 12.82 | −7.18 | −31.18 |
| Portable reception (PO, PI, PO-H, PI-H) | *PR*(*p*) (dB) | 18.84 | −1.16 | −25.16 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 20.20 | 0.20 | −23.80 |

TABLE 44 (*end*)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reference frequency band (MHz) | | 200 MHz VHF Band III | | |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 13.11 | −6.89 | −30.89 |
| Portable reception (PO, PI, PO-H, PI-H) | *PR*(*p*) (dB) | 19.75 | −0.25 | −24.25 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 21.49 | 1.49 | −22.51 |

##### 4.3.4.1.2 DRM interfered with by FM in VHF Band II

The basic protection ratio *PRbasic* for DRM interfered with by FM in VHF Band II is given in Table 45. The values for the combined location correction factors *CF* are given in Table 46, and for the corresponding protection ratios *PR*(*p*), are given in Table 47 for 4-QAM and in Table 48 for 16‑QAM, respectively.

TABLE 45

Basic protection ratios *PRbasic* for DRM interfered with by FM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| DRM (4-QAM. *R* = 1/3) interfered with by FM (stereo) | *PRbasic* (dB) | 11 | −13 | −54 |
| DRM (16-QAM. *R* = 1/2) interfered with by FM (stereo) | *PRbasic* (dB) | 18 | −9 | −49 |

TABLE 46

Combined location correction *CF* factor for DRM interfered with by FM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Location probability *p* (%) | | 70 | 95 | 99 |
| Combined location correction factor in urban and suburban area for fixed and portable reception | *CF* (dB) | 4.79 | 15.02 | 21.24 |
| Combined location correction factor in rural area for mobile reception | *CF* (dB) | 4.65 | 14.57 | 20.61 |

TABLE 47

Corresponding protection ratios *PR*(*p*) to reception modes   
for DRM (4-QAM. *R* = 1/3) interfered with by FM stereo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 15.79 | −8.21 | −49.21 |
| Portable reception (PO, PI, PO-H, PI-H) | *PR*(*p*) (dB) | 26.02 | 2.02 | −38.98 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 31.61 | 7.61 | −33.39 |

TABLE 48

Corresponding protection ratios *PR*(*p*) to reception modes   
for DRM (16-QAM. *R* = 1/2) interfered with by FM stereo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 22.79 | −4.21 | −44.21 |
| Portable reception (PO, PI, PO-H, PI-H) | *PR*(*p*) (dB) | 33.02 | 6.02 | −33.98 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 38.61 | 11.61 | −28.39 |

##### 4.3.4.1.3 DRM interfered with by DAB in VHF Band III

The basic protection ratio *PRbasic* for DRM interfered with by DAB in VHF Band III is given in Table 49. The values for the combined location correction factors CF are given in Table 50, and for the corresponding protection ratios *PR*(*p*)*,* are given in Table 51 for 4-QAM and in Table 52 for 16‑QAM, respectively. For the protection ratios of DRM interfered with DAB+, see § 7.4.4.

TABLE 49

Basic protection ratios *PRbasic* of DRM interfered with by DAB

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Basic protection ratio for DRM (4-QAM. *R* = 1/3) | *PRbasic* (dB) | −7 | −36 | −40 |
| Basic protection ratio for DRM (16-QAM. *R* = 1/2) | *PRbasic* (dB) | −2 | −18 | −40 |

TABLE 50

Combined location correction factor *CF* of DRM interfered with by DAB

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Location probability *p* (%) | | 70 | 95 | 99 |
| Combined location correction factor  **in urban and suburban area for fixed and portable reception** | *CF* (dB) | 3.63 | 11.37 | 16.09 |
| Combined location correction factor  i**n rural area for mobile reception** | *CF* (dB) | 3.42 | 10.72 | 15.16 |

TABLE 51

Corresponding protection ratios *PR*(*p*) to reception modes   
for DRM (4-QAM. *R* = 1/3) interfered with by DAB

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | −3.37 | −32.37 | −50.37 |
| Portable reception (PO, PI, PO-H, PI‑H) | *PR*(*p*) (dB) | 4.37 | −24.63 | −42.63 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 8.16 | −20.84 | −38.84 |

TABLE 52

Corresponding protection ratios *PR*(*p*) to reception modes   
for DRM (16-QAM. *R* = 1/2) interfered with by DAB

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Fixed reception (FX) | *PR*(*p*) (dB) | 1.63 | −14.37 | −45.37 |
| Portable reception (PO, PI, PO-H, PI-H) | *PR*(*p*) (dB) | 9.37 | −6.63 | −37.63 |
| Mobile reception (MO) | *PR*(*p*) (dB) | 13.16 | −2.84 | −33.84 |

##### 4.3.4.1.4 DRM interfered with by DVB-T in VHF Band III

Since the impact mechanisms of DAB into DRM is the same as that of DVB-T it is proposed that the same protection ratios for DRM interfered with by DVB-T in VHF Band III can be assumed as for DRM interfered with by DAB in VHF Band III.

#### 4.3.4.2 Protection ratios for broadcasting systems interfered with by DRM

##### 4.3.4.2.1 Protection ratios for FM in VHF Band II

The FM signal parameters are given in Recommendation ITU‑R BS.412.

Recommendation ITU‑R BS.412, Annex 5 states that interferences can be caused by intermodulation of strong FM signals in a frequency offset greater than 400 kHz. This cross modulation effect from a high interfering signal level in a range up to 1 MHz offset has also to be taken into account when planning OFDM systems into the VHF Band II. Therefore not only the protection ratios *PRbasic* are given in the range 0 kHz to ±400 kHz, and for ±500 kHz and ±1 000 MHz, see Table 53. The values for ±600 kHz to ±900 kHz can be found by linear interpolation.

TABLE 53

Basic protection ratios *PRbasic* for FM interfered with by DRM

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 | ±300 | ±400 | ±500 | ±1 000 |
| Basic protection ratio for FM (stereo) | *PRbasic* (dB) | 49 | 30 | 3 | −8 | −11 | −13 | −21 |

##### 4.3.4.2.2 Protection ratios for DAB in VHF Band III

The DAB signal parameters are given in Recommendation ITU-R BS.1660. In GE06 [1] it is given that the DAB planning should be able to deal with mobile reception with a location probability of 99%, and with portable indoor reception with a location probability of 95%, respectively. In addition the values for fixed reception with a location probability of 70% are given.

The basic protection ratios for DAB interfered with by DRM are given in Table 54, the related combined location correction factors are given in Table 55, and the corresponding protection ratios *PR(p)* are given in Table 56, respectively. For the protection ratios of DAB+ interfered with DRM, see § 7.4.4.

TABLE 54

Basic protection ratios *PRbasic* for DAB interfered with by DRM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| Basic protection ratio for T‑DAB | *PRbasic* (dB) | 10 | −40 | −40 |

TABLE 55

Combined location correction factor *CF* for DAB interfered with by DRM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Location probability *p* (%) | | 70 | 95 | 99 |
| Combined location correction factor  in urban and suburban area for fixed and portable reception | *CF* (dB) | 3.63 | 11.37 | 16.09 |
| Combined location correction factor  in rural area for mobile reception | *CF* (dB) | 3.42 | 10.72 | 15.16 |

TABLE 56

Corresponding protection ratios *PR*(*p*) to reception   
modes for DAB interfered with by DRM

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 |
| DAB fixed reception | *PR*(*p*) (dB) | 13.63 | −36.37 | −36.37 |
| DAB portable reception | *PR*(*p*) (dB) | 21.37 | −28.63 | −28.63 |
| DAB mobile reception | *PR*(*p*) (dB) | 25.16 | −24.84 | −24.84 |

##### 4.3.4.2.3 Protection ratios for DVB-T in VHF Band III

The DVB-T signal parameters are given in Recommendation ITU-R BT.1368.

In VHF Band III not only DAB but also may be DVB-T operated additionally as an interferer into DRM or to be interfered with by DRM.

DRM as an interferer against a DAB wanted signal has the same impact as a DAB interferer under the assumption that more than one DRM interferer with different frequencies in a DAB block has to be included, see Table 54.

The same proposal can be assumed if DVB-T is the wanted signal. If there is more than one DRM interferer with different frequencies in a DVB-T channel the impact may be the same as it is caused by a DAB signal. Therefore, it is proposed that the protection ratios of DVB-T interfered with by DRM are the same as DVB-T is interfered with by DAB.

In Recommendation ITU-R BT.1368 the basic protection ratios for DVB-T interfered with DAB are given, see Table 57. These protection rations are proposed for the interferences by a DRM signal also. In the adjacent channels no impact is proposed.

TABLE 57

Co-channel basic protection ratios *PRbasic* for DVB-T interfered   
with by DAB (Recommendation ITU-R BT.1368) and by DRM

|  |  |
| --- | --- |
| Wanted signal DVB-T constellation-code rate | *PR*  (dB) |
| QPSK-1/2 | 10 |
| QPSK-2/3 | 12 |
| QPSK-3/4 | 14 |
| 16-QAM-1/2 | 15 |
| 16-QAM-2/3 | 18 |
| 16-QAM-3/4 | 20 |
| 64-QAM-1/2 | 20 |
| 64-QAM-2/3 | 24 |
| 64-QAM-3/4 | 26 |
| 64-QAM-7/8 | 31 |

#### 4.3.4.3 Protection ratios for other services interfered with by DRM

##### 4.3.4.3.1 Other services below the radio broadcasting VHF Band II

Below the VHF Band II broadcasting band, land mobile services with security tasks are located. The interference potential of DRM into these services is not higher as the one of FM signals. Provided sufficient additional band-pass filtering of the output of the transmitter is applied, the interference potential of DRM into narrow-band FM (BOS) reception is not substantially higher than that of a standard FM broadcast signal [8].

##### 4.3.4.3.2 Other services above the radio broadcasting VHF Band II

Above the VHF Band II broadcasting band, aeronautical radio navigation services are located. The interference potential of DRM into these services is not higher as the one of FM signals. For frequency offsets of less than 200 kHz, the interference potential of DRM into VOR and ILS localizer reception is much less than of a standard FM broadcast signal (up to 30 dB less). For larger frequency offsets, both signals produce roughly the same interference, provided sufficient additional band-pass filtering of the output of the transmitter is deployed [8].

##### 4.3.4.3.3 Other services in the radio broadcasting VHF Band III

The values and the procedures to take into account other services in VHF Band III is given in GE06. For DRM the same values as for DAB shall be applied.

### 4.3.5 Calculation of the resulting sum field strength of interferers

To calculate the resulting interfering sum field-strength level from several signal sources *Esum*

– **in VHF Band I and VHF Band II** the simplified multiplication method (see Report ITU‑R BS.945) shall be applied according to GE84 [5];

– **in VHF Band III** the log-normal methods (see Report ITU-R BS.945) according to the planning procedures of T-DAB and DVB-T [1] shall be applied.

# 5 Planning parameters for digital terrestrial broadcasting system RAVIS in VHF Bands I and II

The RAVIS system is designed for digital sound and multimedia broadcasting in VHF Bands I and II. The system is nationally standardized in the Russian Federation [9-13]. Main characteristics and features of RAVIS can be found in Report ITU‑R BT.2049 – Broadcasting of multimedia and data applications for mobile reception.

## 5.1 System parameters of RAVIS

### 5.1.1 RAVIS signal parameters

RAVIS supports three types of radio channel bandwidth: 100, 200 and 250 kHz.

RAVIS supports three different coding rates for logical channel of main service: 1/2, 2/3 and 3/4.

RAVIS supports three different modulation types for logical channel of main service: QPSK, 16‑QAM and 64-QAM.

Rounded bit rates for different combinations of system parameters are given in Table 58.

TABLE 58

Bit rates for RAVIS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Modulation type | Code rate | Bit rate (kbit/s) | | |
| 100 kHz channel | 200 kHz channel | 250 kHz channel |
| QPSK | 1/2 | 80 | 160 | 200 |
| 2/3 | 100 | 210 | 270 |
| 3/4 | 120 | 240 | 300 |
| 16-QAM | 1/2 | 150 | 320 | 400 |
| 2/3 | 210 | 420 | 530 |
| 3/4 | 230 | 470 | 600 |
| 64-QAM | 1/2 | 230 | 470 | 600 |
| 2/3 | 310 | 630 | 800 |
| 3/4 | 350 | 710 | 900 |

Main OFDM parameters of RAVIS signal are given in Table 59.

TABLE 59

OFDM parameters of RAVIS

|  |  |  |  |
| --- | --- | --- | --- |
| Channel bandwidth *B* | 100 kHz | 200 kHz | 250 kHz |
| Number of curriers | 215 | 439 | 553 |
| Number of information curriers | 196 | 400 | 504 |
| Distance between first and last curriers | 95.1 kHz | 194.7 kHz | 245.3 kHz |
| Carrier spacing 1/*Tu* | 4 000/9 Hz = 444 4/9 Hz | | |
| Duration of useful part of symbol *Tu* | 2.25 ms | | |
| Duration of guard interval *Tg* | 281.25 ms | | |

TABLE 59 (*end*)

|  |  |
| --- | --- |
| Duration of symbol *Ts = Tu + Tg* | 2.53125 ms |
| *Tg/Tu* | 1/8 |
| Duration of transmission frame *Tf* | 103.8 ms |
| Number of symbols per frame *Ns* | 41 |

### 5.1.2 SFN operation capabilities

RAVIS can operate in single frequency networks (SFN). The maximum transmitter distance that has to go below to prevent self-interferences depends on the length of the OFDM guard interval. The maximum transmitter distance defined by (45) is calculated through the multiplication of velocity of light (3 · 105 km/s) by guard interval duration (~0.28 ms for RAVIS). So maximum transmitter distance is about 84 km.

### 5.1.3 Channel models

Channel models used for simulation of RAVIS operation corresponds to the models defined in DRM standard [6] and used for DRM operation simulation (see Table 28).

## 5.2 RAVIS radio receiver related parameters

RAVIS receiver is intended to receive and decode programmes transmitted according to the RAVIS system standard [9].

The parameters relevant for determining the required minimum field-strength levels are:

–noise figure *Fr* (dB), measured from the antenna input to the I/Q base band RAVIS decoder input (including down conversion and A/D conversion);

–receiver noise input power *Pn* (dBW);

–minimum carrier-to-noise ratio (*C*/*N*)*min* (dB) at the RAVIS decoder input;

–minimum receiver input power level *Ps,min* (dBW).

For having cost effective RAVIS receiver solutions the receiver noise figure *F* is assumed to be *Fr* = 7 dB as for DRM receiver for all VHF bands, see Table 29.

Receiver noise input power *Pn* is calculated according to (16) and depends on input signal bandwidth (*T* = 290 K):

*Pn* (dBW) = –146.98 (dBW) for 100 kHz signal bandwidth;

*Pn* (dBW) = –143.97 (dBW) for 200 kHz signal bandwidth;

*Pn* (dBW) = –143.00 (dBW) for 250 kHz signal bandwidth.

Required (*C*/*N*)*min* for a transmission in VHF Band II to achieve an average coded bit error ratio BER = 1 ⋅ 10−4 (bit) after the channel decoder for system parameters and different channel models are given in Tables 60 to 62. Channel models correspond to the models from [6], Annex B.2. Channel 7 (AWGN) models fixed reception mode, channel 8 (Urban) models portable reception mode, channel 11 (Hilly terrain) models mobile reception mode.

TABLE 60

(*C*/*N*)*min* for RAVIS with 100 kHz channel bandwidth

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Channel model/ reception mode | (*C*/*N*)*min* (dB) | | | | | | | | |
| QPSK | | | 16-QAM | | | 64-QAM | | |
| *R*= 1/2 | *R*= 2/3 | *R* = 3/4 | *R =* 1/2 | *R* = 2/3 | *R* = 3/4 | *R*= 1/2 | *R* = 2/3 | *R* = 3/4 |
| Channel 7 (AWGN)/fixed reception | 5 1.2 | 6 3.4 | 6 4.3 | 8 6.6 | 1 9.2 | 1 10.3 | 1 10.9 | 1 14.2 | 1 15.6 |
| Channel 8 (urban)/ portable reception | 1 6.5 | 1 9.5 | 1 11.7 | 1 12.6 | 1 15.1 | 1 17.2 | 2 16.3 | 2 19.6 | 2 22.2 |
| Channel 11 (hilly terrain)/mobile reception | 9 5.6 | 1 8.7 | 1 10.0 | 1 10.5 | 1 13.3 | 1 15.8 | 1 14.8 | 2 18.1 | 2 20.7 |

TABLE 61

(*C*/*N*)*min* for RAVIS with 200 kHz channel bandwidth

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Channel model/ reception mode | (*C*/*N*)*min* (dB) | | | | | | | | |
| QPSK | | | 16-QAM | | | 64-QAM | | |
| *R*= 1/2 | *R*= 2/3 | *R* = 3/4 | *R =* 1/2 | *R* = 2/3 | *R* = 3/4 | *R*= 1/2 | *R* = 2/3 | *R* = 3/4 |
| Channel 7 (AWGN)/fixed reception | 4 1.1 | 5 3.3 | 6 4.2 | 8 6.4 | 1 9.1 | 1 10.2 | 1 10.8 | 1 14.0 | 1 15.4 |
| Channel 8 (urban)/ portable reception | 1 6.4 | 1 9.4 | 1 11.5 | 1 12.5 | 1 14.9 | 1 17.0 | 2 16.2 | 2 19.4 | 2 22.0 |
| Channel 11 (hilly terrain)/mobile reception | 1 5.5 | 1 8.6 | 1 9.8 | 1 10.4 | 1 13.2 | 1 15.6 | 1 14.7 | 2 17.9 | 2 20.5 |

TABLE 62

(*C*/*N*)*min* for RAVIS with 250 kHz channel bandwidth

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Channel model /reception mode | (*C*/*N*)*min* (dB) | | | | | | | | |
| QPSK | | | 16-QAM | | | 64-QAM | | |
| *R*= 1/2 | *R*= 2/3 | *R* = 3/4 | *R =* 1/2 | *R* = 2/3 | *R* = 3/4 | *R*= 1/2 | *R* = 2/3 | *R* = 3/4 |
| Channel 7 (AWGN) /fixed reception | 5 1.1 | 5 3.2 | 6 4.2 | 8 6.3 | 1 9.1 | 1 10.2 | 1 10.6 | 1 14.0 | 1 15.4 |
| Channel 8 (urban) /portable reception | 1 6.4 | 1 9.4 | 1 11.5 | 1 12.4 | 2 14.9 | 2 17.0 | 2 16.1 | 2 19.4 | 2 22.0 |
| Channel 11 (hilly terrain)/mobile reception | 1 5.5 | 1 8.5 | 1 9.8 | 1 10.3 | 1 13.2 | 1 15.6 | 2 14.6 | 2 17.9 | 2 20.5 |

## 5.3 RAVIS planning parameters

### 5.3.1 Minimum median field-strength

Based on the parameters and equations set above, the minimum median field-strength level for different reception modes and frequency Bands I and II can be calculated for all sets of RAVIS system parameters, as shown in Tables 63 to 80.

TABLE 63

Minimum median field-strength level *Emed* for 100 kHz channel   
bandwidth and QPSK modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 51.2 | 16.5 | 16.5 | 16.5 | 16.5 | 95.6 |
| *R* = 2/3 | 63.4 | 19.5 | 19.5 | 19.5 | 19.5 | 18.7 |
| *R* = 3/4 | 64.3 | 111.7 | 111.7 | 111.7 | 111.7 | 110.0 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R*= 1/2 | −142.78 | −137.48 | −137.48 | −137.48 | −137.48 | −138.38 |
| *R* = 2/3 | −140.58 | −134.48 | −134.48 | −134.48 | −134.48 | −135.28 |
| *R* = 3/4 | −139.68 | −132.28 | −132.28 | −132.28 | −132.28 | −133.98 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | ϕ*min* (dBW/m2) | *R* = 1/2 | −146.12 | −139.72 | −119.16 | −139.72 | −119.16 | −140.40 |
| *R* = 2/3 | −143.92 | −136.72 | −116.16 | −136.72 | −116.16 | −137.30 |
| *R*= 3/4 | −143.02 | −134.52 | −113.96 | −134.52 | −113.96 | −136.00 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(µV/m)) | *R* = 1/2 | −0.32 | 6.08 | 26.64 | 6.08 | 26.64 | 5.40 |
| *R* = 2/3 | 1.88 | 9.08 | 29.64 | 9.08 | 29.64 | 8.50 |
| *R* = 3/4 | 2.78 | 11.28 | 31.84 | 11.28 | 31.84 | 9.80 |
| Allowance for man‑made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 83.56 | 83.56 | 82.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl* (dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(µV/m)) | *R* = 1/2 | 18.06 | 48.18 | 57.32 | 38.97 | 47.51 | 41.26 |
| *R* = 2/3 | 20.26 | 51.18 | 60.32 | 41.97 | 50.51 | 44.36 |
| *R* = 3/4 | 21.16 | 53.38 | 62.52 | 44.17 | 52.71 | 45.66 |

TABLE 64

Minimum median field-strength level *Emed* for 100 kHz channel   
bandwidth and QPSK modulation in Band II

| Reception mode |  |  | FX | PI | PI−H | PO | PO−H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 1.20 | 6.50 | 6.50 | 6.50 | 6.50 | 5.60 |
| *R* = 2/3 | 3.40 | 9.50 | 9.50 | 9.50 | 9.50 | 8.70 |
| *R* = 3/4 | 4.30 | 11.70 | 11.70 | 11.70 | 11.70 | 10.00 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −142.78 | −137.48 | −137.48 | −137.48 | −137.48 | −138.38 |
| *R* = 2/3 | −140.58 | −134.48 | −134.48 | −134.48 | −134.48 | −135.28 |
| *R* = 3/4 | −139.68 | −132.28 | −132.28 | −132.28 | −132.28 | −133.98 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | ϕ*min* (dBW/m2) | *R*= 1/2 | −142.08 | −135.98 | −119.16 | −135.98 | −119.16 | −136.60 |
| *R*= 2/3 | −139.88 | −132.98 | −116.16 | −132.98 | −116.16 | −133.50 |
| *R* = 3/4 | −138.98 | −130.78 | −113.96 | −130.78 | −113.96 | −132.20 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(µV/m)) | *R* = 1/2 | 3.72 | 9.82 | 26.64 | 9.82 | 26.64 | 9.20 |
| *R*= 2/3 | 5.92 | 12.82 | 29.64 | 12.82 | 29.64 | 12.30 |
| *R*= 3/4 | 6.82 | 15.02 | 31.84 | 15.02 | 31.84 | 13.60 |
| Allowance for man‑made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl* (dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(µV/m)) | *R*= 1/2 | 17.23 | 50.19 | 60.63 | 40.01 | 49.91 | 42.42 |
| *R* = 2/3 | 19.43 | 53.19 | 63.63 | 43.01 | 52.91 | 45.52 |
| *R*= 3/4 | 20.33 | 55.39 | 65.83 | 45.21 | 55.11 | 46.82 |

TABLE 65

Minimum median field-strength level *Emed* for 100 kHz channel   
bandwidth and 16‑QAM modulation in Band I

| Reception mode |  |  | FX | PI | PI−H | PO | PO−H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 6.60 | 12.60 | 12.60 | 12.60 | 12.60 | 10.50 |
| *R*= 2/3 | 9.20 | 15.10 | 15.10 | 15.10 | 15.10 | 13.30 |
| *R*= 3/4 | 10.30 | 17.20 | 17.20 | 17.20 | 17.20 | 15.80 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R*= 1/2 | −137.38 | −131.38 | −131.38 | −131.38 | −131.38 | −133.48 |
| *R* = 2/3 | −134.78 | −128.88 | −128.88 | −128.88 | −128.88 | −130.68 |
| *R* = 3/4 | −133.68 | −126.78 | −126.78 | −126.78 | −126.78 | −128.18 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | ϕ*min* (dBW/m2) | *R*= 1/2 | −140.72 | −133.62 | −113.06 | −133.62 | −113.06 | −135.50 |
| *R*= 2/3 | −138.12 | −131.12 | −110.56 | −131.12 | −110.56 | −132.70 |
| *R* = 3/4 | −137.02 | −129.02 | −108.46 | −129.02 | −108.46 | −130.20 |
| Minimum field‑strength level at receiving antenna | *Emin*(dB(μV/m)) | *R* = 1/2 | 5.08 | 12.18 | 32.74 | 12.18 | 32.74 | 10.30 |
| *R* = 2/3 | 7.68 | 14.68 | 35.24 | 14.68 | 35.24 | 13.10 |
| *R*= 3/4 | 8.78 | 16.78 | 37.34 | 16.78 | 37.34 | 15.60 |
| Allowance for man-made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl* (dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb* |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(μV/m)) | *R* = 1/2 | 23.46 | 54.28 | 63.42 | 45.07 | 53.61 | 46.16 |
| *R*= 2/3 | 26.06 | 56.78 | 65.92 | 47.57 | 56.11 | 48.96 |
| *R*= 3/4 | 27.16 | 58.88 | 68.02 | 49.67 | 58.21 | 51.46 |

TABLE 66

Minimum median field-strength level *Emed* for 100 kHz channel   
bandwidth and 16‑QAM modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 |
| Minimum *C*/*N* | (*C*/*N*)*min*  (dB) | *R* = 1/2 | 6.60 | 12.60 | 12.60 | 12.60 | 12.60 | 10.50 |
| *R* = 2/3 | 9.20 | 15.10 | 15.10 | 15.10 | 15.10 | 13.30 |
| *R* = 3/4 | 10.30 | 17.20 | 17.20 | 17.20 | 17.20 | 15.80 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −137.38 | −131.38 | −131.38 | −131.38 | −131.38 | −133.48 |
| *R* = 2/3 | −134.78 | −128.88 | −128.88 | −128.88 | −128.88 | −130.68 |
| *R* = 3/4 | −133.68 | −126.78 | −126.78 | −126.78 | −126.78 | −128.18 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | ϕ*min* (dBW/m2) | *R* = 1/2 | −136.68 | −129.88 | −113.06 | −129.88 | −113.06 | −131.70 |
| *R*= 2/3 | −134.08 | −127.38 | −110.56 | −127.38 | −110.56 | −128.90 |
| *R*= 3/4 | −132.98 | −125.28 | −108.46 | −125.28 | −108.46 | −126.40 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 9.12 | 15.92 | 32.74 | 15.92 | 32.74 | 14.10 |
| *R* = 2/3 | 11.72 | 18.42 | 35.24 | 18.42 | 35.24 | 16.90 |
| *R* = 3/4 | 12.82 | 20.52 | 37.34 | 20.52 | 37.34 | 19.40 |
| Allowance for man-made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl* (dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(μV/m)) | *R* = 1/2 | 22.63 | 56.29 | 66.73 | 46.11 | 56.01 | 47.32 |
| *R* = 2/3 | 25.23 | 58.79 | 69.23 | 48.61 | 58.51 | 50.12 |
| *R*= 3/4 | 26.33 | 60.89 | 71.33 | 50.71 | 60.61 | 52.62 |

TABLE 67

Minimum median field-strength level *Emed* for 100 kHz channel   
bandwidth and 64‑QAM modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 10.90 | 16.30 | 16.30 | 16.30 | 16.30 | 14.80 |
| *R* = 2/3 | 14.20 | 19.60 | 19.60 | 19.60 | 19.60 | 18.10 |
| *R* = 3/4 | 15.60 | 22.20 | 22.20 | 22.20 | 22.20 | 20.70 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −133.08 | −127.68 | −127.68 | −127.68 | −127.68 | −129.18 |
| *R* = 2/3 | −129.78 | −124.38 | −124.38 | −124.38 | −124.38 | −125.88 |
| *R* = 3/4 | −128.38 | −121.78 | −121.78 | −121.78 | −121.78 | −123.28 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | ϕ*min* (dBW/m2) | *R* = 1/2 | −136.42 | −129.92 | −109.36 | −129.92 | −109.36 | −131.20 |
| *R* = 2/3 | −133.12 | −126.62 | −106.06 | −126.62 | −106.06 | −127.90 |
| *R* = 3/4 | −131.72 | −124.02 | −103.46 | −124.02 | −103.46 | −125.30 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 9.38 | 15.88 | 36.44 | 15.88 | 36.44 | 14.60 |
| *R* = 2/3 | 12.68 | 19.18 | 39.74 | 19.18 | 39.74 | 17.90 |
| *R* = 3/4 | 14.08 | 21.78 | 42.34 | 21.78 | 42.34 | 20.50 |
| Allowance for man-made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl* (dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field-strength level | *Emed*(dB(μV/m)) | *R* = 1/2 | 27.76 | 57.98 | 67.12 | 48.77 | 57.31 | 50.46 |
| *R*= 2/3 | 31.06 | 61.28 | 70.42 | 52.07 | 60.61 | 53.76 |
| *R* = 3/4 | 32.46 | 63.88 | 73.02 | 54.67 | 63.21 | 56.36 |

TABLE 68

Minimum median field-strength level *Emed* for 100 kHz channel   
bandwidth and 64‑QAM modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 | −146.98 |
| Minimum *C*/*N* | (*C*/*N*)*min*  (dB) | *R* = 1/2 | 10.90 | 16.30 | 16.30 | 16.30 | 16.30 | 14.80 |
| *R* = 2/3 | 14.20 | 19.60 | 19.60 | 19.60 | 19.60 | 18.10 |
| *R* = 3/4 | 15.60 | 22.20 | 22.20 | 22.20 | 22.20 | 20.70 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −133.08 | −127.68 | −127.68 | −127.68 | −127.68 | −129.18 |
| *R* = 2/3 | −129.78 | −124.38 | −124.38 | −124.38 | −124.38 | −125.88 |
| *R* = 3/4 | −128.38 | −121.78 | −121.78 | −121.78 | −121.78 | −123.28 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux-density at receiving place | ϕ*min*(dBW/m2) | *R* = 1/2 | −132.38 | −126.18 | −109.36 | −126.18 | −109.36 | −127.40 |
| *R*= 2/3 | −129.08 | −122.88 | −106.06 | −122.88 | −106.06 | −124.10 |
| *R* = 3/4 | −127.68 | −120.28 | −103.46 | −120.28 | −103.46 | −121.50 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(µV/m)) | *R* = 1/2 | 13.42 | 19.62 | 36.44 | 19.62 | 36.44 | 18.40 |
| *R* = 2/3 | 16.72 | 22.92 | 39.74 | 22.92 | 39.74 | 21.70 |
| *R*= 3/4 | 18.12 | 25.52 | 42.34 | 25.52 | 42.34 | 24.30 |
| Allowance for man‑made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl*(dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(μV/m)) | *R* = 1/2 | 26.93 | 59.99 | 70.43 | 49.81 | 59.71 | 51.62 |
| *R* = 2/3 | 30.23 | 63.29 | 73.73 | 53.11 | 63.01 | 54.92 |
| *R* = 3/4 | 31.63 | 65.89 | 76.33 | 55.71 | 65.61 | 57.52 |

TABLE 69

Minimum median field-strength level *Emed* for 200 kHz channel   
bandwidth and QPSK modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 |
| Minimum *C*/*N* | (*C*/*N*)*min*(dB) | *R* = 1/2 | 1.10 | 6.40 | 6.40 | 6.40 | 6.40 | 5.50 |
| *R* = 2/3 | 3.30 | 9.40 | 9.40 | 9.40 | 9.40 | 8.60 |
| *R* = 3/4 | 4.20 | 11.50 | 11.50 | 11.50 | 11.50 | 9.80 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −139.87 | −134.57 | −134.57 | −134.57 | −134.57 | −135.47 |
| *R*= 2/3 | −137.67 | −131.57 | −131.57 | −131.57 | −131.57 | −132.37 |
| *R*= 3/4 | −136.77 | −129.47 | −129.47 | −129.47 | −129.47 | −131.17 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | φ*min* (dBW/m2) | *R*= 1/2 | −143.21 | −136.81 | −116.25 | −136.81 | −116.25 | −137.49 |
| *R*= 2/3 | −141.01 | −133.81 | −113.25 | −133.81 | −113.25 | −134.39 |
| *R* = 3/4 | −140.11 | −131.71 | −111.15 | −131.71 | −111.15 | −133.19 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 2.59 | 8.99 | 29.55 | 8.99 | 29.55 | 8.31 |
| *R* = 2/3 | 4.79 | 11.99 | 32.55 | 11.99 | 32.55 | 11.41 |
| *R*= 3/4 | 5.69 | 14.09 | 34.65 | 14.09 | 34.65 | 12.61 |
| Allowance for man-made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl*(dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field-strength level | *Emed* (dB(μV/m)) | *R* = 1/2 | 20.97 | 51.09 | 60.23 | 41.88 | 50.42 | 44.17 |
| *R* = 2/3 | 23.17 | 54.09 | 63.23 | 44.88 | 53.42 | 47.27 |
| *R*= 3/4 | 24.07 | 56.19 | 65.33 | 46.98 | 55.52 | 48.47 |

TABLE 70

Minimum median field-strength level *Emed* for 200 kHz channel   
bandwidth and QPSK modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 1.10 | 6.40 | 6.40 | 6.40 | 6.40 | 5.50 |
| *R* = 2/3 | 3.30 | 9.40 | 9.40 | 9.40 | 9.40 | 8.60 |
| *R*= 3/4 | 4.20 | 11.50 | 11.50 | 11.50 | 11.50 | 9.80 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R*= 1/2 | −139.87 | −134.57 | −134.57 | −134.57 | −134.57 | −135.47 |
| *R* = 2/3 | −137.67 | −131.57 | −131.57 | −131.57 | −131.57 | −132.37 |
| *R* = 3/4 | −136.77 | −129.47 | −129.47 | −129.47 | −129.47 | −131.17 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | φ*min*(dBW/m2) | *R*= 1/2 | −139.17 | −133.07 | −116.25 | −133.07 | −116.25 | −133.69 |
| *R* = 2/3 | −136.97 | −130.07 | −113.25 | −130.07 | −113.25 | −130.59 |
| *R* = 3/4 | −136.07 | −127.97 | −111.15 | −127.97 | −111.15 | −129.39 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 6.63 | 12.73 | 29.55 | 12.73 | 29.55 | 12.11 |
| *R* = 2/3 | 8.83 | 15.73 | 32.55 | 15.73 | 32.55 | 15.21 |
| *R*= 3/4 | 9.73 | 17.83 | 34.65 | 17.83 | 34.65 | 16.41 |
| Allowance for man‑made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl*(dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed*(dB(µV/m)) | *R*= 1/2 | 20.14 | 53.10 | 63.54 | 42.92 | 52.82 | 45.33 |
| *R* = 2/3 | 22.34 | 56.10 | 66.54 | 45.92 | 55.82 | 48.43 |
| *R* = 3/4 | 23.24 | 58.20 | 68.64 | 48.02 | 57.92 | 49.63 |

TABLE 71

Minimum median field-strength level *Emed* for 200 kHz channel   
bandwidth and 16‑QAM modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 |
| Minimum *C*/*N* | (*C*/*N*)*min*  (dB) | *R* = 1/2 | 6.40 | 12.50 | 12.50 | 12.50 | 12.50 | 10.40 |
| *R*= 2/3 | 9.10 | 14.90 | 14.90 | 14.90 | 14.90 | 13.20 |
| *R* = 3/4 | 10.20 | 17.00 | 17.00 | 17.00 | 17.00 | 15.60 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −134.57 | −128.47 | −128.47 | −128.47 | −128.47 | −130.57 |
| *R* = 2/3 | −131.87 | −126.07 | −126.07 | −126.07 | −126.07 | −127.77 |
| *R* = 3/4 | −130.77 | −123.97 | −123.97 | −123.97 | −123.97 | −125.37 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux-density at receiving place | ϕ*min* (dBW/m2) | *R* = 1/2 | −137.91 | −130.71 | −110.15 | −130.71 | −110.15 | −132.59 |
| *R* = 2/3 | −135.21 | −128.31 | −107.75 | −128.31 | −107.75 | −129.79 |
| *R* = 3/4 | −134.11 | −126.21 | −105.65 | −126.21 | −105.65 | −127.39 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 7.89 | 15.09 | 35.65 | 15.09 | 35.65 | 13.21 |
| *R* = 2/3 | 10.59 | 17.49 | 38.05 | 17.49 | 38.05 | 16.01 |
| *R* = 3/4 | 11.69 | 19.59 | 40.15 | 19.59 | 40.15 | 18.41 |
| Allowance for man‑made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b*(dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl*(dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh*(dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb*(dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed*(dB(μV/m)) | *R* = 1/2 | 26.27 | 57.19 | 66.33 | 47.98 | 56.52 | 49.07 |
| *R* = 2/3 | 28.97 | 59.59 | 68.73 | 50.38 | 58.92 | 51.87 |
| *R* = 3/4 | 30.07 | 61.69 | 70.83 | 52.48 | 61.02 | 54.27 |

TABLE 72

Minimum median field-strength level *Emed* for 200 kHz channel   
bandwidth and 16‑QAM modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 6.40 | 12.50 | 12.50 | 12.50 | 12.50 | 10.40 |
| *R* = 2/3 | 9.10 | 14.90 | 14.90 | 14.90 | 14.90 | 13.20 |
| *R* = 3/4 | 10.20 | 17.00 | 17.00 | 17.00 | 17.00 | 15.60 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps min* (dBW) | *R* = 1/2 | −134.57 | −128.47 | −128.47 | −128.47 | −128.47 | −130.57 |
| *R* = 2/3 | −131.87 | −126.07 | −126.07 | −126.07 | −126.07 | −127.77 |
| *R* = 3/4 | −130.77 | −123.97 | −123.97 | −123.97 | −123.97 | −125.37 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | φ*min* (dBW/m2) | *R* = 1/2 | −133.87 | −126.97 | −110.15 | −126.97 | −110.15 | −128.79 |
| *R*= 2/3 | −131.17 | −124.57 | −107.75 | −124.57 | −107.75 | −125.99 |
| *R* = 3/4 | −130.07 | −122.47 | −105.65 | −122.47 | −105.65 | −123.59 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 11.93 | 18.83 | 35.65 | 18.83 | 35.65 | 17.01 |
| *R* = 2/3 | 14.63 | 21.23 | 38.05 | 21.23 | 38.05 | 19.81 |
| *R* = 3/4 | 15.73 | 23.33 | 40.15 | 23.33 | 40.15 | 22.21 |
| Allowance for man-made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl*(dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed*(dB(μV/m)) | *R* = 1/2 | 25.44 | 59.20 | 69.64 | 49.02 | 58.92 | 50.23 |
| *R* = 2/3 | 28.14 | 61.60 | 72.04 | 51.42 | 61.32 | 53.03 |
| *R* = 3/4 | 29.24 | 63.70 | 74.14 | 53.52 | 63.42 | 55.43 |

TABLE 73

Minimum median field-strength level *Emed* for 200 kHz channel   
bandwidth and 64‑QAM modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 10.80 | 16.20 | 16.20 | 16.20 | 16.20 | 14.70 |
| *R* = 2/3 | 14.00 | 19.40 | 19.40 | 19.40 | 19.40 | 17.90 |
| *R* = 3/4 | 15.40 | 22.00 | 22.00 | 22.00 | 22.00 | 20.50 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −130.17 | −124.77 | −124.77 | −124.77 | −124.77 | −126.27 |
| *R*= 2/3 | −126.97 | −121.57 | −121.57 | −121.57 | −121.57 | −123.07 |
| *R*= 3/4 | −125.57 | −118.97 | −118.97 | −118.97 | −118.97 | −120.47 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | ϕ*min*(dBW/m2) | *R* = 1/2 | −133.51 | −127.01 | −106.45 | −127.01 | −106.45 | −128.29 |
| *R* = 2/3 | −130.31 | −123.81 | −103.25 | −123.81 | −103.25 | −125.09 |
| *R* = 3/4 | −128.91 | −121.21 | −100.65 | −121.21 | −100.65 | −122.49 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 12.29 | 18.79 | 39.35 | 18.79 | 39.35 | 17.51 |
| *R* = 2/3 | 15.49 | 21.99 | 42.55 | 21.99 | 42.55 | 20.71 |
| *R* = 3/4 | 16.89 | 24.59 | 45.15 | 24.59 | 45.15 | 23.31 |
| Allowance for man‑made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl*(dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 815.00 | 8.00 | 8.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(μV/m)) | *R* = 1/2 | 30.67 | 60.89 | 70.03 | 51.68 | 60.22 | 53.37 |
| *R* = 2/3 | 33.87 | 64.09 | 73.23 | 54.88 | 63.42 | 56.57 |
| *R*= 3/4 | 35.27 | 66.69 | 75.83 | 57.48 | 66.02 | 59.17 |

TABLE 74

Minimum median field-strength level *Emed* for 200 kHz channel   
bandwidth and 64‑QAM modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 | −143.97 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R*= 1/2 | 10.80 | 16.20 | 16.20 | 16.20 | 16.20 | 14.70 |
| *R* = 2/3 | 14.00 | 19.40 | 19.40 | 19.40 | 19.40 | 17.90 |
| *R* = 3/4 | 15.40 | 22.00 | 22.00 | 22.00 | 22.00 | 20.50 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −130.17 | −124.77 | −124.77 | −124.77 | −124.77 | −126.27 |
| *R*= 2/3 | −126.97 | −121.57 | −121.57 | −121.57 | −121.57 | −123.07 |
| *R* = 3/4 | −125.57 | −118.97 | −118.97 | −118.97 | −118.97 | −120.47 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | φ*min* (dBW/m2) | *R* = 1/2 | −129.47 | −123.27 | −106.45 | −123.27 | −106.45 | −124.49 |
| *R* = 2/3 | −126.27 | −120.07 | −103.25 | −120.07 | −103.25 | −121.29 |
| *R* = 3/4 | −124.87 | −117.47 | −100.65 | −117.47 | −100.65 | −118.69 |
| Minimum field-strength level at receiving antenna | *Emin*(dB(µV/m)) | *R* = 1/2 | 16.33 | 22.53 | 39.35 | 22.53 | 39.35 | 21.31 |
| *R* = 2/3 | 19.53 | 25.73 | 42.55 | 25.73 | 42.55 | 24.51 |
| *R* = 3/4 | 20.93 | 28.33 | 45.15 | 28.33 | 45.15 | 27.11 |
| Allowance for man-made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | µ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl*(dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dBµV/m) | *R* = 1/2 | 29.84 | 62.90 | 73.34 | 52.72 | 62.62 | 54.53 |
| *R*= 2/3 | 33.04 | 66.10 | 76.54 | 55.92 | 65.82 | 57.73 |
| *R* = 3/4 | 34.44 | 68.70 | 79.14 | 58.52 | 68.42 | 60.33 |

TABLE 75

Minimum median field-strength level *Emed* for 250 kHz channel   
bandwidth and QPSK modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 |
| Minimum *C*/*N* | (*C*/*N*)*min*  (dB) | *R* = 1/2 | 1.10 | 6.40 | 6.40 | 6.40 | 6.40 | 5.50 |
| *R =* 2/3 | 3.20 | 9.40 | 9.40 | 9.40 | 9.40 | 8.50 |
| *R* = 3/4 | 4.20 | 11.50 | 11.50 | 11.50 | 11.50 | 9.80 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min*  (dBW) | *R* = 1/2 | −138.90 | −133.60 | −133.60 | −133.60 | −133.60 | −134.50 |
| *R* = 2/3 | −136.80 | −130.60 | −130.60 | −130.60 | −130.60 | −131.50 |
| *R* = 3/4 | −135.80 | −128.50 | −128.50 | −128.50 | −128.50 | −130.20 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | ϕ*min*(dBW/m2) | *R* = 1/2 | −142.24 | −135.84 | −115.28 | −135.84 | −115.28 | −136.52 |
| *R* = 2/3 | −140.14 | −132.84 | −112.28 | −132.84 | −112.28 | −133.52 |
| *R* = 3/4 | −139.14 | −130.74 | −110.18 | −130.74 | −110.18 | −132.22 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 3.56 | 9.96 | 30.52 | 9.96 | 30.52 | 9.28 |
| *R* = 2/3 | 5.66 | 12.96 | 33.52 | 12.96 | 33.52 | 12.28 |
| *R* = 3/4 | 6.66 | 15.06 | 35.62 | 15.06 | 35.62 | 13.58 |
| Allowance for man-made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl* (dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed*(dB(μV/m)) | *R* = 1/2 | 21.93 | 52.06 | 61.20 | 42.85 | 51.39 | 45.14 |
| *R* = 2/3 | 24.03 | 55.06 | 64.20 | 45.85 | 54.39 | 48.14 |
| *R* = 3/4 | 25.03 | 57.16 | 66.30 | 47.95 | 56.49 | 49.44 |

TABLE 76

Minimum median field-strength level *Emed* for 250 kHz channel   
bandwidth and QPSK modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 |
| Minimum *C*/*N* | (*C*/*N*)*min* (dB) | *R* = 1/2 | 1.10 | 6.40 | 6.40 | 6.40 | 6.40 | 5.50 |
| *R* = 2/3 | 3.20 | 9.40 | 9.40 | 9.40 | 9.40 | 8.50 |
| *R* = 3/4 | 4.20 | 11.50 | 11.50 | 11.50 | 11.50 | 9.80 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min*  (dBW) | *R* = 1/2 | −138.90 | −133.60 | −133.60 | −133.60 | −133.60 | −134.50 |
| *R* = 2/3 | −136.80 | −130.60 | −130.60 | −130.60 | −130.60 | −131.50 |
| *R* = 3/4 | −135.80 | −128.50 | −128.50 | −128.50 | −128.50 | −130.20 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | ϕ*min*(dBW/m2) | *R* = 1/2 | −138.20 | −132.10 | −115.28 | −132.10 | −115.28 | −132.72 |
| *R* = 2/3 | −136.10 | −129.10 | −112.28 | −129.10 | −112.28 | −129.72 |
| *R* = 3/4 | −135.10 | −127.00 | −110.18 | −127.00 | −110.18 | −128.42 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 7.60 | 13.70 | 30.52 | 13.70 | 30.52 | 13.08 |
| *R* = 2/3 | 9.70 | 16.70 | 33.52 | 16.70 | 33.52 | 16.08 |
| *R*= 3/4 | 10.70 | 18.80 | 35.62 | 18.80 | 35.62 | 17.38 |
| Allowance for man-made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl* (dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 170.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed*(dB(μV/m)) | *R* = 1/2 | 21.11 | 54.07 | 64.51 | 43.89 | 53.79 | 46.30 |
| *R* = 2/3 | 23.21 | 57.07 | 67.51 | 46.89 | 56.79 | 49.30 |
| *R* = 3/4 | 24.21 | 59.17 | 69.61 | 48.99 | 58.89 | 50.60 |

TABLE 77

Minimum median field-strength level *Emed* for 250 kHz channel   
bandwidth and 16‑QAM modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 |
| Minimum *C*/*N* | (*C*/*N*)*min*  (dB) | *R* = 1/2 | 6.30 | 12.40 | 12.40 | 12.40 | 12.40 | 10.30 |
| *R* = 2/3 | 9.10 | 14.90 | 14.90 | 14.90 | 14.90 | 13.20 |
| *R* = 3/4 | 10.20 | 17.00 | 17.00 | 17.00 | 17.00 | 15.60 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min* (dBW) | *R* = 1/2 | −133.70 | −127.60 | −127.60 | −127.60 | −127.60 | −129.70 |
| *R* = 2/3 | −130.90 | −125.10 | −125.10 | −125.10 | −125.10 | −126.80 |
| *R* = 3/4 | −129.80 | −123.00 | −123.00 | −123.00 | −123.00 | −124.40 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | ϕ*min*(dBW/m2) | *R* = 1/2 | −137.04 | −129.84 | −109.28 | −129.84 | −109.28 | −131.72 |
| *R* = 2/3 | −134.24 | −127.34 | −106.78 | −127.34 | −106.78 | −128.82 |
| *R* = 3/4 | −133.14 | −125.24 | −104.68 | −125.24 | −104.68 | −126.42 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 8.76 | 15.96 | 36.52 | 15.96 | 36.52 | 14.08 |
| *R* = 2/3 | 11.56 | 18.46 | 39.02 | 18.46 | 39.02 | 16.98 |
| *R* = 3/4 | 12.66 | 20.56 | 41.12 | 20.56 | 41.12 | 19.38 |
| Allowance for man-made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl*(dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed*(dB(μV/m)) | *R* = 1/2 | 27.13 | 58.06 | 67.20 | 48.85 | 57.39 | 49.94 |
| *R* = 2/3 | 29.93 | 60.56 | 69.70 | 51.35 | 59.89 | 52.84 |
| *R* = 3/4 | 31.03 | 62.66 | 71.80 | 53.45 | 61.99 | 55.24 |

TABLE 78

Minimum median field-strength level *Emed* for 250 kHz channel   
bandwidth and 16‑QAM modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 |
| Minimum *C*/*N* | (*C*/*N*)*min*(dB) | *R* = 1/2 | 6.30 | 12.40 | 12.40 | 12.40 | 12.40 | 10.30 |
| *R* = 2/3 | 9.10 | 14.90 | 14.90 | 14.90 | 14.90 | 13.20 |
| *R* = 3/4 | 10.20 | 17.00 | 17.00 | 17.00 | 17.00 | 15.60 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min*  (dBW) | *R* = 1/2 | −133.70 | −127.60 | −127.60 | −127.60 | −127.60 | −129.70 |
| *R* = 2/3 | −130.90 | −125.10 | −125.10 | −125.10 | −125.10 | −126.80 |
| *R* = 3/4 | −129.80 | −123.00 | −123.00 | −123.00 | −123.00 | −124.40 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | φ*min*(dBW/m2) | *R* = 1/2 | −133.00 | −126.10 | −109.28 | −126.10 | −109.28 | −127.92 |
| *R* = 2/3 | −130.20 | −123.60 | −106.78 | −123.60 | −106.78 | −125.02 |
| *R* = 3/4 | −129.10 | −121.50 | −104.68 | −121.50 | −104.68 | −122.62 |
| Minimum field-strength level at receiving antenna | *Emin*(dB(µV/m)) | *R* = 1/2 | 12.80 | 19.70 | 36.52 | 19.70 | 36.52 | 17.88 |
| *R* = 2/3 | 15.60 | 22.20 | 39.02 | 22.20 | 39.02 | 20.78 |
| *R*= 3/4 | 16.70 | 24.30 | 41.12 | 24.30 | 41.12 | 23.18 |
| Allowance for man-made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl*(dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed*  (dB(µV/m)) | *R* = 1/2 | 26.31 | 60.07 | 70.51 | 49.89 | 59.79 | 51.10 |
| *R* = 2/3 | 29.11 | 62.57 | 73.01 | 52.39 | 62.29 | 54.00 |
| *R* = 3/4 | 30.21 | 64.67 | 75.11 | 54.49 | 64.39 | 56.40 |

TABLE 79

Minimum median field-strength level *Emed* for 250 kHz channel   
bandwidth and 64‑QAM modulation in Band I

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 |
| Minimum *C*/*N* | (*C*/*N*)*min*  (dB) | *R* = 1/2 | 10.60 | 16.10 | 16.10 | 16.10 | 16.10 | 14.60 |
| *R* = 2/3 | 14.00 | 19.40 | 19.40 | 19.40 | 19.40 | 17.90 |
| *R* = 3/4 | 15.40 | 22.00 | 22.00 | 22.00 | 22.00 | 20.50 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min*  (dBW) | *R*= 1/2 | −129.40 | −123.90 | −123.90 | −123.90 | −123.90 | −125.40 |
| *R* = 2/3 | −126.00 | −120.60 | −120.60 | −120.60 | −120.60 | −122.10 |
| *R* = 3/4 | −124.60 | −118.00 | −118.00 | −118.00 | −118.00 | −119.50 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −22.76 | −2.20 | −22.76 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 4.44 | 2.24 | −18.32 | 2.24 | −18.32 | 2.24 |
| Feeder-loss | *Lf* (dB) |  | 1.10 | 0.00 | 0.00 | 0.00 | 0.00 | 0.22 |
| Minimum power flux‑density at receiving place | ϕ*min* (dBW/m2) | *R*= 1/2 | −132.74 | −126.14 | −105.58 | −126.14 | −105.58 | −127.42 |
| *R*= 2/3 | −129.34 | −122.84 | −102.28 | −122.84 | −102.28 | −124.12 |
| *R* = 3/4 | −127.94 | −120.24 | −99.68 | −120.24 | −99.68 | −121.52 |
| Minimum field-strength level at receiving antenna | *Emin* (dB(μV/m)) | *R* = 1/2 | 13.06 | 19.66 | 40.22 | 19.66 | 40.22 | 18.38 |
| *R* = 2/3 | 16.46 | 22.96 | 43.52 | 22.96 | 43.52 | 21.68 |
| *R*= 3/4 | 17.86 | 25.56 | 46.12 | 25.56 | 46.12 | 24.28 |
| Allowance for man-made noise | *PMMN* (dB) |  | 15.38 | 15.38 | 0.00 | 15.38 | 0.00 | 15.38 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.56 | 3.56 | 3.56 | 3.56 | 3.56 | 2.86 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b* (dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.76 | 6.50 | 4.66 | 5.76 | 3.56 | 5.36 |
| Location correction factor | *Cl*(dB) |  | 3.00 | 10.72 | 7.68 | 9.51 | 5.87 | 12.48 |
| Antenna height loss | *Lh* (dB) |  | 0.00 | 8.00 | 815.00 | 8.00 | 815.00 | 8.00 |
| Building penetration loss | *Lb* (dB) |  | 0.00 | 98.00 | 98.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(μV/m)) | *R* = 1/2 | 31.43 | 61.76 | 70.90 | 52.55 | 61.09 | 54.24 |
| *R* = 2/3 | 34.83 | 65.06 | 74.20 | 55.85 | 64.39 | 57.54 |
| *R* = 3/4 | 36.23 | 67.66 | 76.80 | 58.45 | 66.99 | 60.14 |

TABLE 80

Minimum median field-strength level *Emed* for 250 kHz channel   
bandwidth and 64‑QAM modulation in Band II

| Reception mode |  |  | FX | PI | PI-H | PO | PO-H | MO |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Receiver noise figure | *F* (dB) |  | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 | 7.00 |
| Receiver noise input power | *Pn* (dBW) |  | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 | −143.00 |
| Minimum *C*/*N* | (*C*/*N*)*min*  (dB) | *R* = 1/2 | 10.60 | 16.10 | 16.10 | 16.10 | 16.10 | 14.60 |
| *R*= 2/3 | 14.00 | 19.40 | 19.40 | 19.40 | 19.40 | 17.90 |
| *R* = 3/4 | 15.40 | 22.00 | 22.00 | 22.00 | 22.00 | 20.50 |
| Implementation loss | *Li* (dB) |  | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 | 3.00 |
| Minimum receiver input power level | *Ps,min*  (dBW) | *R* = 1/2 | −129.40 | −123.90 | −123.90 | −123.90 | −123.90 | −125.40 |
| *R* = 2/3 | −126.00 | −120.60 | −120.60 | −120.60 | −120.60 | −122.10 |
| *R* = 3/4 | −124.60 | −118.00 | −118.00 | −118.00 | −118.00 | −119.50 |
| Antenna gain | *Gd* (dBd) |  | 0.00 | −2.20 | −19.02 | −2.20 | −19.02 | −2.20 |
| Effective antenna aperture | *Aa* (dBm2) |  | 0.70 | −1.50 | −18.32 | −1.50 | −18.32 | −1.50 |
| Feeder-loss | *Lf* (dB) |  | 1.40 | 0.00 | 0.00 | 0.00 | 0.00 | 0.28 |
| Minimum power flux‑density at receiving place | ϕ*min*(dBW/m2) | *R* = 1/2 | −128.70 | −122.40 | −105.58 | −122.40 | −105.58 | −123.62 |
| *R* = 2/3 | −125.30 | −119.10 | −102.28 | −119.10 | −102.28 | −120.32 |
| *R* = 3/4 | −123.90 | −116.50 | −99.68 | −116.50 | −99.68 | −117.72 |
| Minimum field-strength level at receiving antenna | *Emin*(dB(μV/m)) | *R* = 1/2 | 17.10 | 23.40 | 40.22 | 23.40 | 40.22 | 22.18 |
| *R* = 2/3 | 20.50 | 26.70 | 43.52 | 26.70 | 43.52 | 25.48 |
| *R* = 3/4 | 21.90 | 29.30 | 46.12 | 29.30 | 46.12 | 28.08 |
| Allowance for man-made noise | *PMMN* (dB) |  | 10.43 | 10.43 | 0.00 | 10.43 | 0.00 | 10.43 |
| Location probability | *p* (%) |  | 70.00 | 95.00 | 95.00 | 95.00 | 95.00 | 99.00 |
| Distribution factor | μ |  | 0.52 | 1.65 | 1.65 | 1.65 | 1.65 | 2.33 |
| Standard deviation of field strength | σ*m* (dB) |  | 3.80 | 3.80 | 3.80 | 3.80 | 3.80 | 3.10 |
| Standard deviation of man-made noise | σ*MMN* (dB) |  | 4.53 | 4.53 | 0.00 | 4.53 | 0.00 | 4.53 |
| Standard deviation of building penetration loss | σ*b*(dB) |  | 0.00 | 3.00 | 3.00 | 0.00 | 0.00 | 0.00 |
| Combined standard deviation of field strength | σ*c* (dB) |  | 5.91 | 6.63 | 4.84 | 5.91 | 3.80 | 5.49 |
| Location correction factor | *Cl* (dB) |  | 3.07 | 10.94 | 7.99 | 9.76 | 6.27 | 12.79 |
| Antenna height loss | *Lh* |  | 0.00 | 10.00 | 17.00 | 10.00 | 17.00 | 10.00 |
| Building penetration loss | *Lb* |  | 0.00 | 9.00 | 9.00 | 0.00 | 0.00 | 0.00 |
| Minimum median field‑strength level | *Emed* (dB(μV/m)) | *R* = 1/2 | 30.61 | 63.77 | 74.21 | 53.59 | 63.49 | 55.40 |
| *R* = 2/3 | 34.01 | 67.07 | 77.51 | 56.89 | 66.79 | 58.70 |
| *R*= 3/4 | 35.41 | 69.67 | 80.11 | 59.49 | 69.39 | 61.30 |

### 5.3.2 Out-of-band emissions

The spectrum masks for RAVIS transmission (for three types of channel bandwidth) [10] compared to spectrum mask for analogue FM (according to ETSI EN 302 018-2 [7]) are given in Tables 81 to 84 and Fig. 3. RAVIS spectrum masks are fitting into analogue FM spectrum mask.

TABLE 81

Spectrum mask for FM transmission

|  |  |
| --- | --- |
| Frequency offset (kHz) | Level (dBc)/(1 kHz) |
| 0 | 0 |
| ±100 | 0 |
| ±200 | −80 |
| ±300 | −85 |
| ±400 | −85 |

TABLE 82

Spectrum mask for RAVIS transmission, 100 kHz channel bandwidth

|  |  |
| --- | --- |
| Frequency offset (kHz) | Level (dBc)/(1 kHz) |
| 0 | −20 |
| ±50 | −20 |
| ±70 | −50 |
| ±100 | −70 |
| ±200 | −80 |
| ±300 | −85 |
| ±400 | −85 |

TABLE 83

Spectrum mask for RAVIS transmission, 200 kHz channel bandwidth

|  |  |
| --- | --- |
| Frequency offset (kHz) | Level (dBc)/(1 kHz) |
| 0 | −23 |
| ±100 | −23 |
| ±120 | −50 |
| ±150 | −70 |
| ±200 | −80 |
| ±300 | −85 |
| ±400 | −85 |


TABLE 84

Spectrum mask for RAVIS transmission, 250 kHz channel bandwidth

|  |  |
| --- | --- |
| Frequency offset (kHz) | Level (dBc)/(1 kHz) |
| 0 | −24 |
| ±125 | −24 |
| ±145 | −50 |
| ±175 | −70 |
| ±200 | −80 |
| ±300 | −85 |
| ±400 | −85 |

Figure 3

Spectrum mask for RAVIS and FM transmission



### 5.3.3 Protection ratios

#### 5.3.3.1 Protection ratios for FM

Basic protection ratios for FM interfered with by RAVIS are given in Table 85.

TABLE 85

Basic protection ratios *PRbasic* for FM interfered with by RAVIS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 | ±300 | ±400 |
| Basic protection ratio, channel bandwidth *B* = 100 kHz | *PRbasic* (dB) | 50 | 35 | 5 | −5 | −10 |
| Basic protection ratio, channel bandwidth *B* = 200 kHz | *PRbasic* (dB) | 50 |  |  |  |  |
| Basic protection ratio, channel bandwidth *B* = 250 kHz | *PRbasic* (dB) | 50 |  |  |  |  |

#### 5.3.3.2 Protection ratios for RAVIS

Basic protection ratios for RAVIS interfered with by RAVIS are given in Table 86.

TABLE 86

Basic protection ratios *PRbasic* for RAVIS interfered with by RAVIS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 | ±300 | ±400 |
| B = 100 kHz, QPSK, R = 1/2 | *PRbasic* (dB) | 8 | 0 | −48 | −55 | −56 |
| B = 100 kHz, QPSK, R = 2/3 | *PRbasic* (dB) | 9 | 2 | −47 | −54 | −55 |
| B = 100 kHz, QPSK, R = 3/4 | *PRbasic* (dB) | 10 | 3 | −46 | −53 | −54 |
| B = 100 kHz, 16-QAM, R = 1/2 | *PRbasic* (dB) | 12 | 6 | −43 | −51 | −52 |
| B = 100 kHz, 16-QAM, R = 2/3 | *PRbasic* (dB) | 14 | 8 | −41 | −49 | −50 |
| B = 100 kHz, 16-QAM, R = 3/4 | *PRbasic* (dB) | 15 | 9 | −40 | −48 | −49 |
| B = 100 kHz, 64-QAM, R = 1/2 | *PRbasic* (dB) | 16 | 10 | −39 | −47 | −48 |
| B = 100 kHz, 64-QAM, R = 2/3 | *PRbasic* (dB) | 19 | 13 | −36 | −44 | −45 |
| B = 100 kHz, 64-QAM, R = 3/4 | *PRbasic* (dB) | 20 | 14 | −35 | −43 | −44 |
| B = 200 kHz, QPSK, R = 1/2 | *PRbasic* (dB) | 8 | 6 | −22 | −51 | −54 |
| B = 200 kHz, QPSK, R = 2/3 | *PRbasic* (dB) | 9 | 7 | −6 | −50 | −53 |
| B = 200 kHz, QPSK, R = 3/4 | *PRbasic* (dB) | 10 | 8 | −1 | −49 | −52 |
| B = 200 kHz, 16-QAM, R = 1/2 | *PRbasic* (dB) | 12 | 10 | 2 | −47 | −49 |
| B = 200 kHz, 16-QAM, R = 2/3 | *PRbasic* (dB) | 14 | 12 | 5 | −45 | −48 |
| B = 200 kHz, 16-QAM, R = 3/4 | *PRbasic* (dB) | 15 | 13 | 6 | −44 | −47 |
| B = 200 kHz, 64-QAM, R = 1/2 | *PRbasic* (dB) | 16 | 14 | 7 | −42 | −46 |
| B = 200 kHz, 64-QAM, R = 2/3 | *PRbasic* (dB) | 19 | 17 | 10 | −39 | −43 |
| B = 200 kHz, 64-QAM, R = 3/4 | *PRbasic* (dB) | 20 | 18 | 11 | −38 | −41 |
| B = 250 kHz, QPSK, R = 1/2 | *PRbasic* (dB) | 8 | 6 | 2 | −47 | −52 |
| B = 250 kHz, QPSK, R = 2/3 | *PR*basic (dB) | 9 | 7 | 3 | −46 | −51 |
| B = 250 kHz, QPSK, R = 3/4 | *PRbasic* (dB) | 10 | 8 | 5 | −44 | −50 |
| B = 250 kHz, 16-QAM, R = 1/2 | *PRbasic* (dB) | 12 | 10 | 7 | −41 | −48 |
| B = 250 kHz, 16-QAM, R = 2/3 | *PRbasic* (dB) | 14 | 12 | 9 | −35 | −46 |

TABLE 86 (*end*)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 | ±300 | ±400 |
| B = 250 kHz, 16-QAM, R = 3/4 | *PRbasic* (dB) | 15 | 13 | 10 | −32 | −45 |
| B = 250 kHz, 64-QAM, R = 1/2 | *PRbasic* (dB) | 16 | 14 | 11 | −30 | −44 |
| B = 250 kHz, 64-QAM, R = 2/3 | *PRbasic* (dB) | 19 | 17 | 14 | −24 | −41 |
| B = 250 kHz, 64-QAM, R = 3/4 | *PRbasic* (dB) | 20 | 18 | 15 | −23 | −40 |

Basic protection ratios for RAVIS interfered with by FM are given in Table 87.

TABLE 87

Basic protection ratios *PRbasic* for RAVIS interfered with by RAVIS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Frequency offset (kHz) | | 0 | ±100 | ±200 | ±300 | ±400 |
| B = 100 kHz, QPSK, R = 1/2 | *PRbasic* (dB) | 8 | 28 | 20 | −55 | −56 |
| B = 100 kHz, QPSK, R = 2/3 | *PRbasic* (dB) | 9 | 29 | 22 | −54 | −55 |
| B = 100 kHz, QPSK, R = 3/4 | *PRbasic* (dB) | 10 | 30 | 23 | −53 | −54 |
| B = 100 kHz, 16-QAM, R = 1/2 | *PRbasic* (dB) | 12 | 29 | 25 | −51 | −52 |
| B = 100 kHz, 16-QAM, R = 2/3 | *PRbasic* (dB) | 14 | 26 | 27 | −49 | −50 |
| B = 100 kHz, 16-QAM, R = 3/4 | *PRbasic* (dB) | 15 | 25 | 28 | −48 | −49 |
| B = 100 kHz, 64-QAM, R = 1/2 | *PRbasic* (dB) | 16 | 24 | 29 | −47 | −48 |
| B = 100 kHz, 64-QAM, R = 2/3 | *PRbasic* (dB) | 19 | 21 | 32 | −44 | −45 |
| B = 100 kHz, 64-QAM, R = 3/4 | *PRbasic* (dB) | 20 | 20 | 33 | −43 | −44 |
| B = 200 kHz, QPSK, R = 1/2 | *PRbasic* (dB) | 8 | 30 | 26 | −51 | −54 |
| B = 200 kHz, QPSK, R = 2/3 | *PRbasic* (dB) | 9 | 31 | 27 | −49 | −53 |
| B = 200 kHz, QPSK, R = 3/4 | *PRbasic* (dB) | 10 | 32 | 28 | −48 | −51 |
| B = 200 kHz, 16-QAM, R = 1/2 | *PRbasic* (dB) | 12 | 34 | 30 | −46 | −49 |
| B = 200 kHz, 16-QAM, R = 2/3 | *PRbasic* (dB) | 14 | 36 | 32 | −45 | −47 |
| B = 200 kHz, 16-QAM, R = 3/4 | *PRbasic* (dB) | 15 | 37 | 33 | −44 | −46 |
| B = 200 kHz, 64-QAM, R = 1/2 | *PRbasic* (dB) | 16 | 38 | 34 | −43 | −45 |
| B = 200 kHz, 64-QAM, R = 2/3 | *PRbasic* (dB) | 19 | 41 | 37 | −40 | −42 |
| B = 200 kHz, 64-QAM, R = 3/4 | *PRbasic* (dB) | 20 | 42 | 38 | −39 | −39 |
| B = 250 kHz, QPSK, R = 1/2 | *PRbasic* (dB) | 8 | 30 | 27 | −45 | −52 |
| B = 250 kHz, QPSK, R = 2/3 | *PRbasic* (dB) | 9 | 31 | 28 | 7 | −51 |
| B = 250 kHz, QPSK, R = 3/4 | *PRbasic* (dB) | 10 | 32 | 29 | 16 | −50 |
| B = 250 kHz, 16-QAM, R = 1/2 | *PRbasic* (dB) | 12 | 34 | 31 | 20 | −48 |
| B = 250 kHz, 16-QAM, R = 2/3 | *PRbasic* (dB) | 14 | 36 | 33 | 23 | −46 |
| B = 250 kHz, 16-QAM, R = 3/4 | *PRbasic* (dB) | 15 | 37 | 34 | 24 | −45 |
| B = 250 kHz, 64-QAM, R = 1/2 | *PRbasic* (dB) | 16 | 38 | 35 | 25 | −44 |
| B = 250 kHz, 64-QAM, R = 2/3 | *PRbasic* (dB) | 19 | 41 | 38 | 28 | −41 |
| B = 250 kHz, 64-QAM, R = 3/4 | *PRbasic* (dB) | 20 | 42 | 39 | 30 | −40 |

### 5.3.4 Sharing criteria with other services

The potential interference from RAVIS to the services in adjacent frequency ranges (for example, to aeronautical radionavigation service in the band above 108.0 MHz) is not higher as the one of analogue FM service.

# 6 Planning parameters for Digital System C (HD Radio) in VHF Band II

The HD Radio hybrid configuration makes use of the existing VHF Band II allocations and embeds new audio and data services along with the existing analogue FM. The In-Band On-Channel (IBOC) implementation preserves the analogue broadcast located on the main frequency assignment and adds low-level digital signals immediately adjacent to the analogue signal. These digital signals, immediately adjacent to the analogue, may be on either side of the analogue signal or on both sides. This approach is defined as System C in Recommendation ITU-R BS.1114.

IBOC, as implemented by the HD Radio system, retains the power of the analogue signal, while adding digital carriers within a controlled bandwidth and at lower power levels. This design allows for adjustment of the bandwidth and power of the digital signal, making possible controllable trade‑offs between coverage of the digital signal and adjacent channel availability.

For the purpose of deploying the HD Radio FM system in the VHF Band II, certain reception performance may be considered.

This Report provides a summary of requirements in order to allow for adequate reception performance. The analysis follows the guidance in the applicable requirements documents. As a complementary measure and where applicable, the analysis follows other applicable guiding documents and practices from ITU Regions 1, 2, 3, and from the USA.

## 6.1 HD Radio system parameters

The HD Radio system is designed to allow for numerous configurations. The configurations allow for different bandwidth settings, frequency positioning, band combining, and different throughput. These configurations are captured in standard documents, such as NRSC-5-D or other design documents. While the system has provision for several configurations, only a subset is initially implemented and proposed for deployment in ITU Regions 1, 2 and 3. However, at a future time, additional configurations may be implemented as suitable for one location or another. A subset of these configurations is briefly described in the present document in conjunction with the provided planning parameters and deployment aspects.

### 6.1.1 System configurations

This analysis includes the configurations that are considered suitable for initial deployment in ITU Regions 1, 2 and 3. At a future time, additional configurations may be considered for deployment in ITU Regions 1, 2 and 3. The analysis can then be expanded to include such additional configurations.

The system can be configured to use a single frequency block that employs 70-kHz digital signal bandwidth or a single frequency block that employs 100-kHz digital signal bandwidth. The configuration is defined by system modes, and provides various combinations of logical channels, bit rates, and protection levels.

When configured to use a single frequency block that employs 70-kHz bandwidth, the system may be configured by mode MP9. It then employs logical channel P1 and provides a throughput (net bit rate) of 98.3 kbit/s. The employed modulation is QPSK.

When configured to use a single frequency block that employs 100-kHz bandwidth, the system may be configured to mode MP12 or mode MP19, which allows for a trade‑off between throughput (net bit rate) and robustness. When configured to mode MP12, the system employs logical channel P1 and provides a throughput (net bit rate) of 98.3 kbit/s. When configured to mode MP19, the system employs logical channels P1 and P3, and provides a throughput (net bit rate) of 122.9 kbit/s. The employed modulation is QPSK.

The HD Radio system also supports joint configurations of two digital bands. These two digital bands are treated as two independent signals, in the context of planning, sharing, and compatibility for Band II. The joint configurations provide higher robustness or otherwise support higher throughput (net bit rate). When configured to use 2 × 70-kHz bandwidth, the system may be configured by mode MP1. It then employs logical channel P1 and provides a throughput (net bit rate) of 98.3 kbit/s. When configured to use 2 × 100-kHz bandwidth, the system may be configured by mode MP11. It then employs logical channels P1, P3 and P4, and provides a throughput (net bit rate) of 147.5 kbit/s.

The essential characteristics of the HD Radio system configurations (operating modes) are summarized in Table 88.

TABLE 88

Characteristics of various HD radio system operating modes

| System mode | Used BW (kHz) | Total (1) bit rate | Channel P1 | | Channel P3 | | Channel P4 | | Comments |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Code rate | Bit (1) rate | Code rate | Bit (1) rate | Code rate | Bit (1) rate | Interleaver span |
| MP9 | 70 | 98.3 | 4/5 | 98.3 | – | – | – | – | P1: ~1.5s |
| MP12 | 100 | 98.3 | 4/7 | 98.3 | – | – | – | – | P1: ~1.5s; additional diversity delay |
| MP19 | 100 | 122.9 | 4/5 | 98.3 | 1/2 | 24.6 | – | – | P1: ~1.5s;  P3: ~3s |
| MP1(2) | 2× 70 | 98.3 | 2/5 | 98.3 | – | – | – | – | P1: ~1.5s |
| MP11(2) | 2× 100 | 147.5 | 2/5 | 98.3 | 1/2 | 24.6 | 1/2 | 24.6 | P1: ~1.5s;  P3/P4: ~3s |
| (1) The bit rates reflect the throughput (‘net’ bit rate) by the application layer, and do not include the overhead used by the physical layer.  (2) Joint configuration of two digital signal blocks for enhanced performance or features. The digital blocks may be adjusted independently for power level. | | | | | | | | | |

Additional HD Radio system signal parameters (physical layer) for VHF Band II are provided in Table 89.

TABLE 89

HD radio system physical layer parameters

| Parameter name | Computed value (rounded) |
| --- | --- |
| Cyclic prefix width α | 0.1586 ms |
| Symbol duration (with prefix) *Ts* | 2.902 ms |
| Number of symbols in a block | 32 |
| Block duration *Tb* | 9.288 ms |
| Number of blocks in a frame | 16 |
| Frame duration *Tf* | 1.486 s |
| OFDM subcarrier spacing Δ*f* | 363.4 Hz |
| Number of carriers | 70 kHz band: 191  100 kHz band: 267 |
| Used bandwidth | 70 kHz band: 69.4 kHz  100 kHz band: 97.0 kHz |

Figure 4

HD radio system 70-kHz digital block positioning examples



Note: PL and PU are used for indicating lower positioning and upper positioning (respectively) of the digital block. The indication is for convenience only, and does not suggest an actual difference in the signal.


In the USA, the fundamental channel raster in VHF Band II is based on 200-kHz spacing. The HD Radio system presumes that the digital signal blocks are at pre-defined positions. As can be seen from the diagrams in Figs 4 and 5, these positions are not centred on the 200-kHz raster but in between. It has to be noted that the block position of 0 kHz in the Figures below corresponds to the reference analogue frequency for the HD Radio signal.

The reference analogue frequency may represent an actual analogue host signal when operating in hybrid configuration and employing a composition of either two signals (one analogue and one digital band) or three signals (one analogue and two digital bands). The analogue reference frequency may represent the centre frequency of a vacant band of a previously existing analogue host signal, while the system operates in all digital configurations. Such reference also demonstrates that a transition from hybrid configuration to all digital configurations does not have to change the digital signal allocation or configuration. Practically, it is expected to be followed by increasing the digital signal power.

Additional configurations allow for expanded signal composition, where two digital blocks of 70 kHz each as shown in Fig. 6, or two digital signal blocks of 100 kHz each as shown in Fig. 7, are employed jointly for providing more options for trade-off between throughput (net bit rate) and robustness.

Figure 5

HD radio system 100-kHz digital block positioning examples



Note: PL and PU are used for indicating lower positioning and upper positioning (respectively) of the digital block. The indication is for convenience only, and does not suggest an actual difference in the signal.

Figure 6

HD radio system 2 × 70-kHz digital block positioning examples



Note: PL and PU are used for indicating lower positioning and upper positioning (respectively) of the digital block. The indication is for convenience only, and does not suggest an actual difference in the signal.

Figure 7

HD radio system 2 × 100-kHz digital block positioning examples



Note: PL and PU are used for indicating lower positioning and upper positioning (respectively) of the digital block. The indication is for convenience only, and does not suggest an actual difference in the signal.

### 6.1.2 Channel models and fading margins

The specific EIA-approved channel (fading) models used in this analysis are provided further. Attempting to address all the reception modes along with the possible channel models may result in a significant number of combinations, thus prolonging the analysis work. For the specific purpose of providing planning parameters and in order to cover all of the combinations by using as few analysis cases as possible, the analysis brings forward the more demanding cases (in terms of required CNR and the resulting field strength), while assuming that the less demanding cases are then accounted for. For example, it may be assumed that reception under urban slow fading is more demanding than reception under suburban slow fading; therefore only the case of using the urban slow fading model has to be analysed. In another example, while considering the urban multipath profile in comparison to the suburban multipath profile, it may be assumed that reception under urban fast (60 km/h) fading is more demanding than reception under suburban fast (150 km/h) fading; therefore only the case of using the urban fast fading model is analysed for planning purposes.

In accordance with the analysis of a reduced number of cases, the reception modes and channel models combinations for planning purposes are provided in Table 90.

TABLE 90

Definition of reception modes and channel models

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | FX | MO | PO | PI | PO-H | PI-H |
| Antenna type | External | External | External | External | Integrated | Integrated |
| Antenna location | Outdoor | Outdoor | Outdoor | Indoor | Outdoor | Indoor |
| Environment | Suburban / Urban | Suburban / Urban | Suburban / Urban | Suburban / Urban | Urban | Urban |
| Reception percentage | 70% | 99% | 95% | 99% | 95% | 99% |
| Analysis speed (km/h) | 0 (static) | 60 (driving) | 2 (walking) | 0 (quasi-static) | 2 (walking) | 0 (quasi-static) |
| Analysis channel model | FXWGN | UFRM | USRM | FXWGN | USRM | FXWGN |

Channel models

The channel models included in this section may apply to the reception modes.

TABLE 91

Fixed Reception under White Gaussian Noise (FXWGN) channel model

|  |  |  |  |
| --- | --- | --- | --- |
| Ray | Delay (µs) | Attenuation (dB) | Doppler Frequency (Hz) |
| 1 | 0.0 | 0.0 | 0 |

TABLE 92

Urban Slow Rayleigh Multipath (USRM) channel model

|  |  |  |  |
| --- | --- | --- | --- |
| Ray | Delay  (µs) | Attenuation  (dB) | Doppler Frequency  (Hz) |
| 1 | 0.0 | 2.0 | 0.174 (reflects ~2 km/h |
| 2 | 0.2 | 0.0 |
| 3 | 0.5 | 3.0 |
| 4 | 0.9 | 4.0 |
| 5 | 1.2 | 2.0 |
| 6 | 1.4 | 0.0 |
| 7 | 2.0 | 3.0 |
| 8 | 2.4 | 5.0 |
| 9 | 3.0 | 10.0 |

TABLE 93

Urban Fast Rayleigh Multipath (UFRM) channel model

|  |  |  |  |
| --- | --- | --- | --- |
| Ray | Delay  (µs) | Attenuation  (dB) | Doppler Frequency  (Hz) |
| 1 | 0.0 | 2.0 | 5.231 (reflects ~60 km/h |
| 2 | 0.2 | 0.0 |
| 3 | 0.5 | 3.0 |
| 4 | 0.9 | 4.0 |
| 5 | 1.2 | 2.0 |
| 6 | 1.4 | 0.0 |
| 7 | 2.0 | 3.0 |
| 8 | 2.4 | 5.0 |
| 9 | 3.0 | 10.0 |

TABLE 94

Rural Fast Rayleigh Multipath (RFRM) channel model

|  |  |  |  |
| --- | --- | --- | --- |
| Ray | Delay  (µs) | Attenuation  (dB) | Doppler Frequency  (Hz) |
| 1 | 0.0 | 4.0 | 13.08 (reflects ~150 km/h |
| 2 | 0.3 | 8.0 |
| 3 | 0.5 | 0.0 |
| 4 | 0.9 | 5.0 |
| 5 | 1.2 | 16.0 |
| 6 | 1.9 | 18.0 |
| 7 | 2.1 | 14.0 |
| 8 | 2.5 | 20.0 |
| 9 | 3.0 | 25.0 |

TABLE 95

Terrain Obstructed Fast Rayleigh Multipath (TORM) channel model

|  |  |  |  |
| --- | --- | --- | --- |
| Ray | Delay  (µs) | Attenuation  (dB) | Doppler Frequency  (Hz) |
| 1 | 0.0 | 10.0 | 5.231 (reflects ~60 km/h |
| 2 | 1.0 | 4.0 |
| 3 | 2.5 | 2.0 |
| 4 | 3.5 | 3.0 |
| 5 | 5.0 | 4.0 |
| 6 | 8.0 | 5.0 |
| 7 | 12.0 | 2.0 |
| 8 | 14.0 | 8.0 |
| 9 | 16.0 | 5.0 |

## 6.2 HD Radio receiver parameters

### 6.2.1 Minimum *C*/*N*

*C*/*N* calculations for various reception scenarios employed various channel models. Followed by long term experience with commercial HD Radio receivers, the models correlation with actual reception conditions has been observed. As a result, the more performance impacting (i.e. requiring higher *C*/*N*) models are provided for planning purposes.

*C*/*N* values (*f* = 100 MHz) are provided for an average decoded BER of 0.5 × 10−4 as a reference operating point for providing services.

In considering the approach for planning parameters as indicated in [[2]](#EBU_TECH_3317) and based on potential (and actual) usage scenarios of various HD Radio receiver types, the following is assumed for planning:

1) Handheld portable receivers may be used while walking or while driving. Slow (up to 2 km/h) fading conditions are likely to affect reception at a walking speed, while fast (60 km/h) fading conditions likely to affect reception while driving. The slow urban fading conditions are expected to have much more severe impact on the reception than fast fading conditions and therefore will be used for planning purpose.

2) Portable receivers may be used in quasi-static (0 km/h) conditions or while driven. Due to their larger form factor in comparison to handheld receivers, it is assumed that they are likely to be used for quasi-static reception. Therefore, quasi-static reception is used in conjunction with portable receivers for planning purposes.

3) For mobile receivers, typical usage is more likely to be experienced in urban areas. In addition, calculations and actual tests have not shown significant difference of impact on reception, between urban conditions (60 km/h) and rural conditions (150 km/h). Therefore, urban reception conditions analysis, which employ more aggressive multipath profiles, are used for planning purposes.

The cases (and models) and their related required *Cd*/*N*0 (digital power to noise density ratio) as analysed for planning purposes are provided in Table 96.

TABLE 96

HD radio receiver required *C*/*N* for various reception modes

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | FX | MO | PO | PI | PO-H | PI-H |
| Channel model symbol | FXWGN | UFRM | USRM | FXWGN | USRM | FXWGN |
| Environment | Fixed | Urban | Urban | Indoor | Urban | Indoor |
| Speed (km/h) | 0 | 60 | 2 (walking) | 0 (quasi-static) | 2 (walking) | 0 (quasi-static) |
| MP9 Required *Cd*/*N*0 (dB-Hz) | 55.3 | 59.7 | 64.3 | 55.3 | 64.3 | 55.3 |
| MP12 Required *Cd*/*N*0 (dB-Hz) | 54.4 | 58.5 | 62.5 | 54.4 | 62.5 | 54.4 |
| MP19 Required *Cd*/*N*0 (dB-Hz) | 56.8 | 61.2 | 65.8 | 56.8 | 65.8 | 56.8 |
| MP1 Required *Cd*/*N*0 (dB-Hz) | 53.8 | 57.2 | 61.3 | 53.8 | 61.3 | 53.8 |
| MP11 Required *Cd*/*N*0 (dB-Hz] | 56.3 | 58.7 | 62.8 | 56.3 | 62.8 | 56.3 |

### 6.2.2 Receiver integrated noise figure

Based on calculations and certain deployments, the HD Radio receiver system noise figure (NF) for link budget calculations is shown in Table 97. Considering the reality of constant device miniaturization and integration, it is believed that for handheld reception, both external (ear bud) antenna and internal integrated antenna should be considered for planning purposes.

The integrated noise figure calculations employ conservative practical values, in accordance with the methodology for antenna for maximum voltage transfer (to the LNA), as indicated in § 3.11 and in [30].

In portable devices, power constraints are assumed to result in LNA NF that may be slightly higher (approximately 1 dB) than LNA NF for fixed or automotive reception which may not have power constraints.

In handheld devices, the best achievable antenna matching may be impacted by limited radiating element dimensions, varying elements and varying spatial orientation, which may collectively result in relatively high integrated noise figures. In all other cases (where the physical antenna, receiver structure, and their spatial orientation may be considered stable and reasonably defined), the antenna matching network is assumed to achieve the best required matching for maximum voltage transfer; thus resulting in values that may be common to those of the receiver only, as indicated in [[2]](#EBU_TECH_3317).

TABLE 97

HD radio overall receiver system NF

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | FX | MO | PO | PI | PO-H | PI-H |
| Antenna type | External fixed | Adapted | External telescopic / ear bud | External telescopic / ear bud | Internal | Internal |
| Receiver System NF (dB) | 7 | 7 | 8 | 8 | 25 | 25 |

The sensitivity (required field strength) based on the overall receiver system NF already assumed antenna gain of 1.5 (‘net physical’ isotropic element, separate of matching loss), while all losses are included in NF. Therefore, the antenna gain correction factor Δ*AG* is applied only where the physical element is different (noticeably larger).

#### 6.2.2.1 Receiver noise input power

This section does not include any operational values and is provided only as a place holder for reiterating that such a legacy approach is irrelevant for HD Radio field strength calculations, since an integrated NF approach is used.

## 6.3 HD Radio planning parameters

### 6.3.1 Minimum wanted field strength used for planning

The minimum median required field strength calculations are according to the integrated approach, as described in §§ 3.10 and 3.11.

In certain configurations (i.e. system modes) where both channels P1 and P3/P4 are active, and where field strength requirements for channel P1 are different from the field strength requirements for channels P3/P4, the more demanding requirements (higher *C*/*N*) are used for planning and are provided in the Tables in this section.

The minimum median field strength *Emed* for the HD Radio system is indicated in Tables 98 to 102.

It is noted that while the calculations follow the ITU guidelines as indicated in the respective sections in this Report, the chosen values are intended to ensure adequate reception in realistic conditions. Specifically, the following is noted:

– The HD Radio system’s approach to signal reception considers 99% for ‘good’ indoor reception, while certain other systems’ approaches may consider only 95% for indoor reception, potentially leading to inadequate reception. This higher requirement (of 99%) results in considering higher field strength requirements of 3.4 dB more than the field strength for only 95% indoor reception. This is relevant for reception modes PI and PI‑H (and reflected in higher total reception location losses for these modes).

– Broad industry experience with advanced and highly integrated small receivers, such as those in handheld devices and particularly their inclusion in smart phones, may require considering higher implementation losses than the implementation losses for discrete classes of receivers (i.e. automotive, portable). These higher losses result in considering higher field strength requirements of 2 dB more than the field strength for only discrete classes of receivers. This is relevant for reception modes PO-H and PI-H.

– The technological advances over the last tens of years have resulted in increased man-made noise, as has been indicated in certain published referenced documents. The HD Radio system’s analysis approach employs such man-made noise data from the year 2000 or later while certain other systems’ approaches may consider other data from referenced documents which have been established in 1974 or earlier. The HD Radio system’s approach considers such old data to be outdated and potentially leading to an inadequate reception. The consideration of the higher man-made noise data results in considering higher field strength requirements of 6.2 dB more than the field strength considered for the lower and potentially non-realistic man-made noise. This is relevant for all outdoor reception modes: FX, MO, PO and PI.

– The HD Radio system’s analysis approach considers the often outdoor use of handheld and portable receivers in both walking speed and driving speed. Adverse reception conditions for walking speed are considered much more demanding (requiring higher *C*/*N*) due to the slow fading impacts. While certain other systems’ approaches may consider analysis in driving speed to be sufficient, the HD Radio system considers the field strength requirements for walking speed to be adequate for planning. The consideration of walking speed reception results in considering higher field strength requirements of up to 4.6 dB more than the field strength considered for driving. This is relevant for all outdoor reception modes PO and PO‑H.

The HD Radio system’s analysis for deriving field strength requirements considers the most probable usage scenarios along with conservative assumptions regarding adverse channel conditions, environmental noise (man-made), and deployment margins. Considering less conservative parameters or outdated data may lead to potential reduction of more than 10 dB in field strength requirements, which may potentially lead to inadequate planning and then inadequate reception.

TABLE 98

HD radio mode MP9 minimum median field strength versus reception modes

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | **FX** | **MO** | **PO** | **PI** | **PO-H** | **PI-H** |
| MP9 Required *Cd*/*N*0 (dB-Hz) | 55.3 | 59.7 | 64.3 | 55.3 | 64.3 | 55.3 |
| Antenna gain correction, Δ*AG* (dB) | 4.4 | 0 | 0 | 0 | 0 | 0 |
| Reception location losses, *Lrl* (dB) | 3.4 | 19.1 | 16.2 | 30.3 | 23.2 | 37.3 |
| Implementation loss, *Lim* (dB) | 3 | 3 | 3 | 3 | 5 | 5 |
| Receiver System, *NF* (dB) | 7 | 7 | 8 | 8 | 25 | 25 |
| Man-made noise allowance, *Pmmn* (dB) | 14.1 | 14.1 | 14.1 | 14.1 | 0 | 0 |
| Minimum median field strength (dBµV/m) | 19.9 | 44.4 | 47.1 | 52.2 | 59.0 | 64.1 |

TABLE 99

HD radio mode MP12 minimum median field strength versus reception modes

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | **FX** | **MO** | **PO** | **PI** | **PO-H** | **PI-H** |
| MP12 Required *Cd*/*N*0 (dB-Hz) | 54.4 | 58.5 | 62.5 | 54.4 | 62.5 | 54.4 |
| Antenna gain correction, Δ*AG* (dB) | 4.4 | 0 | 0 | 0 | 0 | 0 |
| Reception location losses, *Lrl* (dB) | 3.4 | 19.1 | 16.2 | 30.3 | 23.2 | 37.3 |
| Implementation loss, *Lim* (dB) | 3 | 3 | 3 | 3 | 5 | 5 |
| Receiver System, *NF* (dB) | 7 | 7 | 8 | 8 | 25 | 25 |
| Man-made noise allowance, *Pmmn* (dB) | 14.1 | 14.1 | 14.1 | 14.1 | 0 | 0 |
| Minimum median field strength (dBµV/m) | 19.0 | 43.2 | 45.3 | 51.3 | 57.3 | 63.2 |

TABLE 100

HD radio mode MP19 minimum median field strength versus reception modes

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | **FX** | **MO** | **PO** | **PI** | **PO-H** | **PI-H** |
| MP19 Required *Cd*/*N*0 (dB-Hz) | 56.8 | 61.2 | 65.8 | 56.8 | 65.8 | 56.8 |
| Antenna gain correction, Δ*AG* (dB) | 4.4 | 0 | 0 | 0 | 0 | 0 |
| Reception location losses, *Lrl* (dB) | 3.4 | 19.1 | 16.2 | 30.3 | 23.2 | 37.3 |
| Implementation loss, *Lim* (dB) | 3 | 3 | 3 | 3 | 5 | 5 |
| Receiver System, *NF* (dB) | 7 | 7 | 8 | 8 | 25 | 25 |
| Man-made noise allowance, *Pmmn* (dB) | 14.1 | 14.1 | 14.1 | 14.1 | 0 | 0 |
| Minimum median field strength (dBµV/m) | 21.4 | 45.9 | 48.6 | 53.7 | 60.5 | 65.6 |

TABLE 101

HD radio mode MP1 minimum median field strength versus reception modes

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | **FX** | **MO** | **PO** | **PI** | **PO-H** | **PI-H** |
| MP1 Required *Cd*/*N*0 (dB-Hz) | 53.8 | 57.2 | 61.3 | 53.8 | 61.3 | 53.8 |
| Antenna gain correction, Δ*AG* (dB) | 4.4 | 0 | 0 | 0 | 0 | 0 |
| Reception location losses, *Lrl* (dB) | 3.4 | 19.1 | 16.2 | 30.3 | 23.2 | 37.3 |
| Implementation loss, *Lim* (dB) | 3 | 3 | 3 | 3 | 5 | 5 |
| Receiver System, *NF* (dB) | 7 | 7 | 8 | 8 | 25 | 25 |
| Man-made noise allowance, *Pmmn* (dB) | 14.1 | 14.1 | 14.1 | 14.1 | 0 | 0 |
| Minimum median field strength (dBµV/m) | 18.4 | 41.9 | 44.1 | 50.7 | 56.0 | 62.6 |

TABLE 102

HD radio mode MP11 minimum median field strength versus reception modes

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reception mode | **FX** | **MO** | **PO** | **PI** | **PO-H** | **PI-H** |
| MP11 Required *Cd*/*N*0 (dB-Hz) | 56.3 | 58.7 | 62.8 | 56.3 | 62.8 | 56.3 |
| Antenna gain correction, Δ*AG* (dB) | 4.4 | 0 | 0 | 0 | 0 | 0 |
| Reception location losses, *Lrl* (dB) | 3.4 | 19.1 | 16.2 | 30.3 | 23.2 | 37.3 |
| Implementation loss, *Lim* (dB) | 3 | 3 | 3 | 3 | 5 | 5 |
| Receiver System, *NF* (dB) | 7 | 7 | 8 | 8 | 25 | 25 |
| Man-made noise allowance, *Pmmn* (dB) | 14.1 | 14.1 | 14.1 | 14.1 | 0 | 0 |
| Minimum median field strength (dBµV/m) | 20.9 | 43.4 | 45.6 | 53.2 | 57.5 | 65.1 |

# 7 Planning parameters for Digital System A (DAB) in VHF Band III

In May 2018, the European Broadcasting Union (EBU) published the Report Tech 3391 ‘Guidelines for DAB network planning’ [45]. This Report was jointly developed with Broadcast Networks Europe (BNE) and is the basis for the information provided in the present Report.

The use of the term 'DAB' in this Report applies to both DAB and DAB+ systems (see § 7.1). Where there is a difference in the impact on network planning between the two systems, this is explained.

## 7.1 System parameters of DAB

Short review of DAB standards

The DAB digital broadcasting system originated from a European funded project known as Eureka 147. The members of the project team decided to standardize the system at ETSI and the system standard was first published in 1995 as ETS 300 401 [34]. The DAB standard has been supported and developed for many years by the WorldDAB Forum, a not for profit membership organization, and is actively supported by the EBU. The latest version of the DAB standard was published by ETSI in January 2017 as EN 300 401 V2.1.1 [35].

The core DAB standard describes the coding, modulation and transmission system parameters. Two basic data mechanisms are provided: stream mode and packet mode. Also defined is the signalling channel that allows a receiver to make sense of the content of the multiplex. Compared with analogue broadcast radio systems, a DAB transmission is relatively wideband, this extra bandwidth allowing several services to be carried on the transmission. Such a transmission carrying more than one service is known as an ensemble. Originally, the DAB audio coding mechanism, using MPEG Layer II coding, was included in the core specification, ETS 300 401 [34]. Later developments in audio coding efficiency led to the introduction of DAB+ audio coding, based on MPEG 4 AAC coding, which is described in a separate specification, TS 102 563 [58]. With the release of EN 300 401 V2.1.1 [35] the DAB audio coding definition was also transferred into a separate specification, TS 103 466 [59].

DAB is most widely used as a digital radio transmission system for audio services using DAB+ audio coding, with text messages carried as dynamic labels. Additional data can accompany the audio services, visuals via the SlideShow application and logos and programme information via the Service and Programme (SPI) application. The SPI application also allows carriage of other non-audio services such as mobile video services, traffic data and a host of other applications.

Additional standards documents have been created to facilitate additional features, interoperable equipment interfaces, additional transport modes, data applications, etc. A useful guide to the DAB standards is available as ETSI TR 101 495 V2.1.1 [60].

DAB and DAB+: what is the difference?

Some ambiguity surrounds the terms DAB and DAB+, owing to the way that the DAB system has developed over time. Often, DAB+ is used to describe the whole transmission system, although this would more correctly be described as a DAB ensemble with exclusively DAB+ audio services. The coding, modulation and transmission systems are identical whether the ensemble carries DAB audio services, DAB+ audio services, DMB video services, data, or any combination of these.

Today, the majority of DAB ensembles used for digital radio services carry those services using DAB+ audio coding. This is because DAB+ audio is more bandwidth efficient, using around half of the bitrate needed by DAB audio for the same subjective quality, and it is slightly more robust than DAB audio at the same protection level.

DAB audio coding was designed at the same time as the coding, modulation and transmission system. Five levels of Unequal Error Protection (UEP) were specified which provide additional protection to the more sensitive parts of the audio frame. DAB+ audio coding was designed to fit into the existing DAB system, the AAC audio frames are collected into audio super-frames of constant duration and are further protected by a Reed-Solomon (RS) coding. DAB+ audio sub-channels are protected using one of four levels of Equal Error Protection (EEP).

### 7.1.1 Modulation scheme and guard interval

DAB uses the Orthogonal Frequency Division Multiplexing modulation scheme (OFDM). Since it is not the task of this Report to give an introduction into this modulation technique, the present section is restricted to a short description of those OFDM features that are relevant for planning.

Carrier structure

DAB uses a convolutionally coded D-QPSK OFDM signal. The system is based on the use of 1 536 active carriers with a frequency spacing of 1 kHz. All carriers are transmitted at the same power level. Four DAB frequency blocks fit into a single 7 MHz television channel identified by the letters A, B, C and D, with a 176 kHz guard band between blocks A-B, B-C and C-D. Between blocks D and A there is a wider guard band of 320 or 336 kHz in order to align with a 7 MHz television raster.

Frequency interleaving

The decoding algorithm performs poorly when confronted with bit errors that are all bunched together in the data stream, and because the carriers are subject to fading, bit errors usually do occur in groups when a carrier is in a deep fade. To protect against this, DAB uses frequency interleaving. This mechanism randomly spreads the information across all carriers and thus across the whole bandwidth. This avoids the bundling of bit errors caused by frequency selective fading and significantly improves the performance of the decoder.

Time interleaving

An important property of a broadcast system targeting mobile reception is the use of time interleaving. In a mobile radio propagation channel, errors often appear in bursts. This may happen, for example, when field strength is too low at some reception points on the route along which a mobile receiver is moving.

In this case, use of time interleaving ensures that the errors resulting from these outage points are distributed over several transmission frames allowing the error protection/correction to rectify any errors that may occur. In DAB the interleaving depth is 16 logical frames which is equivalent to 384 ms.

Time interleaving is, however, most effective above a certain speed. In the case of DAB the time interleaving is less effective at speeds below roughly 15 km/h. This means that the portable indoor reception case may be a worst case scenario.

Multipath capability

OFDM, when coupled with appropriate channel coding (error correction coding), can achieve a high level of immunity against multipath propagation and co-channel interference.

In OFDM, the individual carriers are modulated by means of phase shift and amplitude modulation techniques. Each carrier has a fixed phase and amplitude for a certain time duration during which a small portion of the information is carried. This unit of data is called a symbol; the time it lasts is called the symbol duration. At the end of the time period the modulation is changed and the next symbol carries the next portion of information.

A DAB receiver has to cope with the adverse conditions of the broadcast transmission channel. Unless measures are taken, signals arriving at a receiver by different paths will have different time delays which will result in inter-symbol interference (ISI) and a degradation in reception. An OFDM system with a multipath capability allows for the constructive combination of such signals. This is achieved by inserting a guard interval, a cyclic prolongation of the period in which useful information can be extracted from symbol’s that are delayed. The FFT-window, i.e. the time period for the OFDM demodulation is then positioned to minimise the inter-symbol interference. The insertion of the guard interval, whilst helping avoid ISI reduces the data capacity because less of the symbol duration is used for "useful" data – the guard interval is a period where the received signal is not used to make received data decisions; it is only used to avoid ISI from the previous symbol due to multipath delays.

All signals with time delays that cannot be absorbed by the guard interval in the way described above introduce a degradation of reception.

OFDM, due to its multicarrier nature, exhibits relatively long symbols. This long symbol period already provides a certain degree of protection against inter-symbol interference caused by multipath propagation. However, as described above, this protection is greatly enhanced by use of the guard interval.

### 7.1.2 Transmission modes

In the first edition of the DAB standard published in 1995, ETSI ETS 300 401 [34], three transmission modes were defined to allow the DAB system to be used in both terrestrial and satellite network configurations and over a wide range of operating frequencies. A fourth transmission mode was later added. With the latest version of the standard, ETSI EN 300 401 V2.1.1 [35], only Mode I, corresponding to use in the VHF band (30 to 300 MHz) has been retained.

Transmission Mode I is intended to be used for terrestrial Single Frequency Networks (SFN) and local-area broadcasting in Bands I, II and III. It may also be used for cable distribution and for Multiple Frequency Networks (MFN) as well.

TABLE 103

Mode I features

|  |  |  |
| --- | --- | --- |
| Typical use | Mode I | |
| Terrestrial VHF (urban/suburban) | Terrestrial VHF (rural) |
| Max speed VHF (km/h) | 260 | 390 |
| Number of carriers | 1 536 | |
| Carrier spacing (kHz) | 1 | |
| Useful symbol duration (µs) | 1 000 | |
| Guard interval (µs) | 246 | |
| Total symbol duration (µs) | 1 246 | |

### 7.1.3 Protection levels, coding and net bit rates

Convolutional encoding is applied to each of the data sources feeding the multiplex to ensure reliable reception (see [35] § 11 “Convolutional coding”). The encoding process involves adding deliberate redundancy to the source data. In the ETSI standard specification for the DAB system [35], five Unequal Error Protection (UEP) levels are available (used for DAB audio) and eight Equal Error Protection (EEP) levels are available (used for DAB+ audio and data) that use punctured convolutional coding.

The total capacity of the Main Service Channel (MSC) can be partitioned into several sub-channels. Depending on the number of sub-channels the net bit rate is calculable. Some net bit rates, using the example of 6, 12 and 18 sub-channels carrying DAB audio services, are given in Table 104 for the UEP protection levels.

TABLE 104

Net bit rates per sub-channel

|  |  |  |  |
| --- | --- | --- | --- |
| Protection level UEP | Net bit rate (kbit/s) | | |
| 6 sub-channels | 12 sub-channels | 18 sub-channels |
| 1 | 128 | 64 | 32 |
| 2 | 128 | 64 | 48 |
| 3 | 192 | 96 | 64 |
| 4 | 192 | 112 | 64 |
| 5 | 256 | 128 | 80 |

In the case of the EEP levels, there are two options, each consisting of four different protection levels. For each option, Level 1 represents the strongest and Level 4 the lowest error protection. Option A has sub-channels in multiples of 8 kbit/s and offers the maximum flexibility for segmentation for service providers and is the option generally chosen for DAB+ audio services. In contrast, Option B has sub-channels in multiples of 32 kbit/s and is designed primarily for DMB video services where the greater bit-rate granularity is less important.

Table 105 shows the corresponding code rates for EEP Options A and B:

TABLE 105

Code rates for EEP Options A and B

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Protection level | EEP-1A | EEP-2A | EEP-3A | EEP-4A |
| Code rate | 1/4 | 3/8 | 1/2 | 3/4 |
| Protection level | EEP-1B | EEP-2B | EEP-3B | EEP-4B |
| Code rate | 4/9 | 4/7 | 4/6 | 4/5 |

Table 106 is a table of net bit rates similar to Table 104, but for an ensemble carrying DAB+ audio protected using EEP option A profiles.

TABLE 106

Net bit rates per sub-channel for DAB+

|  |  |  |  |
| --- | --- | --- | --- |
| **Protection level EEP** | **Net bit rate (kbit/s)** | | |
| **12 sub-channels** | **18 sub-channels** | **24 sub-channels** |
| 1A | 48 | 32 | 24 |
| 2A | 72 | 48 | 32 |
| 3A | 96 | 64 | 48 |
| 4A | 144 | 96 | 72 |

The values shown in Tables 104 and 106 are for the case when all sub-channels have the same bit rate; a situation which will usually result in reduced efficiency. The allocation of different bit rates to each sub-channel (for example, higher bit rates for music and lower for news) enables more efficient use of the spectrum.

### 7.1.4 Channel models

The *C*/*N* value is a fundamental planning parameter for DAB networks. Generally, the *C*/*N* should ensure acceptable audio quality at a Bit Error Ratio (BER) of 1 × 10−4 after Viterbi.

Previously DAB planning has been based on the WI95 [36] and GE06 [1] agreements. The planning values in these two agreements are mainly based on the EBU planning guideline BPN 003 (issues 1 and 2) [37]. The coverage criteria used has been mobile reception assuming DAB audio coding in a Rayleigh channel, in a rural environment (RA) at a speed of 130 km/h with an associated *C*/*N* of 15 dB (values for a typical urban environment (TU) at a speed of 15 km/h are also given).

Measurements quoted in an early ITU-R Recommendation [38] suggested a Gaussian *C*/*N* value for Mode I at UEP-3 of 7.1 dB. This was simplified to 7 dB for the Wiesbaden planning process. A revision of Recommendation ITU-R BS.1114 [14], gave a value of 7.6 dB for Mode I and 7.4 dB for Modes II and III. The value of 7 dB was adopted in EBU planning guideline BPN 003 [37] for all modes in a Gaussian channel.

The EBU guideline TR 021 [39] considered that for UEP-3 protected sub-channels a *C*/*N* value of 7.4 dB is required to achieve a Bit Error Rate (BER) of 1 × 10−4after Viterbi decoding in a Gaussian channel. For Rayleigh channels a figure of between 13 and 13.5 dB is quoted, this being based on operational DAB networks. Corresponding DVB-T planning values are then used to extrapolate / interpolate for all code rates, followed by variable implementation margins for different channel types to derive the results reproduced in Table 107.

TABLE 107

*C*/*N* values for UEP protection

|  |  |  |
| --- | --- | --- |
| Protection level | *C*/*N* (dB) for BER of 1 × 10−4 after Viterbi | |
| Gaussian channel | Rayleigh channel – TU 6 |
| UEP-1 | 5.9 | 12.1 |
| UEP-2 | 6.7 | 12.6 |
| UEP-3 | 7.4 | 13.3 |
| UEP-4 | 8.4 | 14.9 |
| UEP-5 | 10.2 | 18.6 |

Planning values optimised for ensembles carrying DAB+ audio services are given in TR 025 [40]; these values being based on measurements carried out by the IRT. In these measurements, a Gaussian type channel was assumed for fixed reception, a Rayleigh channel (profile TU 12 at 25 km/h and 178 MHz) and Rural Area 6, RA 6 (speed 120 km/h six taps) for mobile and portable reception was assumed.

Most recent *C*/*N* values for DAB ensembles intended to carry EEP protected sub channels have been determined by a set of measurements carried out by the IRT and Rai Way. These measurements were based on nineteen arbitrarily chosen DAB+ receivers and three different profiles, one for fixed reception and two for mobile and portable reception. The two Rayleigh profiles are Typical Urban 12, TU 12 (speed 25 km/h twelve taps), and Rural Area 6, RA 6 (speed 120 km/h six taps). The results, shown in Table 106, are the averages of the minimum values of the proper operation of the receivers.

TABLE 108

*C*/*N* values for EEP-A protection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Protection level | Corresponding code rate | *C*/*N* (dB) | | | Approximate bit-rate (Mbit/s) |
| Gaussian channel (FX) | TU 12 | RA 6 |
| EEP-1A | 1/4 | 3.7 | 7.8 | 7.8 | 0.58 |
| EEP-2A | 3/8 | 4.4 | 9.7 | 9.9 | 0.86 |
| **EEP-3A** | **1/2** | **5.6** | **11.9** | **12.6** | **1.15** |
| EEP-4A | 3/4 | 8.6 | 18.1 | 20.7 | 1.73 |

For both UEP and EEP, the differences between the *C*/*N* values of the various protection levels are not constant and the measurements show that the higher code rate, which results in lower protection, requires significantly more *C*/*N* to achieve reliable reception. Moreover, in EBU TR 021 [39] it is stated that the Protection Level 5 does not work for the mobile high-speed worst-case reception situation. This was confirmed by the tests made with DAB+ audio which proved that some receivers are not able to lock the signal when using the RA 6 profile with EEP-4A. The *C/N* values for EEP‑3A, highlighted in bold in Table 106 have been used in the link budget calculations.

### 7.1.5 SFN performance

#### 7.1.5.1 Theoretical evaluation of SFN performance

In Single Frequency Networks (SFNs) transmitters are required to radiate the same OFDM symbol at the same time. This comes from the fact that “echoes” generated by co‑channel transmitters shall be confined within the guard interval period: outside the guard interval a part of the echo power is associated with the same OFDM symbol as the primary signal, and which therefore contributes positively to the total useful signal power; differently another part of the echo power is associated with the previous or subsequent OFDM symbol and produces inter‑symbol interference (ISI), which has a similar effect to uncorrelated Gaussian noise interference. In Fig. 8 the splitting of a generic signal power into useful and interfering components is shown, where ∆ is the guard interval length and *Tu* is the useful symbol length [47].

Figure 8

DAB model ‑ splitting of a generic signal power into useful and interfering components



For DAB, the rule for splitting the signal power into a useful component and an interfering component is expressed as follows:

(47)

(48)

(49)

where:

*Ci* power contribution from the i‑th signal at the receiver input

*C* total power of the effective useful signal

*I* total effective interfering power

*wi* weighting coefficient for the i‑th component

*Tu* useful symbol length

Δ guard interval length

*t* signal arrival time.

It must be borne in mind that, the total effective interfering power, is weighted by the established DAB‑to‑DAB protection ratio when being regarded as a source of interference in a coverage calculation.

The OFDM receiver has to setup a time window during which it samples the on‑air OFDM signal. The objective is to synchronize this time window with the useful period of the OFDM symbol. If the transmitters deliver the same OFDM symbol at the same instant, or with a sufficiently small time delay, the differential propagation path delay to the OFDM receiver will remain inside the guard interval period. Accordingly, the sum of the received signals will be constructive because they constitute the same OFDM symbol (with no ISI).

In the design of SFNs the inter‑transmitter distance is proportional to the maximum echo delay acceptable by the transmission system, which depends on the guard interval. Actual transmitter spacing can be increased beyond that defined by the guard interval with network optimization in terms of static delays, antenna patterns and power of transmitters.

As an example, considering a 2‑path scenario with power *P*1 = *P* for signal 1 and power *P*2 = *aP* for signal 2; the requirement for an allowed delay of signal 2 is given by:

(50)

where:

γ: required protection ratio for the considered service

*w*: weighting function

*a*: allowed power of signal 2, expressed as a percentage of the power of signal 1.

*w* is a function of *t*, the relative delay of signal 2. All quantities are expressed in linear scale.

The value of the parameter *a* is sought as a function of the delay *t*. It is independent of the particular value of *P*; it can therefore be written as:

(51)

Table 109 gives the results for a protection ratio γ = 13.5 dB and a guard interval ∆ = 246 µs.

TABLE 109

Theoretical values of the required difference in power for a delayed signal

|  |  |  |  |
| --- | --- | --- | --- |
| Relative delay (µs) | *w* | *a* | Required difference between *P*1 and *P*2 → 10 log(*a*) (dB) |
| 0 ≤ *t* ≤ 246 (i.e. inside the guard interval) | 1 | 1 | 0 (i.e. not required) |
| 300 | 0.8949 | 0.6859 | 1.64 |
| 335 | 0.8299 | 0.3358 | 4.74 |
| 365 | 0.7762 | 0.2362 | 6.27 |
| 400 | 0.7157 | 0.1770 | 7.52 |
| *t* > 1246 | 0 | 1/γ = 0.0447 | 13.5 |

It has been found that practical SFN performance (§ 7.1.5.2) aligns quite well with the theoretical considerations based on equations (47) to (49) and shown in Fig. 8 (see also § 2.6 of EBU TR 021 [39]).

The effective planning of the required radiated power and the optimization of static delays at the secondary site(s) will improve SFN performance as well and provide the effective management to eliminate most potential interference problems.

#### 7.1.5.2 Practical SFN performance

In some countries, large area SFNs will need to be considered due to frequency constraints. For this reason, an experimental verification of the behaviour of DAB receivers in presence of signals beyond the guard interval is required, in order to optimize the setup of this kind of network.

Rai Way performed several tests on this issue in the laboratory and in a sample service area.

In both cases a number of models of commercial receivers sold in Italy (Continental, Blaupunkt and Pure) were tested. The transmission Mode I was considered as a reference as it is used in real DAB+ networks deployment in the VHF band in Italy. The theoretical value of the guard interval, ∆, used was 246 µs.

Tests were specifically focused on the identification of the “minimal condition” which allows the commercial receivers to correctly demodulate the content when one or more echoes are beyond the guard interval, taking into account the power levels of the signals and their relative delays. These tests showed that far beyond the guard interval the difference in the signal levels of transmitters at the receiving point represents the discriminating factor which guarantees (or not) a good reception quality, in line with the theoretical analysis of § 7.1.5.1. Therefore, this difference has been named as the required protection ratio ζ to make the reception feasible in presence of signals beyond the guard interval. It is important to notice that the parameter γ (introduced in the previous section) and ζ have a different meaning: ζ expresses the difference in the signal levels of transmitters at the receiving point (only in SFN mode) which might guarantee a good reception quality. Therefore, it does not have a fixed value, but rather a value which varies and depends on the relative delay among the SFN echoes. For this reason, ζ cannot be considered in the same way as γ, although if a specific condition arises in the considered SFN network (see Table 110) the value of the two parameters corresponds.

The behaviour shown by commercial receivers in the service area was very similar to that seen in the laboratory tests. From the results of these studies, Rai Way derived the values in Table 110; the conditions required in a DAB+ SFN in order that commercial receivers may correctly demodulate the audio content with good quality.

TABLE 110

Conditions to be respected by DAB signals in SFN configuration (transmission Mode I)   
to make audio reception feasible with good quality on commercial receivers

|  |  |
| --- | --- |
| Required protection ratio ζ | Relative delay |
| 0 (i.e. not required) | 0 ≤ *t* ≤ 246 µs (i.e. inside the guard interval) |
| 5 dB | 246 < *t* ≤ 350 µs |
| 13.5 dB | *t* > 350 µs |

It is important to notice that for the range 0 µs to ~350 µs the values of Table 109 fit quite well with the figures of Table 110. In the range beyond 400 µs the degradation as reflected in Table 110 is faster than the one derived from the theoretical equation presented in § 7.1.5.1. On the other hand, the conditions shown in Table 110 are quite conservative and might be slightly adjusted after further tests are performed on commercial receivers. Also, a more complex mathematical function that better describes the real behaviour of receivers in presence of echoes beyond the guard interval could be derived.


Additional tests should be performed for case of pre‑echoes those “in advance” of the time window, i.e. for *t* < 0. Unless otherwise demonstrated, planning analysis should not rely on the symmetry of the theoretical DAB model with respect to the time axis, as shown in Fig. 8 (for *t* < 0 a *protection ratio* ζ of about 13.5 dB should be considered).

In Annex H of [45], all the details and the results of the tests performed by Rai Way on SFN performance, both in the laboratory and in a sample service area, are reported.

Laboratory and field testing by CRA has shown situations where SFN performance could be degraded under certain conditions even though the reception of two SFN signals is within the guard band, i.e. less than 246 µs apart. This particular situation occurs when the signals from both transmitters are very close in power, e.g. less than 1 dB difference ‑ the ‘zero dB’ echo case. The two signals are combined at the input to the antenna non‑coherently and consequently the relative phase of each sub‑carrier in the OFDM symbol will determine the resulting power. This is shown in Fig. 9 where the delay between the two equal power signals is 10 µs. The result is that there are several sub‑carriers in the symbol which are significantly reduced in power, in this case by over 20 dB relative to the peak sub‑carrier power. The impact of this ‘scalloping’ is a reduction in receiver performance when the received signal power is less than approximately 20 dB above the minimum received signal power threshold. This reduction is due to the poor *C*/*N* for the specific sub‑carriers in the symbol which effectively propagate through the receiver signal processing as errors and can result in an effective increase in the noise floor. The result can be to raise the minimum receive signal power by typically between 3 and 6 dB for FEC code rate EEP-3A, dependent on the second path delay and the receiver implementation.

Figure 9

The spectrum of two equal power DAB signals combined with 10 µs delay



This situation typically will only occur when the receiver is in a situation where the signal received from both transmitters is not only equal power but also ‘clean’, that is there are no significant multipath signal components present. As the power difference between the two received signals increases the performance is dominated by the stronger signal. Also, the presence of multipath components helps ‘dilute’ the effect by adding further non‑coherent signal components that can reduce the depth of some notches.

## 7.2 Receiver parameters

### 7.2.1 Receiver noise figure

A noise factor of 7 dB has been used since the early days of DAB. This value is also suggested by the EBU in their DAB planning guideline document [37]. However, some receivers, in particular mobile DAB receivers, are likely to perform better, i.e. having a noise figure of about 5 dB or better.

IRT has made measurements of the receiver noise figure [41] and found that values lay in the range 4.7 dB to 6.4 dB. On the basis of these tests and experience with modern receivers, a noise figure of 6 dB is regarded as a reasonable compromise to cover different receiver types.

It is suggested that a noise figure of 6 dB should be used for planning.

### 7.2.2 Minimum receiver signal input levels

To illustrate how the *C*/*N* influences the minimum signal input level to the receiver, the latter has been calculated for representative *C*/*N*, including the implementation margin. For other values simple linear interpolation can be applied.

The receiver noise figure has been chosen as 6 dB (see § 7.2.1). The noise figure is given for all the frequencies within Band III and thus the minimum receiver input signal level is independent of the transmitter frequency. If other noise figures are used in practice, the minimum receiver input signal level will change correspondingly by the same amount.

The minimum receiver input signal levels calculated here are used to derive the minimum power flux densities and corresponding minimum median equivalent field strength values for various reception modes.

|  |  |  |
| --- | --- | --- |
| Definitions: | | |
|  | B | : Receiver noise bandwidth (Hz) |
|  | *S*/*N* | : RF signal-to-noise ratio required by the system (dB) |
|  | *Fr* | : Receiver noise figure (dB) |
|  | *Pn* | : Receiver noise input power (dBW) |
|  | *Ps min* | : Minimum receiver signal input power (dBW) |
|  | *Us min* | : Minimum equivalent receiver input voltage into *Zi* (dBµV) |
|  | *Zi* | : Receiver input impedance (75 Ω) |
|  | *k* | : Boltzmann’s constant = 1.38 × 10−23 Ws/K |
|  | *T*0 | : Absolute temperature = 290 K |
| Equations: | | |
|  | *Pn* | = *Fr* + 10 log(*kT*0*B*) |
|  | *Ps min* | = *Pn* + *C*/*N* |
|  | *Us min* | = *Psmin* + 120 + 10 log(*Zi*) |

TABLE 111

Minimum required input signal levels for different *C*/*N* values

|  |  |  |  |
| --- | --- | --- | --- |
| Band III – 7 MHz channels | | | |
| Channel model |  | TU 12 | RA 6 |
| Equivalent noise bandwidth | *B* (Hz) | 1.536 × 106 | 1.536 × 106 |
| Receiver noise figure | *Fr* (dB) | 6 | 6 |
| Corresponding receiver noise input power | *Pn* (dBW) | −136.1 | −136.1 |
| Signal-to-noise ratio | *S*/*N* (dB) | 11.9 | 12.6 |
| Minimum receiver signal input power | *Ps min* (dBW) | −124.2 | −123.5 |
| Minimum equivalent receiver input voltage, 75 ohm | *Us min* (dBW) | 14.55 | 15.25 |

## 7.3 Additional considerations for DAB planning

### 7.3.1 Coverage prediction height

Two main mechanisms give rise to variations in field strength with height.

The first is simply that diffraction losses will tend to fall as an antenna is raised above the level of surrounding clutter.

The second effect leading to variation of field strength with height is one due to interference between direct and reflected waves, this effect is dependent on polarisation and overall path geometry such as possible ground reflected wave in open/rural environments, however reflected waves are not normally taken into account in prediction models.

Historically radio services were received at rooftop level (clear of the clutter), typically 10 m above ground level (a.g.l.) and hence propagation prediction methods provided field‑strength values at 10 metres. This was necessary since receiver performance was relatively poor compared to todayʼs standards. However, using modern receivers, listening is now predominantly carried out on mobile and indoor portable receivers and a representative height of typically 1.5 m is assumed. An adjustment to 1.5 m would therefore have to be applied.

The alternative prediction approach is to construct the propagation geometry from the transmitter to the receiver on the basis of the required receiver height, i.e. direct to 1.5 m a.g.l.

Advances in computing power and storage and the availability of affordable fine resolution clutter data (density and heights of buildings, trees etc.) for large areas, allows for predictions to be made directly to the intended receiver height. This method is recommended when developing or updating deterministic prediction tools.

Figure 10

Examples of clutter resolution when comparing predictions at 1.5 m a.g.l. with a prediction at 10 m a.g.l. with fixed height loss. The terrain data resolutions matched to the clutter resolution.

These maps have been produced with a low transmit power to demonstrate the differences

|  |  |
| --- | --- |
| image006 | image003 |
| a) 100 m resolution prediction at 10 m a.g.l. and fixed height loss of 12.4 dB (Low Urban) | b) 50 m resolution prediction to 1.5 m a.g.l. |
| image004 |  |
| c) 25 m resolution prediction to 1.5 m a.g.l. | Key to maps |

As the resolution of clutter data becomes finer, the difference in 10 m predictions using a height loss factor compared to a prediction directly to 1.5 m becomes more apparent. Figure 10 compares a 10 m fixed height loss prediction with predictions to 1.5 m at different clutter data resolutions. It demonstrates that the finer resolutions can show more detail in the coverage which otherwise may have been overlooked. The terrain data resolution should be matched to the clutter data resolution and defines the minimum pixel size used in the predictions. The finer the detail of the predictions the more computational power and storage is required. By predicting direct to the receiver height, the need to set height loss values, either a fixed value or by receiving environment, is avoided.

If clutter data of a suitable resolution is not available or computational power or storage is limited then predictions to 10 m a.g.l. with a height loss correction factor, *Lh* (dB), being applied are suggested. This height loss correction factor is the method used in the ITU‑R published empirical based propagation models. The height loss relative to 10 m a.g.l. or the ‘representative clutter height’ can be calculated.

For long distance interference analysis, the deterministic models used for coverage planning may not provide accurate results due to the extended range that interference travels and the impact of tropospheric conditions such as ducting. In this case, the interfering field strength calculations can still be based on empirical models, typically Recommendation ITU‑R P.1546 [18].

The height loss correction factor from 10 m to 1.5 m can be taken directly from the Final Acts of GE06, § 3.2.2.1 of Chapter 3 of Annex 2 (Considerations on height loss) [1]. This factor depends on the frequency and receiving environment.

Some example calculated values at 200 MHz have been populated in Table 112, based on UK and Austrian clutter samples. The Austrian examples represent the clutter categories seen in the map in Fig. 10.

For planning purposes height loss values can be calculated using relevant clutter heights for the country or area in question and based on ITU method [18], some example calculations have been reproduced in Annex D in [45].

TABLE 112

(a and b) Calculated height loss examples for some different environment classes   
in the UK and Austria

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Band III at 200 MHz | Typical UK clutter height | Rec. 1546 Calculated height loss |  | Band III at 200 MHz | Typical Austrian clutter height | Rec. 1546 Calculated height loss |
| Urban | 18 m | 17.6 dB |  | Dense Urban | 30 m | 21.7 dB |
| Suburban | 9 m | 11.4 dB |  | Low Urban | 10 m | 12.4 dB |
| Low Suburban | 6 m | 7.9 dB |  | Suburban | 10 m | 12.4 dB |
| Rural | 6 m | 7.9 dB |  | Rural | 0 m | Not applicable |


Table 112a shows some example calculated height loss values for the UK and Table 112b shows some for Austria which have been used in the map of Figure 10a. These examples show that height loss decreases with lower clutter heights.

In Australia a measurement campaign has been carried out to obtain a better understanding of height loss. Commercial Radio Australia in conjunction with the Australian Broadcast Corporation undertook measurements in a range of different environments from line‑of‑sight to various shadowed environments from high to low field strengths. All measurements were taken in Canberra where there is a single medium power (3.1 kW ERP) high tower transmission, and hence there is no influence from SFN transmissions which tend to reduce the height loss due to multiple sources of received signal. The results are shown in Fig. 11.

The measurement results at 25 out of the 28 measurement sites, i.e. 90%, had height loss values of less than 10.5 dB, and the average height loss value was between 7 and 8 dB.

Figure 11

Height loss measurement results



The measurement results provide a basis for the height loss value used in 10 m to 1.5 m prediction methods, where 90% of values will be less than 10.5 dB, hence Australia has opted for a value of 10 dB as being appropriate, the same value is used in the UK where similar results were found during early Band III DAB survey measurements.

Due to the differences in building types, spacing and construction methods between countries or even areas, it is pragmatic to carry out survey and analysis work when calibrating a prediction model for 1.5 m reception. For predictions based on 10 m a.g.l. and including a height loss factor it is recommended to classify typical environments (such as urban, suburban) with a height loss value for each category. To calibrate and validate a prediction model measurements should be considered in areas where co‑channel interference is at a minimum and there is a single wanted signal, they should be carried out at 10 m a.g.l. (or clear of local clutter) and also at the target receiver height of 1.5 m. Once below the clutter height and diffraction path an omnidirectional receive antenna should be used for measuring due to the much greater importance of reflections. As mobile measurements using a nominally omnidirectional receive antenna are fairly quick and easy to make compared to 10 m measurements, the validation of predictions direct to 1.5 m receiver height can be made much quicker.

Typically, when planning for indoor reception, the urban and dense urban areas which may represent a small percentage of the overall area whilst exhibiting higher building entry loss, will be targeted first and served with high field strengths from one or more transmitters and any increase in height loss becomes less noticeable in the predictions. For these reasons and evidence from survey measurements, the examples of Australia and the UK use a single value representing the Suburban environment. It should be stipulated that these values are examples provided as guidance for the inclusion of height loss in the development of coverage predictions.

#### 7.3.1.1 Height loss values for planning

For planning purposes height loss values can be calculated using the methodology proposed in Recommendation ITU-R P.1546 [18] for different receiving environments and some typical clutter heights for the country or the area under examination as shown in Table 113.

TABLE 113

Height loss for different environment classes and typical clutter heights

|  |  |  |  |
| --- | --- | --- | --- |
| Receiving environment | Reference frequency  (MHz) | Representative clutter height  (m) | Height loss *Lh* from ITU-R P.1546 methodology  (dB) |
| Dense urban | 200 | 30 | 22 |
| Urban | 200 | 20 | 19 |
| Suburban | 200 | 10 | 12 |
| Rural | 200 | 10 | 12 |

### 7.3.2 Building and vehicle entry loss

#### 7.3.2.1 Building entry loss

Portable reception can take place at both outdoor and indoor locations. For indoor locations, depending on the materials, the construction and orientation of the building, the field strength can be significantly attenuated. The ratio between the mean field strength inside a building at a given height above ground level and the mean field strength outside the same building at the same height above ground level expressed in (dB) is the mean building entry loss.

For Band III, in many planning documents, such as [1], [44], [2], [39], the mean building entry loss *Lb* was set to 9 dB and standard deviation σ*b* to 3 dB.

ITU‑R WP 3K has compiled measurement data on building entry loss [43] and Teracom have made additional measurements and have developed a more sophisticated model for building entry loss (see Annex E in [45]).

For example, [42] proposes for 200 MHz a median building entry loss of 10.5 dB for traditional buildings and 34.4 dB for thermally efficient buildings, as calculated in Table 114 below.

TABLE 114

Example of calculation of median building entry loss  
The value of the coefficients *u* and *v* are given in Table 1 of [42]

|  |  |  |
| --- | --- | --- |
|  | Traditional building | Thermally‑efficient building |
| Frequency, *f* | 0.2 GHz | 0.2 GHz |
| Model coefficient, *r* | 12.64 | 28.19 |
| Model coefficient, *s* | 3.72 | −3.00 |
| Model coefficient, *t* | 0.96 | 8.48 |
| Median loss for horizontal paths  *Lh* = *r* + *s* log(f) + *t* [log(*f*)]2 | 10.5 | 34.4 |
| Correction for elevation angle of the path at the building façade  *Le* = 0.212 |θ|  where θ is the elevation angle | ~ 0 | ~ 0 |
| Median building entry loss, *Lh*+ *Le* | 10.5 dB | 34.4 dB |
| σ1 = *u* + v log(*f*) | 8.2 dB | 10.8 dB |

In addition, for both cases the standard deviation σ1, is much higher than the standard deviation given in the previous planning documents. Detailed values may be calculated by the formula given in [42].

This large difference between traditional buildings and thermally efficient buildings and the much higher spread of the building entry loss values is confirmed by the Teracom measurements.

The values given in previous planning documents, *Lb* = 9 dB and σ*b* = 3 dB, represent a reference from which DAB networks have been planned for indoor reception. However, with building regulations changing to provide more thermally efficient buildings which in turn leads to extremely high median value for the building entry loss (Table 114), achieving reliable indoor RF coverage may, in future, be challenging. Network designers may need to consider alternative means for providing a service indoors within thermally efficient buildings.

#### 7.3.2.2 Vehicle (car) entry loss

A study presented in [46] shows in‑car entry losses of 8 dB with an associated standard deviation of 2 dB, based on measurements at 800 MHz. Due to the lack of investigations concerning the car entry loss and its variation with the frequency, the same value is taken for Band III. Furthermore, it is expected that the value of 8 dB will not be sufficient for estimating entry loss into trains.

### 7.3.3 Location percentages

#### 7.3.3.1 Location statistics within a pixel and prediction error

Slow fading effects are due to ground cover variations, which are important for pixel sizes substantially greater than the relevant morphography. Since the local distribution of morphographic influences within the pixel will usually be homogenous and their effects occur in a multiplicative way along the path, the loss due to slow fading fits a log‑normal distribution, independent of the signal’s bandwidth, and consequently slow fading is often called “Log‑normal Fading”. Measurements validate this assumption.

Due to the log‑normal distribution of the slow fading, the logarithm of the field strength (including slow fading only) fits a normal distribution. The field strength is characterized by a median value and its standard deviation within the area of one pixel.

More information on the location variation of field strength and its implementation for coverage prediction is given in Annex F in [45].

In many frequency planning documents, e.g. [1], a standard deviation for wideband signals of 5.5 dB is used.

Recent studies ([48], [49], [50], [51]), where a large number of measurements have been taken, show that the standard deviation of the field strength distribution within a pixel of between 20 × 20 m to 100 × 100 m in size is, depending on the clutter and also the size of the pixel, between about 2 and 4 dB. The larger the pixel size, the higher the standard deviation of the field strength distribution.

The minimum median field strength values calculated in § 7.4.1 use a standard deviation value of 4.0 dB as being a representative value.

#### 7.3.3.2 Location correction factors for different reception modes

In many cases the location correction factor is influenced not only by the location variation but also by the standard deviation of additional losses such as building entry loss or vehicle entry loss as explained in § 7.3.2.

The values used for various DAB reception modes are shown in Table 115. For indoor reception in a building, the values are on the basis of entry loss measured in traditional buildings (see § 7.3.2.1).

TABLE 115

Location Correction value calculations for various reception modes

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Reception mode | Service quality | Location variation   (dB) | Variation of other losses  (dB) | Composite location variation SD  (dB) | Location probability    % | Distribution factor value    µ | Location correction factor   *Cl* (dB) (1) | Comments |
| 1. MO (rural) | Good | 4.0 | 0 | 4.0 | 99 | 2.33 | 9.32 |  |
| Acceptable | 4.0 | 0 | 4.0 | 90 | 1.28 | 5.12 |  |
| 2. PO (suburban) | Good | 4.0 | 0 | 4.0 | 95 | 1.64 | 6.56 |  |
| Acceptable | 4.0 | 0 | 4.0 | 70 | 0.52 | 2.08 |  |
| 3. PI (urban) | Good | 4.0 | 8.2 | 9.12 | 95 | 1.64 | 14.96 | BEL |
| Acceptable | 4.0 | 8.2 | 9.12 | 70 | 0.52 | 4.74 | BEL |
| 4. PO‑H/Ext (suburban) | Good | 4.0 | 0 | 4.0 | 95 | 1.64 | 6.56 |  |
| Acceptable | 4.0 | 0 | 4.0 | 70 | 0.52 | 2.08 |  |
| 5. PI‑H/Ext (urban) | Good | 4.0 | 8.2 | 9.12 | 95 | 1.64 | 14.96 | BEL |
| Acceptable | 4.0 | 8.2 | 9.12 | 70 | 0.52 | 4.74 | BEL |
| 6. MO‑H/Ext (rural) | Good | 4.0 | 2 | 4.47 | 99 | 2.33 | 10.42 | VEL |
| Acceptable | 4.0 | 2 | 4.47 | 90 | 1.28 | 5.72 | VEL |
| BEL = Building entry loss     VEL = Vehicle entry loss  (1) The values in the Location correction factor column do not have any rounding as may be found by using the base numbers in this Table which are shown as having only two decimal places. | | | | | | | | |

## 7.4 Planning parameters

### 7.4.1 Minimum median field strength

In § 7.2.2 the minimum signal levels to overcome noise are given as the minimum receiver input power and the corresponding minimum equivalent receiver input voltage. No account is taken of any propagation effect. However, it is necessary to consider propagation effects when considering reception in a practical environment.

In defining coverage, it is indicated that due to the very rapid transition from near perfect to no reception at all, it is necessary that the minimum required signal level is achieved at a high percentage of locations. These percentages have been set at 95% for “good” and 70% for “acceptable” portable reception. For mobile reception the percentages defined were 99% and 90%, respectively.

In this section, minimum median power flux-densities and equivalent field strengths are presented which are needed for practical planning considerations. Six different reception modes are described which are listed in Table 116. The *C*/*N* values are those described in Table 108 for protection level EEP-3A associated with the reception modes defined in § 2.

TABLE 116

Reception modes, *C*/*N* values

|  |  |  |  |
| --- | --- | --- | --- |
|  | Reception mode | *C*/*N* (dB) | Channel model |
| 1 | Mobile reception / rural (MO) | 12.6 | RA 6 |
| 2 | Portable outdoor reception / suburban (PO) | 11.9 | TU 12 |
| 3 | Portable indoor reception / urban (PI) | 11.9 | TU 12 |
| 4 | Handheld portable outdoor reception / External antenna (PO-H) | 11.9 | TU 12 |
| 5 | Handheld portable indoor reception / External antenna (PI-H) | 11.9 | TU 12 |
| 6 | Handheld mobile reception / External antenna (MO-H) | 12.6 | RA 6 |

Results of calculation according to § 3.10 are provided in Table 117.

TABLE 117

DAB+ in Band III

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | **1. (MO) Mobile / rural** | **2. (PO) Portable outdoor /suburban** | **3. (PI) Portable indoor / urban** | **4. (PO‑H/Ext) Handheld portable outdoor / suburban / External antenna** | **5. (PI‑H/Ext) Handheld portable indoor / urban / External antenna** | **6. (MO‑H/Ext) Handheld mobile / rural / External antenna** |
| Frequency | Freq | MHz | 200 | 200 | 200 | 200 | 200 | 200 |
| Minimum *C*/*N* required by system | *C/N* | dB | 12.6 | 11.9 | 11.9 | 11.9 | 11.9 | 12.6 |
| Receiver noise figure | *Fr* | dB | 6 | 6 | 6 | 6 | 6 | 6 |
| Equivalent noise bandwidth | *B* | MHz | 1.54 | 1.54 | 1.54 | 1.54 | 1.54 | 1.54 |
| Receiver noise input power | *Pn* | dBW | −136.10 | −136.10 | −136.10 | −136.10 | −136.10 | −136.10 |
| Minimum receiver signal input power | *Ps min* | dBW | −123.50 | −124.20 | −124.20 | −124.20 | −124.20 | −123.50 |
| Minimum equivalent receiver input voltage, 75 Ω | *Umin* | dBµV | 15.25 | 14.55 | 14.55 | 14.55 | 14.55 | 15.25 |
| Feeder loss | *Lf* | dB | 0 | 0 | 0 | 0 | 0 | 0 |
| Antenna gain relative to half dipole | *Gd* | dB | −5 | −8 | ‑8 | −13 | −13 | −13 |
| Effective antenna aperture | *Aa* | dBm2 | −10.32 | −13.32 | −13.32 | −18.32 | −18.32 | −18.32 |
| Minimum pfd at receiving location | Φ*min* | dB(W)/m2 | −113.18 | −110.88 | −110.88 | −105.88 | −105.88 | −105.18 |
| Minimum equivalent field strength at receiving location | *Emin* | dBµV/m | 32.62 | 34.92 | 34.92 | 39.92 | 39.92 | 40.62 |
| Allowance for man‑made noise | *Pmmn* | dB | 0.90 | 1.50 | 5.30 | 0.50 | 2.40 | 0.20 |
| Entry loss (building or vehicle) | *Lb*, *Lv* | dB | 0 | 0 | 10.50 | 0 | 10.50 | 8 |
| Standard deviation of the entry loss |  | dB | 0 | 0 | 8.20 | 0 | 8.20 | 2 |
| Location probability |  | % | 90 | 70 | 70 | 70 | 70 | 90 |
| Distribution factor |  |  | 1.28 | 0.52 | 0.52 | 0.52 | 0.52 | 1.28 |
| Standard deviation (1) |  |  | 4 | 4 | 9.12 | 4 | 9.12 | 4.47 |
| Location correction factor | Cl | dB | 5.12 | 2.08 | 4.74 | 2.08 | 4.74 | 5.72 |
| Minimum median pfd at 1.5 m a.g.l.; 50% time and 50% locations (for a location probability of 90 or 70% as indicated) | Φ*med* | dB(W)/m2 | −107.16 | −107.30 | −90.34 | −103.30 | −88.24 | −91.26 |
| Minimum median equivalent field strength at 1.5 m a.g.l.; 50% time and 50% locations (for a location probability of 90 or 70% as indicated) | E*med* | dBµV/m | **38.64** | **38.50** | **55.46** | **42.50** | **57.56** | **54.54** |
| Location probability |  | % | 99 | 95 | 95 | 95 | 95 | 99 |
| Distribution factor |  |  | 2.33 | 1.64 | 1.64 | 1.64 | 1.64 | 2.33 |
| Standard deviation |  |  | 4 | 4 | 9.12 | 4.00 | 9.12 | 4.47 |
| Location correction factor | Cl | dB | 9.32 | 6.56 | 14.96 | 6.56 | 14.96 | 10.42 |
| Minimum median pfd at 1.5 m a.g.l.; 50% time and 50% locations (for a location probability of 99 or 95% as indicated) | Φ*med* | dB(W)/m2 | −102.96 | −102.82 | −80.12 | −98.82 | −78.02 | −86.57 |
| Minimum median equivalent field strength at 1.5 m a.g.l.; 50% time and 50% locations (for a location probability of 99 or 95% as indicated) | *Emed* | dBµV/m | **42.84** | **42.98** | **65.68** | **46.98** | **67.78** | **59.23** |
| **(1)** The minimum median field strength values calculated use a standard deviation value of 4 dB as being a representative value. However, when making field strength predictions for a particular pixel it is suggested to add the prediction error and therefore to use a standard deviation value of 5.5 dB. | | | | | | | | |

### 7.4.2 Transmitter spectrum mask

Outside the 1.5 MHz wide COFDM spectrum, the signal contains natural sidebands, attenuated relative to the main signal by some 40-50 dB. Although a high degree of linearity is employed, commonly used power amplifiers produce intermodulation products that increase the level of the sidebands, in some cases to only 30 dB below the main signal. These sidebands are unwanted, are considered spurious signals and should as far as possible be suppressed to allow optimum usage of the frequency spectrum. This attenuation (also called shoulder attenuation) is of importance because it allows adjacent DAB frequency blocks to be used in adjacent service areas.

The DAB signal spectrum is measured in a 4 kHz bandwidth. Inside the 1.5 MHz block the power level therefore reduces by (10 × log(4 / 1 536)) dB = −26 dB (see [54]) relative to the total power of the signal. The (shoulder) attenuation of the sidebands (out-of-band signals) is expressed in dB relative to this value.

The out-of-band radiated signal spectrum in any 4 kHz band shall be constrained by one of the masks defined in Fig. 12 and Table 118. The solid line mask shall apply to DAB transmitters in critical areas for adjacent channel interference. The dotted line mask shall apply to DAB transmitters in other circumstances for suppression of adjacent channel interference.

Figure 12

Spectrum mask for DAB out-of-band radiation



TABLE 118

Break points for spectrum masks in Fig. 12

|  |  |  |
| --- | --- | --- |
| **Frequency relative to the block centre frequency (MHz)** | **Case 1 (critical cases) relative level (dB)** | **Case 2 (uncritical cases) relative level (dB)** |
| ±0.77 | −26 | −26 |
| ±0.97 | −71 | −56 |
| ±1.75 | −106 | n.a. |
| ±3.00 | −106 | −106 |

### 7.4.3 DAB frequency block raster and bandwidth

A DAB block is a frequency channel 1.536 MHz wide. A 176 kHz guard band separates adjacent DAB blocks. DAB in VHF has been introduced in the pre‑existing 7 MHz raster of analogue TV; therefore 4 DAB blocks fit into one TV channel with a guard band of 320 kHz or 336 kHz between TV channel limits. The blocks are designated according to their TV channel position in Band III (channels 5 to 12) and labelled A through D for each TV channel, e.g. 5A for the lowest DAB block in VHF Band III.

Channel 13 (230 MHz ‑ 240 MHz), which is not covered by GE06 [1] and retains to WI95revCO07 [52], contains 6 DAB blocks with a guard band of 176 kHz. There also remains a plan entry in Band I, labelled 4A.

Figure 13

DAB frequency blocks in Band III



### 7.4.4 Protection ratios

#### 7.4.4.1 DAB versus DAB

##### 7.4.4.1.1 Co‑ channel protection ratios


The Co‑Channel Interference (CCI) Protection Ratio (PR) is used to plan DAB services on the same channel block or frequency. Generally, though the two transmissions on the same frequency should be from distant locations there will be some ‘residual’ signal power which propagates between the two areas.

To calculate the maximum allowed interference power in a specific area, the minimum power ratio between the wanted and interfering signal must be defined. As DAB uses COFDM the interfering signal appears to be AWG Noise added at the front end of the receiver. Consequently, it is reasonable to set the protection ratio at the same value as that used for Rayleigh fading, i.e. a *C*/*N* which is generally between 12 and 13 dB.

CRA undertook a number of bench tests to determine the current PR required by modern receivers. Figure 14 shows the results for a very commonly used table top receiver implementation (2016). The results show the power difference to support non‑errored audio for a range of input equivalent field strengths and channel types.

Figure 14

Protection ratio requirements for a range of channel types



The first observation is that the AWGN result is around 6 dB across the input range of −95 to −70 dBµV/m. This can be compared to the commonly used AWGN reference *C*/*N* of 7.4 dB and the results may indicate that the required AWGN *C*/*N* is less than the standard allowance.

The results for the fading channels show that the required PR is in the range 10‑14 dB with an average of 12 dB.

##### 7.4.4.1.2 Adjacent channel protection

The Protection Ratios for adjacent channel use are very important as they will have a large impact upon the design of the DAB network, in particular when adding other non co‑located services on an adjacent frequency.

National, regional and local broadcast coverage requirements will typically differ leading to alternative network implementations in an area. Introducing a new transmitter into a network has the potential to cause interference not just to co‑channel usage elsewhere, but also adjacent channel interference (ACI) in its close vicinity. The level of ACI impact will depend on many factors such as, the new transmitter power, antenna pattern ‑ both horizontal radiation pattern (HRP) and vertical radiation pattern (VRP), antenna height, whether the new transmitter is in a highly populated area or next to a busy road, and the frequency separation between the new service and the affected service. The level of impact will also depend on the robustness of the affected service and its field strength level in the area around the new transmitter site.

Impact predictions for non co‑sited proposed transmitters should be carried out. These predictions must consider the relevant adjacent channel protection ratio plus the additional margin needed to serve the required percentage locations (forming the Protection Margin). Such impact predictions will identify if the existing services are protected to their planned service level.

A field strength measurement survey can be made for the existing services to validate the coverage prediction. BER measurements should also be taken as an indication of the quality of service. These measurements will be a record of the existing service performance.

The predicted field strength difference between the services in each pixel will indicate areas where the protection margin is exceeded, this method will include pixels that would not actually hear any audible interference and therefore it is essentially very restrictive to new services.

Adjacent channel interference can be regarded as degrading the affected service within a certain area around the additional transmitter (so‑called “hole punching”), in which case the impact may be better represented by counting the proportion of users in each pixel that may be affected. This method examines the existing services predicted percentage locations served in each pixel before and after the proposed new service, the drop in predicted percentage locations multiplied by the number of households in that pixel will indicate the severity and number of households likely to be affected. If the coverage in a pixel drops below 50% locations served then receiver blocking can be assumed and all households in that pixel should be counted as lost. Assessment of many ACI situations in the UK has identified these predicted estimates to align closely with reality.

In many cases this proportional counting, combined with careful consideration of the design of the new transmitter, will reduce the predicted impact to a level that the affected broadcaster will find acceptable and hence allow the new non co‑sited service to launch.


When the new transmitter is brought to air, drive survey measurements can be taken of both services to validate the impact assessment. The proportion of measurement points within a pixel that exceed the relevant protection ratio (from Table 119) should be used to calculate the proportional impact. These results can also be scaled to represent indoor coverage impacts (only counted where the affected service provides enough field strength for an indoor service before the addition of the new transmitter). BER measurements of the affected service should again be taken to indicate where uncorrected errors have increased and to validate the field strength difference results. Annex I in [45] provides a worked example of such an ACI assessment carried out in the UK.

The critical and non‑critical spectrum masks for DAB were specified to allow a reasonable degree of overlap between service areas using adjacent channels. In deciding the masks, it was important to provide sufficient filtering reducing Out-of-Band (OOB) emissions from DAB transmissions into adjacent channels, without making filters too expensive. As such the DAB receiver’s adjacent selectivity itself is generally the main limitation when operating non co‑sited transmitters.

The IRT has carried out a number of measurements of adjacent channel protection ratios [53] during the last few years. The measurements show that these protection ratios strongly depend upon the spectrum of the interfering signal. Measurements were carried out using three differently filtered interfering signals: fulfilling the non‑critical spectrum mask, the critical spectrum mask and using an undistorted signal, shown below in Fig. 15.

Figure 15

Undistorted signal considered in IRT studies [53]



Based on BBC experience (see Annex I in [45]) and the IRT’s measurements it is suggested that, in the case of the use of the critical spectrum mask, the adjacent channel protection ratios used for planning should be based upon the following values (Table 119):

TABLE 119

Suggested adjacent channel protection ratios (together with critical mask)

|  |  |
| --- | --- |
| Interfering DAB block | Protection ratio (dB) |
| N ± 1 | ‑40 |
| N ± 2 | ‑45 |
| N ± 3 | ‑45 |

#### 7.4.4.2 DAB vs other broadcasting and non‑broadcasting systems

##### 7.4.4.2.1 General remarks

Protection ratios of DAB vs other broadcasting systems and other non‑broadcasting systems are well described in several ITU‑R documents: [1], [44], [55]. For Europe, a relevant exception is DVB‑T2 since this is a relatively new system for which no or only very few measurements exist.

The situation is different with regard to DAB+. Apart from intra‑system measurements (DAB+ vs DAB+), practically no figures are available for protection ratios of DAB+ vs other broadcasting systems and other non‑broadcasting systems.

This is not very critical, however, since in most cases an extrapolation from DAB to DAB+ is possible as well as an extrapolation from DVB‑T to DVB‑T2. The basic ideas for these extrapolations are the following:

a) All cases where DAB+ interferes with other broadcasting or non‑broadcasting systems can be treated in the same way as DAB, since both DAB and DAB+ have the same RF characteristics, being OFDM interferers, with the same bandwidth, the same carrier structure, etc.

b) For DVB‑T2 being interfered with by DAB/DAB+, it is proposed that the protection ratios of a corresponding DVB‑T mode (modulation scheme + code rate) be used; in this case, corresponding means having the same (or a similar) *C*/*N* value.

c) For DAB+ being interfered with by DVB‑T/DVB‑T2, it is proposed that the *C*/*N* of DAB+ vs. DAB+ minus 6 dB be used, since the ratio of DAB+ and DVB‑T/T2 bandwidths is 1/4.  
Non fully overlapping DAB+ and DVB‑T/T2 channels should be treated according to Tables A.3.3‑13/14 of [1].

d) For DAB+ being interfered with by other services, it is proposed to use the following procedure:  
The PR for DAB vs the other service (OS) exists: *PRDAB‑OS*, as well as the *C*/*N* of DAB: *C*/*NDAB*.  
These values can be taken from [1] or [37]; typically DAB mode ‘Protection Level 3’ is chosen.

The quantity Δ*OS* = *C*/*NDAB* ‑ *PRDAB*‑*OS* is defined.

It is assumed that Δ*OS* is representative for all protection levels, also for DAB+.

The PR for DAB+ being interfered with by OS is then given by:

*PRDAB+‑OS* = *C*/*NDAB*+ ‑ Δ*OS*

This procedure is a pragmatic but qualitative approach, in view of the lack of measurement results. It may be replaced in the future when results of DAB+ measurements become available.

##### 7.4.4.2.2 DAB vs DVB‑T/T2

Protection ratios for DAB vs DVB‑T are given in Appendix 3.3 to Annex 2 of [1], Tables A.3.3‑13 ‑ 22.

Protection ratios for DAB vs DVB‑T2 and DAB+ vs DVB‑T/T2 may be derived by applying the procedure described in § 7.4.4.2.1.

##### 7.4.4.2.3 DAB vs other services

Protection ratios for DAB vs Other Services are given in Appendix 4.3 to Annex 2 of [1], Tables A.4.3‑2 to A.4.3‑5.

PRs for DAB+ vs Other Services may be derived by applying the procedure described in § 7.4.4.2.1.

# 8 Planning parameters for digital terrestrial broadcasting system ISDB-TSB in VHF bands II and III

ISDB-TSB system (Digital System F) is designed to provide high-quality sound and data broadcasting with high reliability even in mobile reception. The system is also designed to provide flexibility, expandability, and commonality for multimedia broadcasting using terrestrial networks. The system uses OFDM modulation with band segmented transmission, two-dimensional frequency-time interleaving and concatenated error correction codes. The system has commonality with the ISDB‑T system for digital terrestrial television broadcasting in the physical layer.

## 8.1 System parameters of ISDB-TSB

The system has a wide variety of transmission parameters such as carrier modulation scheme, coding rates of the inner error correction code, and length of time interleaving. Some of the carriers are assigned to TMCC carriers which transmit the information on the transmission parameters for receiver control. System parameters of the ISDB-TSB system are described in Annex 3 of Recommendation ITU-R BS.1114.

## 8.2 Receiver parameters

Receiver parameters for different types of reception (mobile, portable, and fixed) of the ISDB-TSB system are described in Annex 2 of Recommendation ITU-R BS.1660.

## 8.3 ISDB-TSB planning parameters

Planning criteria for the the ISDB-TSB system in VHF band II and III are described in Annex 2 of Recommendation ITU-R BS.1660.

# 9 Planning parameters for digital terrestrial broadcasting system CDR in VHF

The CDR system is designed for terrestrial digital sound broadcasting in VHF Bands II. The system is nationally standardized in China. Main characteristics and features of CDR can be found in Recommendation ITU‑R [BS.1114-10](https://www.itu.int/rec/R-REC-BS.1114/en) – Systems for terrestrial digital sound broadcasting to vehicular, portable and fixed receivers in the frequency range 30-3 000 MHz.

## 9.1 System parameters of CDR

### 9.1.1 CDR signal parameters

The choice of system transmission parameters determines the performance of the CDR system. Three selected typical CDR system operating modes (see Table 120) were used for the derivation of the minimum median field-strength.

1 Transmission mode 1-spectral mode B-QPSK-3/4, which is a moderately protected signal with a suitable data rate, is applied for audio services and data services in the case of all digital modes.

2 Transmission mode 1-spectral mode C-QPSK-3/4, as a moderately protected signal with a suitable data rate, is applied for audio services and data services in the case of analog-to-multicast mode.

3 Transmission mode 1-spectral mode B-QPSK-1/2, which keeps a balanced performance between the data rate and the reliability, is applied for audio services and data services in the case of all digital modes.

TABLE 120

CDR System working mode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Transmission mode | Modulation method | Coding rate | Spectrum mode | Payload rate  (kbit/s) |
| 1 | 1 | QPSK | 3/4 | B | 216 |
| 2 | 1 | QPSK | 3/4 | C | 108 |
| 3 | 1 | QPSK | 1/2 | B | 144 |

### 9.1.2 CDR radio receiver related parameters

CDR receiver is intended to receive and decode programmes transmitted according to the CDR system specification.

The parameters relevant for determining the required minimum field-strength levels are:

–noise figure *Fr* (dB), measured from the antenna input to the I/Q base band CDR decoder input (including down conversion and A/D conversion);

– receiver noise input power *Pn* (dBW);

–minimum carrier-to-noise ratio (*C*/*N*)*min* (dB) at the CDR decoder input;

–minimum receiver input power level *Ps,min* (dBW).

Considering the cost-effective CDR receiver solution, the parameters relevant for determining the required minimum field-strength levels are:

–the receiver noise coefficient *Fr* is set to 7 dB. When *K* = 1.38 × 10–23 J/K, *B* = 100 kHz and *T* = 290 K,

–the resulting PLL receiver noise input power for spectral mode Cspectral mode C is *Pn* = −146.98 (dBW); when *K* = 1.38×10–23 J/K, *B* = 200 kHz and *T* = 290 K,

–CDR receiver noise input power of spectrum mode 2 is *Pn* = −143.97 (dBW)

Using the average BER = 1 × 10−4 (bit) as the failure criterion, the (*C*/*N*)*min* of the CDR system is when the receiver under test reaches the failure criterion after the channel decoder for different channel modes. The ratio of the signal to the noise, (*C*/*N*)*min* for three typical modes of operation for different receiving modes is shown in Table 121. Channel models are shown in Tables 122 and 123.

TABLE 121

(*C*/*N*)*min*  Of three typical working modes

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | (*C*/*N*)*min*(dB) | | |
| Receiving mode | channel model | Transmission mode 1, Spectrum mode B,QPSK,3/4 | Transmission mode 1, Spectrum mode C,QPSK,3/4 | Transmission mode 1, Spectrum mode B,QPSK,1/2 |
| Fixed reception | Gaussian channel | 5 | 5 | 2.2 |
| Portable reception  (city static) | Static multipath model  (see Table 122) | 5.5 | 5.5 | 2.5 |
| Mobile reception (city 60 km/h) | Dynamic multipath model  (see Table 123) | 14.3 | 13 | 8.8 |

TABLE 122

Static multipath model

|  |  |  |
| --- | --- | --- |
| Path | Delay  (µs) | Relative amplitude  (dB) |
| 1 | 0.0 | −2.0 |
| 2 | 0.2 | 0.0 |
| 3 | 0.5 | −3.0 |
| 4 | 0.9 | −4.0 |
| 5 | 1.2 | −2.0 |
| 6 | 1.4 | 0.0 |
| 7 | 2.0 | −3.0 |
| 8 | 2.4 | −5.0 |
| 9 | 3.0 | −10.0 |

TABLE 123

Dynamic multipath model

|  |  |  |  |
| --- | --- | --- | --- |
| Path | Delay  (µs) | Relative amplitude  (dB) | Path Type |
| 1 | 0.0 | −2.0 | classical |
| 2 | 0.2 | 0.0 | classical |
| 3 | 0.5 | −3.0 | classical |
| 4 | 0.9 | −4.0 | classical |
| 5 | 1.2 | −2.0 | classical |
| 6 | 1.4 | 0.0 | classical |
| 7 | 2.0 | −3.0 | classical |
| 8 | 2.4 | −5.0 | classical |
| 9 | 3.0 | −10.0 | classical |

## 9.2 Minimum receiver input power level

According to the above values and considering the operation loss, the minimum receiving input power of the three typical working modes of the CDR system under different receiving modes can be calculated. See Tables 124 to 126.

TABLE 124

Minimum receiver input power for  
Transmission Mode 1 – Spectrum Mode B-QPSK-3/4

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Receiving mode | | Fixed reception | Portable reception | Mobile reception |
| Receiver noise coefficient | *Fr* (dB) | 7 | 7 | 7 |
| Receiver noise input power | *Pn* (dBW) | −146.98 | −146.98 | −146.98 |
| *(C*/*N)min* | (*C*/*N*)*min* (dB) | 5 | 5.5 | 14.3 |
| Operating loss | *Li* (dB) | 3 | 3 | 3 |
| Minimum receiver input power | *Ps, min* (dBW) | −138.98 | −138.48 | −129.68 |

TABLE 125

Minimum receiver input power for   
Transmission Mode 1 – Spectrum Mode C-QPSK-3/4

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Receiving mode | | Fixed reception | Portable reception | Mobile reception |
| Receiver noise coefficient | *Fr* (dB) | 7 | 7 | 7 |
| Receiver noise input power | *Pn* (dBW) | −143.97 | −143.97 | −143.97 |
| *(C*/*N)min* | (*C*/*N*)*min* (dB) | 5 | 5.5 | 13 |
| Operating loss | *Li* (dB) | 3 | 3 | 3 |
| Minimum receiver input power | *Ps, min* (dBW) | −135.97 | −135.47 | −127.97 |

TABLE 126

Minimum receiver input power for   
Transmission Mode 1 – Spectrum Mode B-QPSK-1/2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Receiving mode | | Fixed reception | Portable reception | Mobile reception |
| Receiver noise coefficient | *Fr* (dB) | 7 | 7 | 7 |
| Receiver noise input power | *Pn* (dBW) | −146.98 | −146.98 | −146.98 |
| *(C*/*N)min* | (*C*/*N*)*min* (dB) | 2.2 | 2.5 | 8.8 |
| Operating loss | *Li* (dB) | 3 | 3 | 3 |
| Minimum receiver input power | *Ps, min* (dBW) | −141.78 | −141.48 | −135.18 |

## 9.3 Minimum median field-strength for planning

The calculation of the minimum median field-strength can be divided into the following steps under the condition of 50% time probability, 50% location probability and receiving antenna is 10 m above the ground:

(1) Calculate receiver noise input power *Pn*

*Pn* = *Fr*+10log10(*K* · *T*0 · *B*) (dBW) (52)

where:

*Fr* : receiver noise coefficient (dB)

*K* : Boltzmann constant (*k* = 1.38 × 10 – 23(J/K))

*T*0 : absolute temperature (*T*0 = 290(K))

*B* : receiver noise bandwidth (1 × 105Hz or 2 × 105Hz).

(2) Calculate the minimum receiver input power *Ps,min*

*Ps,min* =(*C*/*N*)*min*+ *Pn* (dBW) (53)

where:

(*C*/*N*)*min*: RF input-to-noise ratio at the receiver input required by the system (dB).

(3) Calculate the minimum power flux density at the receiving location ϕ*min*

ϕ*min* = *Ps,min*– *Aa*+ *Lf*(dBW/m2) (54)

*Aa*= *G* + 10 log (1.64λ2/4π) (dBm2) (55)

where:

*Aa* : receive antenna effective aperture (dBm2)

*Lf* : feeder loss (dB)

*G* : antenna gain of the receiving antenna relative to the half-wave dipole (dBd)

λ : signal wavelength (m).

(4) Calculate the minimum equivalent field-strength at the receiving location *Emin*

*Emin* = ϕ*min* +10 log10 (*ZF*0) + 20log10(1V/1μV) (dBμV/m) (56)

where:

        Typical impedance of free space (57)

therefore:

*Emin* = ϕ*min* + 145.8 (dBμV/m) (58)

(5) Calculate the minimum median field-strength *Emed*

The minimum median field-strength for different receiving scenarios is calculated as follows:

*Emed* = *Emin+ Pmmn+ Cl* (dBμV/m), Fixed reception (59)

*Emed* = *Emin+ Pmmn+ Cl + Lh* (dBμV/m), Outdoor portable and mobile reception (60)

*Emed* = *Emin+ Pmmn+ Cl + Lh+ Lb* (dBμV/m), Indoor portable reception (61)

Based on the parameters and equations set above, the minimum median field-strength level for different reception modes and frequency Bands I and II can be calculated for CDR system parameters, as shown in Tables 127 to 132.

TABLE 127

The minimum median field-strength level of  
Transmission Mode 1 – Spectrum ModeB- QPSK-3/4 (urban and suburban)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Receiving mode | | FX | PI | PO | MO |
| Minimum receiver input power | *Ps, min* (dBW) | −138.98 | −138.48 | −138.48 | −129.68 |
| Antenna gain | *G* (dBd) | 0 | −2 | −2 | −2 |
| Effective antenna aperture | *Aa* (dBm2) | 0.7 | −1.3 | −1.3 | −1.3 |
| Feeder loss | *Lc*(dB) | 1.5 | 0 | 0 | 0.3 |
| Minimum power flux density | φ*min* (dBW/m2) | −138.18 | −137.18 | −137.18 | −128.08 |
| Minimum field-strength | *Emin* (dB(μV/m)) | 7.62 | 8.62 | 8.62 | 17.72 |
| Artificial noise tolerance | *Pmmn* (dB) | 14.55 | 14.55 | 14.55 | 14.55 |
| Antenna height loss | *Lh* (dB) | 0 | 10 | 10 | 10 |

TABLE 127 (*end*)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Receiving mode | | FX | PI | PO | MO |
| Building penetration loss | *Lb* (dB) | 0 | 9 | 0 | 0 |
| Location probability | % | 70 | 95 | 95 | 99 |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 2.33 |
| Standard error of CDR field-strength | σ*m*(dB) | 3.8 | 3.8 | 3.8 | 3.8 |
| Standard error of MMN | σ*mmn*(dB) | 6.6 | 6.6 | 6.6 | 6.6 |
| Standard deviation of building penetration loss | σ*b*(dB) | 0 | 3 | 0 | 0 |
| Location correction factor | *Cl*(dB) | 3.96 | 13.42 | 12.49 | 17.74 |
| Minimum median field- strength level | *Emed* (dB(μV/m)) | 26.13 | 55.59 | 45.66 | 60.01 |

TABLE 128

The minimum median field-strength level of  
Transmission Mode 1 – Spectrum Mode C-QPSK-3/4 (urban and suburban)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Receiving mode | | FX | PI | PO | MO |
| Minimum receiver input power | *Ps, min* (dBW) | −135.97 | −135.47 | −135.47 | −127.97 |
| Antenna gain | *G* (dBd) | 0 | −2 | −2 | −2 |
| Effective antenna aperture | *Aa* (dBm2) | 0.7 | −1.3 | −1.3 | −1.3 |
| Feeder loss | *Lc*(dB) | 1.5 | 0 | 0 | 0.3 |
| Minimum power flux density | φ*min* (dBW/m2) | −135.17 | −134.17 | −134.17 | −126.37 |
| Minimum field-strength | *Emin* (dB(μV/m)) | 10.63 | 11.63 | 11.63 | 19.43 |
| Artificial noise tolerance | *Pmmn* (dB) | 14.55 | 14.55 | 14.55 | 14.55 |
| Antenna height loss | *Lh* (dB) | 0 | 10 | 10 | 10 |
| Building penetration loss | *Lb* (dB) | 0 | 9 | 0 | 0 |
| Location probability | % | 70 | 95 | 95 | 99 |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 2.33 |
| Standard error of CDR field-strength | σ*m* (dB) | 3.8 | 3.8 | 3.8 | 3.8 |
| Standard error of MMN | σ*mmn* (dB) | 6.6 | 6.6 | 6.6 | 6.6 |
| Standard deviation of building penetration loss | σ*b*(dB) | 0 | 3 | 0 | 0 |
| Location correction factor | *Cl* (dB) | 3.96 | 13.42 | 12.49 | 17.74 |
| Minimum median field- strength level | *Emed* (dB(μV/m)) | 29.14 | 58.6 | 48.67 | 61.72 |

TABLE 129

The minimum median field-strength level of   
Transmission Mode 1 – Spectrum Mode B-QPSK-1/2 (urban and suburban)

| Receiving mode | | FX | PI | PO | MO |
| --- | --- | --- | --- | --- | --- |
| Minimum receiver input power | *Ps, min* (dB) | −141.78 | −141.48 | −141.48 | −135.18 |
| Antenna gain | *G* (dBd) | 0 | −2 | −2 | −2 |
| Effective antenna aperture | *Aa* (dBm2) | 0.7 | −1.3 | −1.3 | −1.3 |
| Feeder loss | *Lc*(dB) | 1.5 | 0 | 0 | 0.3 |
| Minimum power flux density | φ*min* (dBW/m2) | −140.98 | −140.18 | −140.18 | −133.58 |
| Minimum field-strength | *Emin* (dB(μV/m)) | 4.82 | 5.62 | 5.62 | 12.22 |
| Artificial noise tolerance | *Pmmn* (dB) | 14.55 | 14.55 | 14.55 | 14.55 |
| Antenna height loss | *Lh* (dB) | 0 | 10 | 10 | 10 |
| Building penetration loss | *Lb* (dB) | 0 | 9 | 0 | 0 |
| Location probability | % | 70 | 95 | 95 | 99 |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 2.33 |
| Standard error of CDR field-strength | σ*m*(dB) | 3.8 | 3.8 | 3.8 | 3.8 |
| Standard error of MMN | σ*mmn*(dB) | 6.6 | 6.6 | 6.6 | 6.6 |
| Standard deviation of building penetration loss | σ*b*(dB) | 0 | 3 | 0 | 0 |
| Location correction factor | *Cl* (dB) | 3.96 | 13.42 | 12.49 | 17.74 |
| Minimum median field- strength level | *Emed* (dB(μV/m)) | 23.33 | 52.59 | 42.66 | 54.51 |

TABLE 130

The minimum median field-strength level of  
Transmission Mode 1 – Spectrum Mode B-QPSK-3/4 (rural area)

| Receiving mode | | FX | PI | PO | MO |
| --- | --- | --- | --- | --- | --- |
| Minimum receiver input power | *Ps, min* (dBW) | −138.98 | −138.48 | −138.48 | −129.68 |
| Antenna gain | *G* (dBd) | 0 | −2 | −2 | −2 |
| Effective antenna aperture | *Aa* (dBm2) | 0.7 | −1.3 | −1.3 | −1.3 |
| Feeder loss | *Lc*(dB) | 1.5 | 0 | 0 | 0.3 |
| Minimum power flux density | φ*min* (dBW/m2) | −138.18 | −137.18 | −137.18 | −128.08 |
| Minimum field-strength | *Emin* (dB(μV/m)) | 7.62 | 8.62 | 8.62 | 17.72 |
| Artificial noise tolerance | *Pmmn* (dB) | 14.55 | 14.55 | 14.55 | 14.55 |
| Antenna height loss | *Lh* (dB) | 0 | 10 | 10 | 10 |
| Building penetration loss | *Lb* (dB) | 0 | 9 | 0 | 0 |
| Location probability | % | 70 | 95 | 95 | 99 |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 2.33 |
| Standard error of CDR field-strength | σ*m*(dB) | 3.1 | 3.1 | 3.1 | 3.1 |

TABLE 130 (*end*)

| Receiving mode | | FX | PI | PO | MO |
| --- | --- | --- | --- | --- | --- |
| Standard error of MMN | σ*mmn*(dB) | 5.3 | 5.3 | 5.3 | 5.3 |
| Standard deviation of building penetration loss | σ*b*(dB) | 0 | 3 | 0 | 0 |
| Location correction factor | *Cl* (dB) | 3.19 | 11.21 | 10.07 | 14.31 |
| Minimum median field- strength level | *Emed* (dB(μV/m)) | 25.36 | 53.38 | 43.24 | 56.58 |

TABLE 131

The minimum median field-strength level of   
Transmission Mode 1 – Spectrum ModeC-QPSK-3/4 (rural area)

| Receiving mode | | FX | PI | PO | MO |
| --- | --- | --- | --- | --- | --- |
| Minimum receiver input power | *Ps, min* (dBW) | −135.97 | −135.47 | −135.47 | −127.97 |
| Antenna gain | *G* (dBd) | 0 | −2 | −2 | −2 |
| Effective antenna aperture | *Aa* (dBm2) | 0.7 | −1.3 | −1.3 | −1.3 |
| Feeder loss | *Lc*(dB) | 1.5 | 0 | 0 | 0.3 |
| Minimum power flux density | φ*min* (dBW/m2) | −135.17 | −134.17 | −134.17 | −126.37 |
| Minimum field-strength | *Emin* (dB(μV/m)) | 10.63 | 11.63 | 11.63 | 19.43 |
| Artificial noise tolerance | *Pmmn* (dB) | 14.55 | 14.55 | 14.55 | 14.55 |
| Antenna height loss | *Lh* (dB) | 0 | 10 | 10 | 10 |
| Building penetration loss | *Lb* (dB) | 0 | 9 | 0 | 0 |
| Location probability | % | 70 | 95 | 95 | 99 |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 2.33 |
| Standard error of CDR field-strength | σ*m* (dB) | 3.1 | 3.1 | 3.1 | 3.1 |
| Standard error of MMN | σ*mmn*(dB) | 5.3 | 5.3 | 5.3 | 5.3 |
| Standard deviation of building penetration loss | σ*b*(dB) | 0 | 3 | 0 | 0 |
| Location correction factor | *Cl* (dB) | 3.19 | 11.21 | 10.07 | 14.31 |
| Minimum median field- strength level | *Emed* (dB(μV/m)) | 28.37 | 56.39 | 46.25 | 58.29 |

TABLE 132

The minimum median field-strength level of   
Transmission Mode 1 Spectrum Mode B-QPSK-1/2 (rural area)

| Receiving mode | | FX | PI | PO | MO |
| --- | --- | --- | --- | --- | --- |
| Minimum receiver input power | *Ps, min* (dBW) | −141.78 | −141.48 | −141.48 | −135.18 |
| Antenna gain | *G* (dBd) | 0 | −2 | −2 | −2 |
| Effective antenna aperture | *Aa* (dBm2) | 0.7 | −1.3 | −1.3 | −1.3 |
| Feeder loss | *Lc*(dB) | 1.5 | 0 | 0 | 0.3 |
| Minimum power flux density | φ*min* (dBW/m2) | −140.98 | −140.18 | −140.18 | −133.58 |
| Minimum field-strength | *Emin* (dB(μV/m)) | 4.82 | 5.62 | 5.62 | 12.22 |
| Artificial noise tolerance | *Pmmn* (dB) | 14.55 | 14.55 | 14.55 | 14.55 |
| Antenna height loss | *Lh* (dB) | 0 | 10 | 10 | 10 |
| Building penetration loss | *Lb* (dB) | 0 | 9 | 0 | 0 |
| Location probability | % | 70 | 95 | 95 | 99 |
| Distribution factor | μ | 0.52 | 1.64 | 1.64 | 2.33 |
| Standard error of CDR field-strength | σ*m*(dB) | 3.1 | 3.1 | 3.1 | 3.1 |
| Standard error of MMN | σ*mmn*(dB) | 5.3 | 5.3 | 5.3 | 5.3 |
| Standard deviation of building penetration loss | σ*b* (dB) | 0 | 3 | 0 | 0 |
| Location correction factor | *Cl* (dB) | 3.19 | 11.21 | 10.07 | 14.31 |
| Minimum median field- strength level | *Emed* (dB(μV/m)) | 22.56 | 50.38 | 40.24 | 51.08 |

Annex 1   
  
Symbols and abbreviations

For the purposes of the present Report, the following symbols and abbreviations apply:

φ*min* Minimum power flux-density at receiving place (dBW/m2)

*Aa* Effective antenna aperture (dBm2)

*B* Receiver noise bandwidth (Hz)

BEL Building entry loss

*CF* Combined location correction factor (dB)

*C*l Location correction factor (dB)

*c*0 Velocity of light in free space (km/s)

*d* Antenna directivity

DAB/DAB+ Digital audio broadcasting

*Decho(max)* Maximum echo delay distance (km)

DRM+ DRM mode E

*E* RMS field-strength level (dB)

*Emin* Equivalent minimum RMS field-strength level at receiving place (dB(μV/m))

*Emed* Equivalent median RMS field-strength level, planning value (dB(μV/m))

*Fa* Antenna noise figure (dB)

*Fa,med* Antenna noise figure mean value (dB)

*Fr* Receiver noise figure (dB)

*Fs* System equivalent noise figure (dB)

FM Frequency modulation

*fa* Antenna noise factor

*fr* Receiver noise factor

*g* Linear antenna gain (dB)

*G* Antenna gain (dB)

*GD* Antenna gain with reference to half-wave dipole (dBd)

Δ*G* Antenna gain variation (dB)

η Antenna efficiency

*k* Boltzmann’s constant (J/K)

*K* Correction factor for the macro-scale standard deviation σ*m* (dB)

*l* Cable length (m)

λ Wavelength (m)

*Lb* Mean building entry loss (dB)

*Lf* Feeder loss (dB)

*L′f*  Feeder loss per unit length (dB/m)

*Lh* Height loss correction factor (10 m a.g.l. to 1.5 m. a.g.l.) (dB)

μ Distribution factor

MMN Allowance for man-made noise

MSC Main service channel

*Ns* Number of symbols per frame in DRM mode E (ms)

OFDM Orthogonal Frequency Division Multiplexing

*p* Percentage of receiving locations (location probability) (%)

*PL* Protection level in DRM mode E

*Pmmn* Man-made noise level (dB)

*Pn*  Receiver noise input power (dBW)

*PR* Protection ratio (dB)

*PRbasic* Basic protection ratio (dB)

*Ps*,*min* Minimum receiver signal input power (dBW)

QAM Quadrature amplitude modulation

QPSA Quadrature phase shift keying

*R* Code rate

*RL* Antenna loss resistance (Ω)

*Rr* Antenna radiation resistance (Ω)

σ*b* Building entry loss standard deviation (dB)

σ*c* Combined standard deviation (dB)

σ*m* Macro-scale standard deviation (dB)

σ*m,DRM* Macro-scale standard deviation for DRM (dB)

σ*m*,DAB Macro-scale standard deviation for DAB (dB)

σ*m*,FM Macro-scale standard deviation for FM (dB)

σMMN Man-made noise standard deviation (dB)

SDC Service description channel

SFN Single frequency network

*T* Elementary time period of DRM mode E (ms)

*Tf* Duration of transmission frame of DRM mode E (ms)

*Tg* Duration of guard interval of DRM mode E (ms)

*Ts* Duration of OFDM symbol of DRM mode E (ms)

*Tu* Duration of useful (orthogonal) part of DRM mode E (ms)

*T*0 Absolute temperature (K)

VEL Vehicle entry loss

VHF very high frequency

*ZF*0 Characteristic impedance in free space (Ω).

Annex 2   
  
Technical references

# 1 Position of DRM frequencies

## 1.1 VHF Band II

The DRM centre frequencies are positioned in 100 kHz distance according to the FM frequency grid and ETSI-DRM [6]. The nominal carrier frequencies are, in principle, integral multiples of 100 kHz [5], see Table 133. A 50 kHz channel spacing is considered.

TABLE 133

Position of DRM frequencies in VHF Band II (87.5-108 MHz)

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DRM channel centre frequency *fC* (MHz) | DRM channel number |  | DRM channel centre frequency *fC* (MHz) | DRM channel number |  | DRM channel centre frequency *fC* (MHz) | DRM channel number |  | DRM channel centre frequency *fC* (MHz) | DRM channel number |
| 87.6 | 1 |  | 92.7 | 52 |  | 97.8 | 103 |  | 102.9 | 154 |
| 87.7 | 2 |  | 92.8 | 53 |  | 97.9 | 104 |  | 103.0 | 155 |
| 87.8 | 3 |  | 92.9 | 54 |  | 98.0 | 105 |  | 103.1 | 156 |
| 87.9 | 4 |  | 93.0 | 55 |  | 98.1 | 106 |  | 103.2 | 157 |
| 88.0 | 5 |  | 93.1 | 56 |  | 98.2 | 107 |  | 103.3 | 158 |
| 88.1 | 6 |  | 93.2 | 57 |  | 98.3 | 108 |  | 103.4 | 159 |
| 88.2 | 7 |  | 93.3 | 58 |  | 98.4 | 109 |  | 103.5 | 160 |
| 88.3 | 8 |  | 93.4 | 59 |  | 98.5 | 110 |  | 103.6 | 161 |
| 88.4 | 9 |  | 93.5 | 60 |  | 98.6 | 111 |  | 103.7 | 162 |
| 88.5 | 10 |  | 93.6 | 61 |  | 98.7 | 112 |  | 103.8 | 163 |
| 88.6 | 11 |  | 93.7 | 62 |  | 98.8 | 113 |  | 103.9 | 164 |
| 88.7 | 12 |  | 93.8 | 63 |  | 98.9 | 114 |  | 104.0 | 165 |
| 88.8 | 13 |  | 93.9 | 64 |  | 99.0 | 115 |  | 104.1 | 166 |
| 88.9 | 14 |  | 94.0 | 65 |  | 99.1 | 116 |  | 104.2 | 167 |
| 89.0 | 15 |  | 94.1 | 66 |  | 99.2 | 117 |  | 104.3 | 168 |
| 89.1 | 16 |  | 94.2 | 67 |  | 99.3 | 118 |  | 104.4 | 169 |

TABLE 133 (*end*)

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DRM channel centre frequency *fC* (MHz) | DRM channel number |  | DRM channel centre frequency *fC* (MHz) | DRM channel number |  | DRM channel centre frequency *fC* (MHz) | DRM channel number |  | DRM channel centre frequency *fC* (MHz) | DRM channel number |
| 89.2 | 17 |  | 94.3 | 68 |  | 99.4 | 119 |  | 104.5 | 170 |
| 89.3 | 18 |  | 94.4 | 69 |  | 99.5 | 120 |  | 104.6 | 171 |
| 89.4 | 19 |  | 94.5 | 70 |  | 99.6 | 121 |  | 104.7 | 172 |
| 89.5 | 20 |  | 94.6 | 71 |  | 99.7 | 122 |  | 104.8 | 173 |
| 89.6 | 21 |  | 94.7 | 72 |  | 99.8 | 123 |  | 104.9 | 174 |
| 89.7 | 22 |  | 94.8 | 73 |  | 99.9 | 124 |  | 105.0 | 175 |
| 89.8 | 23 |  | 94.9 | 74 |  | 100.0 | 125 |  | 105.1 | 176 |
| 89.9 | 24 |  | 95.0 | 75 |  | 100.1 | 126 |  | 105.2 | 177 |
| 90.0 | 25 |  | 95.1 | 76 |  | 100.2 | 127 |  | 105.3 | 178 |
| 90.1 | 26 |  | 95.2 | 77 |  | 100.3 | 128 |  | 105.4 | 179 |
| 90.2 | 27 |  | 95.3 | 78 |  | 100.4 | 129 |  | 105.5 | 180 |
| 90.3 | 28 |  | 95.4 | 79 |  | 100.5 | 130 |  | 105.6 | 181 |
| 90.4 | 29 |  | 95.5 | 80 |  | 100.6 | 131 |  | 105.7 | 182 |
| 90.5 | 30 |  | 95.6 | 81 |  | 100.7 | 132 |  | 105.8 | 183 |
| 90.6 | 31 |  | 95.7 | 82 |  | 100.8 | 133 |  | 105.9 | 184 |
| 90.7 | 32 |  | 95.8 | 83 |  | 100.9 | 134 |  | 106.0 | 185 |
| 90.8 | 33 |  | 95.9 | 84 |  | 101.0 | 135 |  | 106.1 | 186 |
| 90.9 | 34 |  | 96.0 | 85 |  | 101.1 | 136 |  | 106.2 | 187 |
| 91.0 | 35 |  | 96.1 | 86 |  | 101.2 | 137 |  | 106.3 | 188 |
| 91.1 | 36 |  | 96.2 | 87 |  | 101.3 | 138 |  | 106.4 | 189 |
| 91.2 | 37 |  | 96.3 | 88 |  | 101.4 | 139 |  | 106.5 | 190 |
| 91.3 | 38 |  | 96.4 | 89 |  | 101.5 | 140 |  | 106.6 | 191 |
| 91.4 | 39 |  | 96.5 | 90 |  | 101.6 | 141 |  | 106.7 | 192 |
| 91.5 | 40 |  | 96.6 | 91 |  | 101.7 | 142 |  | 106.8 | 193 |
| 91.6 | 41 |  | 96.7 | 92 |  | 101.8 | 143 |  | 106.9 | 194 |
| 91.7 | 42 |  | 96.8 | 93 |  | 101.9 | 144 |  | 107.0 | 195 |
| 91.8 | 43 |  | 96.9 | 94 |  | 102.0 | 145 |  | 107.1 | 196 |
| 91.9 | 44 |  | 97.0 | 95 |  | 102.1 | 146 |  | 107.2 | 197 |
| 92.0 | 45 |  | 97.1 | 96 |  | 102.2 | 147 |  | 107.3 | 198 |
| 92.1 | 46 |  | 97.2 | 97 |  | 102.3 | 148 |  | 107.4 | 199 |
| 92.2 | 47 |  | 97.3 | 98 |  | 102.4 | 149 |  | 107.5 | 200 |
| 92.3 | 48 |  | 97.4 | 99 |  | 102.5 | 150 |  | 107.6 | 201 |
| 92.4 | 49 |  | 97.5 | 100 |  | 102.6 | 151 |  | 107.7 | 202 |
| 92.5 | 50 |  | 97.6 | 101 |  | 102.7 | 152 |  | 107.8 | 203 |
| 92.6 | 51 |  | 97.7 | 102 |  | 102.8 | 153 |  | 107.9 | 204 |

## 1.2 VHF Band III

The frequency band of a DAB block has a bandwidth of 1.536 MHz with lower and upper guard channels to fit into the 7 MHz channels of VHF Band III. The DRM centre frequencies are positioned in 100 kHz distance beginning by 174.05 MHz and integral multiples of 100 kHz up to 229.95 MHz, see Table 134.

The nomenclature of the DRM channel identifier is given by:

(No. of the VHF channel) – (No. of the DRM channel suffix in the VHF channel),

e.g. for the first DRM channel in this Table the identifier is “5‑1”.

TABLE 134

Position of DRM frequencies in VHF Band III (174-230 MHz)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DRM channel suffix | DRM channel centre frequency *fC* (MHz) in VHF channel (number) | | | | | | | |
| 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 |
| 1 | 174.050 | 181.050 | 188.050 | 195.050 | 202.050 | 209.050 | 216.050 | 223.050 |
| 2 | 174.150 | 181.150 | 188.150 | 195.150 | 202.150 | 209.150 | 216.150 | 223.150 |
| 3 | 174.250 | 181.250 | 188.250 | 195.250 | 202.250 | 209.250 | 216.250 | 223.250 |
| 4 | 174.350 | 181.350 | 188.350 | 195.350 | 202.350 | 209.350 | 216.350 | 223.350 |
| 5 | 174.450 | 181.450 | 188.450 | 195.450 | 202.450 | 209.450 | 216.450 | 223.450 |
| 6 | 174.550 | 181.550 | 188.550 | 195.550 | 202.550 | 209.550 | 216.550 | 223.550 |
| 7 | 174.650 | 181.650 | 188.650 | 195.650 | 202.650 | 209.650 | 216.650 | 223.650 |
| 8 | 174.750 | 181.750 | 188.750 | 195.750 | 202.750 | 209.750 | 216.750 | 223.750 |
| 9 | 174.850 | 181.850 | 188.850 | 195.850 | 202.850 | 209.850 | 216.850 | 223.850 |
| 10 | 174.950 | 181.950 | 188.950 | 195.950 | 202.950 | 209.950 | 216.950 | 223.950 |
| 11 | 175.050 | 182.050 | 189.050 | 196.050 | 203.050 | 210.050 | 217.050 | 224.050 |
| 12 | 175.150 | 182.150 | 189.150 | 196.150 | 203.150 | 210.150 | 217.150 | 224.150 |
| 13 | 175.250 | 182.250 | 189.250 | 196.250 | 203.250 | 210.250 | 217.250 | 224.250 |
| 14 | 175.350 | 182.350 | 189.350 | 196.350 | 203.350 | 210.350 | 217.350 | 224.350 |
| 15 | 175.450 | 182.450 | 189.450 | 196.450 | 203.450 | 210.450 | 217.450 | 224.450 |
| 16 | 175.550 | 182.550 | 189.550 | 196.550 | 203.550 | 210.550 | 217.550 | 224.550 |
| 17 | 175.650 | 182.650 | 189.650 | 196.650 | 203.650 | 210.650 | 217.650 | 224.650 |
| 18 | 175.750 | 182.750 | 189.750 | 196.750 | 203.750 | 210.750 | 217.750 | 224.750 |
| 19 | 175.850 | 182.850 | 189.850 | 196.850 | 203.850 | 210.850 | 217.850 | 224.850 |
| 20 | 175.950 | 182.950 | 189.950 | 196.950 | 203.950 | 210.950 | 217.950 | 224.950 |
| 21 | 176.050 | 183.050 | 190.050 | 197.050 | 204.050 | 211.050 | 218.050 | 225.050 |
| 22 | 176.150 | 183.150 | 190.150 | 197.150 | 204.150 | 211.150 | 218.150 | 225.150 |
| 23 | 176.250 | 183.250 | 190.250 | 197.250 | 204.250 | 211.250 | 218.250 | 225.250 |
| 24 | 176.350 | 183.350 | 190.350 | 197.350 | 204.350 | 211.350 | 218.350 | 225.350 |
| 25 | 176.450 | 183.450 | 190.450 | 197.450 | 204.450 | 211.450 | 218.450 | 225.450 |
| 26 | 176.550 | 183.550 | 190.550 | 197.550 | 204.550 | 211.550 | 218.550 | 225.550 |
| 27 | 176.650 | 183.650 | 190.650 | 197.650 | 204.650 | 211.650 | 218.650 | 225.650 |

TABLE 134 (*continued*)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DRM channel suffix | DRM channel centre frequency *fC* (MHz) in VHF channel (number) | | | | | | | |
| 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 |
| 28 | 176.750 | 183.750 | 190.750 | 197.750 | 204.750 | 211.750 | 218.750 | 225.750 |
| 29 | 176.850 | 183.850 | 190.850 | 197.850 | 204.850 | 211.850 | 218.850 | 225.850 |
| 30 | 176.950 | 183.950 | 190.950 | 197.950 | 204.950 | 211.950 | 218.950 | 225.950 |
| 31 | 177.050 | 184.050 | 191.050 | 198.050 | 205.050 | 212.050 | 219.050 | 226.050 |
| 32 | 177.150 | 184.150 | 191.150 | 198.150 | 205.150 | 212.150 | 219.150 | 226.150 |
| 33 | 177.250 | 184.250 | 191.250 | 198.250 | 205.250 | 212.250 | 219.250 | 226.250 |
| 34 | 177.350 | 184.350 | 191.350 | 198.350 | 205.350 | 212.350 | 219.350 | 226.350 |
| 35 | 177.450 | 184.450 | 191.450 | 198.450 | 205.450 | 212.450 | 219.450 | 226.450 |
| 36 | 177.550 | 184.550 | 191.550 | 198.550 | 205.550 | 212.550 | 219.550 | 226.550 |
| 37 | 177.650 | 184.650 | 191.650 | 198.650 | 205.650 | 212.650 | 219.650 | 226.650 |
| 38 | 177.750 | 184.750 | 191.750 | 198.750 | 205.750 | 212.750 | 219.750 | 226.750 |
| 39 | 177.850 | 184.850 | 191.850 | 198.850 | 205.850 | 212.850 | 219.850 | 226.850 |
| 40 | 177.950 | 184.950 | 191.950 | 198.950 | 205.950 | 212.950 | 219.950 | 226.950 |
| 41 | 178.050 | 185.050 | 192.050 | 199.050 | 206.050 | 213.050 | 220.050 | 227.050 |
| 42 | 178.150 | 185.150 | 192.150 | 199.150 | 206.150 | 213.150 | 220.150 | 227.150 |
| 43 | 178.250 | 185.250 | 192.250 | 199.250 | 206.250 | 213.250 | 220.250 | 227.250 |
| 44 | 178.350 | 185.350 | 192.350 | 199.350 | 206.350 | 213.350 | 220.350 | 227.350 |
| 45 | 178.450 | 185.450 | 192.450 | 199.450 | 206.450 | 213.450 | 220.450 | 227.450 |
| 46 | 178.550 | 185.550 | 192.550 | 199.550 | 206.550 | 213.550 | 220.550 | 227.550 |
| 47 | 178.650 | 185.650 | 192.650 | 199.650 | 206.650 | 213.650 | 220.650 | 227.650 |
| 48 | 178.750 | 185.750 | 192.750 | 199.750 | 206.750 | 213.750 | 220.750 | 227.750 |
| 49 | 178.850 | 185.850 | 192.850 | 199.850 | 206.850 | 213.850 | 220.850 | 227.850 |
| 50 | 178.950 | 185.950 | 192.950 | 199.950 | 206.950 | 213.950 | 220.950 | 227.950 |
| 51 | 179.050 | 186.050 | 193.050 | 200.050 | 207.050 | 214.050 | 221.050 | 228.050 |
| 52 | 179.150 | 186.150 | 193.150 | 200.150 | 207.150 | 214.150 | 221.150 | 228.150 |
| 53 | 179.250 | 186.250 | 193.250 | 200.250 | 207.250 | 214.250 | 221.250 | 228.250 |
| 54 | 179.350 | 186.350 | 193.350 | 200.350 | 207.350 | 214.350 | 221.350 | 228.350 |
| 55 | 179.450 | 186.450 | 193.450 | 200.450 | 207.450 | 214.450 | 221.450 | 228.450 |
| 56 | 179.550 | 186.550 | 193.550 | 200.550 | 207.550 | 214.550 | 221.550 | 228.550 |
| 57 | 179.650 | 186.650 | 193.650 | 200.650 | 207.650 | 214.650 | 221.650 | 228.650 |
| 58 | 179.750 | 186.750 | 193.750 | 200.750 | 207.750 | 214.750 | 221.750 | 228.750 |
| 59 | 179.850 | 186.850 | 193.850 | 200.850 | 207.850 | 214.850 | 221.850 | 228.850 |
| 60 | 179.950 | 186.950 | 193.950 | 200.950 | 207.950 | 214.950 | 221.950 | 228.950 |
| 61 | 180.050 | 187.050 | 194.050 | 201.050 | 208.050 | 215.050 | 222.050 | 229.050 |
| 62 | 180.150 | 187.150 | 194.150 | 201.150 | 208.150 | 215.150 | 222.150 | 229.150 |
| 63 | 180.250 | 187.250 | 194.250 | 201.250 | 208.250 | 215.250 | 222.250 | 229.250 |
| 64 | 180.350 | 187.350 | 194.350 | 201.350 | 208.350 | 215.350 | 222.350 | 229.350 |
| 65 | 180.450 | 187.450 | 194.450 | 201.450 | 208.450 | 215.450 | 222.450 | 229.450 |
| 66 | 180.550 | 187.550 | 194.550 | 201.550 | 208.550 | 215.550 | 222.550 | 229.550 |

TABLE 134 (*end*)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DRM channel suffix | DRM channel centre frequency *fC* (MHz) in VHF channel (number) | | | | | | | |
| 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 |
| 67 | 180.650 | 187.650 | 194.650 | 201.650 | 208.650 | 215.650 | 222.650 | 229.650 |
| 68 | 180.750 | 187.750 | 194.750 | 201.750 | 208.750 | 215.750 | 222.750 | 229.750 |
| 69 | 180.850 | 187.850 | 194.850 | 201.850 | 208.850 | 215.850 | 222.850 | 229.850 |
| 70 | 180.950 | 187.950 | 194.950 | 201.950 | 208.950 | 215.950 | 222.950 | 229.950 |

# 2 Computations of correction factors

## 2.1 Computation of the antenna gain for portable handheld reception

The antenna (linear) gain *g* is the product of directivity *d* and efficiency η [4].

 (62)

For lossless antennas the efficiency equals one and the gain equals the directivity.

Portable handheld reception antennas are very lossy, and therefore the gain is much lower than directivity. They are also short linear antennas, with small dimensions compared to wavelength, and have a constant directivity of about 1.5 (1.8 dBi or –0.4 dBd). The gain changes with frequency only due to efficiency.

To estimate the efficiency change with frequency a transmitting antenna is considered. That leads to the values for a receiving antenna also, because antennas are reciprocal; their directivity, efficiency and gain are the same as receiving or transmitting antenna [4].

To transfer the maximum energy from a port to an antenna or vice versa the antenna has to be matched to the port impedance. A matched antenna has an equivalent series circuit with radiation resistance *Rr*, antenna loss resistance and a matching circuit loss resistance. It is considered that the reactive part of the serial impedance as zero. The radiation resistance is small and the transmitted energy is dissipated mostly in the antenna loss resistance and the matching circuit. Only the energy in *Rr* is radiated. Combining all losses in *RL* the antenna efficiency:

 (63)

*Rr* can be neglected in the denominator, because *Rr* is much lower than *RL*.

For the antenna length l << λ the radiation resistance magnitude is proportional to the square of the antenna length l relative to wavelength λ [4]:

 (64)

where λ was substituted by *c*/*f*, with *c* the light velocity.

If the antenna dimension is not changed, and it is considered that the losses in the antenna and the matching circuit does not change significantly in the frequency range of interest, the efficiency η2 at a frequency *f*2, compared to the efficiency η1 at a frequency *f*1, changes as follows:

 (65)

The same is true for the gain *G* (dB), since the directivity does not change.

Changing the frequency from *f*1 to *f*2 the gain changes with:

 (66)

## 2.2 Computation of man-made noise allowance from the antenna noise factor

Definition of the antenna noise factor

An antenna for terrestrial communications with efficiency one receives from its environment, no matter what shape its receiving diagram has, thermal noise with a power *n*:

 (67)

where:

*k* : Boltzmann’s constant (J/K)

*T* : environment temperature (K)

*B* : bandwidth (Hz).

If the antenna receives in the same bandwidth B Gaussian noise like man-made noise with a power *i*, the total power received is:

 (68)

An antenna noise factor *fa* can be defined as:

 (69)

and an antenna noise figure *Fa* given in dB [4]:

 (70)

The man-made noise allowance for coverage calculations

In a link budget used for coverage calculations, the receiver is taken into account by its noise figure *Fr*. It can be shown, that the effect of the man-made noise *i* received by the antenna is equivalent to an increase of the receiver noise figure *Fr* by an amount MMN in dB, called man-made noise allowance.

If the antenna does not receive man-made noise, the total equivalent noise at a receiver input is:

 (71)

with:

*p* : power sum (W)

*pr* : receiver noise corresponding to the noise figure and the bandwidth (W)

*n* : thermal noise (*kTB*) (W)

*fr* :receiver noise factor calculated from the noise figure .

The receiver noise factor is defined as:

 (72)

If man-made noise *i* is received, the power at the receiver input is:

 (73)

The interference power is increased by a factor *mmn*:

 (74)

but:

 (75)

and

 (76)

The factor *mmn* can be expressed as a function of *fr* and *fa*:

 (77)

or in dB, the allowance for man-made noise *MMN*:

 (78)

The system equivalent noise figure to be used for coverage calculations is increased to:

 (79)

Special case with antenna gain below 1.8 dBi

The antenna gain is the product of directivity and efficiency. The lowest realistic directivity is the one of a short dipole (length << λ) and it has the value 1.5 (1.8 dBi). Any gain lower than 1.8 dBi (−0.4 dBd) is due to an antenna efficiency η lower than 1.

If the antenna efficiency is η, from the received wanted signal *w* only η*\*w* reaches the receiver, but the Gaussian noise and the man-made noise getting into the receiver are also reduced to η*\*n* and η*\*i*.

The interference power at the receiver input is increased due to man-made noise interference *i* by the factor *mmn*:

 (80)

 (81)

The efficiency η can be calculated from the antenna gain *GD*, for gains lower than −0.4 dBd:

 (82)

References

[1] GE06 – Final Acts of the Regional Radiocommunication Conference for planning of the digital terrestrial broadcasting service in parts of Regions 1 and 3, in the frequency bands 174-230 MHz and 470‑862 MHz (RRC-06) Annex 3: Technical basis and characteristics

[2] EBU-TECH 3317 [July, 2007] *Planning parameters for hand held reception concerning the use of DVB-H and T-DMB in Bands III, IV, V and the 1.5 GHz band*

[3] ETSI TR 101 190; *Digital Video Broadcasting (DVB); Implementation guidelines for DVB terrestrial services; Transmission aspects*

[4] KRAUS, J.D. [December, 2001] *Antennas*, Mc Graw Hill College; 3rd revised edition

[5] GE84 – Final Acts of the Regional Administrative Conference for the Planning of VHF Sound Broadcasting (Region 1 and Part of Region 3); Geneva 1984

[6] ETSI EN 201 980; Digital Radio Mondiale (DRM); *System Specification*

[7] ETSI EN 302 018-2; *Electromagnetic compatibility and Radio spectrum Matters (ERM); Transmitting equipment for the Frequency Modulated (FM) sound broadcasting service*

[8] Documentation G531/00328/07 [September, 2007] *Compatibility Measurements DRM120, DRM and HD Radio interfering with FM Broadcast, Narrowband FM (BOS) and Aeronautical Radionavigation*, German Network Agency and University of Applied Science of Kaiserslautern

[9] Russian Federation national standard GOST R 54309-2011 “Realtime audiovisual information system (RAVIS). Framing structure, channel coding and modulating for digital terrestrial narrowband broadcasting system for the VHF band. Technical specification”

[10] Russian Federation national standard GOST R 55686-2013 “Realtime audiovisual information system (RAVIS). Digital modulator. Main parameters and technical requirements”

[11] Russian Federation national standard GOST R 55687-2013 “Realtime audiovisual information system (RAVIS). Test radio receiver. General technical requirements”

[12] Russian Federation national standard GOST R 55688-2013 “Realtime audiovisual information system (RAVIS). Content creator. Structure and protocols of data transmission”

[13] Russian Federation national standard GOST R 55689-2013 “Realtime audiovisual information system (RAVIS). Norms and methods of metrology support”

[14] Recommendation ITU-R BS.1114-7 – Systems for terrestrial digital sound broadcasting to vehicular, portable and fixed portable, and fixed receivers in the frequency range 30‑3 000 MHz

[15] Recommendation ITU-R BS.412-9 – Planning standards for terrestrial FM sound broadcasting at VHF

[16] Recommendation ITU-R BS.704 – Characteristics of FM sound broadcasting reference receivers for planning purposes

[17] Recommendation ITU-R BS.415-2 – Minimum performance specifications for low-cost sound-broadcasting receivers

[18] Recommendation ITU-R P.1546 – Method for point-to-area predictions for terrestrial services in the frequency range 30 MHz to 3 000 MHz

[19] U.S.A. FCC Title 47, Part 73, Section 73.215: *Contour Protection for Short Spaced Assignment*

[20] U.S. National Radio System Committee NRSC-5-D: In-Band/On-Channel Digital Radio Broadcasting Standard

[21] iBiquity Digital Corporation. Document Number SY\_IDD\_1011s. HD Radio Air Interface Design Description – Layer 1 FM

[22] U.S.A. FCC MM Docket No. 99-325, 17 FCC RCD 19990: *Digital Audio Broadcasting System and Impact on the Terrestrial Radio Broadcast Service*, First Report and Order. October 10, 2002

[23] U.S.A. FCC MM Docket No. 99-325, DA 10-208, FCC RCD 10344: *Digital Audio Broadcasting System and Impact on the Terrestrial Radio Broadcast Service*, Order, Released January 29, 2010. Digital Power Increase for FM Stations Approved

[24] ITU RRC-84: *Final Acts of the Regional Administrative Conference for the Planning of VHF Sound Broadcasting*. Geneva, 1984

[25] Recommendation ITU-R BS.599 – *Directivity of antennas for the reception of sound broadcasting in band 8 (VHF)*

[26] Recommendation ITU-R P.372-9 – *Radio Noise*

[27] RA(OfCom) AY 3952: *Feasibility Study into the Measurement of Man-Made Noise*. 2001

[28] RA(OfCom) AY4119: *Man-Made Noise Measurement Programme*. 2003

[29] J. Rantakko, E. Lofsved, and M. Alexandersson. *Measurement of Man-Made Noise at VHF*. EMC Europe Workshop. 2005

[30] Brian Kroeger and Paul Peyla: *Adaptive impedance matching (AIM) for electrically small radio receiver antennas*. NAB. April 8, 2013

[31] 48th IEEE Vehicular technology Symposium. *Measurements of the vehicle penetration loss characteristics at 800 MHz*. May 199

[32] EBU Document B/BCP 078 – *Man-Made Noise in the VHF- and UHF- Frequency Band: Results of indoor measurements*. Contribution from IRT, Geneva, 2005

[33] Recommendation ITU-R SM.2093 – *Methods for measurements of indoor radio environment*

[34] ETSI ETS 300 401 – *Radio broadcasting systems; Digital Audio Broadcasting (DAB) to mobile, portable and fixed receivers*. February 1995

[35] ETSI EN 300 401 V2.1.1 – *Radio Broadcasting Systems; Digital Audio Broadcasting (DAB) to Mobile, Portable and Fixed receivers*. January 2017

[36] WI95 – *Special Arrangement of the European Conference of Postal and Telecommunications Administrations (CEPT) relating to the use of the bands   
47-68 MHz, 87.5-108 MHz and 230-240 MHz for Terrestrial Digital Audio Broadcasting (T-DAB)*. Wiesbaden 1995

[37] EBU BPN 003, ver. 1 and 2, – *Technical bases for the T-DAB services network planning and compatibility with existing broadcasting services*. Geneva, 1995-1998

[38] Recommendation ITU-R BS.774-1 – *Digital sound broadcasting to vehicular, portable and fixed receivers using terrestrial transmitters in the VHF/UHF bands*. July 1994 (Superseded)

[39] EBU TR 021 (BPN 003, version 3, Feb. 2003) – *Technical bases for the T-DAB services network planning and compatibility with existing broadcasting services*. Geneva, October 2013

[40] EBU TR 025 (BPN 101, Dec. 2012) – *Report of frequency and Network planning parameters related to DAB +*. Geneva, October 2013

[41] *Labormessungen zur Ermittlung der C/N-Werte bei DAB+ und der Rauschzahl der Empfänger*. Raul Schramm, IRT, November 2011 (in German)

[42] Recommendation ITU-R P.2109 0 – *Prediction of building entry loss*. June 2017

[43] Report ITU-R P.2346 2 – *Compilation of measurement data relating to building entry loss*. March 2017

[44] Recommendation ITU‑R BS.1660‑7 – *Technical basis for planning of terrestrial digital sound broadcast in the VHF band*. October 2015

[45] EBU Report Tech 3391 – *Guidelines for DAB network planning*, Geneva May 2018

[46] Measurements of the vehicle penetration loss characteristics at 800 MHz. *48th IEEE Vehicular technology Symposium, May 1998*

[47] EBU TR 024 (BPN 066, July 2005) - SFN frequency planning and network implementation with regard to T-DAB and DVB-T. Geneva, October 2013

[48] Location Factor Standard Deviation Field Trial Results and Analysis. *CRA, Les Sabel and Wilson NG,* May 2016

[49] DAB+ Field Strength Location Variation Standard Deviation Investigation. CRA, Les Sabel and Wilson NG, September 2016

[50] *Signal in Band III.* OFCOM/BBC/Arqiva. Version 1.0, 30 April 2012 ([http://stakeholders.ofcom.org.uk/binaries/broadcast/radio‑ops/coverage/Location\_Variation\_for\_TDAB.pdf](http://stakeholders.ofcom.org.uk/binaries/broadcast/radio-ops/coverage/Location_Variation_for_TDAB.pdf)

[51] *Statistical Analysis of Field Strength Location Variability for UHF Multimedia Broadband Services.* J.A. Arenas *et al.*, IEEE,December 2011

[52] WI95revCO07 ‑ FINAL ACTS of the CEPT T‑DAB *Planning Meeting for the revision of the Special Arrangement of the European Conference of Postal and Telecommunications Administrations (CEPT) relating to the use of the bands 47‑68 MHz, 87.5‑108 MHz, 174‑230 MHz, 230‑240 MHz and 1452‑1492 MHz for the introduction of Terrestrial Digital Audio Broadcasting (T‑DAB)*, Wiesbaden, 1995, as revised by the CEPT T‑DAB planning meeting, Bonn, 1996, as further revised by the CEPT T‑DAB planning meeting, Maastricht, 2002. Constanţa 2007

[53] Schutzabstand bei DAB+ im Gausskanal; Messungen mit Neuen Empfängern. *Raul Schramm, IRT,* July 2013

[54] ETSI EN 302 077 V2.1.0 – Transmitting equipment for the Digital Audio Broadcasting (DAB) service; Harmonised Standard for access to radio spectrum. March 2018

[55] Recommendation ITU‑R BT.1368‑12 – *Planning criteria, including protection ratios, for digital terrestrial television services in the VHF/UHF bands*. February 2015

[56] *Update on Man Made Noise impact due to antenna gain* rev2. L. Sabel, S Comm Technologies and Commercial Radio Australia, November 2017

[57] EBU Document B/BCP 134 – *Effects of negative isotropic antenna gains on the treatment of man-made noise*. IRT, November 2005

[58] ETSI TS 102 563 (V2.1.1) – Digital Audio Broadcasting (DAB); DAB+ Audio Coding (MPEG HE AACv2). January 2017

[59] ETSI TS 103 466 V1.1.1 – Digital Audio Broadcasting (DAB); DAB audio coding (MPEG Layer II). October 2016

[60] ETSI TR 101 495 V2.1.1 – Digital Audio Broadcasting (DAB); Guide to DAB standards. August 2017

1. The calculation presented in [56] is an updated version of the derivation in [57]. [↑](#footnote-ref-1)
2. <http://www.fh-kl.de>; <http://www.drm-radio-kl.eu>. [↑](#footnote-ref-2)
3. <http://www.ikt.uni-hannover.de/>. [↑](#footnote-ref-3)
4. Radio Regulations No. **5.252**: in Botswana, Lesotho, Malawi, Mozambique, Namibia, South Africa, Swaziland, Zambia and Zimbabwe, the bands 230-238 MHz and 246-254 MHz are allocated to the broadcasting service on a primary basis, subject to agreement obtained under No. **9.21**. [↑](#footnote-ref-4)