### CONTENTS

Report ITU-R BT.2408-7  
Policy on Intellectual Property Right (IPR)  
 1 Introduction  
 2 Reference levels and signal format  
 2.1 HDR Reference White  
 2.2 Signal levels for line-up in production  
 2.3 Bit depth  
 2.4 Signal range  
 2.5 Colour representation  
 3 Monitoring  
 3.1 Display of PQ signals  
 3.1.1 Mapping to displays with limited luminance range  
 3.2 Display of HLG signals  
 3.2.1 Display of HLG signals on SDR screens  
 4 Image brightness  
 4.1 Comfortable brightness of static images  
 4.2 Tolerance to programme brightness shifts  
 5 Integrating standard dynamic range and high dynamic range production  
 5.1 Inclusion of standard dynamic range content in high dynamic range  
 5.1.1 Display referred mapping  
 5.1.2 Display referred mapping of SDR into PQ  
 5.1.3 Display referred mapping of SDR into HLG  
 5.1.4 Scene referred mapping  
 5.1.5 Comparing scene-light and display-light direct-mapping  
 5.2 HDR to SDR down-mapping  
 5.3 Handling negative values in format conversion  
 5.4 Adjustments to BT.709 cameras  
 5.5 Use of 8-bit content  
 5.6 Mapping of SDR graphics  
 6 Conversion between PQ and HLG  
 6.1 Transcoding concepts  
 6.2 Conversion concepts using a reference condition at 1 000 cd/m2  
 6.3 Cameras using a common OOTF at a reference peak luminance of 1 000 cd/m2  
 6.4 Handling PQ signals with greater than 1 000 cd/m2 peak luminance  
 6.5 Possible colour differences when converting from PQ to HLG  
 7 Transitioning from SDR BT.709 to HDR BT.2100 production  
 7.1 HDR focused production  
 7.2 SDR focused production  
 7.2.1 PQ production with SDR shading  
 7.2.2 HLG production with SDR shading  
UHD and HD resolution HDR camera outputs  
HDR slow-motion  
HDR to SDR down-mapping  
 7.3 SDR-HDR and HDR-SDR format conversion  
 7.3.1 PQ conversion  
 7.3.2 HLG conversion  
 7.3.3 The displayed “look” of content following format conversion  
 7.3.4 Signal range considerations for HDR to SDR conversion  
 7.4 SDR-HDR-SDR “Round-Tripping”  
 7.5 Hardware colour matrix compensation  
 7.6 Signal line-up  
 7.7 Camera painting  
 8 Conversion practices for camera and display RGB colorimetry  
Annex 1 Study to evaluate levels for PQ content  
Annex 2 Analysis of reference levels  
 A2.1 Introduction  
 A2.2 Analysis of reference levels  
 A2.3 Diffuse white elements in live HLG encoded broadcast content  
 A2.4 Diffuse white in an HDR dataset of 1 000 cd/m2 PQ encoded images  
 A2.5 Discussion  
 A2.6 Conclusions  
Annex 3 Two studies of skin tones, using a reflectance database and using real subjects  
 A3.1 Study 1: using a skin tone database and an ideal model of a camera  
 A3.2 Study 2: using human subjects and a RAW recording camera  
 A3.3 Conclusions  
Annex 4 Study of facial skin tones in broadcast content  
 A4.1 Facial skin tones in SDR news and information programmes in studio  
 A4.2 Comparison of facial skin tones in HLG HDR and SDR content in a music programme  
 A4.3 Conclusion  
Annex 5 Displaying PQ – calculating the EETF  
Annex 6 Comparison of the native looks of HDR and SDR production  
 A6.1 Differences in chromaticity and saturation  
 A6.2 Quantifying the total colour differences  
 A6.3 Comparison with the reference colour pattern data  
Annex 7 Calculating the normalized primary matrix  
 A7.1 Conversion of normalized linear colour signals to Recommendation ITU‑R BT.2100  
 A7.2 Conversion of BT.2100 to arbitrary linear colour signals for display systems  
Annex 8 4K/8K UHD HDR and HD SDR simul-production and simulcast practice in China  
 A8.1 Background  
 A8.2 Basic workflows and principles  
 A8.3 Introduction of related work and research  
 A8.4 Mapping for conversion between HDR and SDR  
 A8.5 Parameter settings  
 A8.6 Converter performance consistency (LUTs usage)  
 A8.7 Signal range  
 A8.8 Consistency of international exchange  
 A8.9 Conclusions  
Annex 9 HDR and SDR monitors in close proximity  
 A9.1 Approach used by BBC  
 A9.2 Approach used by NBCUniversal  
Annex 10 NBCUniversal single-master HDR-SDR workflow  
Annex 11 Conversion between 203 cd/m2 and 100 cd/m2 (BT.2035) SDR signal formats  
Glossary