|  |
| --- |
| **Report ITU-R M.2039-3**  **(11/2014)** |
| **Characteristics of terrestrial IMT-2000 systems for frequency sharing/ interference analyses** |
| **M Series**  **Mobile, radiodetermination, amateur**  **and related satellite services** |

Foreword

The role of the Radiocommunication Sector is to ensure the rational, equitable, efficient and economical use of the radio-frequency spectrum by all radiocommunication services, including satellite services, and carry out studies without limit of frequency range on the basis of which Recommendations are adopted.

The regulatory and policy functions of the Radiocommunication Sector are performed by World and Regional Radiocommunication Conferences and Radiocommunication Assemblies supported by Study Groups.

# Policy on Intellectual Property Right (IPR)

ITU-R policy on IPR is described in the Common Patent Policy for ITU-T/ITU-R/ISO/IEC referenced in Annex 1 of Resolution ITU-R 1. Forms to be used for the submission of patent statements and licensing declarations by patent holders are available from <http://www.itu.int/ITU-R/go/patents/en> where the Guidelines for Implementation of the Common Patent Policy for ITU‑T/ITU‑R/ISO/IEC and the ITU-R patent information database can also be found.

|  |  |
| --- | --- |
| Series of ITU-R Reports  (Also available online at <http://www.itu.int/publ/R-REP/en>) | |
| **Series** | Title |
| **BO** | Satellite delivery |
| **BR** | Recording for production, archival and play-out; film for television |
| **BS** | Broadcasting service (sound) |
| **BT** | Broadcasting service (television) |
| **F** | Fixed service |
| **M** | Mobile, radiodetermination, amateur and related satellite services |
| **P** | Radiowave propagation |
| **RA** | Radio astronomy |
| **RS** | Remote sensing systems |
| **S** | Fixed-satellite service |
| **SA** | Space applications and meteorology |
| **SF** | Frequency sharing and coordination between fixed-satellite and fixed service systems |
| **SM** | Spectrum management |

|  |
| --- |
|  |

|  |
| --- |
| ***Note****: This ITU-R Report was approved in English by the Study Group under the procedure detailed in Resolution ITU-R 1.* |

*Electronic Publication*

Geneva, 2015

© ITU 2015

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without written permission of ITU.

REPORT ITU-R M.2039-3

Characteristics of terrestrial IMT-2000 systems for frequency sharing/interference analyses

(2004-2009-2010-2014)

TABLE OF CONTENTS

Page

1 Introduction 2

2 Acronyms and definitions 3

3 IMT-2000 interfaces 5

4 Non-deployment related parameters 6

4.1 Non-deployment related parameters for IMT-2000 CDMA DS (interface No. 1) 7

4.2 Non-deployment related parameters for IMT-2000 CDMA MC (CDMA 2000, HRPD and UMB) (interface No. 2) 13

4.3 Non-deployment related parameters for IMT-2000 CDMA TDD (interface No. 3) 17

4.4 Non-deployment related parameters for IMT-2000 TDMA SC (interface No. 4) 24

4.5 Non-deployment related parameters for IMT-2000 FDMA/TDMA (interface No. 5) 26

4.6 Non-deployment related parameters for IMT-2000 OFDMA TDD WMAN (interface No. 6) 27

5 Deployment-related parameters in the bands below 1 GHz 31

5.1 Deployment-related parameters for IMT-2000 CDMA DS (interface No. 1) 31

5.2 Deployment-related parameters for IMT-2000 CDMA MC (CDMA 2000, HRPD and UMB) (interface No. 2) 34

5.3 Deployment-related parameters for IMT-2000 CDMA TDD (interface No. 3) 39

5.4 Deployment-related parameters for IMT-2000 OFDMA TDD WMAN (interface No. 6) 41

5.5 Spectrum emission mask for terminal/mobile station equipment operating in the band 3 400-3 600 MHz 43

References 45

# 1 Introduction

International Mobile Telecommunications 2000 (IMT-2000) third generation mobile systems started service around the year 2000, and provide access by means of one or more radio links to a wide range of telecommunications services supported by the fixed telecommunication networks (e.g. PSTN/ISDN/ Internet protocol (IP)) and to other services specific to mobile users. Since then, IMT-2000 has been continually enhanced.

The Radiocommunication Assembly 2007 adopted Resolution ITU-R 56 that resolves that the term “IMT” be the root name that encompasses both IMT-2000 and IMT-Advanced collectively.

Certain bands are identified for IMT in the Radio Regulations (RR) and the frequency arrangements used in those bands can be found in Recommendation ITU-R M.1036.

Frequency sharing studies and interference analyses involving IMT systems and other systems and services operating in bands identified for IMT may need to be undertaken within ITU R.

To perform the necessary sharing studies between IMT systems and systems in other services, characteristics of the terrestrial component of IMT systems are needed.

This Report provides the baseline characteristics of terrestrial IMT-2000 systems only for use in frequency sharing and interference analysis studies involving IMT-2000 systems and between IMT‑2000 systems and other systems.

Recommendations ITU-R M.1457, ITU-R M.1580 and ITU-R M.1581 provide standardization information relating to IMT-2000 interfaces.

Parameters for IMT-Advanced interfaces are not addressed in this Report. They are addressed in Report ITU-R M.2292.

The characteristics of the IMT-2000 interfaces have been grouped by frequency ranges:

– below 1 GHz,

– between 1 and 3 GHz,

– between 3 and 6 GHz.

Band specific variations, if any, are reflected in the tables.

# 2 Acronyms and definitions

3GPP 3rd Generation Partnership Project

3GPP2 3rd Generation Partnership Project 2

ACLR Adjacent channel leakage ratio

ACR Adjacent channel rejection

ACS Adjacent channel selectivity

BS Base station

BW Bandwidth

CDMA Code-division multiple access

DECT Digital enhanced cordless telecommunications

DL Downlink

EDGE Enhanced data rates for GSM evolution

e.i.r.p. Equivalent isotropic radiated power

e.r.p. Effective radiated power

E-UTRA Evolved UTRA

EV-DO Evolution-Data Optimized

EV-DV Evolution-Data/Voice

FDD Frequency division duplex

FDMA Frequency-division multiple access

GMSK Gaussian minimum shift keying

HPSK Hybrid phase shift keying

HRPD High rate packet data

HSPA High speed packet access

HSPA+ Evolved high speed packet access

IMT International Mobile Telecommunications – root name that encompasses both IMT 2000 and IMT-Advanced collectively

IMT-2000 International Mobile Telecommunications 2000

IMT-Advanced International Mobile Telecommunications-Advanced – previously known as systems beyond IMT 2000

*I/N* Interference to noise ratio

LTE Long term evolution

MC Multi-carrier

MS Mobile station

N/A Not applicable

OFDMA Orthogonal frequency-division multiple access

PUSC Partially used sub-channel

QAM Quadrature amplitude modulation

QPSK Quadrature phase shift keying

RF Radio frequency

SC-FDMA Single carrier frequency division multiple access

SDO Standards development organization

TDD Time division duplex

TDMA Time-division multiple access

TD-SCDMA Time division synchronous code-division multiple access

TR Technical report of 3GPP

TS Technical specification of 3GPP

TX Transmitter

UE User equipment

UL Uplink

UMB Ultra mobile broadband

UMTS Universal mobile telecommunication system

UT User terminal

UTRA Universal terrestrial radio access

UWC Universal wireless communications

WCDMA Wideband code-division multiple access

WiMAX Worldwide interoperability for microwave access

# 3 IMT-2000 interfaces

Table 1 provides an explanation of the terminology used for the IMT 2000 terrestrial radio interfaces as given in Recommendation ITU-R M.1457. For IMT-Advanced terrestrial radio interfaces see Recommendation ITU-R M.2012.

TABLE 1

IMT-2000 terrestrial radio interfaces

|  |  |  |
| --- | --- | --- |
| Full name | Common names | Duplex mode |
| IMT‑2000 CDMA Direct Spread  (interface No. 1) | UTRA FDD  WCDMA  UMTS  HSPA, HSPA+  E-UTRA FDD (LTE FDD) | FDD |
| IMT‑2000 CDMA Multi‑Carrier  (interface No. 2) | CDMA2000  CDMA2000 1X and 3X  CDMA2000 HRPD  CDMA2000 1xEV-DV  CDMA2000 1xEV-DO  EVDOHRPD  UMB | FDD and TDD |
| IMT‑2000 CDMA TDD (time‑code)  (interface No. 3) | UTRA TDD 7.68 Mchip/s  UTRA TDD 3.84 Mchip/s  UTRA TDD 1.28 Mchip/s (TD-SCDMA) UMTS  HSPA, HSPA+  E-UTRA TDD (LTE TDD) | TDD |

TABLE 1 (*end*)

|  |  |  |
| --- | --- | --- |
| Full name | Common names | Duplex mode |
| IMT‑2000 TDMA Single‑Carrier  (interface No. 4) | UWC-136  EDGE | FDD |
| IMT‑2000 FDMA/TDMA (frequency-time)  (interface No. 5) | DECT | TDD |
| IMT-2000 OFDMA TDD WMAN  (interface No. 6) | Mobile WiMAX | FDD and TDD |

# 4 Non-deployment related parameters

Specification requirements indicate the minimum acceptable performance. Equipment performance often exceeds this performance significantly. Implementation aspects may also mandate improved performance, e.g. when duplex filters reduce the interference generated in adjacent spectrum.

When equipment performance measurements, band specific parameters or detailed models are available, these factors may be taken into account in sharing analysis.

## 4.1 Non-deployment related parameters for IMT-2000 CDMA DS (interface No. 1)

TABLE 2

Non-deployment related parameters for IMT-2000 CDMA DS (interface No. 1)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | IMT-2000 RADIO INTERFACE | IMT‑2000 CDMA  Direct Spread [1], [2], [3], [4], [5] | | | |
|  |  | UTRA | | E-UTRA | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station |
| 1. | Access Technique | CDMA | CDMA | OFDM | SC-FDMA |
| 2. | Modulation parameters | QPSK 16-QAM 64-QAM | <1 GHz: QPSK 16-QAM  1-3 GHz:  HPSK(10) 16-QAM | QPSK 16-QAM 64-QAM | QPSK 16-QAM 64-QAM |
| 3. | Duplex mode | FDD | | FDD | |
| 4. | Carrier spacing | 5 MHz ± n × 0.2 MHz | | Nominal Channel spacing =  (BW*Channel*(1) + BW*Channel*(2))/2(1) | |
| 5. | Channel bandwidth (MHz)(2) | 5 | 5 | 1.4, 3, 5, 10, 15, 20 | 1.4, 3, 5, 10, 15, 20 |
| 6. | Effective transmitter/receiver bandwidth (MHz) | 3.84 | 3.84 | 1.08, 2.7, 4.5, 9, 13.5 and 18 | 1.08, 2.7, 4.5, 9, 13.5 and 18 |

TABLE 2 (*continued*)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | IMT-2000 RADIO INTERFACE | IMT‑2000 CDMA  Direct Spread [1], [2], [3], [4], [5] | | | |
|  |  | UTRA | | E-UTRA | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station |
| 7. | Transmitter characteristics |  | | | |
| 7.1 | Total power dynamic range for BS (dB) and minimum power (dBm) for MS (Power control) | Total power dynamic range  > 18 dB(3) | Minimum power  < −50 dBm(4) | Total power dynamic range  > 7.7/11.7/13.9/16.9/ 18.7 dB for 1.4/3/5/10/15/20 MHz Channel BW(5) | Minimum power  ≤ −40 dBm(6) |
| 7.2 | Spectral emission mask or Operating band unwanted emissions | (7) | (8) | (9) | (10) |
| 7.3 | ACLR(11) |  | | | |
| 7.3a. | ACLR1 | Macro, Micro, Pico, Femto:  45 dB  (12) | 33 dB  (13) | Macro, Micro, Pico, Femto:  45 dB  @±BW MHz  (14)(15) | 30 dB  (interference to E‑UTRA)  33 dB  (interference to UTRA)  (16) |

TABLE 2 (*continued*)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | IMT-2000 RADIO INTERFACE | IMT‑2000 CDMA  Direct Spread [1], [2], [3], [4], [5] | | | |
|  |  | UTRA | | E-UTRA | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station |
| 7.3b. | ACLR2 | Macro, Micro, Pico, Femto:  50 dB(12) | 43 dB(13) | Macro, Micro, Pico, Femto:  45 dB  @±2\*BW MHz(14)(15) | N/A  for second adjacent E‑UTRA channel  36 dB  for second adjacent UTRA channel)(16) |
| 7.4 | Transmitter power(17) | (dBm/antenna)  Macro:  No limit  Micro:  35  Pico:  24  Femto: < +20 dBm  (1 transmit antenna) (18) | (dBm)  24 (power class 3) / 21 (power class 4)(19) | (dBm/antenna)  Macro:  No limit  Micro:  38 Pico:  24  (20) | (dBm)  23  (21) |
| 7.5 | Transmitter Spurious emissions [1], [2], [3], [5](22) | −36 dBm/100 kHz for 30 MHz – 1 GHz  −30 dBm/1 MHz for 1 GHz – 12.75 GHz  −30 dBm/1 MHz for 12.75 GHz – 5th harmonic of the upper frequency edge of the UL operating band in GHz (applicable to 3GPP E-UTRA Band 22 or UTRA Band XXII) | | | |

TABLE 2 (*continued*)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | IMT-2000 RADIO INTERFACE | IMT‑2000 CDMA  Direct Spread [1], [2], [3], [4], [5] | | | |
|  |  | UTRA | | E-UTRA | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station |
| 8. | Receiver characteristics |  | | | |
| 8.1 | Receiver Noise Figure (NF) (dB) | Macro: 5  Micro: 15  Pico: 19  Femto: 19 | 9 | Macro: 5  Micro: 10  Pico: 13  Femto: 13 | 9 |
| 8.2 | Receiver thermal noise level | RTN = 10 log10(kTB)+NF  k : Boltzmann’s constant = 1.38 × 10–23;  T : 290 K;  B : effective rx bandwidth (Hz). | | | |
| 8.3 | Receiver blocking  (in-band, out-of-band, narrow-band) | (23) | (24) | (25) | (26) |
| 8.4 | ACS(27) (relative ACS) | Macro:  −52 dBm  (46 dB)  Micro:  −42 dBm (46 dB)  Pico / Femto:  –38 dBm (46 dB)  (28) | 33 dB  (29) | (30) | (31)(33 dB)  (up to 10 MHz channel bandwidth)  (30 dB)  (BW = 15 MHz)  (27 dB)  (BW = 20 MHz) |
| 9. | Interference criterion, *I/N* (dB) | *I/N* = −6 dB, −10 dB or −20 dB depending on scenario(32) | | | |

|  |
| --- |
| *Notes relative to Table 2:*  (1) BW*Channel*(1)and BW*Channel*(2) are the channel bandwidths of the two respective E-UTRA carriers. Supported channel bandwidths: 1.4 MHz, 3 MHz, 5 MHz, 10 MHz, 15 MHz and 20 MHz.  (2) This value refers to the transmission bandwidth.  (3) See 3GPP Document: TS 25 104, § 6.4  (4) See 3GPP Document: TS 25 101, § 6.4  (5) See 3GPP Document: TS 36 104, § 6.3  (6) See 3GPP Document: TS 36 101, § 6.3  (7) See 3GPP Documents: TS 25 104, § 6.6.2.1 or TS 37 104, § 6.6.2  (8) See 3GPP Documents: TS 25 101, § 6.6.2.1  (9) See 3GPP Documents: TS 36 104, § 6.6.3 or TS 37 104 § 6.6.2  (10) See 3GPP Documents: TS 36 101, § 6.6.2  (11) These unwanted emission limits are the upper limits from SDO specifications for laboratory testing with maximum transmitting power. It is assumed that when the in-band transmitting power is reduced by x dB through power control, the unwanted emission levels would be reduced by x dB in consequence in the coexistence simulations.  (12) See 3GPP Documents: TS 25 104, § 6.6.2.2 or TS 37 104, § 6.6.4  (13) See 3GPP Documents: TS 25 101, § 6.6.2.2  (14) ACLR applies up to 10 MHz outside the operating band. Stricter limits may apply beyond 10 MHz outside the operating band, see 3GPP Documents TS 36 104 § 6.6.2 or TS 37 104 § 6.6.4  (15) BW represents the channel bandwidth. Supported channel bandwidths: 1.4 MHz, 3 MHz, 5 MHz, 10 MHz, 15 MHz and 20 MHz.  (16) See 3GPP Document TS 36.101, § 6.6.2.3. The ACLR value provided in the table applies to a single-UE occupying the whole channel bandwidth.  (17) Transmit power values refer to maximum values defined in the specifications. For actual powers to be used in sharing studies see the deployment specific parameters.  (18) See 3GPP Documents: TS 25 104, § 6.2 or TS 37 104, § 6.2.  (19) See 3GPP Document TS 25.101, § 6.2.  (20) See 3GPP Documents: TS 36 104, § 6.2 or TS 37 104, § 6.2.  (21) See 3GPP Document TS 36.101, § 6.2.  (22) 3GPP specifies additional spurious emissions for co-existence/co-location between 3GPP technologies. |

|  |
| --- |
| *Notes relative to Table 2 (end):* |

(23) See 3GPP Document TS 25.104, § 7.5 or TS 37 104 § 7.4, § 7.5

(24) See 3GPP Document TS 25.101, § 7.6

(25) See 3GPP Document TS 36.104, §§ 7.5, 7.6 or TS 37 104 §§ 7.4, 7.5

(26) See 3GPP Document TS 36.101, § 7.6

(27) The absolute ACS values are the test values as specified in 3GPP TS 25.104 § 7.4. The following conversion formula:  
ACS\_relative = ACS\_test – Noise\_floor – 10 log10 (10M/10 – 1)  
can be used to derive relative ACS values, where M is the margin (dB) used in the ACS test, which is the useful signal level above the reference sensitivity level. For both IMT 2000 CDMA direct spread and IMT 2000 CDMA TDD (time code), E.g. M = 6 dB for Macro BS. ACS relative values are often used in sharing studies. For values of M see 3GPP Documents: TS 25.104 § 7.4, TS 36.104 § 7.5 or TS 37.104 § 7.4.

(28) See 3GPP Document TS 25.104, § 7.4

(29) See 3GPP Document TS 25.101, § 7.5

(30) E-UTRA BS receiver ACS and blocking test conditions are specified in 3GPP 36.104 § 7.5, those test conditions should be used to derive E-UTRA BS receiver mask with the conversion formula in note (27), special care is needed when deriving the E-UTRA BS receiver mask for channel bandwidth larger than 5 MHz since a 5 MHz interfering signal is specified in the ACS and Blocking test conditions.

(31) E-UTRA UE ACS values are to be used if the E-UTRA victim channel bandwidth is the same as interferer transmitting channel bandwidth. In case that the E-UTRA victim channel bandwidth is different from the interferer transmitting channel bandwidth, the E-UTRA receiver mask needs to be derived with the formula in note (27) using the E-UTRA UE ACS and Blocking test conditions defined in 3GPP TS 36.101 § 7.5, special care is needed when deriving the E‑UTRA UE receiver mask for UE channel bandwidth larger than 5 MHz since a 5 MHz interfering signal is specified in the ACS and Blocking test conditions.

(32) Different protection criteria correspond to different interference situations: *I/N* = −6 dB (corresponding to 1 dB reduction of the receiver sensitivity) is applicable to cases where interference affects one or a few cells, or when the IMT-2000 system is interference limited. In other cases *I/N* = −10 dB (corresponding to 0.4 dB reduction of the receiver sensitivity) is applicable. In case of interference from systems which are allowed to be operated on lower priority basis, including in particular license exempt systems, a requirement of *I/N* = −20 dB applies. In case of multiple interfering services, the allowed interference should be partitioned among the interferers. These criteria may be modified in case of cross-border negotiations.

## 4.2 Non-deployment related parameters for IMT-2000 CDMA MC (CDMA 2000, HRPD and UMB) (interface No. 2)

TABLE 3(1)

Non-deployment related parameters for IMT-2000 CDMA MC (CDMA 2000, HRPD and UMB) (interface No. 2)

|  | IMT-2000 RADIO INTERFACE | | IMT-2000 CDMA MC | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | | cdma2000 | | HRPD | | UMB | |
| No. | Parameter | | Base station | Mobile station | Base station | Mobile station | Base station | Mobile station |
| 1. | Access Technique | | CDMA | CDMA | TDMA | CDMA | OFDMA | CDMA/OFDMA |
| 2. | Modulation parameters | Forward link or downlink | Data modulation: BPSK; QPSK, 8‑PSK, 16‑QAM Spreading modulation: QPSK | | Data modulation: QPSK, 8-PSK, 16‑QAM, and 64-QAM Spreading modulation: QPSK | | Data modulation: QPSK, 8-PSK, 16‑QAM, and 64-QAM | |
| Reverse link or uplink | Data modulation: 64-ary Orthogonal Modulation, BPSK; QPSK, 8-PSK Spreading modulation: HPSK | | Data modulation: BPSK; QPSK, 8‑PSK Spreading modulation: HPSK | | Data modulation: QPSK, 8-PSK, 16‑QAM, and 64-QAM Spreading modulation: QPSK (CDMA control segment) | |
| 3. | Duplex mode | | FDD | | FDD | | FDD/TDD | |
| 4. | Carrier spacing | | Nominal carrier spacing is 1.23 MHz or 1.25 MHz | | Nominal carrier spacing is 1.23 MHz or 1.25 MHz | | Nominal Channel spacing =  (BW*Channel*(1) + BW*Channel*(2))/2(2) | |
| 5. | Channel bandwidth (MHz)  Channel bandwidth(s), some systems being capable of multiple bandwidths | | It has a chip rate of N = 1.2288 Mchip/s (currently, N = 1 and 3 are specified)  Carrier spacing is 1.23 MHz for Band Class 0; 1.25 MHz for all other Band Classes | | M carriers of 1.2288 Mchip/s can be aggregated in a single or multi-carrier operation, where M = 1, 2, 3, 4, …, 15. Carriers in a multi- carrier operation do not have to be contiguous and their spacing is multiple of 30, 50, 25 or 12.5 kHz depending on the Band Class | | Native bandwidth can fit deployment of 1.25 to 20 MHz (0.768 + N × 0.1536 MHz, N × 0, …, 123). Also, multi-carrier configurations can be used to aggregate two or more carriers of possibly different native bandwidths and operating in non‑contiguous spectral allocation | |

TABLE 3(1) (*continued*)

|  | IMT-2000 RADIO INTERFACE | IMT-2000 CDMA MC | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | cdma2000 | | HRPD | | | UMB | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station | | Base station | Mobile station |
| 6. | Effective transmitter/receiver bandwidth (MHz) | 1.2288 per carrier. One or three carriers can be used together, with carriers separated by 1.23 MHz for Band Class 0 and 1.25 MHz in other cases | 1.2288 (1x) and 3.6864 (3x) | 1.2288 per carrier. One to fifteen carriers can be used together, with carriers separated by 1.23 MHz for Band Class 0 and 1.25 MHz in other cases | 1.2288 per carrier. One to fifteen carriers can be used together, separated by 1.23 MHz for Band Class 0 and 1.25 MHz in other cases | | 0.768-19.6608 with step size of 0.1536 | 0.768-19.6608 with step size of 0.1536 |
| 7. | Transmitter characteristics |  | | | | | | |
| 7.1 | Output power dynamic (Power control) (dB) | Open loop and Closed loop (800, 400, 200, 50, 25, 12.5 Hz update rate) with power control steps: 0.25 × N, N = 1, 2, 4 dB | | Open loop and Closed loop (600 and 150 Hz update rate) with power control steps: 0.5 × N, N = 1, 2, 3, 4 dB | | Open loop and Closed loop (Once every N data frames (0.911 ms), N = 4, 8, 16, 32) with power control steps: 0.25 × N, N = 1, 2, 3, ..., 8 dB | | |
| 7.2 | Spectral emission mask or Operating band unwanted emissions | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | See Recommendation ITU‑R M.1581 for CDMA-MC Mobile Stations | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | See Recommendation ITU‑R M.1581 for CDMA-MC Mobile Stations | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | | See Recommendation ITU‑R M.1581 for CDMA‑MC Mobile Stations |
| 7.3 | ACLR | [19] | [20] | [21] | [22] | [31] | | [32] |

TABLE 3(1) (*continued*)

|  | IMT-2000 RADIO INTERFACE | IMT-2000 CDMA MC | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | cdma2000 | | HRPD | | | UMB | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station | | Base station | Mobile station |
| 7.3a | ACLR1 | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | See Recommendation ITU‑R M.1581 for CDMA-MC Mobile Stations | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | See Recommendation ITU‑R M.1581 for CDMA-MC Mobile Stations | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | | See RecommendationsITU‑R M.1581 for CDMA‑MC Mobile Stations |
| 7.3b | ACLR2 | See RecommendationITU-R M.1580 for CDMA‑MC Base Stations | See Recommendation ITU‑R M.1581 for CDMA-MC Mobile Stations | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | See Recommendation ITU‑R M.1581 for CDMA-MC Mobile Stations | See Recommendation ITU-R M.1580 for CDMA‑MC Base Stations | | See Recommendation ITU‑R M.1581 for CDMA‑MC Mobile Stations |
| 7.4 | Transmitter power (dBm/antenna) | Macro: Nominal 43 dBm (vendor dependent subject to regulation)  Pico: ≤ 24 dBm  Femto: ≤ 20 dBm | 23 dBm (single transmit antenna) | Macro: Nominal 43 dBm (vendor dependent subject to regulation)  Pico: ≤ 24 dBm  Femto: ≤ 20 dBm | 23 dBm (single transmit antenna) | Macro: Nominal 43 dBm (vendor dependent subject to regulation)  Pico: ≤ 24 dBm  Femto: ≤ 20 dBm | | 23 dBm (single transmit antenna) |
| 7.5 | Transmitter Spurious emissions | [6] | [7] | [8] | [9] | [10] | | [11] |
| 8. | Receiver characteristics |  | | | | | | |
| 8.1 | Receiver noise figure (NF) (dB) | 5 dB nominal | 10 dB nominal | 5 dB nominal | 10 dB nominal | 5 dB nominal | | 10 dB nominal |

TABLE 3(1) (*end*)

|  | IMT-2000 RADIO INTERFACE | IMT-2000 CDMA MC | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | cdma2000 | | HRPD | | | UMB | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station | | Base station | Mobile station |
| 8.2. | Receiver thermal noise level | RTN = 10 log10(kTB)+NF  k: Boltzmann’s constant = 1.38 × 10–23,  T: 290 K,  B: effective rx bandwidth (Hz). | | | | | | |
| 8.3. | Receiver blocking  (in-band, out-of-band, narrow-band) | [6] | [7] | [8] | [9] | [10] | | [11] |
| 8.4. | ACS (relative ACS) | [6] | [7] | [8] | [9] | [10] | | [11] |
| 9. | Interference criterion, *I/N* (dB) | *I/N* = −6 dB, −10 dB or −20 dB depending on scenario(3) | | | | | | |
| *Notes relative to Table 3:*  (1) Note that some of the parameters in this table are typically not included in the cdma2000 specifications. These include: maximum spectral power density, transmitting antenna type, antenna gain, antenna height, antenna pattern, antenna downtilt, feeder loss, and polarization. Some information in these categories found in this table is listed in 3GPP2 Report C.R1002 (cdma2000 Evaluation Methodology) and may be considered typical in some deployments.  (2) BW*Channel*(1)and BW*Channel*(2) are the channel bandwidths of the two respective UMB carriers. Supported channel bandwidths: 0.768 + N × 0.1536 MHz,  N = 0, …, 123.  (3) Different protection criteria correspond to different interference situations: *I/N* = −6 dB (corresponding to 1 dB reduction of the receiver sensitivity) is applicable to cases where interference affects one or a few cells, or when the IMT-2000 system is interference limited. In other cases *I/N* = −10 dB (corresponding to 0.4 dB reduction of the receiver sensitivity) is applicable. In case of interference from systems which are allowed to be operated on lower priority basis, including in particular license exempt systems, a requirement of *I/N* = −20 dB applies. In case of multiple interfering services, the allowed interference should be partitioned among the interferers. These criteria may be modified in case of cross-border negotiations. | | | | | | | | |

## 4.3 Non-deployment related parameters for IMT-2000 CDMA TDD (interface No. 3)

TABLE 4

Non-deployment related parameters for IMT-2000 CDMA TDD (interface No. 3)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 CDMA TDD (time-code) [2], [5], [12], [13] | | | |
| --- | --- | --- | --- | --- | --- |
|  |  | UTRA | | E-UTRA | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station |
| 1. | Access Technique | TDMA/CDMA | TDMA/CDMA | OFDM in DL  SC-FDMA in UL | OFDM in DL  SC-FDMA in UL |
| 2. | Modulation parameters | 1.28 Mchip/s: QPSK/  8-PSK/16-QAM  3.84 Mchip/s: QPSK/16-QAM  7.68 Mchip/s: QPSK/16-QAM | | QPSK/  16-QAM/64-QAM | |
| 3. | Duplex mode | TDD | | TDD | |
| 4. | Carrier spacing | 1.28 Mchip/s: 1.6 MHz  3.84 Mchip/s: 5 MHz  7.68 Mchip/s: 10 MHz | | Nominal Channel spacing =  (BWChannel(1) + BWChannel(2))/2(1) | |
| 5. | Channel bandwidth (MHz)(2) | 1.6, 5, 10 | 1.6, 5, 10 | 1.4, 3, 5, 10, 15, 20 | 1.4, 3, 5, 10, 15, 20 |
| 6. | Effective transmitter/receiver bandwidth (MHz) | 1.28 Mchip/s:  < 1.6 MHz [13]  3.84 Mchip/s:  < 5 MHz [13]  7.68 Mchip/s:  < 10 MHz [13] | 1.28 Mchip/s:  < 1.6 MHz [12]  3.84 Mchip/s:  < 5 MHz [12]  7.68 Mchip/s:  < 10 MHz [12] | 1.08, 2.7, 4.5, 9, 13.5 and 18 | 1.08, 2.7, 4.5, 9, 13.5 and 18 |

TABLE 4 (*continued*)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 CDMA TDD (time-code) [2], [5], [12], [13] | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | UTRA | | | E-UTRA | | |
| No. | Parameter | Base station | Mobile station | | Base station | Mobile station | |
| 7. | Transmitter characteristics |  | | | | | |
| 7.1 | Total power dynamic range (dB) for BS and minimum power (dBm) for MS (Power control) | Total power dynamic range  ≥ 30(3) | Minimum power  < −49/44/41 dBm for 1.28/3.84/7.68 Mcps(4) | Total power dynamic range  > 7.7/11.7/13.9/16.9/18.7 dB for 1.4/3/5/10/15/20 MHz Channel BW (5) | | Minimum power  ≤ −40 dBm(6) | |
| 7.2 | Spectral emission mask or Operating band unwanted emissions | (7) | (8) | | (9) | (10) | |
| 7.3 | ACLR(11) |  | | | | | |
| 7.3a. | ACLR1 | 1.28 Mchip/s: 40 dB @  ±1.6 MHz  3.84 Mchip/s: 45 dB @  ±5 MHz  7.68 Mchip/s: 45 dB @  ±10 MHz(12) | 33 dB  (for 1.28, 3.84 and 7.68 Mchip/s)(13) | | 45 dB  @ ± BW MHz  (14) (15) | | 30 dB  @ ± BW MHz (interference to E‑UTRA)  33 dB  (interference to UTRA)  (16) |

TABLE 4 (*continued*)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 CDMA TDD (time-code) [2], [5], [12], [13] | | | |
| --- | --- | --- | --- | --- | --- |
|  |  | UTRA | | E-UTRA | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station |
| 7.3b. | ACLR2 | 1.28 Mchip/s: 45 dB @  ±3.2 MHz  3.84 Mchip/s: 55 dB @  ±10 MHz  7.68 Mchip/s: 55 dB @  ±20 MHz  (12) | 43 dB  (for 1.28, 3.84 and 7.68 Mchip/s)  (13) | 45 dB  @ ± 2 × BW MHz  (14) (15) | N/A  for second adjacent E‑UTRA channel  36 dB  for second adjacent UTRA channel)  (16) |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 7.4 | Transmitter power(17) | (dBm/antenna)  25(18)  for 1.28 Mchip/s,  43  for 3.84 Mchip/s  (19)  [13] | 24 dBm for class 3 / 21 dBm for class 4 (20)  [12] | (dBm/antenna)  Macro:  No limit  Micro:  38  Pico:  24  Femto:  20  (1 transmit antenna)(21) | 23 dBm  (22) |

|  |  |  |
| --- | --- | --- |
| 7.5 | Transmitter Spurious emissions(23) [1], [2], [3], [5] | −36 dBm/100 kHz for 30 MHz – 1 GHz  −30 dBm/1 MHz for 1 GHz – 12.75 GHz  −30 dBm/1 MHz for 12.75 GHz– 5th harmonic of the upper frequency edge of the UL operating band in GHz (applicable to 3GPP E-UTRA Band 42 and E-UTRA Band 43) |

TABLE 4 (*continued*)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 CDMA TDD (time-code) [2], [5], [12], [13] | | | |
| --- | --- | --- | --- | --- | --- |
|  |  | UTRA | | E-UTRA | |
| No. | Parameter | Base station | Mobile station | Base station | Mobile station |
| 8. | Receiver characteristics |  | |  | |
| 8.1 | Receiver Noise Figure (NF) (dB) | 1.28 Mchip/s:  – Macro: 7 dB  – Pico: 21 dB  – Femto: 16 dB  3.84 Mchip/s:  – Macro: 5 dB  – Pico: 19 dB  7.68 Mchip/s:  – Macro: 5 dB  – Pico: 19 dB | 9 dB | Macro: 5 dB  Micro: 10 dB  Pico: 13 dB  Femto: 13 dB | 9 dB |
| 8.2 | Receiver thermal noise level | RTN = (log(kTB)+N)  k: Boltzmann’s constant = 1.38 × 10–23;  T: 290 K;  B: effective rx bandwidth (Hz)= 1.08, 2.7, 4.5, 9, 13.5 and 18 | | | |
| 8.3 | Receiver blocking  (in-band, out-of-band, narrow-band) | (24) | (25) | (26) | (27) |

TABLE 4 (*end*)

|  | **IMT-2000 RADIO INTERFACE** | **IMT 2000 CDMA TDD (time-code) [2], [5], [12], [13]** | | | |
| --- | --- | --- | --- | --- | --- |
|  |  | **UTRA** | | **E-UTRA** | |
| **No.** | **Parameter** | **Base station** | **Mobile station** | **Base station** | **Mobile station** |
| 8.4 | ACS(28) (relative ACS) | Macro:  1.28 Mchip/s:  −55 dBm (46 dB)  3.84 Mchip/s:  −52 dBm (46 dB)  7.68 Mchip/s:  −49 dBm  (46 dB)  (29) | 33 dB  (30) | (31) | (32)  (33 dB)  (up to 10 MHz channel bandwidth)  (30 dB)  (BW = 15 MHz)  (27 dB)  (BW = 20 MHz) |
| 9. | Interference criterion, *I/N* (dB) | *I/N* = −6 dB, −10 dB or −20 dB depending on scenario(33) | | | |

|  |
| --- |
| *Notes relative to Table 4:*  (1) BWChannel(1) and BWChannel(2) are the channel bandwidths of the two respective E-UTRA carriers. Supported channel bandwidths: 1.4 MHz, 3 MHz, 5 MHz, 10 MHz, 15 MHz and 20 MHz.  (2) This value refers to the transmission bandwidth.  (3) See 3GPP Documents: TS 25 105, § 6.4.  (4) See 3GPP Documents: TS 25 102, § 6.4.  (5) See 3GPP Document TS 36 104, § 6.3.  (6) See 3GPP Documents: TS 36 101, § 6.3.2.  (7) See 3GPP Documents: TS 25 105, §§ 6.6.2.1, 6.6.2.1A.  (8) See 3GPP Documents: TS 25 102, §§ 6.6.2.1, 6.6.2.1A.  (9) See 3GPP Documents: TS 36 104, § 6.6.3 or TS 37 104 § 6.6.2.  (10) See 3GPP Documents: TS 36 101, Table 6.6.2.  (11) These unwanted emission limits are the upper limits from SDO specifications for laboratory testing with maximum transmitting power. It is assumed that when the in-band transmitting power is reduced by x dB through power control, the unwanted emission levels would be reduced by x dB in consequence in the coexistence simulations.  (12) See 3GPP Documents: TS 25 105, § 6.6.2.2.  (13) See 3GPP Documents: TS 25 102, § 6.6.2.2.  (14) ACLR applies up to 10 MHz outside the operating band. Stricter limits may apply beyond 10 MHz outside the operating band, see 3GPP Documents TS 36 104 § 6.6.2 or TS 37 104 § 6.6.2.  (15) BW represents the channel bandwidth. Supported channel bandwidths: 1.4 MHz, 3 MHz, 5 MHz, 10 MHz, 15 MHz and 20 MHz.  (16) See 3GPP Documents: TS 36 101, § 6.6.2.3.  (17) Transmit power values refer to maximum values defined in the specifications. For actual powers used in sharing studies see the deployment specific parameters.  (18) 8-element smart antenna system is employed for UTRA TDD 1.28 Mchip/s.  (19) See 3GPP Documents: TS 25 105, § 6.2. |

|  |
| --- |
| *Notes relative to Table 4 (end):*  (20) See 3GPP Document TS 25.102, § 6.2.  (21) See 3GPP Documents: TS 36 104, § 6.2 or TS 37 104, § 6.2.  (22) See 3GPP Document TS 36.101, § 6.2.  (23) 3GPP specifies additional spurious emissions for co-existence/co-location between 3GPP technologies.  (24) See 3GPP Documents: TS 25 105, § 7.6.  (25) See 3GPP Documents: TS 25 102, § 7.6.  (26) See 3GPP Documents: TS 36 104, § 7.6. or TS 37 104, §§ 7.4, 7.5.  (27) See 3GPP Documents: TS 36 101, § 7.6.  (28) The absolute ACS values are the test values as specified in 3GPP TS 25 105. The following conversion formula: ACS\_relative = ACS\_test – Noise\_floor – 10 log10 (10M/10 – 1) can be used to derive relative ACS values, where M is the margin (dB) used in the ACS test, which is the useful signal level above the reference sensitivity level. For both IMT‑2000 CDMA direct spread and IMT‑2000 CDMA TDD (time code), e.g. M = 6 dB for macro BS. ACS relative values are often used in sharing studies. For values of M see 3GPP Documents: TS 25.105 § 7.4, TS 36.104 § 7.5 or TS 37.104 § 7.4.  (29) See 3GPP Documents: TS 25 105, see § 7.4.  (30) See 3GPP Documents: TS 25 102, § 7.5.  (31) E-UTRA BS receiver ACS and blocking test conditions are specified in 3GPP 36.104 §§ 7.5 and 7.6, those test conditions should be used to derive EUTRA BS receiver mask with the conversion formula in note (28), special care is needed when deriving the E-UTRA BS receiver mask for channel bandwidth larger than 5 MHz since a 5 MHz interfering signal is specified in the ACS and Blocking test conditions.  (32) E-UTRA UE ACS values are to be used if the E-UTRA victim channel bandwidth is the same as interferer transmitting channel bandwidth. In case that the E-UTRA victim channel bandwidth is different from the interferer transmitting channel bandwidth, the E-UTRA receiver mask needs to be derived with the formula in note (28) using the E-UTRA UE ACS and Blocking test conditions defined in 3GPP TS 36.101 §§ 7.5 and 7.6, special care is needed when deriving the E-UTRA UE receiver mask for UE channel bandwidth larger than 5 MHz since a 5 MHz interfering signal is specified in the ACS and Blocking test conditions.  (33) Different protection criteria correspond to different interference situations: *I/N* = -6 dB (corresponding to 1 dB reduction of the receiver sensitivity) is applicable to cases where interference affects one or a few cells, or when the IMT-2000 system is interference limited. In other cases *I/N* = -10 dB (corresponding to 0.4 dB reduction of the receiver sensitivity) is applicable. In case of interference from systems which are allowed to be operated on lower priority basis, including in particular license exempt systems, a requirement of *I/N* = -20 dB applies. In case of multiple interfering services, the allowed interference should be partitioned among the interferers. These criteria may be modified in case of cross-border negotiations. |

## 4.4 Non-deployment related parameters for IMT-2000 TDMA SC (interface No. 4)

TABLE 5

Non-deployment related parameters for IMT-2000 TDMA SC (interface No. 4)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 TDMA Single-Carrier | | | |
| --- | --- | --- | --- | --- | --- |
| No. | Parameter | Base station | | Mobile station | |
| 1. | Access Technique | TDMA | TDMA | TDMA | TDMA |
| 2. | Modulation parameters | π/4-DQPSK 8-PSK | GMSK 8-PSK | π/4-DQPSK 8-PSK | GMSK 8-PSK |
| 3. | Duplex mode | FDD | FDD | FDD | FDD |
| 4. | Carrier spacing | 30 kHz | 200 kHz | 30 kHz [15] | 200 kHz [16] |
| 5. | Channel bandwidth (MHz) | 24.3 kHz @ −3 dB points | 130 kHz @ −3 dB points | 24.3 kHz @ −3 dB point | 130 kHz @ −3 dB points |
| 6. | Effective transmitter/receiver bandwidth (MHz) | N/A | N/A | [17], [18] | [19] |
| 7. | Transmitter characteristics |  | | | |
| 7.1 | Output power dynamic (Power control) (dB) |  |  | Class IV MS is nominally 32 dB | 50 dB |
| 7.2 | ACLR |  | | | |
| 7.2a. | ACLR1 | 26 dB | 30 dB | 26 dB | 30 dB |
| 7.2b. | ACLR2 | 45 dB | 60 dB 56 dB (8 PSK) | 45 dB | 60 dB 54 dB (8 PSK) |

TABLE 5 (*end*)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 TDMA Single-Carrier | | | |
| --- | --- | --- | --- | --- | --- |
| No. | Parameter | Base station | | Mobile station | |
| 7.3 | Transmitter power (dBm/antenna) (maximum) | ≥43 | ≥43 | 30 [14] | 30 [20] |
| 7.3a. | Transmitter power (dBm/antenna) (typical)(2) | Macro: 40 | Macro: 40 | 20 | 20 |
| 7.4 | Spurious emissions | −30 dBm (1 GHz – 2.1 GHz) | [10] | −30 dBm (1 GHz – 2.1 GHz) | [10] |
| 8. | Receiver characteristics |  |  |  |  |
| 8.1 | Receiver noise figure (NF) | 5 dB | 5 dB | 9 dB | 9 dB |
| 8.2 | Receiver thermal noise level | −125 dBm(3) | −117 dBm(4) | −119 dBm | −112 dBm |
| 8.3 | ACS (relative ACS) | N/A | N/A | N/A | N/A |
| 9. | Interference criterion, *I/N* (dB) | *I/N* = −6 dB, −10 dB or −20 dB depending on scenario(5) | | | |
| *Notes relative to Table 5:*  (1) TDMA, comprising 8 timeslots (577 μs) per single TDMA frame (4.615 ms). For user packet data service, 1-4 timeslots per frame may be used by mobile stations having multi-slot classes that do not require simultaneous transmission and reception, i.e. classes for which a duplexer is not required.  (2) May not be appropriate for all scenarios, for example when calculating aggregate interference from all users in a cell.  (3) In bandwidth equal to data rate: for IMT-2000 CDMA multicarrier, values are given for 9 600 bit/s speech services and nominal supported rate for data services.  (4) In bandwidth equal to data rate: for IMT-2000 CDMA multicarrier, values are given for 9 600 bit/s speech services and nominal supported rate for data services.  (5) Different protection criteria correspond to different interference situations: *I/N* = −6 dB (corresponding to 1 dB reduction of the receiver sensitivity) is applicable to cases where interference affects one or a few cells, or when the IMT-2000 system is interference limited. In other cases *I/N* = −10 dB (corresponding to 0.4 dB reduction of the receiver sensitivity) is applicable. In case of interference from systems which are allowed to be operated on lower priority basis, including in particular license exempt systems, a requirement of *I/N* = −20 dB applies. In case of multiple interfering services, the allowed interference should be partitioned among the interferers. These criteria may be modified in case of cross-border negotiations. | | | | | |

## 4.5 Non-deployment related parameters for IMT-2000 FDMA/TDMA (interface No. 5)

TABLE 6

Non-deployment related parameters for IMT-2000 FDMA/TDMA (interface No. 5)

|  |  |  |  |
| --- | --- | --- | --- |
|  | IMT-2000 RADIO INTERFACE | IMT 2000 FDMA/TDMA (frequency-time) [21] | |
| No. | Parameter | Base station | Mobile station |
| 1. | Access Technique | MC/  TDMA | MC/TDMA(1) |
| 2. | Modulation parameters | GMSK  (BT = 0.5)  (+ multi-level modulation options) | GMSK (BT = 0.5)  (+ multi-level modulation options) |
| 3. | Duplex mode | TDD | TDD |
| 4. | Carrier spacing | 1.728 MHz | 1.728 MHz |
| 5. | Effective transmitter/receiver bandwidth (MHz) | [21] | [21] |
| 6. | ACLR |  | [21] |
| 7. | Transmitter power (dBm/antenna) (maximum) |  | 24 |
| 8. | Transmitter power (dBm/antenna) (typical)(2) | 24 | 10 |
| 9. | Receiver noise figure (NF) | 10 dB | 10 dB |
| 10. | Receiver thermal noise level | −103 dBm in 1.152 MHz | −102 dBm in 1.728 MHz |
| 11. | Receiver blocking response/levels |  | [21] |
| 12. | Interference criterion | −105 dBm typical  (−97 dBm for speech specification) |  |
| *Notes relative to Table 6:*  (1) Ten frequency channels with 24 time slots (32 kbit/s) per frame. The frame length is 10 ms.  (2) May not be appropriate for all scenarios, for example when calculating aggregate interference from all users in a cell. | | | |

## 4.6 Non-deployment related parameters for IMT-2000 OFDMA TDD WMAN (interface No. 6)

TABLE 7

Non-deployment related parameters for IMT-2000 OFDM TDD WMAN (interface No. 6)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 OFDMA TDD WMAN | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | Mobile WiMAX (OFDMA) | | | | | |
| No. | Parameter | Base station | | | Mobile station | | |
| 1. | Access Technique | TDMA/ OFDMA | TDMA/ OFDMA | TDMA/ OFDMA | TDMA/ OFDMA | TDMA/ OFDMA | TDMA/ OFDMA |
| 2. | Modulation parameters | QPSK 16-QAM 64-QAM, Repetition factor (R) 2, 4, 6 | QPSK 16-QAM 64-QAM, Repetition factor (R) 2, 4, 6 | QPSK 16-QAM 64-QAM, Repetition factor (R) 2, 4, 6 | QPSK 16-QAM 64-QAM  (64-QAM optional), Repetition factor  (*R*) 2, 4, 6 | QPSK 16-QAM 64-QAM  (64-QAM optional), Repetition factor  (*R*) 2, 4, 6 | QPSK 16-QAM 64-QAM,  (64-QAM optional), Repetition factor (*R*) 2, 4, 6 |
| 3. | Duplex mode | TDD | TDD | TDD | TDD | TDD | TDD |
| 4. | Carrier spacing | 5 MHz | 8.75 MHz | 10 MHz | 5 MHz | 8.75 MHz(1) | 10 MHz |
| 5. | Channel bandwidth (MHz) | 4.60 MHz(2) | 6.57 MHz(2) | 9.20 MHz(2) | 4.60 MHz(2) | 6.57 MHz(2) | 9.20 MHz(2) |
| 6. | Effective transmitter/receiver bandwidth (MHz) | 4.75 MHz as defined by –1 dB bandwidth (3), (4) | 8.447MHz  as defined by  –1 dB bandwidth | 9.5 MHz as defined by –1 dB bandwidth (3), (5) | 4.75 MHz as defined by  –1 dB bandwidth(6) | 8.447 MHz | 9.5 MHz as defined by  –1 dB bandwidth(6) |
| 7. | Transmitter characteristics |  | | | | | |
| 7.1 | Spectral emission mask or Operating band unwanted emissions | An example of regulatory requirements for unwanted emission can be found in the FCC regulations(7) §§ 27.53 and 90.543 for the 700 MHz band (698-806 MHz). These are representative of the levels for mobile WiMAX emission masks. | | | | | |

TABLE 7 (*continued*)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 OFDMA TDD WMAN | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | Mobile WiMAX (OFDMA) | | | | | |
| No. | Parameter | Base station | | | Mobile station | | |
| 7.2 | ACLR | (8) |  | (8) | (9) | (9) | (9) |
| 7.2a | ACLR1 | For Macro/Micro/ Pico BS: 45  53.5 dB  (3.84 MHz Rx) @ ±5 MHz inter-system case(10) 45 dB  (4.75 MHz Rx)  @ ±5 MHz  Intra-system case |  | For Macro/Micro/ Pico BS: 45  53.5 dB  (7.68 MHz Rx) @ ±10 MHz inter-system case(10) 45 dB (9.5 MHz Rx)  @ ±10 MHz  Intra-system case | 33 dB  (3.84 MHz Rx) 30 dB  (4.75 MHz Rx) @ ±5 MHz | 30 dB  (8.447 MHz Rx)  @ ±8.75 MHz | 33 dB  (7.68 MHz Rx) 30 dB (9.5 MHz Rx) @ ±10 MHz |
| 7.2b | ACLR2 | For Macro/Micro/ Pico BS: 50(11)  66 dB (3.84 MHz Rx) @ ±10 MHz  Inter-system case(10)  55 dB  (4.75 MHz Rx)  @ ±10 MHz  Intra-system case(10) |  | For Macro/Micro/ Pico BS: 50(11)  66 dB  (7.68 MHz Rx) @ ±20 MHz  inter-system case(10)  55 dB  (9.5 MHz Rx)  @ ±20 MHz  Intra-system case(10) | 43 dB (3.84 MHz Rx) 44 dB (4.75 MHz Rx) @ ±10 MHz | 44 dB  (8.447 MHz Rx)  @ ±17.5 MHz | 43 dB (7.68 MHz Rx) 44 dB (9.5 MHz Rx) @ ±20 MHz |

TABLE 7 (*continued*)

|  | IMT-2000 RADIO INTERFACE | IMT 2000 OFDMA TDD WMAN | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | Mobile WiMAX (OFDMA) | | | | | |
| No. | Parameter | Base station | | | Mobile station | | |
| 7.3. | Transmitter power (dBm) (maximum) | 55(12) | 55(12) | 55(12) | 23(13) | 23(13) | 23(13) |
| 7.3a | Transmitter power (dBm) (typical)(14) | 36(15) | 36(15) | 36(15) | 20(16) | 20(16) | 20(16) |
| 8. | Receiver characteristics |  | | | | | |
| 8.1 | Receiver noise figure (NF) | 3 dB with tower top LNA, 5 dB otherwise | 3 dB with tower top LNA, 5 dB otherwise | 3 dB with tower top LNA, 5 dB otherwise | 5 dB for single band and 8 dB for multi-band designs | 5 dBm | 5 dB for single band and 8 dB for multi-band designs |
| 8.2 | Receiver thermal noise level(17) | –104 dBm for tower top LNA case and  –102 dBm for other cases in 4.75 MHz | –101.51 dBm for tower top LNA case and  –99.51 dBm for other cases in 8.447 MHz | –101 dBm for tower top LNA case and  –99 dBm for other cases in 9.5 MHz | –102 dBm in 4.75 MHz for 5 dB NF and  –99 for 8 dB NF | –99.51 dBm  In 8.447 MHz | –99 dBm in 9.5 MHz for  5 dB NF and –96 for 8 dB NF |
| 8.3 | ACS (relative ACS) | 46 dB(18) |  | 46 dB(18) | 33 dB(19) |  | 33 dB |
| 9. | Interference threshold(20) |  |  |  | –108 dBm or in 4.75 MHz for single band and  –105 dBm for multi-band devices | –105.51 dBm in 8.447 MHz for single band and  –102.51 dBm for multi-band devices | –105 dBm in 9.5 MHz for single band and  –102 dBm for multi-band devices |

|  |
| --- |
| *Notes relative to Table 7:*  (1) Only applicable to the band 2 300-2 400 MHz band.  (2) These values are corresponding to the utilized spectrum within 5, 7 and 10 MHz channel bandwidths in Up Link when PUSC is used.  (3) Receiver thermal noise level as defined by thermal noise in specified bandwidth + receiver NF.  (4) Please refer to Recommendation ITU-R M.1580, Annex 6 for more information.  (5) For a 10−3 raw bit error rate, theoretical *Eb*/*N*0.  (6) Please refer to Recommendation ITU-R M.1581, Annex 6 for more information.  (7) US Code of Federal Regulations, Title 47, FCC Rules Parts 27 and 90.  (8) ACLR values are specified in Recommendation ITU-R M.1580, Annex 6.  (9) ACLR values are specified in Recommendation ITU-R M.1581, Annex 6.  (10) For the 2.5 GHz band only.  (11) Applicable to the 1 800 MHz and 2.3 GHz bands.  (12) This value does not take account of the effect of multiple transmit antennas.  (13) WiMAX numbers for MS related to Item 7 are preliminary numbers. WiMAX Forum profiles 7.A and 7.E of Table 15, in general, cover a range of power classes.  (14) May not be appropriate for all scenarios, for example when calculating aggregate interference from all users in a cell.  (15) TX power reported is typical and higher values may be available based on region. TX power is the RF power averaged during the transmit burst, without considering traffic statistics or lowered-power operation or UL/DL ratio.  (16) TX power reported is typical and higher values may be available based on region. TX power is the RF power averaged during the transmit burst, without considering traffic statistics or lowered-power operation or UL/DL ratio.  (17) Receiver thermal noise level as defined by thermal noise in specified bandwidth + receiver NF.  (18) ACS = SNRmin + implementation loss + M –10 log10 (10M/10 – 1) + ACR, where the test margin, M, and the ACR are contained in the global core specification (WiMAX Forum Mobile Radio Specification version 0.3.1).  (19) ACS = SNRmin + implementation loss + pilot boosting offset + M –10 log10(10M/10 – 1) + ACR, where the test margin, M , is given in IEEE802.16 as 3 dB, and the ACR values are contained in the global core specification (WiMAX Forum Mobile Radio Specification version 0.3.1).  (20) Different protection criteria correspond to different interference situations: *I/N* = −6 dB (corresponding to 1 dB reduction of the receiver sensitivity) is applicable to cases where interference affects one or a few cells, or when the IMT-2000 system is interference limited. In other cases *I/N* = −10 dB (corresponding to 0.4 dB reduction of the receiver sensitivity) is applicable. In case of interference from systems which are allowed to be operated on lower priority basis, including in particular license exempt systems, a requirement of *I/N* = −20 dB applies. In case of multiple interfering services, the allowed interference should be partitioned among the interferers. These criteria may be modified in case of cross-border negotiations. |

# 5 Deployment-related parameters in the bands below 1 GHz

## 5.1 Deployment-related parameters for IMT-2000 CDMA DS (interface No. 1)

TABLE 8

Deployment-related parameters for IMT-2000 CDMA DS (interface No. 1) below 1 GHz

|  | IMT-2000 RADIO INTERFACES | IMT‑2000 CDMA  Direct Spread | |
| --- | --- | --- | --- |
| No. | Parameter | UTRA | E-UTRA |
|  | Base station parameters |  | |
| 1. | Coverage radius | > 5 km (typical 8 km) for macro rural scenario  0.5-5 km (typical 2 km) for macro urban/suburban scenario | > 5 km (typical 8 km) for macro rural scenario  0.5-5 km (typical 2 km) for macro urban/suburban scenario |
| 2. | Typical height of the transmitting BS antenna (m) | 30 | 30 |
| 3. | Antenna type  (sectorized/omnidirectional) | 3 sectors | 3 sectors |
| 4. | Antenna downtilt for macro base stations | 3° | 3° |
| 5. | Frequency reuse factor | 1 | 1 |

TABLE 8 (*continued*)

|  | IMT-2000 RADIO INTERFACES | IMT‑2000 CDMA  Direct Spread | |
| --- | --- | --- | --- |
| No. | Parameter | UTRA | E-UTRA |
|  | Base station parameters |  | |
| 6. | Antenna pattern | Sector Antenna: Rec. ITU-R F.1336 (*recommends* 3.1)  • ka = 0.7  • kp = 0.7  • kh = 0.7  • kv = 0.3  Horizontal 3 dB beamwidth: 65 degrees  Vertical 3 dB beamwidth: determined from the horizontal beamwidth by equations in Recommendation ITU‑R F.1336 (*recommends* 3.3). Vertical beamwidths of actual antennas may also be used when available. | Sector Antenna: Rec. ITU-R F.1336 (*recommends* 3.1)  • ka = 0.7  • kp = 0.7  • kh = 0.7  • kv = 0.3  Horizontal 3 dB beamwidth: 65 degrees  Vertical 3 dB beamwidth: determined from the horizontal beamwidth by equations in Recommendation ITU‑R F.1336 (*recommends* 3.3). Vertical beamwidths of actual antennas may also be used when available. |
| 7. | Polarization | linear / ±45 degrees | linear / ±45 degrees |
| 8. | Feeder loss (dB) | 3 | 3 |
| 9. | Maximum BS transmitter power per sector (dBm) | 43 | 43 for BW ≤ 5 MHz  46 for BW ≥ 10 MHz |
| 10. | Maximum BS transmitter e.i.r.p. per sector (dBm/channel bandwidth) | 55 | 55 for BW ≤ 5 MHz  58 for BW ≥ 10 MHz |
| 11. | Transmitting BS antenna gain (dBi) | 15 | 15 |
| 12. | Average base station activity factor (%) | 50 | 50 |
| 13. | Average base station e.i.r.p. per sector taking into account the base station activity factor (dBm/channel bandwidth) | 52 | 52 for BW ≤ 5 MHz  55 for BW ≥ 10 MHz |
|  | TDD activity factor (%) | N/A | |

TABLE 8 (*end*)

|  |  |  |  |
| --- | --- | --- | --- |
|  | IMT-2000 RADIO INTERFACES | IMT‑2000 CDMA  Direct Spread | |
| No. | Parameter | UTRA | E-UTRA |
| 14. | **User terminal parameters** |  | |
| 15. | Indoor usage | 50% for macro rural scenario  70% for macro urban/suburban scenario | 50% for macro rural scenario  70% for macro urban/suburban scenario |
| 16. | Average indoor user terminal penetration loss | 15 dB for macro rural scenario  20 dB for macro urban/suburban scenario | 15 dB for macro rural scenario  20 dB for macro urban/suburban scenario |
| 17. | Density of the user equipment in active mode(1) (number/km2) | 0.17 / 5 MHz/km2 for macro rural scenario 2.16 / 5 MHz/km2 for urban/suburban scenario | 0.17 / 5 MHz/km2 for macro rural scenario 2.16 / 5 MHz/km2 for urban/suburban scenario |
| 17.1 | User terminal transmitter output power (dBm) |  | |
| 17.2 | Maximum user terminal transmitter output power (dBm/5 MHz) | 24 | 23 |
| 18. | Average user terminal transmitter output power in active mode(1) (dBm/5 MHz) | 2 dBm for macro rural scenario  –9 dBm for macro urban/suburban scenario | 2 dBm for macro rural scenario  –9 dBm for macro urban/suburban scenario |
| 19. | Transmitting user terminal antenna gain (dBi) | –3 dBi | –3 dBi |
| 20. | Body loss | 4 dB | 4 dB |
| *Note relative to Table 8:*  (1) By “active mode” it should be understood that these are terminals with an active communication session but which are not necessarily transmitting. If only transmitting terminals are used in a study, the average power levels for user equipment in active mode cannot be used. In that case power levels need to be computed differently, e.g. by simulations (including power control). | | | |

## 5.2 Deployment-related parameters for IMT-2000 CDMA MC (CDMA 2000, HRPD and UMB) (interface No. 2)

TABLE 9(1)

Deployment-related parameters for IMT-2000 CDMA MC (CDMA 2000, HRPD and UMB) (interface No. 2) below 1 GHz

|  | IMT-2000 RADIO INTERFACES | IMT-2000 CDMA MC | | |
| --- | --- | --- | --- | --- |
| No. | Parameter | cdma2000 | HRPD | UMB |
|  | Base station parameters |  | | |
| 1. | Coverage radius | > 5 km (typical 8 km) for macro rural scenario  0.5-5 km (typical 2 km) for macro urban/suburban scenario | > 5 km (typical 8 km) for macro rural scenario  0.5-5 km (typical 2 km) for macro urban/suburban scenario | > 5 km (typical 8 km) for macro rural scenario  0.5-5 km (typical 2 km) for macro urban/suburban scenario |
| 2. | Typical height of the transmitting BS antenna (m) | 30 | 30 | 30 |
| 3. | Antenna type (sectorized/omnidirectional) | 3 sectors | 3 sectors | 3 sectors |
| 4. | Antenna downtilt for macro base stations | 3° | 3° | 3° |
| 5. | Frequency reuse factor | 1 | 1 | 1 |

TABLE 9(1) (*continued*)

|  | IMT-2000 RADIO INTERFACES | IMT-2000 CDMA MC | | |
| --- | --- | --- | --- | --- |
| No. | Parameter | cdma2000 | HRPD | UMB |
|  | Base station parameters |  | | |
| 6. | Antenna pattern | Sector Antenna: Rec. ITU-R F.1336 (*recommends* 3.1)  • ka = 0.7  • kp = 0.7  • kh = 0.7  • kv = 0.3  Horizontal 3 dB beamwidth: 65 degrees  Vertical 3 dB beamwidth: determined from the horizontal beamwidth by equations in Recommendation ITU-R F.1336 (*recommends* 3.3). Vertical beamwidths of actual antennas may also be used when available. | Sector Antenna: Rec. ITU-R F.1336 (*recommends* 3.1)  • ka = 0.7  • kp = 0.7  • kh = 0.7  • kv = 0.3  Horizontal 3 dB beamwidth: 65 degrees  Vertical 3 dB beamwidth: determined from the horizontal beamwidth by equations in Recommendation ITU-R F.1336 (*recommends* 3.3). Vertical beamwidths of actual antennas may also be used when available. | Sector Antenna: Rec. ITU-R F.1336 (*recommends* 3.1)  • ka = 0.7  • kp = 0.7  • kh = 0.7  • kv = 0.3  Horizontal 3 dB beamwidth: 65 degrees  Vertical 3 dB beamwidth: determined from the horizontal beamwidth by equations in Recommendation ITU-R F.1336 (*recommends* 3.3). Vertical beamwidths of actual antennas may also be used when available. |
| 7. | Polarization | linear / ± 45 degrees | linear / ± 45 degrees | linear / ± 45 degrees |
| 8. | Feeder loss (dB) | 2 | 2 | 2 |
| 9. | Maximum BS transmitter e.i.r.p.  (dBm/5 MHz) per sector | 61(4) | 61(4) | N/A |
| 10. | Transmitting BS antenna gain (dBi) | 15 | 15 | 15 |
| 11. | Average base station activity factor | 0.58(5) | 1(7) | N/A |
| 12. | Average base station e.i.r.p. per sector taking into account the base station activity factor (dBm) | 58.6(6) | 61 | N/A |
| 13. | TDD activity factor (dB) | N/A | N/A | N/A |

TABLE 9(1) (*end*)

|  | IMT-2000 RADIO INTERFACES | IMT-2000 CDMA MC | | |
| --- | --- | --- | --- | --- |
| No. | Parameter | cdma2000 | HRPD | UMB |
|  | User terminal parameters |  |  |  |
| 14. | Average indoor user terminal penetration loss | 15 dB for macro rural scenario  20 dB for macro urban/suburban scenario | 15 dB for macro rural scenario  20 dB for macro urban/suburban scenario | 15 dB for macro rural scenario  20 dB for macro urban/suburban scenario |
| 15. | Density of the user equipment in active mode(2) (number/km2) | (3) | (3) | (3) |
| 16. | User terminal transmitter output power (dBm) | 23 dBm is the minimum when commanded to transmit as maximum power. Typical maximum transmit power is no more than a few dB higher | 23 dBm is the minimum when commanded to transmit as maximum power. Typical maximum transmit power is no more than a few dB higher | 22.5 ± 2 dBm |
| 16.1 | Maximum user terminal transmitter output power (dBm/5 MHz) | 23 dBm is the minimum when commanded to transmit as maximum power. Typical maximum transmit power is no more than a few dB higher | 23 dBm is the minimum when commanded to transmit as maximum power. Typical maximum transmit power is no more than a few dB higher | N/A |
| 17. | Transmitting user terminal antenna gain (dBi) | 0 dBi (omnidirectional) | 0 dBi (omnidirectional) | 0 dBi (omnidirectional) |
| 18. | Body loss | 4 dB | 4 dB | 4 dB |

|  |
| --- |
| *Notes relative to Table 9*:  (1) Note that some of the parameters in this table are typically not included in the cdma2000 specifications. These include: maximum spectral power density, transmitting antenna type, antenna gain, antenna height, antenna pattern, antenna downtilt, feeder loss, and polarization. Some information in these categories found in this table is listed in 3GPP2 Report C.R1002 (cdma2000 Evaluation Methodology) and may be considered typical in some deployments.  (2) By “active mode” it should be understood that these are terminals with an active communication session but are not necessarily transmitting. If only transmitting terminals are used in a study, the average power levels for user equipment in active mode cannot be used. In that case power levels need to be computed differently, e.g. by simulations (including power control).  (3) This is a function of frequency, coverage desired, propagation, data rates desired, etc.  (4) Assuming 43 dBm per carrier transmit power, 15 dBi antenna gain, 2 dB feeder loss, and 3 carriers within 5 MHz.  (5) Assuming 30% overhead power, fully loaded sector, and 40% voice activity factor.  (6) Time averaged e.i.r.p.  (7) Assuming the base station is fully loaded. |

TABLE 10

Maximum power for IMT-2000 CDMA MC mobile stations and HRPD access   
terminals for band classes in the 698-862 MHz range

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Band class | Mobile station class/  access terminal class | Radiating measurement | Lower limit | Upper limit |
| 0 and 3 | Class I | e.r.p. | 1 dBW (1.25 W) | 8 dBW (6.3 W) |
| Class II | e.r.p. | −3 dBW (0.5 W) | 4 dBW (2.5 W) |
| Class III | e.r.p. | −7 dBW (0.2 W) | 0 dBW (1.0 W) |
| 7 and 10 | Class I | e.r.p. | −3 dBW (0.5 W) | 4 dBW (2.5 W) |
| Class II | e.r.p. | −7 dBW (0.2 W) | 0 dBW (1.0 W) |

Table 11 maps the band classes defined in Table 10 to the actual frequencies.

TABLE 11

Band class designations in the 698-862 MHz range

|  |  |  |
| --- | --- | --- |
| Band  class | Transmit frequency band  (MHz) | |
| Mobile station | Base station |
| 0 | 815-849 | 860-894 |
| 3 | 887-889 893-901 915-925 | 832-834 838-846 860-870 |
| 7 | 776-788 | 746-758 |
| 10 | 806-824 896-901 | 851-869 935-940 |
| 18 | 787-799 | 757-769 |
| 19 | 698-716 | 728-746 |

With regard to the band class 5 (450-470 MHz band), the following parameters have to be adjusted:

– BS antenna gain, which would be 14 dBi.

– The MS power levels are given below (Table 12). A typical MS uses class III.

TABLE 12

Maximum power for IMT-2000 CDMA MC terminals for band classes   
in the 450-470 MHz range

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Band class | Mobile station class/ access terminal class | Radiating measurement | Lower limit | Upper limit |
| 5 | Class I | e.r.p. | 3 dBW (2 W) | 10 dBW (10 W) |
| Class II | e.r.p. | −2 dBW (0.63 W) | 5 dBW (3.2 W) |
| Class III | e.r.p. | −7 dBW (0.2 W) | 0 dBW (1.0 W) |
| Class IV | e.r.p. | –12 dBW (0.063 W) | –5 dBW (0.32 W) |

## 5.3 Deployment-related parameters for IMT-2000 CDMA TDD (interface No. 3)

TABLE 13

Deployment-related parameters for IMT-2000 CDMA TDD (interface No. 3) below 1 GHz

|  | IMT-2000 RADIO INTERFACES | IMT‑2000 CDMA  TDD |
| --- | --- | --- |
| No. | Parameter | E-UTRA |
|  | Base station parameters |  |
| 1. | Coverage radius | > 5 km (typical 8 km) for macro rural scenario  0.5-5 km (typical 2 km) for macro urban/suburban scenario |
| 2. | Typical height of the transmitting BS antenna (m) | 30 |
| 3. | Antenna type (sectorized/omnidirectional) | 3 sectors |
| 4. | Antenna downtilt for macro base stations | 3° |
| 5. | Frequency reuse factor | 1 |
| 6. | Antenna pattern | Sector Antenna: Rec. ITU-R F.1336 (*recommends* 3.1)  • ka = 0.7  • kp = 0.7  • kh = 0.7  • kv = 0.3  Horizontal 3 dB beamwidth: 65 degrees  Vertical 3 dB beamwidth: determined from the horizontal beamwidth by equations in Recommendation ITU-R F.1336 (*recommends* 3.3). Vertical beamwidths of actual antennas may also be used when available. |
| 7. | Polarization | linear / ± 45 degrees |
| 8. | Feeder loss (dB) | 3 |
| 9. | Maxim BS transmitter power per sector (dBm) | 43 for BW ≤ 5 MHz  46 for BW ≥ 10 MHz |

TABLE 13 (*end*)

|  |  |  |
| --- | --- | --- |
|  | IMT-2000 RADIO INTERFACES | IMT‑2000 CDMA  TDD |
| No. | Parameter | E-UTRA |
|  | Base station parameters |  |
| 10. | Maximum BS transmitter e.i.r.p. per sector (dBm/channel bandwidth) | 55 for BW ≤ 5 MHz  58 for BW ≥ 10 MHz |
| 11. | Transmitting BS antenna gain (dBi) | 15 |
| 12. | Average base station activity factor (%) | 50 |
| 13. | Average base station e.i.r.p. per sector taking into account the base station activity factor (dBm/channel bandwidth) | 52 for BW ≤ 5 MHz  55 for BW ≥ 10 MHz |
| 14. | TDD activity factor (%)(1) | subject to specific DL/UL ratio |
|  | **User terminal parameters** |  |
| 15. | Indoor usage | 50% for macro rural scenario  70% for macro urban/suburban scenario |
| 16. | Average indoor user terminal penetration loss | 15 dB for macro rural scenario  20 dB for macro urban/suburban scenario |
| 17. | Density of the user equipment in active mode(2) (number/km2) | 0.17 / 5 MHz/km2 for macro rural scenario 2.16 / 5 MHz/km2 for urban/suburban scenario |
| 18. | User terminal transmitter output power (dBm) |  |
| 18.1 | Maximum user terminal transmitter output power (dBm/5 MHz) | 23 |
| 18.2 | Average user terminal transmitter output power in active mode(2)(dBm/5 MHz) | 2 dBm for macro rural scenario –9 dBm for macro urban/suburban scenario |
| 19. | Transmitting user terminal antenna gain (dBi) | –3 dBi (omnidirectional) |
| 20. | Body loss | 4 dB |
| *Notes relative to Table 13:*  (1) In case TDD is used, base station downlink transmission occurs only part of the time, which will further reduce average base station power.  (2) By “active mode” it should be understood that these are terminals with an active communication session but which are not necessarily transmitting. If only transmitting terminals are used in a study, the average power levels for user equipment in active mode cannot be used. In that case power levels need to be computed differently, e.g. by simulations (including power control). | | |

## 5.4 Deployment-related parameters for IMT-2000 OFDMA TDD WMAN (interface No. 6)

TABLE 14

Deployment-related parameters for IMT-2000 OFDMA TDD WMAN   
(interface No. 6) below 1 GHz

|  | IMT-2000 RADIO INTERFACES | IMT 2000 OFDMA TDD WMAN |
| --- | --- | --- |
| No. | Parameter |  |
|  | **Base station parameters** |  |
| 1. | Coverage radius | Rural: 3.46 km  Urban: 2.698 km |
| 2. | Typical height of the transmitting BS antenna (m) | 25 (Urban macro)  35 (Suburban/Rural Macro)  Per ITU-R M.2135-1 |
| 3. | Antenna type (sectorized/omnidirectional) | 3 sectors |
| 4. | Antenna downtilt for macro base stations | 3° |
| 5. | Frequency reuse factor | 1 |
| 6. | Antenna pattern | Sector Antenna: Rec. ITU-R F.1336 (*recommends* 3.1)  • ka = 0.7  • kp = 0.7  • kh = 0.7  • kv = 0.3  Horizontal 3 dB beamwidth: 65 degrees  Vertical 3 dB beamwidth: determined from the horizontal beamwidth by equations in Recommendation ITU-R F.1336 (*recommends* 3.3). Vertical beamwidths of actual antennas may also be used when available. |
| 7. | Feeder loss (dB) | 3 |
| 8. | Maximum BS transmitter e.i.r.p.  (dBm/5 MHz) per sector | 55(1) |
| 9. | Transmitting BS antenna gain (dBi) | 15 |
|  | **User terminal parameters** |  |
| 10. | Density of the user equipment in active mode(2) (number/km2) | Deployment dependent |
| 11. | Maximum user terminal transmitter e.i.r.p. (dBm/5 MHz) | 23(3) |
| 12. | Average user terminal transmitter e.i.r.p. in active mode(2) (dBm/5 MHz) | 3 (rural)  −8 (urban) |

|  |
| --- |
| *Notes relative to Table 14*:  (1) This value does not take account of the effect of multiple transmit antennas.  (2) By “active mode” it should be understood that these are terminals with an active communication session but are not necessarily transmitting. If only transmitting terminals are used in a study, the average power levels for user equipment in active mode cannot be used. In that case power levels need to be computed differently, e.g. by simulations (including power control).  (3) WiMAX numbers for MS related to Item 4 are preliminary numbers. WiMAX Forum profiles 7.A and 7.E of Table 15, in general, cover a range of power classes. |

TABLE 15

Complementary information about IMT-2000 OFDMA TDD WMAN (Mobile WiMAX)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Band Class Group (BCG) | Frequency range UL (MHz) | Frequency range DL (MHz) | Channel bandwidth (MHz) | Duplex mode | Comments |
| 7.A | 698-862 | 698-862 | 5, 7 and 10 | TDD | The bandwidths are applicable to both the MS and BS |
| 7.B | 776-787 | 746-757 | 2 × 5 and 2 × 10 | FDD |
| 7.C | 788-793, 793‑798 | 758-763, 763‑768 | 2 × 5 | FDD |
| 7.D | 788-798 | 758-768 | 2 × 10 | FDD |
| 7.E | 698-862 | 698-862 | 5, 7 and 10 (TDD)  2 × 5, 2 × 7 and 2 × 10 (FDD) | TDD/FDD |
| 7.G | 880-915 | 925-960 | 2 × 5 and 2 × 10 | FDD |

## 5.5 Spectrum emission mask for terminal/mobile station equipment operating in the band 3 400-3 600 MHz

Emission mask for 5 MHz channel bandwidth

The spectrum emission mask of the MS applies to frequency offsets between 2.5 MHz and 12.5 MHz on both sides of the MS centre carrier frequency. The out-of-channel emission is specified as power level measured over the specified measurement bandwidth relative to the total mean power of the MS carrier measured in the 5 MHz channel.

The MS emission shall not exceed the levels specified in Table 16. Assuming specific power classes, the relative requirements of Table 16 can be converted to absolute values for testing purposes.

TABLE 16

Spectrum emission mask requirement for 5 MHz channel bandwidth

|  |  |  |
| --- | --- | --- |
| Frequency offset Δ*f* | Minimum requirement | Measurement bandwidth |
| 2.5 MHz to 3.5 MHz |  | 30 kHz |
| 3.5 to 7.5 MHz |  | 1 MHz |
| 7.5 to 8.5 MHz |  | 1 MHz |
| 8.5 to 12.5 MHz | −47.5 dBc | 1 MHz |
| NOTE 1 − Δ*f* is the separation between the carrier frequency and the centre of the measuring filter.  NOTE 2 − The first measurement position with a 30 kHz filter is at Δ*f* equals 2.515 MHz; the last is at Δ*f* equals 3.485 MHz.  NOTE 3 − The first measurement position with a 1 MHz filter is at Δf equals 4 MHz; the last is at Δ*f* equals 12 MHz. As a general rule, the resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. To improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth can be different from the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.  NOTE 4 − Note that equivalent PSD type mask can be derived by applying 10\*log ((5 MHz)/(30 kHz)) = 22.2 dB and 10\*log((5 MHz)/(1 MHz)) = 7 dB scaling factor for 30 kHz and 1 MHz measurement bandwidth respectively. | | |

Emission mask for 7 MHz channel bandwidth

The spectrum emission mask of the MS applies to frequency offsets between 3.5 MHz and 17.5 MHz on both sides of the MS centre carrier frequency. The out-of-channel emission is specified as power level measured over the specified measurement bandwidth relative to the total mean power of the MS carrier measured in the 7 MHz channel.

The MS emission shall not exceed the levels specified in Table 17. Assuming specific power classes, the relative requirements of Table 17 can be converted to absolute values for testing purposes.

TABLE 17

Spectrum emission mask requirement for 7 MHz channel bandwidth

|  |  |  |
| --- | --- | --- |
| Frequency offset Δ*f* | Minimum requirement | Measurement bandwidth |
| 3.5 MHz to 4.75 MHz |  | 30 kHz |
| 4.75 to 10.5 MHz |  | 1 MHz |
| 10.5 to 11.9 MHz |  | 1 MHz |
| 11.9 to 17.5 MHz | −49.0 dBc | 1 MHz |
| NOTE 1 − Δ*f* is the separation between the carrier frequency and the centre of the measuring filter.  NOTE 2 −The first measurement position with a 30 kHz filter is at Δ*f* equals 3.515 MHz; the last is at Δ*f* equals 4.735 MHz.  NOTE 3 − The first measurement position with a 1 MHz filter is at Δ*f* equals 5.25 MHz; the last is at Δ*f*equals 17 MHz. As a general rule, the resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. To improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth can be different from the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.  NOTE 4 − Note that equivalent PSD type mask can be derived by applying 10\*log ((7 MHz)/(30 kHz)) = 23.7 dB and 10\*log((7 MHz)/(1 MHz)) = 8.5 dB scaling factor for 30 kHz and 1 MHz measurement bandwidth respectively. | | |

Emission mask for 10 MHz channel bandwidth

The spectrum emission mask of the MS applies to frequency offsets between 5.0 MHz and 25.0 MHz on both sides of the MS centre carrier frequency.

The out-of-channel emission is specified as power level measured over the specified measurement bandwidth relative to the total mean power of the MS carrier measured in the 10 MHz channel.

The MS emission shall not exceed the levels specified in Table 18. Assuming specific power classes, the relative requirements of Table 18 can be converted to absolute values for testing purposes.

TABLE 18

Spectrum emission mask requirement for 10 MHz channel bandwidth

|  |  |  |
| --- | --- | --- |
| Frequency offset Δ*f* | Minimum requirement | Measurement bandwidth |
| 5.0 MHz to 7.0 MHz |  | 30 kHz |
| 7.0 to 15.0 MHz |  | 1 MHz |
| 15.0 to 17.0 MHz |  | 1 MHz |
| 17.0 to 25.0 MHz | −50.5 dBc | 1 MHz |

|  |
| --- |
| *Notes relative to Table 18*:  NOTE 1 − Δ*f* is the separation between the carrier frequency and the centre of the measuring filter.  NOTE 2 − The first measurement position with a 30 kHz filter is at Δ*f* equals 510.015 MHz; the last is at Δ*f* equals 6.985 MHz.  NOTE 3 − The first measurement position with a 1 MHz filter is at Δ*f* equals 7.5 MHz; the last is at Δ*f* equals 24.5 MHz. As a general rule, the resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. To improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth can be different from the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.  NOTE 4 − Equivalent PSD type mask can be derived by applying 10\*log ((10 MHz)/(30 kHz)) = 25.2 dB and 10\*log((10 MHz)/(1 MHz)) = 10 dB scaling factor for 30 kHz and 1 MHz measurement bandwidth respectively. |

References

[1] 3GPP TS 25.101: 3rd Generation Partnership Project; Technical Specification Group Radio Access Networks; UE Radio Transmission and Reception (FDD) (Release 9).

[2] 3GPP TS 36.101: 3rd Generation Partnership Project; Technical Specification Group Radio Access Networks; Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio transmission and reception (Release 9).

[3] 3GPP TS 25.104 v9.3.0 (2010-03): 3rd Generation Partnership Project; Technical Specification Group Radio Access Networks; BS Radio Transmission and Reception (FDD) (Release 9).

[4] 3GPP TR 25.951: 3rd Generation Partnership Project; Technical Specification Group Radio Access Networks, FDD Base Station Classification (Release 9).

[5] 3GPP TS 36.104: 3rd Generation Partnership Project; Technical Specification Group Radio Access Networks; Evolved Universal Terrestrial Radio Access (E-UTRA); Base Station (BS) radio transmission and reception (Release 9).

[6] TIA-97-H; Recommended minimum performance Standards for cdma2000® spread spectrum base stations, Feb 2012.

[7] TIA-98-H; Recommended minimum performance Standards for cdma2000® spread spectrum mobile stations, April 2012.

[8] TIA-864-D; Recommended minimum performance Standards for cdma2000® High Rate Packet Data Access Network, May 2012.

[9] TIA-866-D; Recommended minimum performance Standards for cdma2000® High Rate Packet Data Access Terminal, May 2012.

[10] TIA-1170: Recommended Minimum Performance Standards for cdma2000 Ultra Mobile Broadband (UMB) Access Network, February 2010.

[11] TIA-1171: Recommended Minimum Performance Standards for cdma2000 Ultra Mobile Broadband Access Terminal, February 2010.

[12] 3GPP TS 25.102: 3rd Generation Partnership Project; Technical Specification Group Radio Access Networks; UE Radio Transmission and Reception (TDD) (Release 9).

[13] 3GPP TS 25.105: 3rd Generation Partnership Project; Technical Specification Group Radio Access Networks; BS Radio Transmission and Reception (TDD) (Release 9).

[14] TR45 technical specification, SP-4027-270b); Mobile Station Minimum Performance, clause 1.4 and clause 3.2.2. Refers To Power Class Ii Mobile Station.

[15] TR45 technical specification, SP-4027-270b); Mobile Station Minimum Performance, clause 2.3.1.3.1.

[16] TR45 technical specification, TIA/EIA-136-290); RF Minimum performance requirements 136HS Outdoor and 136HS Indoor Bearers, clause 2.

[17] TR45 technical specification, SP-4027-270b); Mobile Station Minimum Performance, clause 3.4.1.1.3.

[18] TR45 technical specification, SP-4027-270b); Mobile Station Minimum Performance, clause 2.3.2.4.3:

TABLE 19

Blocking and spurious response rejection

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency band | Desired signal (frequency, *Fc*) | Blocking signal (frequency, *F*0) | Spurious  response limit  (frequency, *F*0) | Error rate (%) |
| | *fc* – f0 | > 3 MHz (π/4 DQPSK) | −102 | −30 | −45 | 3 |
| 3 MHz > | *fc* – *f*0 | > 90 kHz (π/4 DQPSK) | −102 | −45 | −45 | 3 |
| | *fc* – *f*0 | > 3 MHz (8-PSK) | −99 | −30 | −45 | 3 |
| 3 MHz > | *fc*– *f*0 | > 90 kHz (8-PSK) | −99 | −45 | −45 | 3 |

[19] TR45 technical specification, TIA/EIA-136-290; RF Minimum performance requirements 136HS Outdoor and 136HS Indoor Bearers, clause 5.1:

The mobile station shall meet the requirements set forth in clause 6.2 in the presence of an unmodulated carrier at the following frequencies and amplitudes:

TABLE 20

Requirements of clause 6.2

|  |  |
| --- | --- |
| Frequency of blocking signal | Amplitude of blocking signal (dBm) |
| 600 kHz < ⎜*f* – *f*0| < 800 kHz | −43 |
| 800 kHz < ⎜*f* – *f*0| < 1.6 MHz | −43 |
| 1.6 MHz < = < ⎜*f* – *f*0| < 3 MHz | −33 |
| 3 MHz = ⎜*f* – *f*0| | −26 |

[20] TR45 technical specification, TIA/EIA-136-290; RF Minimum performance requirements 136HS Outdoor and 136HS Indoor Bearers, clause 4.1.1.2 refers to Power Class II mobile station.

[21] Final Draft ETSI EN 300 175-2: Digital Enhanced Telecommunications (DECT) Common Interface (CI) part 2: Physical Layer.