Table IV-14:  Statistics of duration of intervals between precipitations (7)



	Station number	_ _ _ _ _ _
RG site name	_ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _ _
RG country(1)	_ _
RG latitude (–90..+90) (degrees)	_ _ _  _ _ _ _
RG longitude (0..360) (degrees) E 	_ _ _  _ _ _ _
RG altitude amsl hg (m)	_ _ _ _

Measurement: Experiment No.	_ _ _
	Rain gauge type	_ _ _ _ _ _ _ _ _ _
RG resolution (mm/h)	_ _ _ _  _ _ _
RG integration time (s)	_ _ _ _
RG accumulation per tip (mm/tip)	_  _ _ _ _
RG aperture (cm2)	_ _ _ _  _
Start date (yyyy.mm.dd)	_ _ _ _  _ _  _ _
End date (yyyy.mm.dd)	_ _ _ _  _ _  _ _
Duration of measurements d (days) (2,3,6)	_ _ _ _ _  _ _ 






Table a: Parameters of rain inter-events

Total number of rain inter-events, total rain inter-event time accumulated and average duration of inter-events, given that the rain rate is greater than R (mm/h). 

	Duration of rain inter-events

	Rain rate 
	Total number of rain inter-events
	Total rain inter-event time (4) (min)
	Average duration of inter-events (min)

		0.25 mm/h 
   	5 mm/h
	10 mm/h
	20 mm/h
	30 mm/h
	40 mm/h
	50 mm/h
	60 mm/h
	70 mm/h
	80 mm/h
	90 mm/h
	100 mm/h
	110 mm/h
	120 mm/h
	130 mm/h
	140 mm/h
	150 mm/h
	-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
	-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
	-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
-
-





































Table b: Cumulative probability of occurrence of rain inter-events (5)

Probability of occurrence (from 0 to 1) of rain inter-events of duration equal or shorter than D (min), given that the rain rate is greater than R (mm/h). 

	Probability for rainfall rate threshold exceeded in the first row (mm/h)

	Duration (min)
	0.25
	5
	10
	20
	30
	40
	50
	60
	70
	80
	90
	100
	110
	120
	130
	140
	150

	30
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	40
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	60
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	90
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	120
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	240
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	300
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	360
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	720
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	1 080
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	1 440
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	2 160
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	2 880
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	4 320
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	7 200
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	11 520
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	14 400
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	21 600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	28 800
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	43 200
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	86 400
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	129 600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	262 800
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	525 600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	788 400
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	1 051 200
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	



Table c: Cumulative distribution of inter-event time (5)

Total percentage of time (%) due to rain inter-events of duration equal or shorter than D (min), given that the rain rate is greater than R (mm/h)

	Percentage of time (%) for rainfall rate threshold exceeded in the first row (mm/h)

	Duration (min)
	0.25
	5
	10
	20
	30
	40
	50
	60
	70
	80
	90
	100
	110
	120
	130
	140
	150

	30
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	40
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	60
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	90
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	120
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	240
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	300
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	360
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	720
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	1 080
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	1 440
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	2 160
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	2 880
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	4 320
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	7 200
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	11 520
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	14 400
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	21 600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	28 800
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	43 200
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	86 400
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	129 600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	262 800
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	525 600
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	788 400
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	1 051 200
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	











References:

Comments:


(1)	Use ISO 3166-1 alpha-2 country codes..
(2)	In geographic locations where precipitation in the form of ice or snow may occur, an explanation should be given as to when and how long these conditions prevail and how the rain gauge data is treated during these intervals.
(3)	If outages occurred in the measurement of rain, explain under Comments whether rainfall occurred during the outage or not.
(4)	The duration of inter-events is calculated for the whole period of rain rate data, which can be several years. The whole duration for each threshold is limited by the time the first event ends and the last event starts. 
(5)	Both Tables b and c have to be filled in. Distributions are calculated for the whole period of rain rate data, which can be several years.
(6)	Duration is the total time of valid measurements for this dataset, expressed as a real number (e.g. 339.888 days). The ratio of duration to the period identified by the start and the end dates of this dataset is the availability (e.g. start=2001/1/1, end=2001/12/31, duration= 339.888 days corresponds to 93.12 % availability). 
(7)	Submissions should comply with the acceptance criteria specified in Rec. ITU-R P.311.


