|  |
| --- |
| **Recommendation ITU-R M.2122-0**  **(01/2019)** |
| **Technical and operational characteristics for aeronautical mobile service systems limited to aircraft transmissions of aeronautical mobile telemetry for flight testing in the band 5 150-5 250 MHz in Region 1 and in Brazil in accordance  with RR No. 5.446C** |
| **M Series**  **Mobile, radiodetermination, amateur**  **and related satellite services** |

**Foreword**

The role of the Radiocommunication Sector is to ensure the rational, equitable, efficient and economical use of the radio-frequency spectrum by all radiocommunication services, including satellite services, and carry out studies without limit of frequency range on the basis of which Recommendations are adopted.

The regulatory and policy functions of the Radiocommunication Sector are performed by World and Regional Radiocommunication Conferences and Radiocommunication Assemblies supported by Study Groups.

**Policy on Intellectual Property Right (IPR)**

ITU-R policy on IPR is described in the Common Patent Policy for ITU-T/ITU-R/ISO/IEC referenced in Resolution ITU‑R 1. Forms to be used for the submission of patent statements and licensing declarations by patent holders are available from <http://www.itu.int/ITU-R/go/patents/en> where the Guidelines for Implementation of the Common Patent Policy for ITU‑T/ITU‑R/ISO/IEC and the ITU-R patent information database can also be found.

|  |  |
| --- | --- |
| **Series of ITU-R Recommendations**  (Also available online at <http://www.itu.int/publ/R-REC/en>) | |
| **Series** | **Title** |
| **BO** | Satellite delivery |
| **BR** | Recording for production, archival and play-out; film for television |
| **BS** | Broadcasting service (sound) |
| **BT** | Broadcasting service (television) |
| **F** | Fixed service |
| M | Mobile, radiodetermination, amateur and related satellite services |
| **P** | Radiowave propagation |
| **RA** | Radio astronomy |
| **RS** | Remote sensing systems |
| **S** | Fixed-satellite service |
| **SA** | Space applications and meteorology |
| **SF** | Frequency sharing and coordination between fixed-satellite and fixed service systems |
| **SM** | Spectrum management |
| **SNG** | Satellite news gathering |
| **TF** | Time signals and frequency standards emissions |
| **V** | Vocabulary and related subjects |

|  |
| --- |
|  |

|  |
| --- |
| ***Note***: *This ITU-R Recommendation was approved in English under the procedure detailed in Resolution ITU-R 1.* |

*Electronic Publication*

Geneva, 2019

© ITU 2019

All rights reserved. No part of this publication may be reproduced, by any means whatsoever, without written permission of ITU.

RECOMMENDATION ITU-R M.2122-0

Technical and operational characteristics for aeronautical mobile service systems limited to aircraft transmissions of aeronautical mobile telemetry for flight testing in the band 5 150-5 250 MHz in Region 1 and in Brazil   
in accordance with RR No. 5.446C

(2019)

Scope

This Recommendation provides technical and operational characteristics for aeronautical mobile telemetry (AMT) operated in countries of Region 1 (except in Algeria, Saudi Arabia, Bahrain, Egypt, United Arab Emirates, Jordan, Kuwait, Lebanon, Morocco, Oman, Qatar, Syrian Arab Republic, Sudan, South Sudan and Tunisia) and in Brazil in the frequency range 5 150-5 250 MHz in accordance with RR No. **5.446C** which recognizes an allocation to the aeronautical mobile service on a primary basis, limited to aeronautical telemetry transmissions from aircraft stations.

Related ITU Recommendations, Reports

Recommendation ITU-R S.580 – Radiation diagrams for use as design objectives for antennas of earth stations operating with geostationary satellites

Recommendation [ITU-R M.1459](https://www.itu.int/rec/R-REC-M.1459/en) – Protection criteria for telemetry systems in the aeronautical mobile service and mitigation techniques to facilitate sharing with geostationary broadcasting-satellite and mobile-satellite services in the frequency bands 1 452-1 525 MHz and 2 310‑2 360 MHz

Recommendation [ITU-R M.1828](http://www.itu.int/rec/R-REC-M.1828/en) –Technical and operational requirements for aircraft stations of aeronautical mobile service limited to transmissions of telemetry for flight testing in the bands around 5 GHz

Report [ITU-R M.2221](http://www.itu.int/pub/R-REP-M.2221) – Feasibility of MSS operations in certain frequency bands

Report [ITU-R M.2238](http://www.itu.int/pub/R-REP-M.2238) – Compatibility study to support line of sight control and non-payload communications links for unmanned aircraft systems proposed in the frequency band 5 091‑5 150 MHz

Keywords

Telemetry, aircraft

Abbreviations/Glossary

AMS: Aeronautical mobile service

AMT: Aeronautical mobile telemetry

*I*/*N*: Interference-to-noise ratio

The ITU Radiocommunication Assembly,

considering

*a)* that various technically and operationally different aeronautical mobile service (AMS) limited to transmissions of telemetry systems for flight testing networks are already in operation in the 5 GHz frequency band subject to Resolution **418 (Rev.WRC-15)**;

*b)* that the operation of aircraft station is usually a subject of national and international rules and regulations including satisfactory conformance to a mutually agreed technical standard and operational requirements;

*c)* that there is a need for identifying the technical and operational characteristics for performing sharing analysis involving AMS limited to aircraft transmissions of telemetry systems for flight testing;

*d)* that the identification of technical and operational requirements for aircraft stations is presented in Recommendation ITU-R M.1828 and provides a common technical basis for facilitating conformance testing of aircraft station by various national and international authorities and the development of mutual recognition arrangements for conformance of aircraft stations,

recognizing

*a)* that in the frequency band 5 150‑5 250 MHz there are global allocations to aeronautical radionavigation, fixed-satellite (Earth-to-space) and mobile except aeronautical mobile services on a primary basis;

*b)* that, pursuant to RR No. **5.446C**, in Region 1 (except in Algeria, Saudi Arabia, Bahrain, Egypt, United Arab Emirates, Jordan, Kuwait, Lebanon, Morocco, Oman, Qatar, Syrian Arab Republic, Sudan, South Sudan and Tunisia) and in Brazil, the band 5 150‑5 250 MHz is also allocated to the aeronautical mobile service on a primary basis, limited to aeronautical telemetry transmissions from aircraft stations;

*c)* that under RR No. **5.446C**, aeronautical mobile telemetry (AMT) aircraft stations shall not claim protection from other stations operating in accordance with Article **5**;

*d)* that the characteristics of the telemetry equipment operated in the frequency band 5 150‑5 250 MHz may also be applicable for the frequency band 5 091-5 150 MHz if this equipment is also operated in that frequency band in the administrations referenced in *recognizing b)*,

noting

that Recommendation ITU-R M.1459, and Reports ITU-R M.2221 and ITU-R M.2238, also contain technical parameters and protection criteria for telemetry systems for flight testing,

recommends

**1** that the technical and operational characteristics for transmitting aircraft stations and receiving aeronautical stations of the aeronautical mobile service limited to transmissions of telemetry for flight testing in the frequency band 5 150-5 250 MHz given in Annex, should be used to perform sharing analysis;

**2** that the aggregate interference protection criterion for ground AMT receiving stations of *I*/*N* of −6 dB should be used.

Annex  
  
Technical and operational characteristics of aeronautical mobile stations limited to aircraft transmissions of aeronautical mobile telemetry for flight testing   
in the frequency band 5 150-5 250 MHz in Region 1 and in Brazil  
in accordance with RR No. 5.446C

# 1 Aeronautical mobile telemetry characteristics

The following Table provides the aeronautical mobile telemetry transmitting and receiving stations characteristics relevant for performing sharing analysis with other services in co-frequency.

TABLE 1

Aeronautical mobile telemetry characteristics

|  |  |
| --- | --- |
|  | Aeronautical mobile telemetry system |
| **Transmitter (onboard aircraft)** | |
| Frequency range (MHz) | 5 150-5 160 |
| Channel bandwidth (MHz) | 8 |
| Modulation | Single Carrier-SOQPSK or COFDM-QPSK |
| Maximum transmit power (dBW) (1) | 20 |
| Aircraft antennas location | One antenna on the bottom of the aircraft and another antenna on the top of the aircraft |
| Tx antenna gain (dBi) | 0 |
| Cable loss (dB) | 2 |
| Aircraft altitude (m) | 0 – 15 000 |
| Aircraft deployment | Typical: 3 Aircraft in flight at the same time but not co-frequency (each aircraft use different channels)  Maximum: 5 Aircraft in flight at the same time but not co-frequency (each aircraft use different channels) |
| **Receiver (on ground)** | |
| Antenna pattern | Steering Parabolic antenna  Recommendation ITU-R S.580 |
| Receiver antenna gain (dBi) | 40 |
| Noise figure (dB) | 9 |
| Receiver frequency range (MHz) | 5 150-5 160MHz |
| Receiver bandwidth (MHz) | 8 |
| Receiver altitude from ground level (m) | Between 6 and 40 |
| Receiver antenna elevation range (degree) | Between −5 and 90 (99% of time the elevation is between −2° and 5°) |
| (1) The effective power is adjusted to comply with the pfd limits defined in Annex 1 of Resolution **418 (Rev.WRC‑15)**. | |