Data Generated by the ITS LFMF Driver
lfmf.dll Version          v1.1
LFMFDrvr.exe Version      v1.1.0
Date Generated            Thu May  6 20:48:09 2021

Input Arguments          -i point_input.txt -o point_output.txt -mode point -method 

Inputs
h_tx__meter              5            (meters)
h_rx__meter              5            (meters)
N_s                      315.00       (N-Units)
f__mhz                   1.00         (MHz)
pol                      1            [Vertical]
epsilon                  15
sigma                    0.005        (S/m)
P_tx__watt               1000         (Watts)
d__km                    500.00       (km)
Mode                     Point

Distance:                     500.000 (km)
Basic Transmission Loss:      145.475 (dB)
Field Strength:                -3.489 (dB(uV/m))
Received Power:               -75.919 (dBm)
Solution Method:                1     [Residue Series]
