|  |  |  |  |
| --- | --- | --- | --- |
| CTI - Côte d'Ivoire | | | |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| National Spectrum Control Centre - Office of the Director Frequency Spectrum Centre National de Contrôle (CNC) Direction du Contrôle du Spectre (DCS)  Abidjan – Marcory | Agence Ivoirienne de la Gestion des Fréquences Radioélectriques de Côte d’Ivoire 17 B.P. 444 Abidjan 17 | TF : +225 20 344670 TF : +225 20 345960 TF : +225 20 345987 TF : +225 20 345958 FAX : +225 20 344965 |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |  |
| --- | --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** | |
|  |  |  |  |
| **Abidjan** | Agence Ivoirienne de Gestion des Fréquences Radioélectriques de Côte d’Ivoire 17 B.P. 444 Abidjan 17 Côte d'Ivoire | TF : +225 20 344670 TF : +225 20 345960 TF : +225 20 345987 TF : +225 20 345958 FAX : +225 20 344965 | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 05°18'00''N 003°58'00''W | Frequency measurements | 1 MHz - 30 MHz | 0800-1200 | Except Saturdays, Sundays and public holidays.  Can operate on request.  The system is portable and can be used at any site.  Dipole. |
| 05°18'00''N 003°58'00''W | Frequency measurements | 1 MHz - 30 MHz | 1300-1700 | Except Saturdays, Sundays and public holidays.  Can operate on request.  The system is portable and can be used at any site.  Dipole. |
| 05°18'00''N 003°58'00''W | Frequency measurements | 1 MHz - 500 MHz | 0800-1200 | Except Saturdays, Sundays and public holidays.  Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.  Dipole.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Frequency measurements | 1 MHz - 500 MHz | 1300-1700 | Except Saturdays, Sundays and public holidays.  Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.  Dipole.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Field strength or power flux-density measurements | 10 kHz - 30 MHz |  | The system is portable and can be used at any site.  Can operate on request. |
| 05°18'00''N 003°58'00''W | Field strength or power flux-density measurements | 25 MHz - 1000 MHz | 0800-1200 | Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.  Except Saturdays, Sundays and public holidays.  Dipole.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Direction-finding measurements | 25 MHz - 1000 MHz | 1300-1700 | Except Saturdays, Sundays and public holidays.  Dipole.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Direction-finding measurements | 25 MHz - 3000 MHz | 0800-1200 | Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.  Except Saturdays, Sundays and public holidays.  Dipole.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Direction-finding measurements | 25 MHz - 3000 MHz | 1300-1700 | Except Saturdays, Sundays and public holidays.  Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.  Dipole.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Bandwidth measurements | 10 kHz - 30 MHz | 0800-1200 |  |
| 05°18'00''N 003°58'00''W | Bandwidth measurements | 10 kHz - 30 MHz | 1300-1700 |  |
| 05°18'00''N 003°58'00''W | Bandwidth measurements | 20 MHz - 1000 MHz | 0800-1200 | Except Saturdays, Sundays and public holidays.  Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Bandwidth measurements | 20 MHz - 1000 MHz | 1300-1700 | Except Saturdays, Sundays and public holidays.  Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Automatic spectrum occupancy surveys | 10 kHz - 30 MHz | 0800-1200 | The system is portable and can be used at any site.  Can operate on request. |
| 05°18'00''N 003°58'00''W | Automatic spectrum occupancy surveys | 10 kHz - 30 MHz | 1300-1700 | Can operate on request.  The system is portable and can be used at any site. |
| 05°18'00''N 003°58'00''W | Automatic spectrum occupancy surveys | 20 MHz - 3000 MHz | 0800-1200 | Except Saturdays, Sundays and public holidays.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Automatic spectrum occupancy surveys | 20 MHz - 3000 MHz | 1300-1700 | Except Saturdays, Sundays and public holidays.  Log-periodic antenna. |
| 05°18'00''N 003°58'00''W | Automatic spectrum occupancy surveys | 3 GHz - 26.5 GHz | 0800-1200 | Can operate on request.  The system is portable and can be used at any site.  Mobile monitoring stations. |
|  | Automatic spectrum occupancy surveys | 3 GHz - 26.5 GHz | 1300-1700 | Mobile monitoring stations.  The system is portable and can be used at any site.  Can operate on request. |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_