|  |
| --- |
| CTI - Côte d'Ivoire |
| **Centralizing office** | **Postal address** | **Telephone, Telefax, Electronic-mail** | **Remarks** |
|  |  |  |  |
| National Spectrum Control Centre - Office of the DirectorFrequency SpectrumCentre National de Contrôle (CNC)Direction du Contrôle du Spectre (DCS) Abidjan – Marcory | Agence Ivoirienne de la Gestiondes Fréquences Radioélectriquesde Côte d’Ivoire17 B.P. 444Abidjan 17 | TF : +225 20 344670TF : +225 20 345960TF : +225 20 345987TF : +225 20 345958FAX : +225 20 344965 |  |
|  |  |  |  |

Stations in the Terrestrial radiocommunication services

|  |  |  |
| --- | --- | --- |
| **Name of the station** | **Postal address** | **Telephone, Telefax, Electronic-mail** |
|  |  |  |  |
| **Abidjan**  | Agence Ivoirienne de Gestion des FréquencesRadioélectriques de Côte d’Ivoire17 B.P. 444Abidjan 17Côte d'Ivoire   | TF : +225 20 344670TF : +225 20 345960TF : +225 20 345987TF : +225 20 345958FAX : +225 20 344965   |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Geographical coordinates** | **Types of measurements** | **Ranges of frequencies for each measurement** | **Hours of service (UTC)** | **Remarks** |
| 05°18'00''N003°58'00''W | Frequency measurements   | 1 MHz - 30 MHz   | 0800-1200   | Except Saturdays, Sundays and public holidays.Can operate on request.The system is portable and can be used at any site.Dipole.   |
| 05°18'00''N003°58'00''W | Frequency measurements   | 1 MHz - 30 MHz   | 1300-1700   | Except Saturdays, Sundays and public holidays.Can operate on request.The system is portable and can be used at any site.Dipole.   |
| 05°18'00''N003°58'00''W | Frequency measurements   | 1 MHz - 500 MHz   | 0800-1200   | Except Saturdays, Sundays and public holidays.Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.Dipole.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Frequency measurements   | 1 MHz - 500 MHz   | 1300-1700   | Except Saturdays, Sundays and public holidays.Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.Dipole.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Field strength or power flux-density measurements   | 10 kHz - 30 MHz   |   | The system is portable and can be used at any site.Can operate on request.   |
| 05°18'00''N003°58'00''W | Field strength or power flux-density measurements   | 25 MHz - 1000 MHz   | 0800-1200   | Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.Except Saturdays, Sundays and public holidays.Dipole.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Direction-finding measurements   | 25 MHz - 1000 MHz   | 1300-1700   | Except Saturdays, Sundays and public holidays.Dipole.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Direction-finding measurements   | 25 MHz - 3000 MHz   | 0800-1200   | Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.Except Saturdays, Sundays and public holidays.Dipole.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Direction-finding measurements   | 25 MHz - 3000 MHz   | 1300-1700   | Except Saturdays, Sundays and public holidays.Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.Dipole.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Bandwidth measurements   | 10 kHz - 30 MHz   | 0800-1200   |   |
| 05°18'00''N003°58'00''W | Bandwidth measurements   | 10 kHz - 30 MHz   | 1300-1700   |   |
| 05°18'00''N003°58'00''W | Bandwidth measurements   | 20 MHz - 1000 MHz   | 0800-1200   | Except Saturdays, Sundays and public holidays.Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Bandwidth measurements   | 20 MHz - 1000 MHz   | 1300-1700   | Except Saturdays, Sundays and public holidays.Monitoring station devoted to the Aeronautical, Maritime and Land Mobile Services.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Automatic spectrum occupancy surveys   | 10 kHz - 30 MHz   | 0800-1200   | The system is portable and can be used at any site.Can operate on request.   |
| 05°18'00''N003°58'00''W | Automatic spectrum occupancy surveys   | 10 kHz - 30 MHz   | 1300-1700   | Can operate on request.The system is portable and can be used at any site.   |
| 05°18'00''N003°58'00''W | Automatic spectrum occupancy surveys   | 20 MHz - 3000 MHz   | 0800-1200   | Except Saturdays, Sundays and public holidays.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Automatic spectrum occupancy surveys   | 20 MHz - 3000 MHz   | 1300-1700   | Except Saturdays, Sundays and public holidays.Log-periodic antenna.   |
| 05°18'00''N003°58'00''W | Automatic spectrum occupancy surveys   | 3 GHz - 26.5 GHz   | 0800-1200   | Can operate on request.The system is portable and can be used at any site.Mobile monitoring stations.   |
|   | Automatic spectrum occupancy surveys   | 3 GHz - 26.5 GHz   | 1300-1700   | Mobile monitoring stations.The system is portable and can be used at any site.Can operate on request.   |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_