|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Source: Document 5A/TEMP/282 | **Annex 7 toDocument 5A/636-E** |
| **10 November 2014** |
| **English only** |
| Annex 7 to Working Party 5A Chairman’s Report |
| Elements for consideration in future discussions on Recommendation ITU-R M.2015 |
|  |

**Proposed PPDR within 700 MHz**

Figure 4

Scenario based on 2 x 10 MHz for harmonized PPDR IMT starting at 698 MHz + 2 x 3 MHz for expansion or special PPDR applications



**Figure 1. Scenario for PPDR in 700MHz based on UAE proposed arrangement for the 700 MHz band of 2x40MHz**



**Figure 2. Scenario for PPDR in 700MHz if the Frequency arrangement adopted starts at 703 MHz harmonized with APT lower Duplexer**



**Figure 3. Scenario for PPDR in 700 MHz based on arrangements that are partially harmonized with APT arrangement with additional 2x5 MHz for PPDR expansion during disasters or for other government users like Military using LTE**

