ADD CHN/28A8/6#50275

5.GMDSS-B4-2 The use of the band 1 621.35-1 626.5 MHz by the maritime mobile-satellite to support GMDSS is subject to the application of RR No. **9.11A** and its associated Rules of Procedure.     (WRC‑19)