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Abstract:	

The H.310 Draft Recommendation currently identifies the use of the OSI Transport stack to carry the H.245 and T.120 control protocols. 

The T.120 Conference Control Standard supports a variety of different transport profiles for carrying the T.120 protocols.  These are specified in the T.123 Recommendation.  T.123 allows the use of TCP/IP to carry T.120.   The LAN Conferencing Standard, H.323 allows the use of TCP/IP to carry both H.245 and T.120. 

This contribution 
suggests
 the TCP/IP protocol stack
 
be 
considered 
for transporting H.245 and T.120 in 
H.310
.
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Using H.245 in H.310         

The H.310 Draft Recommendation currently identifies the use of the OSI Transport stack to carry the H.245 control protocol.   The following picture shows H.245’s use of the OSI X.224 (Class 0) sitting on LAPF (Q.922) and using AAL5.
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H.310 also recommends that the same protocol stack be used to transport the ITU T.120 Conference Control Protocol.



T.120 Recommendation

The T.120 Recommendation is depicted in the following figure.  
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Applications use the services of the Generic Application Template (T.121),  Generic Conference Control (T.124), and the Multi-point Communication Services (T.122/T.125) to perform conference related functions such as sharing data, conference admission (join/leave), multi-point data distribution, as well as controlling who speaks.            



These functions sit on top of different transport protocols defined by the T.123 Recommendation.   As depicted in the following figure, T.123 specifies transport profiles for a variety of different kinds of networks.
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T.123 defines transport stacks for each of the following:

Public Switched Telephone Networks

Integrated Services Digital Networks (ISDN)

Circuit Switched Digital Networks 

Packet Switched Digital Networks

TCP/IP (via reference profile)



The TCP/IP profile uses the IETF RFC 1006 to provide the X.224\0 level of support to T.120.  



In addition to T.120,  the H.323 Conferencing Standard also supports the TCP/IP stack for carrying the H.245 protocol.



Proposal


H.310 should consider
 the TCP/IP protocol stack for transporting H.245 and T.120
.
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