* Bitstream file name
  - TRANS_D_Chipsnmedia_4.bit

* Explanation of bitstream features
  - 64 transform on
  - LFNST off
  - DepQuant off
  - Bitstream for 'ParkRunning3' scaled test sequence with QP 22 and random access gop

* Profile, tier, and level for the bitstream
  - main_10 profile, main tier, level 4.0

* Max picture width and height, and any additional picture width and height values used
  - 1280x720

* Picture rate
  - 50

* VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
  - The bitstream could be decoded using VVC software, tagged VTM-12.0 in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM.

* VTM release version number used to generate the bitstream, if applicable
  - VVC software, tagged VTM-12.0 in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM.
  - The bitstream was encoded in random access configuration.

* Contact name and email
  - J.-O. Lee (gretta.lee@chipsnmedia.com)
  - D.-Y. Kim (brad.kim@chipsnmedia.com)
  - M.-W. Kim (bentley.kim@chipsnmedia.com)
