* Bitstream file name
  - 10b444_A_Kwai_1.bit
* Explanation of bitstream features
  - The bitstream is provided for the conformance test of Main 444 10 profile with no 444-specific tools enabled
  - 10-bit YUV444 sequences "VenueVu" with QP 27, all intra configuration of 19 frames
* Profile, tier, and level for the bitstream
  - Main 444 10 profile, main tier, level 6
* Max picture width and height
  - Max picture width and height are 1920 and 1080
* Picture rate 
  - Picture rate is 30
* VTM decoder release version number able to correctly decode the bitstream with identical output
  - The bitstream could be decoded using VVC software, tagged ¡§VTM-9.0¡¨ in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM
* VTM release version number used to generate the bitstream, if applicable
  - The bitstream is generated using VVC software, tagged ¡§VTM-9.0¡¨ in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM
* VTM encoder command line used to generate the bitstream
  - EncoderAppStatic -c 10b444_A_Kwai_1.cfg -b 10b444_A_Kwai_1.bit -o 10b444_A_Kwai_1.yuv --PrintHexPSNR=1 --SEIDecodedPictureHash=1 
* Contact name and email of bitstream submitter
  - Xiaoyu Xiu ( xiaoyuxiu@kwai.com )