* Bitstream file name
  - 16b444etsrc_A_3.bit
* Explanation of bitstream features
  - The bitstream is provided to verify the ETSRC tool
  - Slice level signal of the Rice parameter in TSRC
  - 16-bit RGB sequences "OldTownCross_1920x1080_50_16bit_444" with QP -33 ~ 13, low-delay configuration of 8 frames
* Profile, tier, and level for the bitstream
  - Main 16 4:4:4, high tier, level 4.1
* Max picture width and height
  - Max picture width and height are 1920 and 1080
* Picture rate 
  - Picture rate is 50
* VTM decoder release version number able to correctly decode the bitstream with identical output
  - The bitstream could be decoded using VVC software, tagged VTM-23.10 in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM
* VTM release version number used to generate the bitstream, if applicable
  - The bitstream is generated using VVC software, tagged VTM-23.10 in https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM
* Contact name and email of bitstream submitter
  - Hong-Jheng Jhu ( jhuhong-jheng@kwai.com )