Bitstream  : 12b444SPerrc_A_1.bit
Resolution : 1920x1080
Format     : 4:4:4 progressive
Profile    : Main 12 444  Still Picture
Tier       : Main Tier
Frame Rate : 60 fps
Level      : 5.1
Bit Depth  : 12
Encoder    : VTM-14.0
Decoder    : VTM-14.0

Description:
12 bits video data with 4:4:4 chroma format is being coded in still image profile configuration, testing of the ERRC functionality, PRRC is enabled.

Contact Info:
Dmytro Rusanovskyy

