Bitstream  : 16b444prrc_A_1.bit
Resolution : 1920x1080
Format     : 4:4:4 progressive
Profile    : Main 16 444
Tier       : Main Tier
Level      : 6.2
Frame Rate : 50 fps
Bit Depth  : 16
Encoder    : Modified VTM-14.0 (range of QPs)
Decoder    : VTM-14.0

Description:
16 bits RGB video data with is being coded with random access picture types, testing of the PRRC functionality, ERRC is enabled.

Contact Info:
Dmytro Rusanovskyy

