BMS1.0_BCBR1_bms.xlsm and  BMS1.0_BCBR1_vtm.xlsm corresponds to CE11.1 "No limitation on block update refresh rate".
BMS1.0_BCBR2_bms.xlsm and  BMS1.0_BCBR2_vtm.xlsm corresponds to CE11.1 "1/2 block update refresh rate".
BMS1.0_BCBR8_bms.xlsm and  BMS1.0_BCBR8_vtm.xlsm corresponds to CE11.1 "1/8 block update refresh rate".
BMS1.0_BCBR10_bms.xlsm and  BMS1.0_BCBR10_vtm.xlsm corresponds to CE11.1 "1/10 block update refresh rate".
BMS1.0_BCBR10_bms_RA2IP.xlsm and BMS1.0_BCBR10_vtm_RA2IP.xlsm corresponds to CE11.2 "2 times intra period".
BMS1.0_BCBR10_bms_RA5IP.xlsm and BMS1.0_BCBR10_vtm_RA5IP.xlsm corresponds to CE11.2 "5 times intra period".