
test a1, 
use code in source_reduce_coeff.zip
use cfg file in folder cfg_without_shift
set macro CROSS_COMPONENT_LAMBDA_ADJUSTMENT 0
set macro CCALF_NUM_COEFF 6

test a2, 
use code in source_reduce_coeff.zip
use cfg file in folder cfg_without_shift
set macro CROSS_COMPONENT_LAMBDA_ADJUSTMENT 0
set macro CCALF_NUM_COEFF 7

test a3, 
use code in source_reduce_coeff.zip
use cfg file in folder cfg_without_shift
set macro CROSS_COMPONENT_LAMBDA_ADJUSTMENT 0
set macro CCALF_NUM_COEFF 8

test b, 
use code in source_clipping.zip
use cfg file in folder cfg_without_shift
set macro CROSS_COMPONENT_LAMBDA_ADJUSTMENT 0


.......................................................
additional information

test a1, 
use code in source_reduce_coeff.zip
use cfg file in folder cfg_with_shift
set macro CROSS_COMPONENT_LAMBDA_ADJUSTMENT 1
set macro CCALF_NUM_COEFF 6

test a2:
use code in source_reduce_coeff.zip
use cfg file in folder cfg_with_shift
set macro CROSS_COMPONENT_LAMBDA_ADJUSTMENT 1
set macro CCALF_NUM_COEFF 7

test a3:
use code in source_reduce_coeff.zip
use cfg file in folder cfg_with_shift
set macro CROSS_COMPONENT_LAMBDA_ADJUSTMENT 1
set macro CCALF_NUM_COEFF 8
