purpose: Check that the decoder can properly decode texture and depth view components with inter view prediction.
conformance:    3DV-ATMv11.0 and above
Level:          4.1
resolution:     1920x1088 (texture:depth=1:0.5)
# of views:     3+3
# of frames:    8
Coding Structure(time): IBP
Coding Structure(view): IBP
