purpose: Check that the decoder can properly decode texture and depth view components with inter view prediction.
conformance:    3DV-ATMv12
Level:          5.1
resolution:     1024x768 (texture:dpeth=1:1)
# of views:     3+3
# of frames:    8
Coding Structure(time): IbBbP
Coding Structure(view): IBP
