purpose: Check that the decoder can properly decode UP-MVD scheme where base view depth map is excluded from the bitstream.
conformance:    3DV-ATMv11.0 and above
resolution:     1024x768 (texture:depth=1:0.5)
# of views:     3T+2D
# of frames:    8
Coding Structure(views): PIP
HP configuration