purpose: 	Check that the decoder can properly decode various view configurations.
conformance:    3DV-ATMv11.0 and above
Level:          3.1
resolution:     1024x768 (texture:depth=1:0.5)
# of views:     3+3
# of frames:    8
Coding Structure(time): IBP
Coding Structure(view): PIP
