Name: 3DHC_D1_D
Specification: The bitstream is coded with AI configuration as well as 3-view configuration. In addition, SDC is enabled for depth coding.
Functional stage: Decoding of three views with SDC enabled for depth. 
Purpose: To conform SDC in AI configuration.

Software: HTM13.0