Purpose: To conform the single depth mode in all intra configurations. 
Specification: The bitstream is coded with AI configuration as well as 3-view configuration. In addition, single depth mode is enabled for depth coding.
Software version: HTM13.0
Sequence: Balloons ( 1024x768)
# of views:     3T+3D
# of frames:    30