purpose: Check that the decoder can properly decode various view configurations
conformance:    3DV-ATMv8.0r1
Level:          4.0
resolution:     1920x1088 (texture:dpeth=1:1)
# of views:     2+2
# of frames:    8
Coding Structure(time): IBP
Coding Structure(view): IP
