
bitstream file : DQ_B_HHI_3.bit
picture format : YUV 420
picture size   : 1920x1080 luma samples
picture rate   : 24 Hz
profile        : Main 10
tier           : Main Tier
level          : 4
decoder        : VTM-10.0
encoder        : modified VTM-10.0

description    :
This bitstream exercises dependent quantization in combination with related features.
The bitstream consists of three coded video sequences (CVSs) with the following properties:
- The first CVS uses dependent quantization for all pictures, all non-related features (inter tools, ALF, ...) are disabled, and MTS and LFNST are disabled.
- The second CVS uses dependent quantization for all pictures, all non-related features (inter tools, ALF, ...) are disabled, and MTS (for intra) and LFNST are enabled.
- The thrid CVS exercises a picture-level selection between dependent quantization, sign data hiding, and standard quantization, , all non-related features (inter tools, ALF, ...) are disabled, and MTS (for intra) and LFNST are enabled.

contact info   : Heiko Schwarz (heiko.schwarz@hhi.fraunhofer.de)
