–	Bitstream file name
ENTROPY_A_Qualcomm_2


–	Explanation of bitstream features
CABAC initialization: sweeping QP from 0 to 63


–	Profile, tier, and level for the bitstream
Main10 profile
Main tier
Level 3.1


–	Max picture width and height, and any additional picture width and height values used (i.e., for reference picture resample or scalability)  
width = 416
height = 240

–	Picture rate 
frame rate = 30


–	VTM decoder release version number able to correctly decode the bitstream with identical output, or description of VTM decoder incompatibility (preferably including a corresponding error tracking issue number.) 
VTM-10.0

–	VTM release version number used to generate the bitstream, if applicable
VTM-10.0

–	Contact name and email of bitstream submitter
Jie Dong, jiedong@qti.qualcomm.com