bitstream file : LFNST_D_HHI_3.bit
picture format : YUV 420
picture size   : 1920x1080 luma samples
picture rate   : 60 Hz
profile        : Main
tier           : Main Tier
level          : 4.1
decoder        : VTM-10.0
encoder        : modified VTM-10.0

description    :
This bitstream exercises LFNST an its signaling in different combination with other tools.
The bitstream consists of four coded video sequences with the following properties:
- The first CVS enables LFNST and explicit MTS; ISP and MIP are enabled.
- The second CVS enables LFNST and explicit MTS; ISP and MIP are disabled.
- The third CVS enables LFNST and explicit MTS; ISP is enabled and MIP is disabled.
- The fourth CVS enables LFNST and explicit MTS; ISP is disabled and MIP is enabled.

contact info   : Mischa Siekmann (mischa.siekmann@hhi.fraunhofer.de)
