
Bitstream:             APSLMCS_B_Dolby_1.bit

Resolution:            1920x1080 pixels

Format:                4:2:0 Frame Pictures

Profile:               Main 10 Profile

Tier:                  Main Tier

Frame Rate:            50 frames/sec

Level:                 4.1

Bit Depth:             10

VTM release version number used to generate the bitstream, if applicable:  VTM-8.0 (837b7dfe) with modifications at encoder side to produce a wide range of lmcsCW. 

VTM decoder release version number able to correctly decode the bitstream with identical output: VTM-8.0 (837b7dfe) 
 

Description:

The bitstream tests the use of LMCS APS with a large variation of lmcs CW values ([15 ~ 320]) in each of the 16 bins.

 

Contact Info:

Taoran Lu
tlu@dolby.com